# Fan Status

Device > Configure > Fan Status

This dialog box provides information on the fans maintained by the environmental monitor. The following data is displayed:

The following data is displayed:

- Fan Status Index (ciscoEnvMonFanStatusIndex)

- Fan Status Description (ciscoEnvMonFanStatusDescr)

- Fan State (ciscoEnvMonFanState)

Do one of the following:

- Click OK to continue.

- Click Apply to save the changes in the dialog box.

- Click Cancel to close the dialog box.

- Click Refresh to update the contents of the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

- Click Stop to stop device monitoring.

Fan Status Index (ciscoEnvMonFanStatusIndex)

Unique identifier for the fan being used. This value is used for SNMP purposes only, and has no intrinsic signficance.

Fan Status Description (ciscoEnvMonFanStatusDescr)

Textual description of the fan being used.

Fan State (ciscoEnvMonFanState)

Current state of the fan being used.