# SRP Media Dependent Statistics

Use this option to monitor media dependent statistics of an interface side with a specific interval number.

## Procedure

To access higher layer interval statistics information:

1. Right-click the port and select SRP Interface Statistics from the popup menu.

Media Dependent Statistics dialog box appears.

3. Select Media Dependent Statistics from the Category menu to display higher layer interval statistics information.

Media Dependent Statistics dialog box displays:

Interface Side (srpRingIntInterfaceSide)

Interval Number (srpRingIntNumber)

### Interface Side (srpRingIntInterfaceSide)

Indication of the side of the interface for which this row contains information.

### Interval Number (srpRingIntNumber)

A number between 1 and 96, which identifies the intervals for which the set of statistics is available. The interval identified by 1 is the most recently completed 15 minute interval, and interval identified by N is the interval immediately preceding the one identified by N-1.

## Related Topics

The CiscoView Monitor Window

Monitoring Ports

Monitoring the Device

Monitoring the Device Environment

Monitoring Devices and Components

##