# FDDI/Ethernet Bridge

Device>Configure>FDDI/Ethernet Bridge (not supported on 4000-series devices).

The FDDI/Ethernet Bridge window displays the following information:

IP Fragmentation (brouterEnableIpFragmentation)

Whether IP fragmentation is enabled or disabled.

IPX FDDI Snap to Ethernet (brouterIpxSnapToEther)

Default translation method for IPX packets when bridging from FDDI SNAP to Ethernet. Possible values are snap, ethernetII, iso8023, or raw8023.

IPX Ethernet to FDDI (brouterIpx8023RawToFddi)

Default translation for IPX packets when bridging. Possible values are snap, fddiRaw, and iso8022.

IPX FDDI 802.2 To Ethernet (brouterIpx8022ToEther)

Default translation method for IPX packets when bridging from FDDI 802.2 to Ethernet. Possible values are snap, ethernetII, iso8023, or raw8023.

FDDI Check (brouterEnableFddiCheck)

Whether MAC addresses learned on one side of a translational bridge should not be allowed to be learned on the other side of the bridge.

APaRT (brouterEnableAPaRT)

Whether Automatic Packet Recognition and Translation (APaRT) is enabled on translational bridges in the device.

ICMP Unreachables (brouterEnableUnreachables)

Whether ICMP unreachable messages are sent.

Click Apply to make your changes take effect, or click Cancel to close the dialog box without making any changes. Click Print to print the contents of the dialog box.