# Physical

## Navigation

Right-click on the Persistent Storage Device (PSD) card and then select Configure.

In the Physical dialog box, you can view general information about this PSD card.

The following information is displayed:

- Name of the Module (moduleName)

- Module Model (moduleModel)

- Serial Number (moduleSerialNumberString)

- Hardware Version (moduleHwVersion)

- Firmware Version (moduleFwVersion)

- Software Version (moduleSwVersion)

- Status (moduleStatus)

- IP Address (moduleIPAddress)

- Diagnostic Errors (moduleTestResult)

Name of the Module (moduleName)

Name assigned to the module or card by the network administrator (for example, London).

Module Model (moduleModel)

Manufacturer’s model number for the card or module.

Serial Number (moduleSerialNumberString)

Serial number of the card or module (for example, 900000023).

Hardware Version (moduleHwVersion)

Version number of the card being managed (for example, 3.1).

Firmware Version (moduleFwVersion)

Firmware version of the card being managed (for example, 2.0).

Software Version (moduleSwVersion)

Software version of the card being managed (for example, 3.2).

Status (moduleStatus)

Current status of the module or card. Possible values include:

- other

- ok

- minorFault

- majorFault

If the status is not ok, refer to the value of the Diagnostic Errors field for more information about the cause of the problem.

IP Address (moduleIPAddress)

IP address of the module or card.

The value 0.0.0.0 may initially be set for this object. As a result, you will be prompted to enter the appropriate IP address when you right-click on the card and then select PSD Details from the context menu. After you specify an IP address, this object will display the value you entered.

Note: This field is only displayed on IDS, NAM, and PSD modules.

Diagnostic Errors (moduleTestResult)

Result of the module’s self-test. The value none indicates that the module passed all tests.