# Host Result Details

## Navigation

Device > Configure > EOU > Host Result Details

The following information appears:

> Associated Interface (cnnEouHostResultAssocIf)

> IP Addr Type (cnnEouHostResultIpAddrType)

> IP Address (cnnEouHostResultIpAddr)

> Mac Address (cnnEouHostResultMacAddr)

> Auth Type (cnnEouHostResultAuthType)

> Posture Token (cnnEouHostResultPostureToken)

> Query Period (cnnEouHostResultStatusQryPeriod)

> Revalidation Period (cnnEouHostResultRevalidatePeriod)

> Detected Host State (cnnEouHostResultState)

> URL String (cnnEouHostResultUrlRedir)

> Posture Token String (cnnEouHostResultPostureTokenStr)

### Associated Interface (cnnEouHostResultAssocIf)

An index value that uniquely identifies an interface to which the endpoint device is currently connected.

### IP Addr Type (cnnEouHostResultIpAddrType)

Type of Internet address by which the detected host is reachable.

### IP Address (cnnEouHostResultIpAddr)

Internet address for the detected host. The IP address type is indicated by the value of cnnEouHostResultIpAddrType.

### Mac Address (cnnEouHostResultMacAddr)

MAC address of the detected host

### Auth Type (cnnEouHostResultAuthType)

Authentication type used in the posture validation process for the detected host.

### Posture Token (cnnEouHostResultPostureToken)

Indicates the posture token of the detected host.

During the posture validation process, the host is placed into a category and has a token assigned to it. The assignment depends on the current state of the software residing on the host. The host will have the specific right to access the network based on the assigned token.

### Query Period (cnnEouHostResultStatusQryPeriod)

Timeout period, in seconds, for the status query sent after this interface is revalidated.

### Revalidation Period (cnnEouHostResultRevalidatePeriod)

Timeout period, in seconds, for the revalidation of this interface.

### Detected Host State (cnnEouHostResultState)

Current EOU state of this detected host.

### URL String (cnnEouHostResultUrlRedir)

Indicates the URL from which you can download the latest anti-virus file. If the detected host fails credential validation, then it may require remediation.

### Posture Token String (cnnEouHostResultPostureTokenStr)

Posture token string of the detected host. During the posture validation process, the host is placed into a particular category and has a token assigned to it. This assignment will depend on the state of the software that resides on the host. The host will have specific rights to access the network based on the token assigned.