# Receive Side Low Priority Traffic Statistics

Use this option to monitor statistics of low priority traffic reception from physical medium-dependent layer for a particular side of a particular SRP interface.

## Procedure

To access low priority traffic information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

Media Dependent Statistics dialog box appears.

2. Select Rx Physical Layer Statistics from the Category menu to display Receive Physical Layer Statistics dialog box.

3. Select Low Priority Traffic from the Category menu to display low priority traffic information.

Low Priority Traffic dialog box displays:

Unicast Low Priority Packets (srpRingIntUcastLowPriPktsIn)

Unicast Low Priority Octets (srpRingIntUcastLowPriOctetsIn)

Multicast Low Priority Packets (srrpRingIntMcastLowPriPktsIn)

Multicast Low Priority Octets (srpRingIntMcastLowPriOctetsIn)

### Unicast Low Priority Packets (srpRingIntUcastLowPriPktsIn)

Number of low priority unicast packets received from physical medium-dependent layer during a 15-minute interval.

### Unicast Low Priority Octets (srpRingIntUcastLowPriOctetsIn)

Number of low priority unicast octets received from physical medium-dependent layer during a 15-minute interval

### Multicast Low Priority Packets (srrpRingIntMcastLowPriPktsIn)

Number of low priority multicast packets received from physical medium-dependent layer during a 15-minute interval

### Multicast Low Priority Octets (srpRingIntMcastLowPriOctetsIn)

Number of low priority multicast octets received from physical medium-dependent layer during a 15-minute interval

## Related Topics

The CiscoView Monitor Window

Monitoring Ports

Monitoring the Device

Monitoring the Device Environment

Monitoring Devices and Components