# Frame Relay Port Configuration Information

The dialog box displays the frame relay port configuration information for the selected port.

## Procedure

> 1. In the rear view, right-click on an A/S serial port and select Configure from the pop up menu or double-click on an A/S serial port. The port configuration dialog box appears.

> 2. Select Frame Relay Circuits from the Category menu.

The following information appears:

> Data link connection management information:

> State (frDlcmiState)

> Address(frDlcmiAddress)

> Address Length(frDlcmiAddressLen)

> Status Enq Msg Intervals (frDlcmiPollingInterval)

> Max Errs Enq Status Msg (frDlcmiErrorThreshold)

> Multicast Service (frDlcmiMulticast)

> Max Virtual Circuits(frDlcmiMaxSupportedVCs)

> Data Link Connection Identifier(frCircuitDlci)

> Creation Time (frCircuitCreationTime)

> Throughput (frCircuitThroughput)

> Data link connection identifier information:

> Oper State (frCircuitState)

> Last Change (frCircuitLastTimeChange)

> Max Committed Bits (frCircuitCommittedBurst)

> Max Uncommitted Bits (frCircuitExcessBurst)

> Monitored Events (frDlcmiMonitoredEvents)

This information is displayed in the CiscoView configure port window for a Frame Relay port.

### State (frDlcmiState)

Type of connection management scheme that is active at this interface.

Values are:

noLmiConfigured |
lmiRev1 |
ansiT1-617-D |
ansiT1-617-B |

### Address (frDlcmiAddress)

Shows the address format used. Possible values are as follows:

Address Format | Meaning
q921 | 13-bit DLCI
q922March90 | 11-bit DLCI
q922November90 | 10-bit DLCI
q922 | final standard

### Address Length (frDlcmiAddressLen)

Address length in octets. Possible values are two-octets, three-octets, and four-octets. For the address format q922, the length includes address and control portions.

### Status Enq Msg Intervals (frDlcmiPollingInterval)

The number of seconds between successive status enquiry messages. The value range from 1 to 255.

### Max Errs Enq Status Msg (frDlcmiErrorThreshold)

The maximum number of unanswered status inquiries allowed before the interface is declared down. The value range from 1 to 10.

### Multicast Service (frDlcmiMulticast)

Indicates whether the interface uses a multicast service. Possible values are nonBroadcast and broadcast.

### Max Virtual Circuits (frDlcmiMaxSupportedVCs)

The maximum number of virtual circuits allowed for this interface.

### Oper State (frCircuitState)

The operational state of the circuit. Possible values are invalid, active, and inactive.

If you set an entry to invalid, the circuit is deleted.

### Last Change(frCircuitLastTimeChange)

The sysUpTime the state of virtual circuit last changed.

### Max Committed Bits (frCircuitCommittedBurst)

The maximum number of bits of data that the network agrees to transfer under normal conditions during the measurement interval.

### Max Uncommitted Bits (frCircuitExcessBurst)

The number of uncommitted bits of data that the network attempts to transfer under normal conditions during the measurement interval.

### Monitored Events (frDlcmiMonitoredEvents)

The number of status polling intervals over which the error threshold is counted.

### Data Link Connection Identifier (frCircuitDlci)

The data link connection identifier for a virtual circuit.

### Creation Time (frCircuitCreationTime)

The sysUpTime when the virtual circuit was created, whether by the Data Link Connection Management interface or by a SetRequest.

### Throughput (frCircuitThroughput)

The average number of 'Frame Relay Information Field' bits transferred per second across a user network interface in one direction, measured over the measurement interval.

If the configured committed burst rate and throughput are both non-zero, the measurement interval (T) is equal to the value of frCircuitCommittedBurst/frCircuitThroughput.

If the configured committed burst rate and throughput are both zero, the measurement interval (T) is equal to the value of frCircuitExcessBurst/ifSpeed.