# PAE Port

## Navigation

Port > Configure > PAE > PAE Port

The following information appears:

> Protocol Version (dot1xPaePortProtocolVersion)

> Capability (dot1xPaePortCapabilities)

> Intialization (dot1xPaePortInitialize)

> ReAuthentication (dot1xPaePortReauthenticate)

> Multiple Host (cpaeMultipleHost)

> Port Mode (cpaePortMode)

> Vlan No (cpaeGuestVlanNumber)

> Guest Vlan (cpaeInGuestVlan)

> Shutdown Timeout (cpaeShutdownTimeoutEnabled)

> Auth-Fail Vlan (cpaePortAuthFailVlan)

> Assigned Vlan (cpaePortOperVlan)

> Assigned Vlan Type (cpaePortOperVlanType)

> VLAN Max Attempts (cpaeAuthFailVlanMaxAttempts)

> Mab Port Track Enabled (cpaeMabPortIpDevTrackEnabled)

> Port Track Enabled (cpaePortIpDevTrackEnabled)

### Protocol Version (dot1xPaePortProtocolVersion)

Protocol version associated with this port.

### Capability (dot1xPaePortCapabilities)

Indicates the PAE functionality this port supports. It will show what functionality is supported, whether it supports Authenticator functions or supplicant functions.

### Intialization (dot1xPaePortInitialize)

Initialization control for this port. Setting this attribute to true causes the port to be initialized. The attribute reverts to false after initialization is complete.

Note: This attribute can only be set to true when a port has network connectivity and port control is in automatic mode.

### ReAuthentication (dot1xPaePortReauthenticate)

Reauthentication control for this port. Setting this attribute to true causes the Authenticator PAE state machine for the Port to reauthenticate the supplicant.

Note: This attribute can only be set to true when a port has network connectivity, port control is in automatic mode, and port status is authorized.

### Multiple Host (cpaeMultipleHost)

Specifies whether the port allows multiple-host connection.

### Port Mode (cpaePortMode)

Specifies the dot1x operation mode configured for the port.

There are three possible values:

> singleHost(1): The port allows one host to connect and be authenticated.

> multiHost(2): The port allows multiple hosts to connect. After one host is authenticated, the remaining hosts are also authenticated.

> multiAuth(3): The port allows multiple hosts to connect and be authenticated.

Note: If the port security feature is enabled on the interface, the port security configuration settings (such as the number of the hosts allowed, the security violation action, etc.) are applied to the interface.

### Vlan No (cpaeGuestVlanNumber)

Indicates the Guest VLAN configured for the interface. An interface with a cpaePortMode value of singleHost is moved to its Guest VLAN if the interface's supplicant is not capable of IEEE-802.1x authentication.

When the value of this object is zero, it indicates that no Guest VLAN is configured for the interface.

### Guest Vlan (cpaeInGuestVlan)

Indicates whether the interface is currently in its Guest VLAN.

Note: The object is deprecated by cpaePortOperVlanType.

### Shutdown Timeout (cpaeShutdownTimeoutEnabled)

Indicates whether the shutdown timeout feature is enabled on the interface.

### Auth-Fail Vlan (cpaePortAuthFailVlan)

Specifies the Authentication Fail (Auth-Fail) VLAN for this port. A port with a cpaePortMode value of singleHost is moved to its Auth-Fail VLAN if the corresponding supplicant supports IEEE-802.1x authentication but is unsuccessfully authenticated.
When the value of this object is zero, it indicates that no Auth-Fail VLAN is configured for this port.

### Assigned Vlan (cpaePortOperVlan)

Value of VlanIndex for the VLAN assigned to this port via IEEE-802.1x authentication.
When the value of this object is zero, it indicates that no VLAN is assigned to this port.

### Assigned Vlan Type (cpaePortOperVlanType)

Type of VLAN assigned to this port via IEEE-802.1x authentication.

There are four possible values:

> other: The VLAN assigned to this port is not of a type specified by the other possible values for this object.

> none: No VLAN has been assigned to this port. In this case, the corresponding value of cpaePortOperVlan is zero.

> guest: A Guest VLAN has been assigned to this port. This VLAN is specified by the corresponding cpaeGuestVlanNumber object.

> authFail: An Auth-Fail VLAN has been assigned to this port. This VLAN is specified by the corresponding cpaeAuthFailVlanNumber object.

### VLAN Max Attempts (cpaeAuthFailVlanMaxAttempts)

The maximum number of authentication attempts made before a port is moved into the Auth-Fail VLAN.

### MabPort Track Enabled (cpaeMabPortIpDevTrackEnabled)

Indicates whether IP device tracking is enabled on this port for the corresponding MAC Auth-bypass authenticated host.

### Port Track Enabled (cpaePortIpDevTrackEnabled)

Indicates whether IP device tracking is enabled on this port for the corresponding 802.1x authenticated host.