# Authorized IP Table

## Navigation

Device > Configure > EOU > Authorized IP Table

The following information appears:

> IP Address (cnnEouAuthIpAddr)

> IP Mask (cnnEouAuthIpAddrMask)

> IP Policy Name (cnnEouAuthIpPolicy)

## Button Descriptions

> Click Create to launch the Row Creation dialog box. Enter the required information (described below) and then click OK.

> With a table entry selected, click Delete to remove that entry.

### IP Address (cnnEouAuthIpAddr)

IP address of the statically authorized device. The address type is determined by the value of cnnEouAuthIpAddrType.

### IP Mask (cnnEouAuthIpAddrMask)

Mask used with the source IP address to specify which traffic is exempted from EAP validation.

CiscoView supports IP wildcards by making use of inverse masks. For example:

> If the value of cnnEouAuthIpAddr is 10.0.0.0 and the value of cnnEouAuthIpAddrMask is 0.255.255.255, then any IP address with a value of 10.x.x.x is exempted from posture validation.

> If the value of cnnEouAuthIpAddr is 10.1.2.1 and the value of cnnEouAuthIpAddrMask is 0.0.0.0, the IP address 10.1.2.1 is exempted from posture validation.

> If the value of cnnEouAuthIpAddr is 10.0.0.0 and the value of cnnEouAuthIpAddrMask is 255.255.255.255, all IP addresses are exempted from posture validation.

### IP Policy Name (cnnEouAuthIpPolicy)

Name of the policy associated with the statically authorized device identified by cnnEouAuthIpAddr. The policy must be present in the policy database before a statically authorized device can be associated with it.