# CDMA PDSN Service Option Table

The Service Option Table category of the Device Configuration dialog box allows you to view the service option details.

## Procedure

1. Right-click the device, then select Configure or double-click the device. The Device Configuration dialog box appears.

2. Select Service Option Table from the Category list.

The following information appears:

Service Option (cCdmaServiceOptionIndex)

Rp Session Success (cCdmaServiceOptionSucesses)

Rp Session Failure (cCdmaServiceOptionFailures)

### Service Option (cCdmaServiceOptionIndex)

Service option as defined by IOS 4.1. Service option is used to uniquely index entries in the table. Service options (as defined in 3GPP2 4.1) are:

Value | Description
6 | smsRate1
9 | loopback13K
12 | asyncDataRate2
13 | group3FaxRate2
14 | smsRate2
15 | packetData144k
18 | otapaRate1
19 | otapaRate2
22 | packetDataRs1fRs1r
23 | packetDataRs1fRs2r
24 | packetDataRs2fRs1r
25 | packetDataRs2fRs2
32 | is2000TestData
33 | packetData3G
37 | isdn64k
54 | is2000Markov
55 | is2000Loopback
4103 | packetDataRev1

### Rp Session Success (cCdmaServiceOptionSucesses)

Number of times the device succeeded in setting up a radio packet (RP) session for a particular service option defined by IOS 4.1.

### Rp Session Failure (cCdmaServiceOptionFailures)

Number of times the device failed in setting up a radio packet (RP) session for a particular service option defined by IOS 4.1.