# SRP Higher Layer Errors

Use this option to view higher layer error statistics traffic reception for a particular interval of a particular side of a particular SRP interface.

## Procedure

> 1. Right-click the SRP interface and select Configure from the popup menu.

> The Configure Port dialog box appears.

> 2. Select SRP Error Statistics - History from the Category menu.

> The SRP Error Statistics - History dialog box appears.

3. Select an Interval.

4. Click the Statistics button.

5. Select Higher Layer Errors from the Category menu.

The SRP Error Statistics - History dialog box displays the following higher layer error information:

Discarded Packets (srpErrCntIntHostRxDiscardPkts)

Short Packets (srpErrCntIntHostRxShortPkts)

Giant Packets (srpErrCntIntHostRxGiantPkts)

## Related Topics

SRP Physical Layer Errors

### Discarded Packets (srpErrCntIntHostRxDiscardPkts)

Number of packets discarded due to resource limitations, received from layer 1 physical medium during a 15 minute interval in the past 24 hours.

### Short Packets (srpErrCntIntHostRxShortPkts)

Number of packets discarded for being short for the higher layer, during a 15 minute interval in the past 24 hours.

### Giant Packets (srpErrCntIntHostRxGiantPkts)

Number of packets discarded for being too big for the higher layer, during a 15 minute interval in the past 24 hours.