# RP Registration Denied Statistics

From this dialog box, you can view Packet Control Function (PCF) and Service Option (SO)-based RP registration denied statistics.

## Navigation

1. Right-click the Mobile Wireless Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN PCF & SO Based Statistics.

4. With an entry selected in the PCFs & Service Options table, click RP Registration Statistics.

5. Select RP Registration Denied Statistics.

The following information is displayed:

> Registration Requests Denied (cCdmaPcfSoRpRegDeniedReqs)

> Registration Requests Discarded (cCdmaPcfSoRpRegDiscardedReqs)

> New Connection Requests Denied (cCdmaPcfSoRpInitRegDeniedReqs)

> Re-registration Requests Denied (cCdmaPcfSoRpReRegDeniedReqs)

> De-registration Requests Denied (cCdmaPcfSoRpDeRegDeniedReqs)

> Handoff A11 Reg Req Denied (cCdmaPcfSoRpHandoffRegDeniedReqs)

### Registration Requests Denied (cCdmaPcfSoRpRegDeniedReqs)

Number of A11 registration requests denied since system startup.

### Registration Requests Discarded (cCdmaPcfSoRpRegDiscardedReqs)

Number of A11 registration requests discarded since system startup.

### New Connection Requests Denied (cCdmaPcfSoRpInitRegDeniedReqs)

Number of A11 registration requests meant for establishing new RP connections that have been denied since system startup.

### Re-registration Requests Denied (cCdmaPcfSoRpReRegDeniedReqs)

Number of A11 registration requests meant for refreshing established RP connections that have been denied since system startup.

### De-registration Requests Denied (cCdmaPcfSoRpDeRegDeniedReqs)

Number of A11 registration requests meant for closing established RP connections that have been denied since system startup.

### Handoff A11 Reg Req Denied (cCdmaPcfSoRpHandoffRegDeniedReqs)

Total number of denied handoff A11 Registration Requests meant for already existing session, since the system was last restarted.

Note: This object is available for PDSN version 3.0 and later.