# GGSN Charging Alarms

The GGSN Charging Alarms dialog box provides a history of the charging gateways and all charging-related alarms.

Note: This dialog box is available only if the value of cGtpGSNService is set to ggsn.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select GGSN Charging Alarms from the Category drop-down box.

The following information is displayed:

> Charging Gateway ID (cgprsCgAlarmHistIndex)

> Gateway Type (cgprsCgAlarmHistType)

> Address Type (cgprsCgAlarmHistAddrType)

> IP Address (cgprsCgAlarmHistAddress)

> Alarm Severity (cgprsCgAlarmHistSeverity)

> Detailed Information (cgprsCgAlarmHistInfo)

### Charging Gateway ID (cgprsCgAlarmHistIndex)

Monotonically increasing integer that indexes charging gateways and charging-related alarms. The value of this object is wrapped back to one when it reaches the maximum value of 4294967295.

### Gateway Type (cgprsCgAlarmHistType)

Type of GPRS charging gateway or charging-related alarm.

### Address Type (cgprsCgAlarmHistAddrType)

Type of internet address given in cgprsCgAlarmHistAddress.

### IP Address (cgprsCgAlarmHistAddress)

IP address that uniquely identifies the charging gateway.

### Alarm Severity (cgprsCgAlarmHistSeverity)

Indicates the severity of the alarm.

### Detailed Information (cgprsCgAlarmHistInfo)

Provides detailed information on when a GPRS charging gateway or charging-related alarm is generated.