# Mapping Tables

Configuration > Mapping Tables

Mapping tables are used for computing the final DSCP value using the CoS, IP Precedence, and DSCP values in the headers of incoming packets. Depending on the trust state of the port and ACE, the final DSCP value is determined using these mapping tables.

The following list specifies buttons in this dialog box, as well as their function:

- Click Print to print the contents of the dialog box.

- Click Help to access the online help.