# CDMA PDSN Traffic (Pkts) Statistics Contd

1. Right click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Statistics button.

4. Select category CDMA PDSN Traffic (Pkts) Statistics Contd.

5. Select a row and click on Monitor.

The following information appears:

> SDB Marked Data Packets (cCdmaTransmittedSDBPkts)

> GRE Key Missing Discarded Packets (cCdmaNoGREKeyPktDiscards)

> Session Not Found Discarded Packets (cCdmaNoSessionPktDiscards)

> GRE Protocol Discarded Packets (cCdmaInvGREProtoPktDiscards)

> Invalid Checksum Discarded Packets (cCdmaInvCheckSumPktDiscards)

### SDB Marked Data Packets (cCdmaTransmittedSDBPkts)

Total number of SDB marked data packets sent to PCF from PDSN since the system was last restarted.

### GRE Key Missing Discarded Packets (cCdmaNoGREKeyPktDiscards)

Total number of packets discarded from PCF because GRE Key is missing since the system was last restarted.

### Session Not Found Discarded Packets (cCdmaNoSessionPktDiscards)

Total number of packets discarded from PCF because the session is not found since the system was last restarted.

### GRE Protocol Discarded Packets (cCdmaInvGREProtoPktDiscards)

Total number of packets discarded from PCF because GRE protocol is invalid since the system was last restarted.

### Invalid Checksum Discarded Packets (cCdmaInvCheckSumPktDiscards)

Total number of packets discarded from PCF due to invalid checksum since the system was last restarted.