; Jungo Confidential. Copyright (c) 2016 Jungo.  http://www.jungo.com
; Generated by DriverWizard v10.11.
; Installation file (.inf) for "DEVICE" device
;
; You can create a customized version of this file
; by modifying the specified sections.
;
; Refer to Windows DDK documentation for more information on INF files
;

; Version Information
; -------------------
[Version]
Signature="$CHICAGO$"  ; Represents all Windows OS's
Provider=%Provider%
; For WHQL, you should obtain a catalog signed by Microsoft Hardware Compatibility Labs
CatalogFile=asabusb.cat
DriverVer=04/24/2016, 12.2.0

; Select an appropriate class for the device.
; There are several options:
; - Use the Jungo class.
; - Define your own class by generating a private GUID and a class description.
; - Use a system-defined class. This is required for a device that belongs to 
;   a device class that is supported by system-provided drivers, i.e. HID or USB Audio.
;   For example, to replace a default USB mouse driver you have to specify the 
;   description and GUID of HID class:
;       Class=HIDClass
;       ClassGuid={745a17a0-74d3-11d0-b6fe-00a0c90f57da}
;
; We use a Jungo class, you may modify here and use a different class:
Class=Portable Devices
ClassGuid={31f0bc93-edad-45b6-a61e-c25255adf725}

; Driver Information
; ------------------
[Manufacturer]
; You may modify the manufacturer name by changing the Mfg variable in the [Strings]
; section in this INF file.
%Mfg%=DeviceList,NTamd64

; The 'Install' lines under the [DeviceList] include the device name that will
; be displayed in the Device Manager and the hardware ID's. 
; You may modify the device names and the hardware ID's.
; The Vendor ID is 1768, and the Product ID is 0010

; x86 platform, Windows 2000 and later
[DeviceList]
; For a multiple-interface USB device, all selected interfaces are listed here:
"DECT Handset"=Install, USB\VID_1768&PID_0010

; x64 platform, Windows XP x64 edition and later
[DeviceList.NTamd64]
; For a multiple-interface USB device, all selected interfaces are listed here:
"DECT Handset"=Install, USB\VID_1768&PID_0010

; Installation Section
; --------------------
[Install.NT]  ; Installation script for Windows 2000 and later
CopyFiles=FilesToCopy
AddReg=UpDateRegistry

[FilesToCopy]
; To copy asabusb.sys upon installation remove the ';' from the start of the following line
;asabusb.sys ,,,0x40  ; 0x40 == COPYFLG_OVERWRITE_OLDER_ONLY

[ClassInstall32]  ; Register a new class in Windows 2000 and later
AddReg=UpDateRegistry

[UpDateRegistry]
HKR,,,,Portable Devices
HKR,,Icon,,-20
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,, asabusb.sys

[ControlFlags]
ExcludeFromSelect = *  ; Remove all devices listed in this INF file from certain user 
;    interface displays, from which a user is expected to select a particular device 
;    for installation.

[PreCopySection]
HKR,,NoSetupUI,,1

; Defining asabusb Service
; ---------------------------
[Install.NT.Services]
Addservice=asabusb, 0x00000002, Service_Info

[Service_Info]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\asabusb.sys

; Source File Information
; -----------------------
[SourceDisksFiles]
asabusb.sys=1  ; This indicates that the asabusb.sys file is located on
    ; disk number 1 of "MANUFACTURER Installation disks" set.

[SourceDisksNames]
1="Ascom Installation Disk",,  ; This indicates that disk number 1
    ; has the label "MANUFACTURER Installation Disk". The installer will
    ; search for asabusb.sys in this disk.

[DestinationDirs]
DefaultDestDir=10, System32\Drivers  ; The location to which the asabusb.sys
    ; file will be copied (10 translates to the correct Windows directory
    ; on the target machine).


;---------------------------------------------------------------;

[_InstKitData]
Vid=1768
Pid=0010

[Strings]
Provider="Ascom"
Mfg="Ascom"

;
; Localizable Strings, modify as required
;

; Edit the strings in this section according to your needs.
; Some of the strings are shown at the user interface.

; provider name
S_Provider="Ascom (Sweden) AB"

; manufacturer name
S_Mfg="Ascom (Sweden) AB"

; device class display name, shown in Device Manager
S_DeviceClassDisplayName="Portable Devices"

S_DeviceId="Vid_1768&Pid_0010"

; device description
S_DeviceDesc="DECT Handset"

; disk name
S_DiskName="DECT Handset (0010)"

; File name of driver executable.
; If the name is modified, the [_CopyFiles_sys] and [SourceDisksFiles]
; sections must also be modified !
S_DriverName="ASAB_0010"

; *** EOF ***
