## Avaya SMBS
## IP Office Version 3.1
## June 2005
##
## 46xxsettings.txt
##
## Please see the LAN Administrators Guide
## for more details on using this file.
##
## Use "##" without quotes to comment out a line.
## To activate a setting below, set the parameter
## to the appropriate value for your network and
## remove the "## " from the begining of the line.
##
## To include whitespaces in a value, 
## the entire value must be enclosed in double quotes.
## example:
## SET PARAM "value1 value2"
##
## To set different set types to different values, use
## the "IF" keyword statement.
## See the LAN Administrators Guide for more details.
##
## Some of the values listed below have default settings which
## are used by the IP Telephones even if they are commented out
## in this file. For a list of those settings and their default
## values, see the LAN Administrators Guide.
##
## Note that settings as defined for 4610 and 4620 IP
## telephones also apply to the 5610 and 5620 handsets
## respectively.


#############################################################
##### COMMON SETTINGS - Applies to all 4600 IP Telephones####

###### Domain Settings ######

## Your domain
## NOTE: It is recommended that DOMAIN be set via DHCP.
## If you set your DOMAIN via DHCP, do not set it here
## as it will over ride your DHCP setting.
## example:
## SET DOMAIN mycompany.com

## Your Domain Name Server
## NOTE: It is recommended that Domain Name Server be set via DHCP.
## If you set your Domain Name Server via DHCP, do not set it here
## as it will over ride your DHCP setting.
## example:
## SET DNSSRVR 198.152.15.15


#############################################################
############# ==== END OF COMMON SETTINGS ==== ##############


###############################################################
######### Settings for the 4610 and 4620 IP Telephones ########

############## Enhanced Local Dialing Rules #################

## These settings effect certain dialing behaviors on the 4610
## and 4620 phones. These include "Click to Dial" and 
## "Add to Speed Dial" links shown on the web browser applications
## and incoming and missed call log entries. 

## Telephone Country Code
## example: For United States it is '1'
## SET PHNCC 1

## Telephone dial plan length (the length of an internal extension number).
## For example, if your extension is 12345, your dial plan
## length is 5.
## example:
## SET PHNDPLENGTH 5

## Telephone international access code
## For the USA, the code is 011.
## example:
## SET PHNIC 011

## Telephone long distance access code
## example:
## SET PHNLD 1

## Length of national telephone number
## For example, 800-555-1111 is a length of 10.
## example:
## SET PHNLDLENGTH 10

## Outside line access code
## The number you press to make an outside call.
## example:
## SET PHNOL 9
SET PHNOL ""
#####################################################################

################# Application Access Settings #######################

## Use this setting to restrict access to certain 4610 and 4620
## applications.

## When APPSTAT is set to 0, Call Log and Redial are suppressed and, 
## changes to Speed Dial are not allowed.

## when APPSTAT is set to 1, Call Log, Redial and, Speed Dial work 
## without restrictions.

## when APPSTAT is set to 2, Call Log is suppressed, for Redial the 
## Last-6-numbers 

## when APPSTAT is set to 3, changes to Speed Dial are not allowed.

## example:
## SET APPSTAT 1
#####################################################################

###################### Option Access Settings #######################

## Use this setting to enable or disable access to certain 4610 and 
## 4620 user options.

## When OPSTAT is set to 000, the user options are not accessible.

## When OPSTAT is set to 001, the user can only invoke the Log-Off
## Option on the 4610 and 4620. 

## When OPSTAT is set to 010, the user can only invoke view-only options.   
## The user cannot change any setting. 

## When OPSTAT is set to 011, the user can only invoke view-only options   
## and the Log-Off Option on the 4610 and 4620. 

## When OPSTAT is set to 100, the user can access all options except the
## view-only options and the Log-Off option on the 4610 and 4620.

## When OPSTAT is set to 101, the user options can access all options 
## except the view-only options. 

## When OPSTAT is set to 110, the user can invoke all the options except  
## the Log-Off option on the 4610 and 4620. 

## When OPSTAT is set to 111, the user can invoke any or all of the user 
## options. 

## example:
## SET OPSTAT 111

######################################################################
######### ====  END OF 4610 and 4620 IP Phone Settings ==== ##########

#####################################################################
############## 4610 and 4620 Specific IP Phone Settings #############

################ FTP Server for Backup/Restore ###################### 

## NOTE: Setting the FTP backup/restore server address here will cause
## all 4610 and 4620 IP telephones to use the same settings
## and over write each other's backup files. To use this
## feature to perform backup and restores of individual
## IP telephones, these parameters must be set individually
## at each telephone. See the LAN Administrators Guide for
## more details.

## The IP Address of your FTP Server
## example:
## SET FTPSRVR 135.18.18.18 
#####################################################################

####### 4610 and 4620 IP Phone Multi-Language Administration ########

## Use this value to set the local display
## language of your 4610 and 4620.

## For all 4610SW 4620 sets, and 4620SW sets that have
## been loaded with single-byte software, use one of the
## following settings:
## For English use keyword "English"
## For French use keyword "Francais"
## For Italian use keyword "Italiano"
## For Japanese use keyword "Katakana"
## For Dutch use keyword "Nederlands"
## For German use keyword "Deutsch"
## For Portuguese use keyword "Portugues"
## For Spanish use keyword "Espanol"

## For 4620SW sets that have been loaded with multi-byte software
## to support Chinese/Russian/English fonts, use one of
## the following settings:
## For English use keyword "English"
## For Chinese use keyword "Chinese"
## For Russian use keyword "Russian"

## For 4620SW sets that have been loaded with multi-byte software
## to support Japanese/Russian/English fonts, use one of
## the following settings:
## For English use keyword "English"
## For Japanese use keyword "Japanese"
## For Russian use keyword "Russian"

## example:
## SET SYSLANG English
#####################################################################

#####################################################################
########## End of 4610 and 4620 Specific IP Phone Settings ##########

## END OF SETTINGS SCRIPT FILE
