                SOFTWARE RELEASE NOTES
                ======================

Products involved: AXIS 2100 Network Camera

Release date: 2004-08-27

Release type: Production

Software version: 2.42

Filename: 2100_242.bin

Last preceding release:  2.40

---------------------------------------------------------------------

Upgrade instructions:
         
Important: 

0. Upgrade to version 2.42 is only possible if version 2.12 or later 
   is installed. 

1. Make sure that "active applications" such as continuous transmission 
   of images via ftp or smtp from the Axis Network Camera  are disabled 
   prior to initiating upgrade.

2. Make sure to take notes of your application/layout and other 
   settings prior to upgrading since these settings will be 
   lost during upgrade. 

3. You must be at the command prompt and in the directory that 
   contains the Upgrade File.
   Example: C:\Axis\2100\2_42>

4. Open an ftp connection to the unit you want to upgrade from a 
   command prompt.
   (Do not use a Windows based FTP-program for this, use only command 
   line FTP programs!)

5. Login as root. The default password for the root user is "pass" 
   unless changed by the user. You must be logged in as the root user 
   to upgrade the unit.

6. Change to binary transfer mode by typing "bin" and press enter.

7. Type "hash" and press enter. (This will allow you to see how the 
   upgrade progresses)

8. Type the command "put XXX.bin flash_all" where XXX.bin is replaced
   by the name of the name of upgrade file you downloaded 
   (and maybe decompressed) from our site. It is typically named 
   2100_242.bin or axis2100.bin. 

9. Wait for the flash load to finish, this may take 1-10 minutes.
   Always wait at least 10 minutes for the flash upgrade to complete.

10. Your unit will automatically restart using the new firmware. 

11. Reconfigure your settings.


RELEASE 2.42
============

New in 2.42
===========

2.42:1 Corrections for security issues that enable a remote attacker 
       to execute arbitrary shell script commands.

2.42:2 Third party software licenses text added to the product's web 
       interface.


Application developer / scripting in 2.42:
==========================================


The following HTTP API groups are supported by the AXIS 2100. For more 
information, please see the HTTP API document available at www.axis.com.

Group		Exceptions
=====      	==========
General		Get property
Jpeg/Mjpg
Audio
I/O control		
PPP

The new improved audio functionality uses G723 as the default audio codec, 
which gives a higher compression compared to the former G721. It uses 
singlepart instead of multipart communication to reduce overhead. For 
backward compatibility change the following parameters in the product: 

root.Audiod.audioEncoding="G721"
root.Audiod.httpMessageType="multipart"


Known limitations in version 2.42 
=================================

L1. Up to 350KB of RAM memory is available for pre/post alarm image storage.
