SOFTWARE RELEASE NOTES
======================

Products involved: AXIS 2130 PTZ Network Camera

Release date: 2004-08-29

Release type: Production

Software version: 2.42

Filename: 2130_242.bin

Last preceding release:  2.40

-----------------------------------------------------------------------

Upgrade instructions:
      
   
Important: 

0.  Upgrade to version 2.42 can only be done if version 2.12 or later 
    is installed. 

1.  Make sure that "active applications" such as continuous transmission 
    of images via ftp or smtp from the Axis Network Camera  are disabled 
    prior to initiating upgrade.


2.  You must be at the command prompt and in the directory that 
    contains the Upgrade File.
    Example: C:\Axis\2130\2_42>

3.  Open an ftp connection to the unit you want to upgrade from a 
    command prompt.
    (Do not use a "windows" based ftp-program for this, use only command 
    line ftp programs!)

4.  Login as root. The default password for the root user is "pass" 
    unless changed by the user. You must be logged in as the root user 
    to flash upgrade the unit.

5.  Change to binary transfer mode by typing "bin" and press enter.

6.  Type "hash" and press enter. (This will allow you to see how the 
    upgrade progresses)

7.  Type the command "put XXX.bin flash" where XXX.bin is replaced
    by the name of the name of upgrade file you downloaded 
    (and maybe decompressed) from our site, it is typically named 
    2130_242.bin or axis2130.bin. 

8.  Wait for the flash load to finish, this may take 1-10 minutes.
    Always wait at least 10 minutes for the flash upgrade to complete.

9.  Your unit will automatically restart using the new firmware. 

10. In case the product was running an application, you will need to 
    enable it again.


RELEASE 2.42
============


New in 2.42
===========

2.42:1 Corrections for security issues that enable a remote attacker 
       to execute arbitrary shell script commands.

2.42:2 Third party software licenses text added to the product's web 
       interface.


Application developer / scripting in 2.42:
==========================================

The following HTTP API groups are supported by the AXIS 2130. For more 
information please check the HTTP API document available at www.axis.com.

Group		Exceptions
=====           ==========
General	        Get property
Jpeg/Mjpg
PTZ
I/O control		


Known limitations in version 2.40
=================================

L1. Up to 4 MB of RAM memory is available for pre/post alarm image storage.
