-- *****************************************************************
-- CISCO-IMAGE-MIB.my:  Router Image MIB file
--   
-- Jan 1995, Yunsen Wang
--   
-- Copyright (c) 1995, 2009 by cisco Systems Inc.
-- All rights reserved.
--   
-- *****************************************************************

CISCO-IMAGE-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Integer32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    DisplayString
        FROM SNMPv2-TC
    ciscoMgmt
        FROM CISCO-SMI;


ciscoImageMIB MODULE-IDENTITY
    LAST-UPDATED    "9508150000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-snmp@cisco.com"
    DESCRIPTION
        "Router image MIB which identify the capabilities
        and characteristics of the image"
    REVISION        "9508150000Z"
    DESCRIPTION
        "Specify a correct (non-negative) range for an index
        object."
    REVISION        "9501160000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 25 }


-- This group is present in all IOS based products.

ciscoImageMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoImageMIB 1 }


ciscoImageTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CiscoImageEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table provides content information describing the
        executing IOS image."
    ::= { ciscoImageMIBObjects 1 }

ciscoImageEntry OBJECT-TYPE
    SYNTAX          CiscoImageEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A image characteristic string entry."
    INDEX           { ciscoImageIndex } 
    ::= { ciscoImageTable 1 }

CiscoImageEntry ::= SEQUENCE {
        ciscoImageIndex  Integer32,
        ciscoImageString DisplayString
}

ciscoImageIndex OBJECT-TYPE
    SYNTAX          Integer32 (0..2147483647)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A sequence number for each string stored
        in the IOS image." 
    ::= { ciscoImageEntry 1 }

ciscoImageString OBJECT-TYPE
    SYNTAX          DisplayString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The string of this entry." 
    ::= { ciscoImageEntry 2 }
 

-- conformance information

ciscoImageMIBConformance  OBJECT IDENTIFIER
    ::= { ciscoImageMIB 2 }

ciscoImageMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoImageMIBConformance 1 }

ciscoImageMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoImageMIBConformance 2 }


-- compliance statements

ciscoImageMIBCompliance MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for entities which implement
        the Cisco Image MIB"
    MODULE          -- this module
    MANDATORY-GROUPS { ciscoImageMIBGroup }
    ::= { ciscoImageMIBCompliances 1 }

-- units of conformance

ciscoImageMIBGroup OBJECT-GROUP
    OBJECTS         { ciscoImageString }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing IOS image characteristics"
    ::= { ciscoImageMIBGroups 1 }

END



