-- *********************************************************************
-- CISCO-CALLHOME-MIB.my: Call Home Mib
--   
-- October 2002, Vinay Gaonkar, Dipesh Gorashia
--   
-- Copyright (c) 2002-2004, 2006-2007, 2009-2012 by cisco Systems Inc.
-- All rights reserved.
--   
-- *********************************************************************

CISCO-CALLHOME-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
    Unsigned32,
    Counter32,
    Counter64
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    TEXTUAL-CONVENTION,
    TruthValue,
    RowStatus,
    TimeStamp,
    StorageType
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    InetAddressType,
    InetAddress
        FROM INET-ADDRESS-MIB
    sysName
        FROM SNMPv2-MIB
    InterfaceIndexOrZero
        FROM IF-MIB
    SyslogSeverity
        FROM CISCO-SYSLOG-MIB
    CiscoURLString,
    EntPhysicalIndexOrZero,
    CiscoVrfName
        FROM CISCO-TC
    ciscoMgmt
        FROM CISCO-SMI;


ciscoCallHomeMIB MODULE-IDENTITY
    LAST-UPDATED    "201204270000Z"
    ORGANIZATION    "Cisco Systems Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service
            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA
            Tel: +1 800 553 -NETS
            E-mail: cs-san@cisco.com, cs-lan-switch-snmp@cisco.com"
    DESCRIPTION
        "The MIB module for the management of Call Home feature
        within the framework of Cisco's Call Home architecture.
        Customers deploying solutions to run mission critical
        applications such as storage solutions demand very high
        availability and Serviceability from their products
        and/or support partners.
        To meet these requirements, a feature called 
        'Call Home' is provided which allows the system
        experiencing Hardware/Software problems to 
        automatically send the relevant failure information 
        back to the Support Center at the Support Partners for 
        troubleshooting or to get replacement hardware 
        dispatched. This feature also provides advanced
        features that allow storage systems to send 
        performance, accounting and system health information 
        in addition to just the fault information."
    REVISION        "201204270000Z"
    DESCRIPTION
        "Added following enum to callHomeAlertGroupCapability:
        - periodicHourly(6)
        - periodicMinutes(7)
        Added following enum to ccmPeriodicAlertGroupInterval:
        - hourly(4)
        - minutes(5)
        Added following OBJECT-GROUP:
        - ccmCallHomePeriodicMinutesGroup
        - ccmOnDemandCliMsgGroup
        - ccmCallHomeDiagSignatureGroup
        - ccmCallHomeSecurityLevelGroup
        - ccmCallHomeAnonymousReportingGroup
        - ccmCallHomeAaaGroup
        Added new compliance
        - chMIBCompliance9."
    REVISION        "201011080000Z"
    DESCRIPTION
        "chSingleSmtpServerGroup is deprecated and
        replaced by the following new group:
        - ccmSingleSmtpServerGroup
        Added following objects in ccmSmtpServersTable
        - ccmSmtpServersUseVrf
        Added following OBJECT-GROUP 
        - ccmSmtpServersVrfGroup 
        - ccmHttpProxyServerGroup 
        - ccmHttpTransportVrfGroup 
        - ccmMessageSourceGroup
        Added following objects
        - ccmHttpProxyServerAddrType
        - ccmHttpProxyServerAddr
        - ccmHttpProxyServerPort
        - ccmHttpProxyServerUseEnable
        - ccmHttpTransportUseVrf
        - callHomeSmtpServerUseVrf and
        Added new compliance  
        - chMIBCompliance8."
    REVISION        "200905040000Z"
    DESCRIPTION
        "Added ccmCallHomeVrfGroup."
    REVISION        "200904090000Z"
    DESCRIPTION
        "Added the following notification objects :
        - ccmEventDescription
        - ccmEventTime
        - ccmEventUrgencyLevel 
        Added new notification  
        - ccmEventNotif
        Added new Group 
        - ccmEventNotifGroup and 
        Added new compliance  
        - chMIBCompliance6."
    REVISION        "200807010000Z"
    DESCRIPTION
        "Added support for ccmOnDemandMsgSendControlGroup,
        ccmOnDemandMsgStatusGroup, ccmSmartCallHomeGroup and
        ccmEventStatsGroup. Modified callHomeAlertGroupCapability 
        to include the following two enum values:
                       onDemand(4),
                       onDemandPerEntity(5)"
    REVISION        "200712190000Z"
    DESCRIPTION
        "Refined the DESCRIPTION clauses for the objects
        callHomeDestProfileAlertGroups and
        callHomeAlertGroupCapability."
    REVISION        "200703290000Z"
    DESCRIPTION
        "chConfigurationGroup2 is deprecated and replaced by the
        following new groups:
        - ccmConfigurationGroup3
        - ccmAlertActionGroup
        - ccmProfileMessageLevelGroup
        - ccmProfileAlertGroupsGroup
        - ccmThrottleConfigurationGroup
        chSystemInformationGroup is deprecated and replaced by the
        following two new groups:
        - chSystemInformationGroup1,
        - chSystemServicePriorityGroup.
        Add the following groups for the new objects:
        - ccmPeriodicSwInventoryInfoGroup1,
        - ccmProfileTestGroup,
        - ccmProfileActivationGroup, 
        - ccmProfileAlertGroupControlGroup, 
        - ccmSmtpServersPriorityGroup, 
        - ccmAlertGroupCapabilityGroup, 
        - ccmHttpCfgGroup,
        - ccmSeverityAlertGroupCfgGroup,
        - ccmPeriodicAlertGroupCfgGroup,
        - ccmPatternAlertGroupCfgGroup,
        - ccmEventAlertGroupCfgGroup,
        - ccmSmtpMsgSendFailNotifCtrlGroup,
        - ccmSmtpMsgSendFailNotifGroup,
        - ccmAlertHCStatisticsGroup,
        - ccmAlertRateLimitGroup,
        - ccmSmtpServerStatusGroup,
        - ccmProfileHiMessageSizeGroup,
        - chSystemInformationGroup1,
        - chSystemServicePriorityGroup."
    REVISION        "200603300000Z"
    DESCRIPTION
        "Add ccmUserDefCmdGroup."
    REVISION        "200408020000Z"
    DESCRIPTION
        "Added new compliance section 'chMIBCompliance3'."
    REVISION        "200402110000Z"
    DESCRIPTION
        "New Table 'callHomeSwInventoryTable' has been added
        to provide the Call Home inventory information about
        the software services. 
        New objects 'ccmPeriodicSwInventoryMsgEnable', 
        'ccmPeriodicSwInventoryTimeFrame' and
        'ccmMsgThrottlingEnable' has been added."
    REVISION        "200402090000Z"
    DESCRIPTION
        "Max size of 'callHomeDestProfileName' has been
        changed to 31 chars."
    REVISION        "200310300000Z"
    DESCRIPTION
        "New object 'callHomeDestProfileAlertGroups' has been
        added to the callHomeDestProfileTable.
        Row creation support has been added in the 
        callHomeDestProfileTable. 
        New Table 'callHomeAlertGroupTypeTable' has been added."
    REVISION        "200305200000Z"
    DESCRIPTION
        "New object 'callHomeDestProfileMsgLevel' has been
        added to the callHomeDestProfileTable."
    REVISION        "200210280000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 300 }


ccmCallHomeNotifications  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIB 0 }

ciscoCallHomeMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIB 1 }

chMIBConformance  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIB 2 }

ccmCallHomeConfiguration  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 1 }

ccmCallHomeStats  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 2 }

ccmCallHomeStatus  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 3 }

ccmCallHomeOnDemandActions  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 4 }

ccmSmartCallHomeActions  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 5 }

ccmCallHomeVrf  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 6 }

ccmCallHomeMessageSource  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 7 }

ccmCallhomeEvents  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 8 }

ccmCallHomeDiagSignature  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 9 }

ccmCallHomeSecurity  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 10 }

ccmCallHomeReporting  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 11 }

ccmCallHomeHttpProxy  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 12 }

ccmCallHomeAaa  OBJECT IDENTIFIER
    ::= { ciscoCallHomeMIBObjects 13 }


-- Textual Conventions

CallHomeAlert ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The type of the Call Home alert.
        noOp (1)      - no alert             
        test (2)      - alert name 'Test'
        inventory (3) - alert name 'Inventory'
        ."
    SYNTAX          INTEGER  {
                        noOp(1),
                        test(2),
                        inventory(3)
                    }

CallHomeMsgFormat ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Call Home Message format.
        xml (1)       - XML (Extensible Markup Language) 
                      - encoded.            
        fullText (2)  - Plain text without any encoding.
        shortText (3) - Short text without any encoding

        The context of the Call Home message depends on the 
        message. In general, all the Call Home message is sent 
        with following information : 

        'Subject : System Notification from '
        'TimeStamp :' 
        'Message Name :' 
        'Message Type :' 
        'Level :'  
        'Message Device ID :'  
        'Customer ID :' (optional) 
        'Contract ID :' (optional) 
        'Site ID :'     (optional) 
        'Server ID :'  
        'Message Description :' 
        'Device Name :' 
        'Contact Name :'  
        'Contact email :'  
        'Contact Phone :' (optional) 
        'Street Address :'  (optional) 
        'Model Name :' 
        'Serial Number :' 
        'Part Number :' 
        'Chassis Hardware Version :' 
        'Supervisor Software Version :' 

        Following information are required only if a hardware 
        event caused the Call Home message : 
        'Affected FRU' 
        'Affected FRU Serial Number' 
        'Affected FRU Slot :'  
        'Affected FRU Hardware Version :' 
        'Affected FRU Software Version :' 

        Following is required for all the messages : 
        'Command Output :'

        The command output may depend on the implementation and
        severity of the Call Home message. But at minimum, 
        following information which are contained in the output
        of the CLI commands must be included.
        - Hardware model
        - software version
        - context information explaining the state of the device.
        - uptime
        - brief inventory information

        The exact format depends on the format type chosen.
        For 'xml', the above information is encoded in the XML
        format. For 'fullText', above information is sent out in
        plain text. For 'shortText', only following information 
        is provided in plain text:
        'Subject : System Notification from '
        'Device Id : ' 
        'TimeStamp : ' 
        'Error Message : ' 
        'Severity Level :'  
        ."

    REFERENCE
        "For more information on the XML, refer to RFC3023."
    SYNTAX          INTEGER  {
                        xml(1),
                        fullText(2),
                        shortText(3)
                    }

CallHomeTransportMethod ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Call Home transport mechanism used to deliver the alert
        messages.
           email (1),       - via email
           ftp (2),         - via ftp
           http (3),        - via http
           emailAndHttp (4) - via both email and http
        ."
    SYNTAX          INTEGER  {
                        email(1),
                        ftp(2),
                        http(3),
                        emailAndHttp(4)
                    }

CallHomeMsgLevel ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This object contains the severity level for use as a
        threshold for filtering the alerts sent to a destination 
        profile. 
        It ranges from 1 to 10, with 10 being highest severity."
    SYNTAX          INTEGER  {
                        debug(1),
                        normal(2),
                        notification(3),
                        warning(4),
                        minor(5),
                        major(6),
                        critical(7),
                        fatal(8),
                        disaster(9),
                        catastrophic(10)
                    }

AlertGroupList ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "AlertGroups are a pre-defined set of Call Home alerts.
        Users can specify these alert groups for a destination
        profile, to choose the Call Home alerts messages to be
        sent out to the destination. This object represents 
        the list of alert groups (alert group types)
        configured for a destination profile.

        Each 'bit' within the value of an object of this type,
        specifies a configured alert group type.
        Bit position '0' ( most significant bit) in the value 
        of this object is reserved.

        The value of each 'bit' (set/reset) represents whether 
        an alert group type is configured or not for a 
        particular destination profile.

        Bit position 1, represents whether the 
        'callHomeAlertGroupName' corresponding to the 
        'callHomeAlertGroupTypeIndex' 1 in the 
        'callHomeAlertGroupTypeTable' is configured or
        not for a particular destination profile.

        Bit position 2, represents whether the 
        'callHomeAlertGroupName' corresponding to the 
        'callHomeAlertGroupTypeIndex' 2 in the 
        'callHomeAlertGroupTypeTable' is configured or
        not for a particular destination profile.

        If there is no entry in the 'alertGroupTypeTable',
        with 'alertGroupTypeIndex' 'n', then
        bit position 'n' in the value of this object is
        irrelevant. 

        If the length of an object of this type is less
        than 8 bytes, then the alert group types which are 
        not represented are not considered to be part of this
        list, i.e., effectively, the string is extended to
        be of length 8 bytes by appending bytes
        containing x'00'. Note that this means that the
        zero length string represents the 'list is empty'
        value."
    SYNTAX          OCTET STRING (SIZE (0..8))

-- Call Home MIB objects

callHomeEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object enables/disables the Call Home infrastructure
        on the local device." 
    ::= { ccmCallHomeConfiguration 1 }

sysContactPhoneNumber OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0 | 12 | 13..17))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The phone number of the contact person for this managed
        node. The phone number must start with '+' and contains 
        only numeric characters except for space and '-'.
        Some valid phone numbers are 
           +44 20 8332 9091
           +45 44886556
           +81-46-215-4678
           +1-650-327-2600
        A set operation on this object with a invalid format will
        result in an error." 
    ::= { ccmCallHomeConfiguration 2 }

sysContactEmailAddress OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The email address of the contact person for this managed
        node. The format of this object is an e-mail address
        which conforms to RFC822 and RFC1123 'addr-spec'
        syntax.
        Some valid Email Addresses are
                       raj@helpme.com,
                       bob@service.com,
                       mtom@abc.caview.ca.us

        A set operation on this object with a invalid format will
        result in an error." 
    ::= { ccmCallHomeConfiguration 3 }

sysStreetAddress OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The mailing address of this managed node." 
    ::= { ccmCallHomeConfiguration 4 }

callHomeCustomerId OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "A string, in whatever format is appropriate, to identify
        the customer." 
    ::= { ccmCallHomeConfiguration 5 }

callHomeContractId OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "A string, in whatever format is appropriate, to identify
        the support contract between the customer and support 
        partner." 
    ::= { ccmCallHomeConfiguration 6 }

callHomeSiteId OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "A location identifier of this device." 
    ::= { ccmCallHomeConfiguration 7 }

callHomeDeviceServicePriority OBJECT-TYPE
    SYNTAX          SyslogSeverity
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The service priority of the device.
        This determines how fast the device has to be serviced."
    DEFVAL          { debug } 
    ::= { ccmCallHomeConfiguration 8 }

callHomeAlertAction OBJECT-TYPE
    SYNTAX          CallHomeAlert
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object acts as a trigger by which the generation of
        a particular type of alert can be verified.  Specifically,
        setting this object to a type of alert triggers the
        sending of a Call Home message for the specified type
        so that the Call Home backend is activated.

        No action is taken if this object is set to 'noOp'.
        The value of the object when read is always 'noOp'." 
    ::= { ccmCallHomeConfiguration 9 }

callHomeAlertActionStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        successful(2),
                        inprogress(3),
                        failed(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides the status of the last Call Home action
        invocation. 
           unknown (1)     - unknown
           successful (2)  - successful 
           inprogress (3)  - action in progress
           failed (4)      - failed

        If the value of this object is 'failed', then the 
        callHomeAlertActionFailureCause provides the cause for the 
        failure.

        Management stations could read value of this object after a 
        successful set to the callHomeAlertAction object to find
        out the result of the test." 
    ::= { ccmCallHomeConfiguration 10 }

callHomeAlertActionFailureCause OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides the failure cause for the last
        Call Home test invocation. 

        Note that this object is valid only if value of 
        callHomeAlertActionStatus is 'failed'." 
    ::= { ccmCallHomeConfiguration 11 }
-- callHomeDestProfileTable

callHomeDestProfileTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CallHomeDestProfileEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains destination profiles.
        The Call Home feature requires the destination profiles to be
        setup to be able to send the Call Home messages to 
        destinations configured."
    ::= { ccmCallHomeConfiguration 12 }

callHomeDestProfileEntry OBJECT-TYPE
    SYNTAX          CallHomeDestProfileEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing information about a Call Home
        destination."
    INDEX           { callHomeDestProfileName } 
    ::= { callHomeDestProfileTable 1 }

CallHomeDestProfileEntry ::= SEQUENCE {
        callHomeDestProfileName         SnmpAdminString,
        callHomeDestProfileMsgFormat    CallHomeMsgFormat,
        callHomeDestProfileMaxMsgSize   Unsigned32,
        callHomeDestProfileTrnsprtMthd  CallHomeTransportMethod,
        callHomeDestProfileStatus       RowStatus,
        callHomeDestProfileMsgLevel     CallHomeMsgLevel,
        callHomeDestProfileAlertGroups  AlertGroupList,
        callHomeDestProfileActive       TruthValue,
        callHomeDestProfileHiMaxMsgSize Unsigned32
}

callHomeDestProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..31))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Name of the destination profile." 
    ::= { callHomeDestProfileEntry 1 }

callHomeDestProfileMsgFormat OBJECT-TYPE
    SYNTAX          CallHomeMsgFormat
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The Call Home format used with profile while sending
        the message."
    DEFVAL          { xml } 
    ::= { callHomeDestProfileEntry 2 }

callHomeDestProfileMaxMsgSize OBJECT-TYPE
    SYNTAX          Unsigned32 (0..1000000)
    UNITS           "bytes"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Maximum message size that can be sent to destination
        pointed to by this destination profile.

        Implementations are allowed to assign default value.

        A value of 0 for this object indicates no limitation
        on maximum message size that can be sent to destination
        pointed to by this destination profile.

        If the maximum message size is greater than the maximum value
        reportable by this object then this object should report its
        maximum value (1,000,000) and callHomeDestProfileHiMaxMsgSize
        must be used to report the maximum message size." 
    ::= { callHomeDestProfileEntry 3 }

callHomeDestProfileTrnsprtMthd OBJECT-TYPE
    SYNTAX          CallHomeTransportMethod
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Call Home transport method used to deliver the alert
        messages."
    DEFVAL          { email } 
    ::= { callHomeDestProfileEntry 4 }

callHomeDestProfileStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Status of this row." 
    ::= { callHomeDestProfileEntry 5 }

callHomeDestProfileMsgLevel OBJECT-TYPE
    SYNTAX          CallHomeMsgLevel
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object contains the threshold level, used for
        filtering alert messages sent to a destination. 
        Call Home alert message with severity level lower than 
        the configured threshold level would not be sent. 
        The default threshold level is debug (1), which means 
        all the alert messages will be sent."
    DEFVAL          { debug } 
    ::= { callHomeDestProfileEntry 6 }

callHomeDestProfileAlertGroups OBJECT-TYPE
    SYNTAX          AlertGroupList
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represent the list of configured alert
        groups for this destination profile.
        User can modify the configured alert groups, by
        Setting/Resetting the appropriate bits in this
        object.

        Setting a bit to '1' means that the alert group
        is configured and alerts for this alert group
        would be sent to the destination profile.

        Resetting a bit to '0', means that alert group
        is not configured and alerts for this alert group
        would not be sent to the destination profile." 
    ::= { callHomeDestProfileEntry 7 }

callHomeDestProfileActive OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The object specifies whether the profile is active.

        A value of 'true' indicates that the profile is active.

        A value of 'false' indicates that the profile is not
        active."
    DEFVAL          { true } 
    ::= { callHomeDestProfileEntry 8 }

callHomeDestProfileHiMaxMsgSize OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "bytes"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Maximum size of the message that can be sent to destination
        pointed to by this destination profile.

        A value of zero for this object indicates that there is no
        limitation on maximum size of message that can be sent to
        destination pointed to by this destination profile." 
    ::= { callHomeDestProfileEntry 9 }
 


callHomeEmailAddrTblMaxEntries OBJECT-TYPE
    SYNTAX          Unsigned32 (0..65535)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum number of entries that the agent supports in
        the callHomeDestEmailAddressTable.

        A value of zero indicates no limitation on the number of entries
        in callHomeDestEmailAddressTable." 
    ::= { ccmCallHomeConfiguration 13 }
-- callHomeDestEmailAddressTable

callHomeDestEmailAddressTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CallHomeDestEmailAddressEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains email addresses and HTTP URLs
        for the destination profiles."
    ::= { ccmCallHomeConfiguration 14 }

callHomeDestEmailAddressEntry OBJECT-TYPE
    SYNTAX          CallHomeDestEmailAddressEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing information about a Call Home
        destination email address or a destination HTTP URL."
    INDEX           {
                        callHomeDestProfileName,
                        callHomeDestEmailAddressIndex
                    } 
    ::= { callHomeDestEmailAddressTable 1 }

CallHomeDestEmailAddressEntry ::= SEQUENCE {
        callHomeDestEmailAddressIndex  Unsigned32,
        callHomeDestEmailAddress       SnmpAdminString,
        callHomeDestEmailAddressStatus RowStatus,
        callHomeDestType               INTEGER,
        callHomeDestHttpUrl            CiscoURLString
}

callHomeDestEmailAddressIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..65535)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An arbitrary integer value, greater than zero, and less
        than and equal to callHomeEmailAddrTblMaxEntries, which 
        identifies an Email address. 

        The object can be any value in the supported range if the 
        value of callHomeEmailAddrTblMaxEntries is zero.

        These integer values should be non-volatile." 
    ::= { callHomeDestEmailAddressEntry 1 }

callHomeDestEmailAddress OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The email address associated this destination profile. The
        format of this object is an e-mail address which conforms
        to RFC822 and RFC1123 'addr-spec' syntax. Some examples are
                       raj@helpme.com,
                       bob@service.com,
                       mtom@abc.caview.ca.us.
        A set operation on this object with a invalid format will
        result in an error.

        This object may not be modified while the value of the
        corresponding instance of callHomeDestEmailAddressStatus is
        'active'." 
    ::= { callHomeDestEmailAddressEntry 2 }

callHomeDestEmailAddressStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Status of this row." 
    ::= { callHomeDestEmailAddressEntry 3 }

callHomeDestType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        email(1),
                        http(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The type of this destination address.

        email - This destination address is an email address.
                Object callHomeDestHttpUrl is irrelevant and
                can not be set.
        http  - This destination address is an HTTP URL address.
                Object callHomeDestEmailAddress is irrelevant and
                can not be set.

        This object may not be modified while the value of the
        corresponding instance of callHomeDestEmailAddressStatus is
        'active'."
    DEFVAL          { email } 
    ::= { callHomeDestEmailAddressEntry 4 }

callHomeDestHttpUrl OBJECT-TYPE
    SYNTAX          CiscoURLString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The HTTP URL associated with this destination profile.

        This object may not be modified while the value of the
        corresponding instance of callHomeDestEmailAddressStatus is
        'active'." 
    ::= { callHomeDestEmailAddressEntry 5 }
 


-- Transport configurations

callHomeEmailFrom OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The email address that is to be used in the 'From' field
        when sending the email using SMTP. The format of this object
        is an e-mail address which conforms to RFC822 and RFC1123 
        'addr-spec' syntax.
        Some examples are
                       raj@helpme.com,
                       bob@service.com,
                       mtom@abc.caview.ca.us.
        A set operation on this object with a invalid format will
        result in an error."
    REFERENCE
        "RFC 2821 - Simple Mail Transfer Protocol and 
               RFC822 - Standard for the Format of Arpa Internet Text 
               Messages." 
    ::= { ccmCallHomeConfiguration 15 }

callHomeEmailReplyTo OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The email address that is to be used in the 'Reply-To'
        field when sending the email using SMTP. The format of 
        this object is an e-mail address which conforms to RFC822 
        and RFC1123 'addr-spec' syntax.
        Some examples are
                       raj@helpme.com,
                       bob@service.com,
                       mtom@abc.caview.ca.us.
        A set operation on this object with a invalid format will
        result in an error."
    REFERENCE
        "RFC 2821 - Simple Mail Transfer Protocol and 
               RFC822 - Standard for the Format of Arpa Internet Text 
               Messages." 
    ::= { ccmCallHomeConfiguration 16 }

callHomeEmailMsgDispNotification OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The email address to which the Message Disposition
        Notification (also called 'Return Receipt') sent when the 
        email sent from this device is read by the receiver. The 
        format of this object is an e-mail address which conforms
        to RFC822 and RFC1123 'addr-spec' syntax.
        Some examples are
                       raj@helpme.com,
                       bob@service.com,
                       mtom@abc.caview.ca.us.
        A set operation on this object with a invalid format will
        result in an error."
    REFERENCE
        "RFC 2298 - An Extensible Message Format
               for Message Disposition Notifications." 
    ::= { ccmCallHomeConfiguration 17 }

callHomeSmtpServerAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Address Type of the SMTP server." 
    ::= { ccmCallHomeConfiguration 18 }

callHomeSmtpServerAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Address of the SMTP server."
    REFERENCE       "RFC 2821 - Simple Mail Transfer Protocol." 
    ::= { ccmCallHomeConfiguration 19 }

callHomeSmtpServerPort OBJECT-TYPE
    SYNTAX          Unsigned32 (1..65535)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Port of the SMTP server."
    REFERENCE       "RFC 2821 - Simple Mail Transfer Protocol."
    DEFVAL          { 25 } 
    ::= { ccmCallHomeConfiguration 20 }

-- -
-- - Call Home multiple smtp server configuration
-- -

ccmSmtpServersTblMaxEntries OBJECT-TYPE
    SYNTAX          Unsigned32 (0..65535)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Indicates the maximum number of SMTP servers supported by
        this device.  A value of zero indicates no limitation on
        the number of SMTP servers." 
    ::= { ccmCallHomeConfiguration 21 }

ccmSmtpServersTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CcmSmtpServersEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains a list of SMTP servers that may be
        used to send out Call Home e-mail messages.

        An entry is created and deleted by using ccmSmtpServersStatus.

        The maximum number of entries that can be created in this
        table is limited by the object ccmSmtpServersTblMaxEntries."
    ::= { ccmCallHomeConfiguration 22 }

ccmSmtpServersEntry OBJECT-TYPE
    SYNTAX          CcmSmtpServersEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing information about an SMTP server."
    INDEX           {
                        ccmSmtpServersAddrType,
                        ccmSmtpServersAddr
                    } 
    ::= { ccmSmtpServersTable 1 }

CcmSmtpServersEntry ::= SEQUENCE {
        ccmSmtpServersAddrType InetAddressType,
        ccmSmtpServersAddr     InetAddress,
        ccmSmtpServersPort     Unsigned32,
        ccmSmtpServersStatus   RowStatus,
        ccmSmtpServersPriority Unsigned32,
        ccmSmtpServersUseVrf   CiscoVrfName
}

ccmSmtpServersAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Address Type of the SMTP server." 
    ::= { ccmSmtpServersEntry 1 }

ccmSmtpServersAddr OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (1..64))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Address of the SMTP server."
    REFERENCE       "RFC 2821 - Simple Mail Transfer Protocol." 
    ::= { ccmSmtpServersEntry 2 }

ccmSmtpServersPort OBJECT-TYPE
    SYNTAX          Unsigned32 (1..65535)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Port of the SMTP server."
    REFERENCE       "RFC 2821 - Simple Mail Transfer Protocol."
    DEFVAL          { 25 } 
    ::= { ccmSmtpServersEntry 3 }

ccmSmtpServersStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The status object used to manage the rows in this table.

        Objects in this conceptual row may not be modified while the
        value of this object is 'active'." 
    ::= { ccmSmtpServersEntry 4 }

ccmSmtpServersPriority OBJECT-TYPE
    SYNTAX          Unsigned32 (1..100)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The priority of this entry relative to other entries.
        System will attempt to contact SMTP servers in the order of
        their priority values.

        For servers with different values of ccmSmtpServersPriority,
        the server with lowest value has highest priority.

        For servers with same value of ccmSmtpServersPriority
        the relative priority is determined by the system."
    DEFVAL          { 50 } 
    ::= { ccmSmtpServersEntry 5 }

ccmSmtpServersUseVrf OBJECT-TYPE
    SYNTAX          CiscoVrfName
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The Virtual Routing and Forwarding (VRF) domain configured
        for this SMTP server. A zero length string indicates that 
        there is no VRF domain configured and the default VRF domain
        is used"
    DEFVAL          { "default" } 
    ::= { ccmSmtpServersEntry 6 }
 


-- Call Home statistics

callHomeLastAlertSent OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The value of sysUpTime when the last Call Home alert
        was sent." 
    ::= { ccmCallHomeStats 1 }

callHomeAlerts OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of  Call Home alerts sent." 
    ::= { ccmCallHomeStats 2 }

callHomeHCAlerts OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of Call Home alerts sent. This object is a 64-bit
        version of callHomeAlerts" 
    ::= { ccmCallHomeStats 3 }

ccmAlertsDropped OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of Call Home alerts dropped due to rate
        limiting configured through ccmAlertRateLimit." 
    ::= { ccmCallHomeStats 4 }

ccmEventStatsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CcmEventStatsEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains a list of Call Home message type for
        each Call Home event.

        An entry will exist for each call-home message type which
        supports Call Home event statistics."
    ::= { ccmCallHomeStats 5 }

ccmEventStatsEntry OBJECT-TYPE
    SYNTAX          CcmEventStatsEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing Call Home event statistics for a particular
        Call Home message type."
    INDEX           {
                        ccmEventStatsTypeIndex,
                        ccmEventStatsMsgTypeIndex
                    } 
    ::= { ccmEventStatsTable 1 }

CcmEventStatsEntry ::= SEQUENCE {
        ccmEventStatsTypeIndex     INTEGER,
        ccmEventStatsMsgTypeIndex  INTEGER,
        ccmEventStatsTotal         Counter64,
        ccmEventStatsConfiguration Counter64,
        ccmEventStatsDiagnostic    Counter64,
        ccmEventStatsEnvironment   Counter64,
        ccmEventStatsInventory     Counter64,
        ccmEventStatsSystemLog     Counter64,
        ccmEventStatsTest          Counter64,
        ccmEventStatsRequest       Counter64,
        ccmEventStatsSendCliOutput Counter64
}

ccmEventStatsTypeIndex OBJECT-TYPE
    SYNTAX          INTEGER  {
                        successful(1),
                        inQueue(2),
                        dropped(3),
                        failed(4)
                    }
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the type of Call Home event.

        'successful' - Call Home messages were generated successfully
                       for corresponding Call Home event.

        'inQueue'    - Call Home events are queued for processing.

        'dropped'    - Call Home events were dropped due to the Rate
                       Limiting feature within Call Home component.

        'failed'     - Call Home events which failed to generate 
                       Call Home messages." 
    ::= { ccmEventStatsEntry 1 }

ccmEventStatsMsgTypeIndex OBJECT-TYPE
    SYNTAX          INTEGER  {
                        total(1),
                        email(2),
                        http(3)
                    }
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the type of Call Home message.

        'total' - statistics based on all the message types.

        'email' - statistics for Call Home messages which use
                  e-mail transport.

        'http'  - statistics for Call Home messages which use
                  http transport." 
    ::= { ccmEventStatsEntry 2 }

ccmEventStatsTotal OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Total number of Call Home events." 
    ::= { ccmEventStatsEntry 3 }

ccmEventStatsConfiguration OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of Configuration Call Home events." 
    ::= { ccmEventStatsEntry 4 }

ccmEventStatsDiagnostic OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of Diagnostic Call Home events." 
    ::= { ccmEventStatsEntry 5 }

ccmEventStatsEnvironment OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of Environment Call Home events." 
    ::= { ccmEventStatsEntry 6 }

ccmEventStatsInventory OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of Inventory Call Home events." 
    ::= { ccmEventStatsEntry 7 }

ccmEventStatsSystemLog OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of System Log Call Home events." 
    ::= { ccmEventStatsEntry 8 }

ccmEventStatsTest OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of Test Call Home events." 
    ::= { ccmEventStatsEntry 9 }

ccmEventStatsRequest OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of Request Call Home events." 
    ::= { ccmEventStatsEntry 10 }

ccmEventStatsSendCliOutput OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of Send-CLI-Output Call Home events." 
    ::= { ccmEventStatsEntry 11 }
 


-- Call Home Status Objects

ccmSmtpServerStatusTimeStamp OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the time when ccmSmtpServerStatusTable
        was last updated, either by a SNMP Servers check by 
        ccmSmtpServerStatusInitiate or by a change in the SMTP
        servers configured in ccmSmtpServersTable." 
    ::= { ccmCallHomeStatus 1 }

ccmSmtpServerStatusInitiate OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "A control object used to initiate the availability status
        check of the SMTP Servers configured in ccmSmtpServersTable.

        Setting this object to 'true' will check the status of
        the SMTP servers and update the status in 
        ccmSmtpServerStatusTable. This object cannot be set to 'true'
        when the value of ccmSmtpServerStatusResult is 'inprogress'.

        Setting this object to 'false' has no effect.

        When read, this object always returns 'false'." 
    ::= { ccmCallHomeStatus 2 }

ccmSmtpServerStatusResult OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        successful(2),
                        inprogress(3),
                        failed(4),
                        noSmtpServerConfigured(5)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides the status of the last SMTP status
        check initiated by ccmSmtpServerStatusInitiate.

        Management stations could read value of this object after a
        successful set of the ccmSmtpServerStatusInitiate object to
        find out the result of the SMTP server status check." 
    ::= { ccmCallHomeStatus 3 }

ccmSmtpServerStatusTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CcmSmtpServerStatusEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A list of SMTP servers.  An entry will exist for each SMTP
        server which is configured in the ccmSmtpServersTable if the
        value of ccmSmtpServerStatusResult is 'successful'."
    ::= { ccmCallHomeStatus 4 }

ccmSmtpServerStatusEntry OBJECT-TYPE
    SYNTAX          CcmSmtpServerStatusEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing availability status of a particular
        SMTP Server."
    INDEX           {
                        ccmSmtpServersAddrType,
                        ccmSmtpServersAddr
                    } 
    ::= { ccmSmtpServerStatusTable 1 }

CcmSmtpServerStatusEntry ::= SEQUENCE {
        ccmSmtpServerStatusAvailability INTEGER
}

ccmSmtpServerStatusAvailability OBJECT-TYPE
    SYNTAX          INTEGER  {
                        available(1),
                        notAvailable(2),
                        unknown(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This variable indicates whether the SMTP Server
        is currently available." 
    ::= { ccmSmtpServerStatusEntry 1 }
 


ccmOnDemandMsgServAvailable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates whether the system is ready to generate
        on demand Call Home messages.

        A value of 'true' indicates that the system is ready to generate
        on demand Call Home messages. A value of 'false' indicates that
        sending of on demand Call Home messages can not be initiated." 
    ::= { ccmCallHomeStatus 5 }

ccmSysLogSeverity OBJECT-TYPE
    SYNTAX          SyslogSeverity
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Different devices implementing this mib may use
        different criteria for issuing Call Home alerts.

        For the devices that issue Call Home alerts based on
        severity level of the syslog messages generated on
        the device, this object determines syslog severity
        levels beyond which a Call Home alert message will be
        issued.

        Any syslog message with a severity value greater than
        the value set for this object will be ignored by the agent.
        Note: severity numeric values increase as their
        severity decreases, e.g. error(4) is more severe
        than debug(8).

        For the devices that do not issue Call Home alerts based
        on syslog severity levels this object has no effect." 
    ::= { ccmCallHomeConfiguration 23 }

ccmEnableSmtpServerNotif OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This variable indicates whether the system produces
        the ccmSmtpServerFailNotif.

        A false value for this object will prevent
        ccmSmtpServerFailNotif notification being generated
        by the device." 
    ::= { ccmCallHomeConfiguration 24 }
-- Call Home Alert Group Type Table

callHomeAlertGroupTypeTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CallHomeAlertGroupTypeEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains information about all the alert groups
        types supported in the system.

        An entry is created if a new alert group becomes available
        in the system.

        An entry is deleted if the alert group becomes unavailable."
    ::= { ccmCallHomeConfiguration 25 }

callHomeAlertGroupTypeEntry OBJECT-TYPE
    SYNTAX          CallHomeAlertGroupTypeEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing information about a
        particular Call Home alert group type 
        in the system."
    INDEX           { callHomeAlertGroupTypeIndex } 
    ::= { callHomeAlertGroupTypeTable 1 }

CallHomeAlertGroupTypeEntry ::= SEQUENCE {
        callHomeAlertGroupTypeIndex  Unsigned32,
        callHomeAlertGroupName       SnmpAdminString,
        callHomeAlertGroupEnable     TruthValue,
        callHomeAlertGroupCapability BITS
}

callHomeAlertGroupTypeIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..256)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the index corresponding
        to the particular alert group type configured 
        in the system." 
    ::= { callHomeAlertGroupTypeEntry 1 }

callHomeAlertGroupName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..255))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the name of
        alert group configured in the system." 
    ::= { callHomeAlertGroupTypeEntry 2 }

callHomeAlertGroupEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object enables or disables the alert group for the
        system.

        A value of 'true' for this object enables and a value of
        'false' for this object disables the alert group.

        Call Home messages are generated only for those alert groups
        which are enabled in the system." 
    ::= { callHomeAlertGroupTypeEntry 3 }

callHomeAlertGroupCapability OBJECT-TYPE
    SYNTAX          BITS {
                        callHomeMessageSeverity(0),
                        periodic(1),
                        regularExpression(2),
                        event(3),
                        onDemand(4),
                        onDemandPerEntity(5),
                        periodicHourly(6),
                        periodicMinutes(7)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the method used by alert group
        to generate Call Home messages.

        callHomeMessageSeverity -
            Call Home alert is generated based only on the level
            of severity.

        periodic - 
            Call Home alert is generated periodically.

        regularExpression -
            Call Home alert is generated based on the configured
            regular expression.

        event - 
            Call Home alert is generated based on change event.

        onDemand -
            Call Home alert is generated at user request.

        onDemandPerEntity -
            Call Home alert is generated for specific entities
            at user request.

        periodicHourly -
            Call Home alert is generated hourly.

        periodicMinutes -
            Call Home alert is generated periodically after
            specified number of minutes." 
    ::= { callHomeAlertGroupTypeEntry 4 }
 

-- Call Home Software Inventory Table

callHomeSwInventoryTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CallHomeSwInventoryEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains inventory information about all the
        software services currently enabled in the system.
        When a software service is disabled from the system, all
        the entries corresponds to that software service will be
        deleted automatically from the table."
    ::= { ccmCallHomeConfiguration 26 }

callHomeSwInventoryEntry OBJECT-TYPE
    SYNTAX          CallHomeSwInventoryEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing information about the name value
        pair for a particular software service enabled in the
        system."
    INDEX           {
                        callHomeSwServiceName,
                        callHomeInventoryNVPairIndex
                    } 
    ::= { callHomeSwInventoryTable 1 }

CallHomeSwInventoryEntry ::= SEQUENCE {
        callHomeSwServiceName        SnmpAdminString,
        callHomeInventoryNVPairIndex Unsigned32,
        callHomeInventoryInfoName    OCTET STRING,
        callHomeInventoryInfoValue   OCTET STRING
}

callHomeSwServiceName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the name of software service
        enabled in the system." 
    ::= { callHomeSwInventoryEntry 1 }

callHomeInventoryNVPairIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..256)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the index corresponds to the name
        value pair for a particular software service enabled in
        the system. 
        The name value pair is a 'tuple' of (inventory info-name, 
        and inventory info-value) and this object uniquely 
        identifies a value of the tuple, for a particular
        software service enabled in the system." 
    ::= { callHomeSwInventoryEntry 2 }

callHomeInventoryInfoName OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (1..1024))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the name of a feature , for a
        particular software service enabled in the system.
        For example, the value of this object could be
        'number of VSAN' for the software service 'vsan_manager'." 
    ::= { callHomeSwInventoryEntry 3 }

callHomeInventoryInfoValue OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (1..1024))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the value for the feature name
        specified in the corresponding instance of
        'callHomeInventroyInfoName' object.
        For example, the value of this object could be '10' for
        the corresponding instance of 'callHomeInventroyInfoName'
        object with value 'number of VSAN'." 
    ::= { callHomeSwInventoryEntry 4 }
 


-- Objects for Enabling Periodic Software Inventory
-- Call Home Messages

ccmPeriodicSwInventoryMsgEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object enables/disables the sending of periodic
        software inventory Call Home message on the system."
    DEFVAL          { true } 
    ::= { ccmCallHomeConfiguration 27 }

ccmPeriodicSwInventoryTimeFrame OBJECT-TYPE
    SYNTAX          Unsigned32 (1..30)
    UNITS           "days"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the time frame for sending the
        periodic software inventory Call Home message, if the
        periodic software inventory is enabled on the system
        i.e., the value of 'ccmPeriodicSwInventoryMsgEnable'
        object  is set to 'true'."
    DEFVAL          { 7 } 
    ::= { ccmCallHomeConfiguration 28 }

-- Object to Enable Message Throttling Mechanism.

ccmMsgThrottlingEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object enables/disables the message throttling
        mechanism implemented on the system.

        The message throttling mechanism limits the number
        of Call Home messages for a alert type, sent with in  
        a time frame. The maximum number of Call Home alert
        messages that can be sent out for a particular alert 
        type is '30' in a time frame of 2 hours.

        That means, if the number of message sent exceeds the 
        maximum limit (30), with in the given time frame 
        (2 hours) then any further messages for that alert type 
        will be discarded within that time frame. 

        Only 30 messages for each alert type will be sent until 
        2 hours from the time the first message was sent. In case 
        2 hours has already elapsed since the first such message 
        was sent, then time frame and the count for the number of 
        messages will be reset to '0'."
    DEFVAL          { true } 
    ::= { ccmCallHomeConfiguration 29 }
ccmCallHomeAlertGroupCfg  OBJECT IDENTIFIER
    ::= { ccmCallHomeConfiguration 30 }

-- Call Home Severity Alert Group Configuration Table

ccmSeverityAlertGroupTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CcmSeverityAlertGroupEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A list of severity type alert groups which are currently
        configured for each of the profiles in the device.

        An entry is created if a configured alert group
        whose callHomeAlertGroupCapability has
        'callHomeMessageSeverity'.

        An entry is deleted if the destination profile unsubscribes
        an severity based alert group."
    ::= { ccmCallHomeAlertGroupCfg 1 }

ccmSeverityAlertGroupEntry OBJECT-TYPE
    SYNTAX          CcmSeverityAlertGroupEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing severity configuration information
        for a particular alert group in a profile."
    INDEX           {
                        callHomeDestProfileName,
                        callHomeAlertGroupTypeIndex
                    } 
    ::= { ccmSeverityAlertGroupTable 1 }

CcmSeverityAlertGroupEntry ::= SEQUENCE {
        ccmAlertGroupSeverity CallHomeMsgLevel
}

ccmAlertGroupSeverity OBJECT-TYPE
    SYNTAX          CallHomeMsgLevel
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the minimum severity level,
        associated with alert group for a destination profile.

        Call Home alert messages for this alert group with 
        severity level lower than one configured for this object
        will not be issued by the system.

        The default severity level is 'debug', which means
        all the alert messages for an alert group will be issued."
    DEFVAL          { debug } 
    ::= { ccmSeverityAlertGroupEntry 1 }
 

-- Call Home Periodic Alert Group Configuration Table

ccmPeriodicAlertGroupTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CcmPeriodicAlertGroupEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A list of periodic type alert groups which are currently
        configured in the device.

        An entry is created if a configured alert group
        whose callHomeAlertGroupCapability has 'periodic'.

        An entry is deleted if the destination profile unsubscribes
        an periodic alert group."
    ::= { ccmCallHomeAlertGroupCfg 2 }

ccmPeriodicAlertGroupEntry OBJECT-TYPE
    SYNTAX          CcmPeriodicAlertGroupEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing periodic configuration information for a
        particular alert group in a profile."
    INDEX           {
                        callHomeDestProfileName,
                        callHomeAlertGroupTypeIndex
                    } 
    ::= { ccmPeriodicAlertGroupTable 1 }

CcmPeriodicAlertGroupEntry ::= SEQUENCE {
        ccmPeriodicAlertGroupInterval        INTEGER,
        ccmPeriodicAlertGroupDayOfWeek       INTEGER,
        ccmPeriodicAlertGroupDayOfMonth      Unsigned32,
        ccmPeriodicAlertGroupHour            Unsigned32,
        ccmPeriodicAlertGroupMinute          Unsigned32,
        ccmPeriodicAlertGroupEnable          TruthValue,
        ccmPeriodicAlertGroupIntervalMinutes Unsigned32
}

ccmPeriodicAlertGroupInterval OBJECT-TYPE
    SYNTAX          INTEGER  {
                        daily(1),
                        weekly(2),
                        monthly(3),
                        hourly(4),
                        minutes(5)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the type of periodic configuration
        for this alert group.

        This object is only instantiated when the value of
        corresponding instance of ccmPeriodicAlertGroupEnable
        is 'true'.

        A value of 'daily' indicates that periodic message will be
        generated everyday at time specified by the objects
        ccmPeriodicAlertGroupHour and ccmPeriodicAlertGroupMinute.

        A value of 'weekly' indicates that periodic message will be
        generated once every week on the day specified by the object
        ccmPeriodicAlertGroupDayOfWeek and at the time specified
        by the objects ccmPeriodicAlertGroupHour and
        ccmPeriodicAlertGroupMinute.

        A value of 'monthly' indicates that periodic message will be
        generated once every month on day of the month specified by
        the object ccmPeriodicAlertGroupDayOfMonth and at time
        specified by the objects ccmPeriodicAlertGroupHour and
        ccmPeriodicAlertGroupMinute.

        A value of 'hourly' indicates that periodic messages will be
        generated once every hour. ccmPeriodicAlertGroupMinute specifies
        the minute of hour at which the hourly message is generated.

        A value of 'minutes' indicates that a message will be
        generated periodically after the interval specified in 
        ccmPeriodicAlertGroupIntervalMinutes expires."
    DEFVAL          { daily } 
    ::= { ccmPeriodicAlertGroupEntry 1 }

ccmPeriodicAlertGroupDayOfWeek OBJECT-TYPE
    SYNTAX          INTEGER  {
                        sunday(1),
                        monday(2),
                        tuesday(3),
                        wednesday(4),
                        thursday(5),
                        friday(6),
                        saturday(7)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the day of the week on which user
        wishes to receive periodic Call Home alert messages for this
        entry.

        This object is only instantiated when the value of
        corresponding instance of ccmPeriodicAlertGroupEnable
        is 'true' and the value of corresponding instance of
        ccmPeriodicAlertGroupInterval is 'weekly'."
    DEFVAL          { sunday } 
    ::= { ccmPeriodicAlertGroupEntry 2 }

ccmPeriodicAlertGroupDayOfMonth OBJECT-TYPE
    SYNTAX          Unsigned32 (1..31)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the day of the month on which user
        wishes to receive periodic Call Home alert messages for this
        entry.

        If the day specified is beyond the last day of a month, the
        alert message will be generated on the last day of that month.

        This object is only instantiated when the value of
        corresponding instance of ccmPeriodicAlertGroupEnable
        is 'true' and the value of corresponding instance of
        ccmPeriodicAlertGroupInterval is 'monthly'."
    DEFVAL          { 1 } 
    ::= { ccmPeriodicAlertGroupEntry 3 }

ccmPeriodicAlertGroupHour OBJECT-TYPE
    SYNTAX          Unsigned32 (0..23)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the hours component of time
        (24 hour format) at which the daily/weekly/monthly periodic
        Call Home alert messages will be generated for this entry.

        This object is only instantiated when the value of
        corresponding instance of ccmPeriodicAlertGroupEnable
        is 'true'."
    DEFVAL          { 0 } 
    ::= { ccmPeriodicAlertGroupEntry 4 }

ccmPeriodicAlertGroupMinute OBJECT-TYPE
    SYNTAX          Unsigned32 (0..59)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the minutes component of time at which
        the hourly/daily/weekly/monthly periodic Call Home alert
        messages will be generated for this entry.

        This object is only instantiated when the value of
        corresponding instance of ccmPeriodicAlertGroupEnable
        is 'true'."
    DEFVAL          { 0 } 
    ::= { ccmPeriodicAlertGroupEntry 5 }

ccmPeriodicAlertGroupEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether sending Call Home messages
        periodically is enabled."
    DEFVAL          { false } 
    ::= { ccmPeriodicAlertGroupEntry 6 }

ccmPeriodicAlertGroupIntervalMinutes OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "minutes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the number of minutes after which
        periodic message will be generated for this entry.

        This object is only instantiated for the alert groups for which
        callHomeAlertGroupCapability has the 'periodicMinutes' bit set
        and the ccmPeriodicAlertGroupInterval is 'minutes'."
    DEFVAL          { 60 } 
    ::= { ccmPeriodicAlertGroupEntry 7 }
 


-- Call Home Syslog Pattern Configuration

ccmMaxSyslogAlertGroupPatterns OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The object dictates the maximum number of entries in the
        ccmPatternAlertGroupTable which may be created with same
        value for index callHomeDestProfileName.

        A value of zero for this object indicates that there is no
        limitation on maximum number of entries that can be created
        in this table with same value of callHomeDestProfileName." 
    ::= { ccmCallHomeAlertGroupCfg 3 }

ccmPatternAlertGroupTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CcmPatternAlertGroupEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A list of pattern used by the pattern type alert groups
        which are currently configured in the device.

        An entry is created if a configured alert group
        whose callHomeAlertGroupCapability has 'regularExpression'.

        An entry is deleted if the destination profile unsubscribes
        a pattern based alert group.

        Additional entry can also be created through
        ccmPatternAlertGroupStatus.

        Deleting all the entries for a destination profile alert
        group combination will result in profile unsubscribing to
        that alert group."
    ::= { ccmCallHomeAlertGroupCfg 4 }

ccmPatternAlertGroupEntry OBJECT-TYPE
    SYNTAX          CcmPatternAlertGroupEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing properties for a pattern which is used
        to match against system syslog messages."
    INDEX           {
                        callHomeDestProfileName,
                        callHomeAlertGroupTypeIndex,
                        IMPLIED ccmAlertGroupPattern
                    } 
    ::= { ccmPatternAlertGroupTable 1 }

CcmPatternAlertGroupEntry ::= SEQUENCE {
        ccmAlertGroupPattern         SnmpAdminString,
        ccmPatternAlertGroupSeverity CallHomeMsgLevel,
        ccmPatternAlertGroupStorage  StorageType,
        ccmPatternAlertGroupStatus   RowStatus
}

ccmAlertGroupPattern OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..80))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The object contains a regular expression.

        Regular Expressions:
        -------------------

        A regular expression is a pattern (a phrase, number, or more
        complex pattern):

        Regular expressions are case sensitive and allow for complex
        matching requirements. Simple regular expressions include
        entries like Serial, misses, or 138.

        Complex regular expressions include entries like 00210... , 
        (is ), or [Oo]utput.

        Some Practical examples of regular expressions:
        ----------------------------------------------
        The examples correspond with the various ways that you can
        use regular expressions in your configurations.

        For example, syslog messages on IOS look as follows:
        a.
        --
        2004 Jul 21 13:26:55 %SYS-5-REDUNDANTCLOCK_OK: Redundant
        clock recovered
        b.
        --
        2004 Jul 21 13:26:59 %SYS-5-REDUNDANTCLOCK_FAIL: Redundant
        clock failed
        c.
        --
        2004 Jul 26 16:53:47 %MGMT-5-LOGIN_FAIL:User failed to log
        in from 171.69.48.75 via Telnet - max attempt reached


        A pattern of REDUNDANTCLOCK.* would cause all the syslogs 
        with severity greater than specified by
        ccmProfileAlertGroupSeverity
        and having a pattern  REDUNDANTCLOCK followed by
        REDUNDANTCLOCK followed by any number of occurrences (*)
        of any character (.) resulting in corresponding Call Home
        messages being generated for syslog alert group.

        So both messages a and b in above examples will be resulting
        in issuance of Call Home messages for the pattern 
        REDUNDANTCLOCK.*.

        Next, a pattern of ^Telnet would cause all the syslogs 
        with severity greater than specified by
        ccmProfileAlertGroupSeverity and having a string starting 
        and with Telnet resulting in corresponding Call Home
        messages being generated for syslog alert group.

        A pattern of LOGIN_FAIL$ would cause all the syslogs with
        severity greater than specified by 
        ccmProfileAlertGroupSeverity and having a string ending in
        LOGIN_FAIL resulting in corresponding Call Home messages
        being generated for syslog alert group." 
    ::= { ccmPatternAlertGroupEntry 1 }

ccmPatternAlertGroupSeverity OBJECT-TYPE
    SYNTAX          CallHomeMsgLevel
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the severity level, used for
        filtering Call Home messages in conjunction with 
        ccmAlertGroupPattern to be issued to destinations
        associated with this entry.

        Call Home alert messages for this alert group, with
        severity level lower than one configured for this object
        will not be issued by the system.

        The default severity level is 'debug', which means
        all the alert messages will be sent."
    DEFVAL          { debug } 
    ::= { ccmPatternAlertGroupEntry 2 }

ccmPatternAlertGroupStorage OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The storage type for this conceptual row."
    DEFVAL          { volatile } 
    ::= { ccmPatternAlertGroupEntry 3 }

ccmPatternAlertGroupStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Object to manage creation and deletion of rows in this table." 
    ::= { ccmPatternAlertGroupEntry 4 }
 


-- Call Home User Specified CLI Command specifications table

callHomeUserDefMaxCmds OBJECT-TYPE
    SYNTAX          Unsigned32 (0..65535)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum number of CLI commands that the system
        supports
        in the callHomeUserDefCmdTable for a particular alert
        group type represented by the
        callHomeAlertGroupTypeIndex object.

        A value of zero for this object indicates that the number
        of CLI commands system supports for a particular alert
        group type is only limited by resources available on
        system." 
    ::= { ccmCallHomeAlertGroupCfg 5 }

ccmEventDescription OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates the description of the Call Home
        event that occurred in the system." 
    ::= { ccmCallhomeEvents 1 }

ccmEventTime OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object indicates Time when the last
        Call Home alert was triggered." 
    ::= { ccmCallhomeEvents 2 }

ccmEventUrgencyLevel OBJECT-TYPE
    SYNTAX          CallHomeMsgLevel
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object specifies the minimum urgency level, associated
        with Call Home event that occurred in the system." 
    ::= { ccmCallhomeEvents 3 }

callHomeUserDefCmdTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CallHomeUserDefCmdEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Call Home alert messages are sent with output of some
        pre-defined commands run in the system.

        This table provides an option for the user to specify
        a CLI(Command Line Interface) command or set of CLI
        commands to be executed when some important failures
        occur in the system, and whose output should be sent
        with the Call Home alert messages. The user should
        associate these commands with an alert group type.

        Whenever an alert message is to be sent, the Call Home
        server would find out if any commands are specified by
        the user for the alert group associated with the
        alert message, and attach the output of those
        commands in the Call Home alert message.

        This table contains information about all the user
        specified CLI commands for the alert groups types
        supported in the system.

        GLOSSARY :
        CLI - Command Line Interface provided by the system."
    ::= { ccmCallHomeAlertGroupCfg 6 }

callHomeUserDefCmdEntry OBJECT-TYPE
    SYNTAX          CallHomeUserDefCmdEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing information about a user specified
        CLI command for a Call Home alert group type in
        the system.

        The index object 'callHomeAlertGroupTypeIndex' represents
        the alert group type to which the user specified CLI
        command should be associated.

        User can not configure any CLI commands for a
        callHomeAlertGroupTypeIndex, whose corresponding
        instance callHomeAlertGroupName object is configured
        with value 'Cisco-TAC'."
    INDEX           {
                        callHomeAlertGroupTypeIndex,
                        callHomeUserDefCmdIndex
                    } 
    ::= { callHomeUserDefCmdTable 1 }

CallHomeUserDefCmdEntry ::= SEQUENCE {
        callHomeUserDefCmdIndex     Unsigned32,
        callHomeUserDefCmdName      SnmpAdminString,
        callHomeUserDefCmdRowStatus RowStatus
}

callHomeUserDefCmdIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An arbitrary integer identifying the user specified
        CLI command for a particular callHomeAlertGroupTypeIndex." 
    ::= { callHomeUserDefCmdEntry 1 }

callHomeUserDefCmdName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..255))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents a CLI command to be executed
        and whose output should be sent with the Call Home
        alert message.
        The implementation of this object does not do any 
        syntax or semantic validation of the CLI command 
        specified as a value of the object. 

        The value of this object can not be modified
        when the value of the corresponding instance of
        'callHomeUserDefCmdRowStatus' is 'active'.
        To modify the value this object the corresponding
        entry must be deleted and re-created with new
        value for this object." 
    ::= { callHomeUserDefCmdEntry 2 }

callHomeUserDefCmdRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Status of this row." 
    ::= { callHomeUserDefCmdEntry 3 }
 

-- Call Home Event Alert Group Configuration Table

ccmEventAlertGroupTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CcmEventAlertGroupEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A list of event type alerts groups which are currently
        configured in the device.

        An entry is created if a configured alert group 
        whose callHomeAlertGroupCapability has 'event'.

        An entry is deleted if the destination profile unsubscribes
        an event alert group."
    ::= { ccmCallHomeAlertGroupCfg 7 }

ccmEventAlertGroupEntry OBJECT-TYPE
    SYNTAX          CcmEventAlertGroupEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing configuration information about the
        'event' alert group configured for a profile."
    INDEX           {
                        callHomeDestProfileName,
                        callHomeAlertGroupTypeIndex
                    } 
    ::= { ccmEventAlertGroupTable 1 }

CcmEventAlertGroupEntry ::= SEQUENCE {
        ccmEventAlertGroupEnable       TruthValue,
        ccmEventAlertGroupOperSeverity CallHomeMsgLevel
}

ccmEventAlertGroupEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether sending Call Home messages
        based on alert group event is enabled."
    DEFVAL          { true } 
    ::= { ccmEventAlertGroupEntry 1 }

ccmEventAlertGroupOperSeverity OBJECT-TYPE
    SYNTAX          CallHomeMsgLevel
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the severity level used in the
        Call Home messages." 
    ::= { ccmEventAlertGroupEntry 2 }
 

ccmCallHomeProfileTestControl  OBJECT IDENTIFIER
    ::= { ccmCallHomeConfiguration 31 }


ccmDestProfileTestTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CcmDestProfileTestEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table lists status information about the profiles
        configured on this device.

        An entry will be created in this table, for each
        destination profile configured in callHomeDestProfileTable.

        An entry will be deleted from this table if a destination
        profile is removed from callHomeDestProfileTable."
    ::= { ccmCallHomeProfileTestControl 1 }

ccmDestProfileTestEntry OBJECT-TYPE
    SYNTAX          CcmDestProfileTestEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing control and status information
        pertaining to test on a destination profile."
    INDEX           { callHomeDestProfileName } 
    ::= { ccmDestProfileTestTable 1 }

CcmDestProfileTestEntry ::= SEQUENCE {
        ccmDestProfileTestTrigger      TruthValue,
        ccmDestProfileTestMessage      SnmpAdminString,
        ccmDestProfileTestStatus       INTEGER,
        ccmDestProfileTestFailureCause SnmpAdminString
}

ccmDestProfileTestTrigger OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object acts as a trigger by which the generation of
        test message for a profile can be triggered.

        Setting this object to 'true' will cause system to generate
        a test message for a corresponding destination profile.

        Setting this object to 'false' has no effect.

        When read, this object always returns 'false'." 
    ::= { ccmDestProfileTestEntry 1 }

ccmDestProfileTestMessage OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the content of the message
        used for the test operation.

        If this object contains zero-length string,
        a default test message will be used." 
    ::= { ccmDestProfileTestEntry 2 }

ccmDestProfileTestStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        successful(2),
                        inprogress(3),
                        failed(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides the status of the last test
        triggered for this destination profile.

           unknown (1)     - unknown
           successful (2)  - successful
           inprogress (3)  - action in progress
           failed (4)      - failed

        If the value of this object is 'failed', then the
        ccmDestProfileTestFailureCause provides the cause for the
        failure.

        Management stations could read value of this object after a
        successful set to the ccmDestProfileTestTrigger object to 
        find out the result of the test." 
    ::= { ccmDestProfileTestEntry 3 }

ccmDestProfileTestFailureCause OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides the failure cause for the last
        test performed on this profile.

        Note that this object is valid only if value of
        ccmDestProfileTestStatus is 'failed'." 
    ::= { ccmDestProfileTestEntry 4 }
 

ccmCallHomeNotifConfig  OBJECT IDENTIFIER
    ::= { ccmCallHomeConfiguration 32 }


ccmSmtpMsgSendFailNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This variable controls generation of
        ccmSmtpMsgSendFailNotif. 

        A value of 'true' for this object will enable
        ccmSmtpMsgSendFailNotif notification on the
        system.

        A value of 'false' for this object will disable
        ccmSmtpMsgSendFailNotif notification on the 
        system." 
    ::= { ccmCallHomeNotifConfig 1 }
ccmPeriodicSwInventoryCfg  OBJECT IDENTIFIER
    ::= { ccmCallHomeConfiguration 33 }


ccmPeriodicSwInventoryTimeOfDay OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (5))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the time of day for sending the
        periodic software inventory Call Home message, if the
        periodic software inventory is enabled on the system
        i.e., the value of 'ccmPeriodicSwInventoryMsgEnable'
        object is set to 'true'. The input should be in HH:MM
        format ranging from 00:00 to 23:59."
    DEFVAL          { "08:00" } 
    ::= { ccmPeriodicSwInventoryCfg 1 }

ccmAlertRateLimit OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "alerts per minute"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The rate-limit, in alerts per minute, of call home
        alerts generated by the system.  Upon exceeding the rate,
        the alert is dropped." 
    ::= { ccmCallHomeConfiguration 34 }

ccmHttpProxyServerAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the type of the HTTP proxy server as
        represented by the value 'ccmHttpProxyServerAddr'." 
    ::= { ccmCallHomeConfiguration 35 }

ccmHttpProxyServerAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the address of the HTTP proxy server.
        The type of this address is indicated by the value of 
        'ccmHttpProxyServerAddrType'." 
    ::= { ccmCallHomeConfiguration 36 }

ccmHttpProxyServerPort OBJECT-TYPE
    SYNTAX          Unsigned32 (1..65535)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the port of the HTTP proxy server." 
    ::= { ccmCallHomeConfiguration 37 }

ccmHttpProxyServerUseEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object enables/disables the use of HTTP proxy
        server configured for sending callhome messages over HTTP.

        A value of 'true' specifies that proxy server will be
        used. 

        A value of 'false' specifies that the proxy server will
        not be used." 
    ::= { ccmCallHomeConfiguration 38 }

callHomeSmtpServerUseVrf OBJECT-TYPE
    SYNTAX          CiscoVrfName
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The Virtual Routing and Forwarding (VRF) domain configured
        for this SMTP server. A zero length string indicates that 
        there is no VRF domain configured and the default VRF domain
        is used

        A 'set' operation with zero length string indicates that there
        is no VRF domain configured. A subsequent 'get' operation on
        this object will return 'default'"
    DEFVAL          { "default" } 
    ::= { ccmCallHomeConfiguration 39 }

ccmHttpTransportUseVrf OBJECT-TYPE
    SYNTAX          CiscoVrfName
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The Virtual Routing and Forwarding (VRF) domain configured
        for HTTP transport in Call Home. A zero length string 
        indicates that there is no VRF domain configured and the 
        default VRF domain is used

        A 'set' operation with zero length string indicates that there
        is no VRF domain configured. A subsequent 'get' operation on
        this object will return 'default'"
    DEFVAL          { "default" } 
    ::= { ccmCallHomeConfiguration 40 }
ccmOnDemandMsgSendControl  OBJECT IDENTIFIER
    ::= { ccmCallHomeOnDemandActions 1 }


ccmOnDemandMsgSendAlertGroup OBJECT-TYPE
    SYNTAX          Unsigned32 (1..256)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object specifies the alert group for which on demand
        Call Home message should be generated.

        Only those alert groups whose corresponding instance
        of callHomeAlertGroupCapability has 'onDemand' or
        'onDemandPerEntity', may be set for this object.

        Value of this object should be ignored if the value of
        ccmOnDemandMessageType is other than 'alertGroup'." 
    ::= { ccmOnDemandMsgSendControl 1 }

ccmOnDemandMsgSendProfile OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..31))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the name of the profile for which
        the on demand Call Home messages should be generated.

        A zero length string for this object indicates that
        on demand Call Home messages are generated for all profiles.

        Value of this object should be ignored if the value of
        ccmOnDemandMessageType is other than 'alertGroup'." 
    ::= { ccmOnDemandMsgSendControl 2 }

ccmOnDemandMsgSendEntPhyIndex OBJECT-TYPE
    SYNTAX          EntPhysicalIndexOrZero
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the value of entPhysicalIndex of the
        physical entity for which the on demand Call Home messages
        should be generated.

        Only those entities which support generation of on demand
        Call Home messages may be specified for this object. 

        The value of this object should be ignored if alert group
        specified by ccmOnDemandMsgSendAlertGroup does not have
        'onDemandPerEntity' capability.

        Value of this object should be ignored if the value of
        ccmOnDemandMessageType is other than 'alertGroup'." 
    ::= { ccmOnDemandMsgSendControl 3 }

ccmOnDemandMsgSendTrigger OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Object to trigger on demand Call Home messages.

        Setting the object to 'true' triggers on demand Call Home
        messages.

        Setting the object to 'false' has no effect.

        When read, this object always returns 'false'." 
    ::= { ccmOnDemandMsgSendControl 4 }
ccmOnDemandCliMsgControl  OBJECT IDENTIFIER
    ::= { ccmCallHomeOnDemandActions 2 }


ccmOnDemandCliMsgCliList OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object specifies a list of commands that will be executed
        and the output of which will be part of on demand Call Home
        message.

        The list contains one or more commands which are separated by
        ';'.

        Examples of command list: 
          - show version
          - show version;show module;show vlan" 
    ::= { ccmOnDemandCliMsgControl 1 }

ccmOnDemandCliMsgTransport OBJECT-TYPE
    SYNTAX          INTEGER  {
                        email(1),
                        http(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object specifies the transport method used to deliver the
        on demand Call Home messages with CLI output.

        'email'      -- Indicates that on demand message will be
                        delivered via e-mail.

        'http'       -- Indicates that on demand message will be
                        delivered via HTTP." 
    ::= { ccmOnDemandCliMsgControl 2 }

ccmOnDemandCliMsgEmail OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object specifies the e-mail address to which the on demand
        Call Home message with CLI output will be sent if
        ccmOnDemandCliMsgTransport is 'email'.

        The object specifies the e-mail address to which the
        Smart Call Home backend will forward the on demand Call Home
        message with CLI output if ccmOnDemandCliMsgTransport is
        'http'." 
    ::= { ccmOnDemandCliMsgControl 3 }

ccmOnDemandCliMsgFormat OBJECT-TYPE
    SYNTAX          CallHomeMsgFormat
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the format of the on demand Call Home
        message with CLI output." 
    ::= { ccmOnDemandCliMsgControl 4 }

ccmOnDemandCliMsgTacServiceReqId OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the Service Request Identifier
        associated with on demand Call Home message with CLI output." 
    ::= { ccmOnDemandCliMsgControl 5 }

ccmOnDemandCliMsgTrigger OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Object to trigger on demand Call Home messages with CLI output.

        Setting the object to 'true' triggers on demand Call Home
        messages.

        Setting the object to 'false' has no effect.

        When read, this object always returns 'false'." 
    ::= { ccmOnDemandCliMsgControl 6 }

ccmSmartCallHomeProfile OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..31))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the name of the profile for which
        the Smart Call Home messages should be generated.

        A zero length string for this object indicates that the
        Smart Call Home messages are generated only for Cisco-TAC
        profile." 
    ::= { ccmSmartCallHomeActions 1 }

ccmSmartCallHomeServiceType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        commandReference(1),
                        configSanity(2),
                        bugsList(3),
                        outputAnalysis(4),
                        productAdvisory(5)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object specifies the type of service requested from
        Smart Call Home server.

        'commandReference' indicates a request for command reference
        to Smart Call Home server.

        'configSanity' indicates a request for config-sanity request
        to Smart Call Home server. 

        'bugsList' indicates a request for bugs-list
        to Smart Call Home server.

        'outputAnalysis' indicates a request for output-analysis
        to Smart Call Home server. 

        'productAdvisory' indicates a request for exceptions
        report/advisory to Smart Call Home server." 
    ::= { ccmSmartCallHomeActions 2 }

ccmSmartCallHomeAnalysisCmd OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object specifies an existing display/show command on the
        the system. The output of the command will be included in
        the Call Home message and be processed by Cisco backend OI
        (Output Interpreter) tool for further analysis.

        This object is applicable only if the value of the
        corresponding ccmSmartCallHomeServiceType is 'outputAnalysis'." 
    ::= { ccmSmartCallHomeActions 3 }

ccmSmartCallHomeCcoId OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object specifies registered CCO ID (Cisco Connection
        Online) ID to which the response to Smart Call Home requests
        should be directed.

        Response from Cisco will be directed to system contact
        address specified in the Smart Call Home request if value
        of this object is a zero length string." 
    ::= { ccmSmartCallHomeActions 4 }

ccmSmartCallHomeTrigger OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Object to trigger Smart Call Home request messages.

        Setting the object to 'true' triggers Smart Call Home
        request message.

        The object can be set to the value of 'true' only if 
        ccmOnDemandMsgServAvailable returns 'true'.

        Setting the object to 'false' has no effect.

        When read, this object always returns 'false'." 
    ::= { ccmSmartCallHomeActions 5 }

ccmCallHomeVrfName OBJECT-TYPE
    SYNTAX          CiscoVrfName
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The name of Virtual Routing and Forwarding (VRF) domain
        configured for Call Home feature.

        A zero length string indicates that there is no VRF domain
        configured and the default VRF domain is used by Call Home
        feature." 
    ::= { ccmCallHomeVrf 1 }

ccmMsgSourceIpAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The type of Internet address to be used as the source address
        while generating Call Home messages.

        Changing the value of this object may change the value of  
        ccmMsgSourceInterface." 
    ::= { ccmCallHomeMessageSource 1 }

ccmMsgSourceIpAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The Internet address to be used as the source address while
        generating Call Home messages. The type of this address is
        determined by the ccmMessageSourceIpAddrType object." 
    ::= { ccmCallHomeMessageSource 2 }

ccmMsgSourceInterface OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The interface to be used while generating Call Home messages.

        A value of zero indicates that a source interface is not
        specified.

        Changing the value of this object may change the value of
        ccmMsgSourceIpAddrType and ccmMsgSourceIpAddr." 
    ::= { ccmCallHomeMessageSource 3 }

ccmDiagSignatureActive OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object specifies if the Diagnostic Signature functionality
        of Call Home is active.

        Diagnostic signatures allow customers to download Cisco
        digitally signed signatures to devices, and call home will be
        able to support new events and new actions without upgrading
        the software.

        A value of 'true' makes the Diagnostic Signature functionality
        active." 
    ::= { ccmCallHomeDiagSignature 1 }

ccmDiagSignatureProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..31))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the profile that will use
        the Diagnostic Signature functionality.

        A zero length string for this object indicates that
        Cisco-TAC profile will use the Diagnostic Signature
        functionality." 
    ::= { ccmCallHomeDiagSignature 2 }

ccmCallHomeDiagSignatureInfoTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CcmCallHomeDiagSignatureInfoEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A list of Call Home Diagnostic Signatures installed on the
        device."
    ::= { ccmCallHomeDiagSignature 3 }

ccmCallHomeDiagSignatureInfoEntry OBJECT-TYPE
    SYNTAX          CcmCallHomeDiagSignatureInfoEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing management information of a
        Call Home Diagnostic Signature."
    INDEX           { IMPLIED ccmCallHomeDiagSignatureName } 
    ::= { ccmCallHomeDiagSignatureInfoTable 1 }

CcmCallHomeDiagSignatureInfoEntry ::= SEQUENCE {
        ccmCallHomeDiagSignatureName         SnmpAdminString,
        ccmCallHomeDiagSignatureType         INTEGER,
        ccmCallHomeDiagSignatureFuncDescr    SnmpAdminString,
        ccmCallHomeDiagSignatureRev          SnmpAdminString,
        ccmCallHomeDiagSignatureSigner       INTEGER,
        ccmCallHomeDiagSignatureTriggerCount Counter32,
        ccmCallHomeDiagSignatureAvgRuntime   Unsigned32,
        ccmCallHomeDiagSignatureMaxRuntime   Unsigned32
}

ccmCallHomeDiagSignatureName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..31))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The name of Call Home Diagnostic Signature installed on the
        device." 
    ::= { ccmCallHomeDiagSignatureInfoEntry 1 }

ccmCallHomeDiagSignatureType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        meta(1),
                        tcl(2),
                        applet(3),
                        mixed(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The type of this Call Home Diagnostic Signature." 
    ::= { ccmCallHomeDiagSignatureInfoEntry 2 }

ccmCallHomeDiagSignatureFuncDescr OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "A user friendly string providing functionality description
        for this Call Home Diagnostic Signature." 
    ::= { ccmCallHomeDiagSignatureInfoEntry 3 }

ccmCallHomeDiagSignatureRev OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The revision information of Call Home Diagnostic Signature." 
    ::= { ccmCallHomeDiagSignatureInfoEntry 4 }

ccmCallHomeDiagSignatureSigner OBJECT-TYPE
    SYNTAX          INTEGER  {
                        cisco(1),
                        partner(2),
                        thirdParty(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The entity who signed this Call Home Diagnostic Signature.

        'cisco'      - Diagnostic Signature has been signed by Cisco.
        'partner'    - Diagnostic Signature has been signed by
                       a Cisco partner.
        'thirdParty' - Diagnostic Signature has been signed by
                       a third-party." 
    ::= { ccmCallHomeDiagSignatureInfoEntry 5 }

ccmCallHomeDiagSignatureTriggerCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times this Call Home Diagnostic Signature
        has been triggered." 
    ::= { ccmCallHomeDiagSignatureInfoEntry 6 }

ccmCallHomeDiagSignatureAvgRuntime OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "milli seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average run time of this Call Home Diagnostic Signature." 
    ::= { ccmCallHomeDiagSignatureInfoEntry 7 }

ccmCallHomeDiagSignatureMaxRuntime OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "milli seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The maximum amount of time it took to run this Call Home
        Diagnostic Signature." 
    ::= { ccmCallHomeDiagSignatureInfoEntry 8 }
 


ccmCallHomeSecurityLevel OBJECT-TYPE
    SYNTAX          INTEGER  {
                        normal(1),
                        high(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the security level for Call Home.

        normal - running configuration and show CLI output are not
                 changed within Call Home messages.
        high   - system reveal subset of running configuration and
                 show CLI output within Call Home messages due to
                 privacy and security concern." 
    ::= { ccmCallHomeSecurity 1 }

ccmAnonymousReportingEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies if anonymous reporting functionality is
        enable for Call Home.

        A value of 'true' enables the anonymous reporting
        functionality." 
    ::= { ccmCallHomeReporting 1 }

ccmAaaAuthEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object specifies if the AAA authorization is required
        when running the CLI commands in Call Home messages.

        A value of 'true' enables the AAA authorization for the
        CLI commands in Call Home messages." 
    ::= { ccmCallHomeAaa 1 }

ccmAaaAuthUserName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The object specifies the user name used by Call Home for AAA
        authorization.

        Value of this object should be ignored if ccmAaaAuthEnable
        is 'false'." 
    ::= { ccmCallHomeAaa 2 }

-- Notifications

ccmSmtpServerFailNotif NOTIFICATION-TYPE
    OBJECTS         { ccmSmtpServersPort }
    STATUS          current
    DESCRIPTION
        "A ccmSmtpServerFailNotif is sent if the device fails on
        sending an e-mail notification through an SMTP server in
        ccmSmtpServersTable.

        For each SMTP server, an agent should not generate more
        than one ccmSmtpServerFailNotif 'notification-event'
        in a given time interval (ten seconds is the suggested
        default). A 'notification-event' is the transmission of
        a single trap or inform PDU to a list of notification
        destinations.

        If within the throttling period, additional failures to
        send a message through same server occur, then 
        notification-events for these failure should be suppressed
        by the agent until the current throttling period expires."
   ::= { ccmCallHomeNotifications 1 }

ccmAlertGroupTypeAddedNotif NOTIFICATION-TYPE
    OBJECTS         { callHomeAlertGroupName }
    STATUS          current
    DESCRIPTION
        "A ccmAlertGroupTypeAddedNotif is sent, when
        a new entry corresponds to the 
        'callHomeAlertGroupName' object in this 
        notification is added into the 
        callHomeAlertGroupTypeTable."
   ::= { ccmCallHomeNotifications 2 }

ccmAlertGroupTypeDeletedNotif NOTIFICATION-TYPE
    OBJECTS         { callHomeAlertGroupName }
    STATUS          current
    DESCRIPTION
        "A ccmAlertGroupTypeAddedNotif is sent, when an
        entry corresponds to 'callHomeAlertGroupName'
        object in this notification is deleted 
        from the callHomeAlertGroupTypeTable."
   ::= { ccmCallHomeNotifications 3 }

ccmSmtpMsgSendFailNotif NOTIFICATION-TYPE
    STATUS          current
    DESCRIPTION
        "A ccmSmtpMsgSendFailNotif is generated if the device
        fails to send an e-mail notification through all of the
        SMTP servers in ccmSmtpServersTable."
   ::= { ccmCallHomeNotifications 4 }

ccmEventNotif NOTIFICATION-TYPE
    OBJECTS         {
                        sysName,
                        ccmEventDescription,
                        ccmEventTime,
                        ccmEventUrgencyLevel
                    }
    STATUS          current
    DESCRIPTION
        "This notification is generated every time a Call Home
        external event is triggered in the system. Internal events 
        like Periodic Configuration and Inventory events do not 
        generate notifications."
   ::= { ccmCallHomeNotifications 5 }
-- Conformance

chMIBCompliances  OBJECT IDENTIFIER
    ::= { chMIBConformance 1 }

chMIBGroups  OBJECT IDENTIFIER
    ::= { chMIBConformance 2 }


chMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which
        implement the Call Home feature.

        OBJECT ccmSmtpServersAddrType 
        SYNTAX  INTEGER { ipv4(1) }
        DESCRIPTION
                An implementation is only required to 
                support IPv4 addresses.

        OBJECT callHomeDestProfileName
        SYNTAX  SnmpAdminString (SIZE (1..11))
        DESCRIPTION
                An implementation is only required to
                support a profile name of size 1 to 11
                octets."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        chConfigurationGroup,
                        chStatisticsGroup
                    }

    GROUP           chSystemInformationGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chEmailMsgDispGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSingleSmtpServerGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        single SMTP server."

    GROUP           chMultipleSmtpServersGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        multiple SMTP servers."

    GROUP           ccmSysLogSeverityGroup
    DESCRIPTION
        "This group is mandatory for devices that issue
        Call Home alerts based on  severity level of the 
        syslog messages generated on the device."

    GROUP           ccmMIBNotificationsConfigGroup
    DESCRIPTION
        "The ccmMIBNotificationsConfigGroup is optional."

    GROUP           ccmMIBNotificationsGroup
    DESCRIPTION
        "The ccmMIBNotificationsGroup is optional."

    OBJECT          callHomeDestProfileTrnsprtMthd
    SYNTAX          INTEGER  {
                        email(1)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'email' needs to be supported."

    OBJECT          callHomeDestProfileMsgFormat
    SYNTAX          INTEGER  {
                        shortText(3)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'shortText' needs to be supported."

    OBJECT          callHomeDestProfileStatus
    SYNTAX          INTEGER  {
                        active(1)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'active' needs to be supported."

    OBJECT          callHomeDestEmailAddress
    SYNTAX          SnmpAdminString (SIZE (1..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 1 to 63
        octets."

    OBJECT          callHomeDestEmailAddressStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          ccmSmtpServersPort
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmSmtpServersStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          callHomeEmailFrom
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."

    OBJECT          callHomeEmailReplyTo
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."

    OBJECT          callHomeEmailMsgDispNotification
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."
    ::= { chMIBCompliances 1 }

chMIBCompliance1 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which
        implement the Call Home feature.

        OBJECT ccmSmtpServersAddrType 
        SYNTAX  INTEGER { ipv4(1) }
        DESCRIPTION
                An implementation is only required to 
                support IPv4 addresses.

        OBJECT callHomeDestProfileName
        SYNTAX  SnmpAdminString (SIZE (1..31))
        DESCRIPTION
                An implementation is only required to
                support a profile name of size 1 to 31
                octets."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        chConfigurationGroup1,
                        chStatisticsGroup
                    }

    GROUP           chSystemInformationGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chEmailMsgDispGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSingleSmtpServerGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        single SMTP server."

    GROUP           chMultipleSmtpServersGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        multiple SMTP servers."

    GROUP           ccmSysLogSeverityGroup
    DESCRIPTION
        "This group is mandatory for devices that issue
        Call Home alerts based on  severity level of the 
        syslog messages generated on the device."

    GROUP           ccmMIBNotificationsConfigGroup
    DESCRIPTION
        "The ccmMIBNotificationsConfigGroup is optional."

    GROUP           ccmMIBNotificationsGroup1
    DESCRIPTION
        "The ccmMIBNotificationsGroup is optional."

    OBJECT          callHomeDestProfileTrnsprtMthd
    SYNTAX          INTEGER  {
                        email(1)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'email' needs to be supported."

    OBJECT          callHomeDestProfileMsgFormat
    SYNTAX          INTEGER  {
                        shortText(3)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'shortText' needs to be supported."

    OBJECT          callHomeDestProfileStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'active' needs to be supported."

    OBJECT          callHomeDestEmailAddress
    SYNTAX          SnmpAdminString (SIZE (1..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 1 to 63
        octets."

    OBJECT          callHomeDestEmailAddressStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          ccmSmtpServersPort
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmSmtpServersStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          callHomeEmailFrom
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."

    OBJECT          callHomeEmailReplyTo
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."

    OBJECT          callHomeEmailMsgDispNotification
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."
    ::= { chMIBCompliances 2 }

chMIBCompliance2 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which
        implement the Call Home feature.

        OBJECT ccmSmtpServersAddrType 
        SYNTAX  INTEGER { ipv4(1) }
        DESCRIPTION
                An implementation is only required to 
                support IPv4 addresses.

        OBJECT callHomeDestProfileName
        SYNTAX  SnmpAdminString (SIZE (1..31))
        DESCRIPTION
                An implementation is only required to
                support a profile name of size 1 to 31
                octets."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        chConfigurationGroup2,
                        chStatisticsGroup,
                        chSwInventoryInfoGroup
                    }

    GROUP           chSystemInformationGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chEmailMsgDispGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSingleSmtpServerGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        single SMTP server."

    GROUP           chMultipleSmtpServersGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        multiple SMTP servers."

    GROUP           ccmSysLogSeverityGroup
    DESCRIPTION
        "This group is mandatory for devices that issue
        Call Home alerts based on  severity level of the 
        syslog messages generated on the device."

    GROUP           ccmMIBNotificationsConfigGroup
    DESCRIPTION
        "The ccmMIBNotificationsConfigGroup is optional."

    GROUP           ccmMIBNotificationsGroup1
    DESCRIPTION
        "The ccmMIBNotificationsGroup is optional."

    OBJECT          callHomeDestProfileTrnsprtMthd
    SYNTAX          INTEGER  {
                        email(1)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'email' needs to be supported."

    OBJECT          callHomeDestProfileMsgFormat
    SYNTAX          INTEGER  {
                        shortText(3)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'shortText' needs to be supported."

    OBJECT          callHomeDestProfileStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'active' needs to be supported."

    OBJECT          callHomeDestEmailAddress
    SYNTAX          SnmpAdminString (SIZE (1..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 1 to 63
        octets."

    OBJECT          callHomeDestEmailAddressStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          ccmSmtpServersPort
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmSmtpServersStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          callHomeEmailFrom
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."

    OBJECT          callHomeEmailReplyTo
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."

    OBJECT          callHomeEmailMsgDispNotification
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."
    ::= { chMIBCompliances 3 }

chMIBCompliance3 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which
        implement the Call Home feature.

        OBJECT ccmSmtpServersAddrType 
        SYNTAX  INTEGER { ipv4(1) }
        DESCRIPTION
                An implementation is only required to 
                support IPv4 addresses.

        OBJECT callHomeDestProfileName
        SYNTAX  SnmpAdminString (SIZE (1..31))
        DESCRIPTION
                An implementation is only required to
                support a profile name of size 1 to 31
                octets."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        chConfigurationGroup2,
                        chStatisticsGroup
                    }

    GROUP           chSystemInformationGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chEmailMsgDispGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chPeriodicSwInventoryInfoGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSingleSmtpServerGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        single SMTP server."

    GROUP           chMultipleSmtpServersGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        multiple SMTP servers."

    GROUP           ccmSysLogSeverityGroup
    DESCRIPTION
        "This group is mandatory for devices that issue
        Call Home alerts based on  severity level of the 
        syslog messages generated on the device."

    GROUP           ccmMIBNotificationsConfigGroup
    DESCRIPTION
        "The ccmMIBNotificationsConfigGroup is optional."

    GROUP           ccmMIBNotificationsGroup1
    DESCRIPTION
        "The ccmMIBNotificationsGroup is optional."

    OBJECT          callHomeDestProfileTrnsprtMthd
    SYNTAX          INTEGER  {
                        email(1)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'email' needs to be supported."

    OBJECT          callHomeDestProfileMsgFormat
    SYNTAX          INTEGER  {
                        shortText(3)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'shortText' needs to be supported."

    OBJECT          callHomeDestProfileStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'active' needs to be supported."

    OBJECT          callHomeDestEmailAddress
    SYNTAX          SnmpAdminString (SIZE (1..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 1 to 63
        octets."

    OBJECT          callHomeDestEmailAddressStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          ccmSmtpServersPort
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmSmtpServersStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          callHomeEmailFrom
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."

    OBJECT          callHomeEmailReplyTo
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."

    OBJECT          callHomeEmailMsgDispNotification
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."
    ::= { chMIBCompliances 4 }

chMIBCompliance4 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which
        implement the Call Home feature.

        OBJECT ccmSmtpServersAddrType 
        SYNTAX  INTEGER { ipv4(1) }
        DESCRIPTION
                An implementation is only required to 
                support IPv4 addresses.

        OBJECT callHomeDestProfileName
        SYNTAX  SnmpAdminString (SIZE (1..31))
        DESCRIPTION
                An implementation is only required to
                support a profile name of size 1 to 31
                octets."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ccmConfigurationGroup3,
                        chStatisticsGroup
                    }

    GROUP           chSystemInformationGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSystemServicePriorityGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chEmailMsgDispGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmAlertActionGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which generate test messages for all
        (and not any particular) of configured destination
        profiles which meet test message generation criteria
        determined by platform."

    GROUP           ccmProfileMessageLevelGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which allow user to filter Call Home 
        messages based on their associated levels."

    GROUP           ccmProfileActivationGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which provide user control to enable or
        disable configured Call Home profiles."

    GROUP           ccmProfileTestGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which are capable of generating test
        messages specifically for a configured destination
        profile."

    GROUP           ccmProfileAlertGroupsGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which categorize various events that result
        in Call Home messages in different alert-groups and
        provide user control to associate different alert-groups
        to configured profiles."

    GROUP           ccmProfileAlertGroupControlGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which implement ccmProfileAlertGroupsGroup
        and can enable or disable various alert-groups."

    GROUP           ccmThrottleConfigurationGroup
    DESCRIPTION
        "Implementation of this group is only for the systems
        which support such message throttling functionality."

    GROUP           chSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chPeriodicSwInventoryInfoGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmPeriodicSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSingleSmtpServerGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        single SMTP server."

    GROUP           chMultipleSmtpServersGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        multiple SMTP servers."

    GROUP           ccmSmtpServersPriorityGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        prioritization among multiple SMTP servers."

    GROUP           ccmSysLogSeverityGroup
    DESCRIPTION
        "This group is mandatory for devices that issue
        Call Home alerts based on  severity level of the 
        syslog messages generated on the device."

    GROUP           ccmMIBNotificationsConfigGroup
    DESCRIPTION
        "The ccmMIBNotificationsConfigGroup is optional."

    GROUP           ccmMIBNotificationsGroup1
    DESCRIPTION
        "The ccmMIBNotificationsGroup1 is optional."

    GROUP           ccmHttpCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support http as a transport method to deliver
        Call Home messages."

    GROUP           ccmSeverityAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support severity based alert groups."

    GROUP           ccmPeriodicAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support periodic alert groups."

    GROUP           ccmPatternAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support pattern based alert groups."

    GROUP           ccmEventAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support event based alert groups."

    GROUP           ccmAlertGroupCapabilityGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support alert group capabilities."

    GROUP           ccmUserDefCmdGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmSmtpMsgSendFailNotifCtrlGroup
    DESCRIPTION
        "Implementation of ccmSmtpMsgSendFailNotifCtrlGroup
        is optional."

    GROUP           ccmSmtpMsgSendFailNotifGroup
    DESCRIPTION
        "Implementation of ccmSmtpMsgSendFailNotifCtrlGroup
        is optional."

    GROUP           ccmAlertHCStatisticsGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support 64 bit Call Home alert statistics."

    GROUP           ccmAlertRateLimitGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support Call Home alert rate limit feature."

    GROUP           ccmSmtpServerStatusGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support Call Home SMTP Server status
        check feature."

    GROUP           ccmProfileHiMessageSizeGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support the maximum size of message 
        greater than 1000,000 bytes."

    OBJECT          callHomeDestProfileTrnsprtMthd
    SYNTAX          INTEGER  {
                        email(1)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'email' needs to be supported."

    OBJECT          callHomeDestProfileMsgFormat
    SYNTAX          INTEGER  {
                        shortText(3)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'shortText' needs to be supported."

    OBJECT          callHomeDestProfileStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'active' needs to be supported."

    OBJECT          callHomeDestEmailAddress
    SYNTAX          SnmpAdminString (SIZE (1..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 1 to 63
        octets."

    OBJECT          callHomeDestEmailAddressStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          ccmSmtpServersPort
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmSmtpServersStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          callHomeEmailFrom
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          callHomeEmailReplyTo
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          callHomeEmailMsgDispNotification
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."
    ::= { chMIBCompliances 5 }

chMIBCompliance5 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which
        implement the Call Home feature.

        OBJECT ccmSmtpServersAddrType 
        SYNTAX  INTEGER { ipv4(1) }
        DESCRIPTION
                An implementation is only required to 
                support IPv4 addresses."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ccmConfigurationGroup3,
                        chStatisticsGroup
                    }

    GROUP           chSystemInformationGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSystemServicePriorityGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chEmailMsgDispGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmAlertActionGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which generate test messages for all
        (and not any particular) of configured destination
        profiles which meet test message generation criteria
        determined by platform."

    GROUP           ccmProfileMessageLevelGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which allow user to filter Call Home 
        messages based on their associated levels."

    GROUP           ccmProfileActivationGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which provide user control to enable or
        disable configured Call Home profiles."

    GROUP           ccmProfileTestGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which are capable of generating test
        messages specifically for a configured destination
        profile."

    GROUP           ccmProfileAlertGroupsGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which categorize various events that result
        in Call Home messages in different alert-groups and
        provide user control to associate different alert-groups
        to configured profiles."

    GROUP           ccmProfileAlertGroupControlGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which implement ccmProfileAlertGroupsGroup
        and can enable or disable various alert-groups."

    GROUP           ccmThrottleConfigurationGroup
    DESCRIPTION
        "Implementation of this group is only for the systems
        which support such message throttling functionality."

    GROUP           chSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chPeriodicSwInventoryInfoGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmPeriodicSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSingleSmtpServerGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        single SMTP server."

    GROUP           chMultipleSmtpServersGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        multiple SMTP servers."

    GROUP           ccmSmtpServersPriorityGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        prioritization among multiple SMTP servers."

    GROUP           ccmSysLogSeverityGroup
    DESCRIPTION
        "This group is mandatory for devices that issue
        Call Home alerts based on  severity level of the 
        syslog messages generated on the device."

    GROUP           ccmMIBNotificationsConfigGroup
    DESCRIPTION
        "The ccmMIBNotificationsConfigGroup is optional."

    GROUP           ccmMIBNotificationsGroup1
    DESCRIPTION
        "The ccmMIBNotificationsGroup1 is optional."

    GROUP           ccmHttpCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support http as a transport method to deliver
        Call Home messages."

    GROUP           ccmSeverityAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support severity based alert groups."

    GROUP           ccmPeriodicAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support periodic alert groups."

    GROUP           ccmPatternAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support pattern based alert groups."

    GROUP           ccmEventAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support event based alert groups."

    GROUP           ccmAlertGroupCapabilityGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support alert group capabilities."

    GROUP           ccmUserDefCmdGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmSmtpMsgSendFailNotifCtrlGroup
    DESCRIPTION
        "Implementation of ccmSmtpMsgSendFailNotifCtrlGroup
        is optional."

    GROUP           ccmSmtpMsgSendFailNotifGroup
    DESCRIPTION
        "Implementation of chSmtpMsgSendFailNotifGroup
        is optional."

    GROUP           ccmAlertHCStatisticsGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support 64 bit Call Home alert statistics."

    GROUP           ccmAlertRateLimitGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support Call Home alert rate limit feature."

    GROUP           ccmSmtpServerStatusGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support Call Home SMTP Server status
        check feature."

    GROUP           ccmProfileHiMessageSizeGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support the maximum size of message 
        greater than 1000,000 bytes."

    GROUP           ccmOnDemandMsgSendControlGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support on demand Call Home messages."

    GROUP           ccmOnDemandMsgStatusGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which do not support concurrent generation of
        on demand Call Home messages."

    GROUP           ccmSmartCallHomeGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support Smart Call Home messages."

    GROUP           ccmEventStatsGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which maintain statistical information Call Home
        events."

    OBJECT          callHomeDestProfileTrnsprtMthd
    SYNTAX          INTEGER  {
                        email(1)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'email' needs to be supported."

    OBJECT          callHomeDestProfileMsgFormat
    SYNTAX          INTEGER  {
                        shortText(3)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'shortText' needs to be supported."

    OBJECT          callHomeDestProfileStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'active' needs to be supported."

    OBJECT          callHomeDestEmailAddress
    SYNTAX          SnmpAdminString (SIZE (1..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 1 to 63
        octets."

    OBJECT          callHomeDestEmailAddressStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          ccmSmtpServersPort
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmSmtpServersStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          callHomeEmailFrom
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          callHomeEmailReplyTo
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          callHomeEmailMsgDispNotification
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."
    ::= { chMIBCompliances 6 }

chMIBCompliance6 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which
        implement the Call Home feature. It is deprecated 
        and superseded by chMIBCompliance7 statement.

        OBJECT ccmSmtpServersAddrType 
        SYNTAX  INTEGER { ipv4(1) }
        DESCRIPTION
                An implementation is only required to 
                support IPv4 addresses."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ccmConfigurationGroup3,
                        chStatisticsGroup
                    }

    GROUP           chSystemInformationGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSystemServicePriorityGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chEmailMsgDispGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmAlertActionGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which generate test messages for all
        (and not any particular) of configured destination
        profiles which meet test message generation criteria
        determined by platform."

    GROUP           ccmProfileMessageLevelGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which allow user to filter Call Home 
        messages based on their associated levels."

    GROUP           ccmProfileActivationGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which provide user control to enable or
        disable configured Call Home profiles."

    GROUP           ccmProfileTestGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which are capable of generating test
        messages specifically for a configured destination
        profile."

    GROUP           ccmProfileAlertGroupsGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which categorize various events that result
        in Call Home messages in different alert-groups and
        provide user control to associate different alert-groups
        to configured profiles."

    GROUP           ccmProfileAlertGroupControlGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which implement ccmProfileAlertGroupsGroup
        and can enable or disable various alert-groups."

    GROUP           ccmThrottleConfigurationGroup
    DESCRIPTION
        "Implementation of this group is only for the systems
        which support such message throttling functionality."

    GROUP           chSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chPeriodicSwInventoryInfoGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmPeriodicSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSingleSmtpServerGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        single SMTP server."

    GROUP           chMultipleSmtpServersGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        multiple SMTP servers."

    GROUP           ccmSmtpServersPriorityGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        prioritization among multiple SMTP servers."

    GROUP           ccmSysLogSeverityGroup
    DESCRIPTION
        "This group is mandatory for devices that issue
        Call Home alerts based on  severity level of the 
        syslog messages generated on the device."

    GROUP           ccmMIBNotificationsConfigGroup
    DESCRIPTION
        "The ccmMIBNotificationsConfigGroup is optional."

    GROUP           ccmMIBNotificationsGroup1
    DESCRIPTION
        "The ccmMIBNotificationsGroup1 is optional."

    GROUP           ccmHttpCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support http as a transport method to deliver
        Call Home messages."

    GROUP           ccmSeverityAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support severity based alert groups."

    GROUP           ccmPeriodicAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support periodic alert groups."

    GROUP           ccmPatternAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support pattern based alert groups."

    GROUP           ccmEventAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support event based alert groups."

    GROUP           ccmAlertGroupCapabilityGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support alert group capabilities."

    GROUP           ccmUserDefCmdGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmSmtpMsgSendFailNotifCtrlGroup
    DESCRIPTION
        "Implementation of ccmSmtpMsgSendFailNotifCtrlGroup
        is optional."

    GROUP           ccmSmtpMsgSendFailNotifGroup
    DESCRIPTION
        "Implementation of chSmtpMsgSendFailNotifGroup
        is optional."

    GROUP           ccmAlertHCStatisticsGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support 64 bit Call Home alert statistics."

    GROUP           ccmAlertRateLimitGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support Call Home alert rate limit feature."

    GROUP           ccmSmtpServerStatusGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support Call Home SMTP Server status
        check feature."

    GROUP           ccmProfileHiMessageSizeGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support the maximum size of message 
        greater than 1000,000 bytes."

    GROUP           ccmOnDemandMsgSendControlGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support on demand Call Home messages."

    GROUP           ccmOnDemandMsgStatusGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which do not support concurrent generation of
        on demand Call Home messages."

    GROUP           ccmSmartCallHomeGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support Smart Call Home messages."

    GROUP           ccmEventStatsGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which maintain statistical information Call Home
        events."

    GROUP           ccmEventNotifGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmCallhomeEventsGroup
    DESCRIPTION
        "Implementation of this group is optional."

    OBJECT          callHomeDestProfileTrnsprtMthd
    SYNTAX          INTEGER  {
                        email(1)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'email' needs to be supported."

    OBJECT          callHomeDestProfileMsgFormat
    SYNTAX          INTEGER  {
                        shortText(3)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'shortText' needs to be supported."

    OBJECT          callHomeDestProfileStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'active' needs to be supported."

    OBJECT          callHomeDestEmailAddress
    SYNTAX          SnmpAdminString (SIZE (1..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 1 to 63
        octets."

    OBJECT          callHomeDestEmailAddressStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          ccmSmtpServersPort
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmSmtpServersStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          callHomeEmailFrom
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          callHomeEmailReplyTo
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          callHomeEmailMsgDispNotification
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63 
        octets."
    ::= { chMIBCompliances 7 }

chMIBCompliance7 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which
        implement the Call Home feature.

        OBJECT ccmSmtpServersAddrType
        SYNTAX  INTEGER { ipv4(1) }
        DESCRIPTION
                An implementation is only required to
                support IPv4 addresses."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ccmConfigurationGroup3,
                        chStatisticsGroup
                    }

    GROUP           chSystemInformationGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSystemServicePriorityGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chEmailMsgDispGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmAlertActionGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which generate test messages for all
        (and not any particular) of configured destination
        profiles which meet test message generation criteria
        determined by platform."

    GROUP           ccmProfileMessageLevelGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which allow user to filter Call Home
        messages based on their associated levels."

    GROUP           ccmProfileActivationGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which provide user control to enable or
        disable configured Call Home profiles."

    GROUP           ccmProfileTestGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which are capable of generating test
        messages specifically for a configured destination
        profile."

    GROUP           ccmProfileAlertGroupsGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which categorize various events that result
        in Call Home messages in different alert-groups and
        provide user control to associate different alert-groups
        to configured profiles."

    GROUP           ccmProfileAlertGroupControlGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which implement ccmProfileAlertGroupsGroup
        and can enable or disable various alert-groups."

    GROUP           ccmThrottleConfigurationGroup
    DESCRIPTION
        "Implementation of this group is only for the systems
        which support such message throttling functionality."

    GROUP           chSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chPeriodicSwInventoryInfoGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmPeriodicSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSingleSmtpServerGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        single SMTP server."

    GROUP           chMultipleSmtpServersGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        multiple SMTP servers."

    GROUP           ccmSmtpServersPriorityGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        prioritization among multiple SMTP servers."

    GROUP           ccmSysLogSeverityGroup
    DESCRIPTION
        "This group is mandatory for devices that issue
        Call Home alerts based on  severity level of the
        syslog messages generated on the device."

    GROUP           ccmMIBNotificationsConfigGroup
    DESCRIPTION
        "The ccmMIBNotificationsConfigGroup is optional."

    GROUP           ccmMIBNotificationsGroup1
    DESCRIPTION
        "The ccmMIBNotificationsGroup1 is optional."

    GROUP           ccmHttpCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support http as a transport method to deliver
        Call Home messages."

    GROUP           ccmSeverityAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support severity based alert groups."

    GROUP           ccmPeriodicAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support periodic alert groups."

    GROUP           ccmPatternAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support pattern based alert groups."

    GROUP           ccmEventAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support event based alert groups."

    GROUP           ccmAlertGroupCapabilityGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support alert group capabilities."

    GROUP           ccmUserDefCmdGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmSmtpMsgSendFailNotifCtrlGroup
    DESCRIPTION
        "Implementation of ccmSmtpMsgSendFailNotifCtrlGroup
        is optional."

    GROUP           ccmSmtpMsgSendFailNotifGroup
    DESCRIPTION
        "Implementation of chSmtpMsgSendFailNotifGroup
        is optional."

    GROUP           ccmAlertHCStatisticsGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support 64 bit Call Home alert statistics."

    GROUP           ccmAlertRateLimitGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support Call Home alert rate limit feature."

    GROUP           ccmSmtpServerStatusGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support Call Home SMTP Server status
        check feature."

    GROUP           ccmProfileHiMessageSizeGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support the maximum size of message
        greater than 1000,000 bytes."

    GROUP           ccmOnDemandMsgSendControlGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support on demand Call Home messages."

    GROUP           ccmOnDemandMsgStatusGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which do not support concurrent generation of
        on demand Call Home messages."

    GROUP           ccmSmartCallHomeGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support Smart Call Home messages."

    GROUP           ccmEventStatsGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which maintain statistical information Call Home
        events."

    GROUP           ccmEventNotifGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmCallhomeEventsGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmCallHomeVrfGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which maintain VRF information for Call Home."

    OBJECT          callHomeDestProfileTrnsprtMthd
    SYNTAX          INTEGER  {
                        email(1)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'email' needs to be supported."

    OBJECT          callHomeDestProfileMsgFormat
    SYNTAX          INTEGER  {
                        shortText(3)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'shortText' needs to be supported."

    OBJECT          callHomeDestProfileStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'active' needs to be supported."

    OBJECT          callHomeDestEmailAddress
    SYNTAX          SnmpAdminString (SIZE (1..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 1 to 63
        octets."

    OBJECT          callHomeDestEmailAddressStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          ccmSmtpServersPort
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmSmtpServersStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          callHomeEmailFrom
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          callHomeEmailReplyTo
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          callHomeEmailMsgDispNotification
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          ccmCallHomeVrfName
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { chMIBCompliances 8 }

chMIBCompliance8 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which
        implement the Call Home feature.

        OBJECT ccmSmtpServersAddrType
        SYNTAX  INTEGER { ipv4(1) }
        DESCRIPTION
                An implementation is only required to
                support IPv4 addresses."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ccmConfigurationGroup3,
                        chStatisticsGroup
                    }

    GROUP           chSystemInformationGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSystemServicePriorityGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chEmailMsgDispGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmAlertActionGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which generate test messages for all
        (and not any particular) of configured destination
        profiles which meet test message generation criteria
        determined by platform."

    GROUP           ccmProfileMessageLevelGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which allow user to filter Call Home
        messages based on their associated levels."

    GROUP           ccmProfileActivationGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which provide user control to enable or
        disable configured Call Home profiles."

    GROUP           ccmProfileTestGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which are capable of generating test
        messages specifically for a configured destination
        profile."

    GROUP           ccmProfileAlertGroupsGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which categorize various events that result
        in Call Home messages in different alert-groups and
        provide user control to associate different alert-groups
        to configured profiles."

    GROUP           ccmProfileAlertGroupControlGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which implement ccmProfileAlertGroupsGroup
        and can enable or disable various alert-groups."

    GROUP           ccmThrottleConfigurationGroup
    DESCRIPTION
        "Implementation of this group is only for the systems
        which support such message throttling functionality."

    GROUP           chSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chPeriodicSwInventoryInfoGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmPeriodicSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chMultipleSmtpServersGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        multiple SMTP servers."

    GROUP           ccmSmtpServersPriorityGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        prioritization among multiple SMTP servers."

    GROUP           ccmSysLogSeverityGroup
    DESCRIPTION
        "This group is mandatory for devices that issue
        Call Home alerts based on  severity level of the
        syslog messages generated on the device."

    GROUP           ccmMIBNotificationsConfigGroup
    DESCRIPTION
        "The ccmMIBNotificationsConfigGroup is optional."

    GROUP           ccmMIBNotificationsGroup1
    DESCRIPTION
        "The ccmMIBNotificationsGroup1 is optional."

    GROUP           ccmHttpCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support http as a transport method to deliver
        Call Home messages."

    GROUP           ccmSeverityAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support severity based alert groups."

    GROUP           ccmPeriodicAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support periodic alert groups."

    GROUP           ccmPatternAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support pattern based alert groups."

    GROUP           ccmEventAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support event based alert groups."

    GROUP           ccmAlertGroupCapabilityGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support alert group capabilities."

    GROUP           ccmUserDefCmdGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmSmtpMsgSendFailNotifCtrlGroup
    DESCRIPTION
        "Implementation of ccmSmtpMsgSendFailNotifCtrlGroup
        is optional."

    GROUP           ccmSmtpMsgSendFailNotifGroup
    DESCRIPTION
        "Implementation of chSmtpMsgSendFailNotifGroup
        is optional."

    GROUP           ccmAlertHCStatisticsGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support 64 bit Call Home alert statistics."

    GROUP           ccmAlertRateLimitGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support Call Home alert rate limit feature."

    GROUP           ccmSmtpServerStatusGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support Call Home SMTP Server status
        check feature."

    GROUP           ccmProfileHiMessageSizeGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support the maximum size of message
        greater than 1000,000 bytes."

    GROUP           ccmOnDemandMsgSendControlGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support on demand Call Home messages."

    GROUP           ccmOnDemandMsgStatusGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which do not support concurrent generation of
        on demand Call Home messages."

    GROUP           ccmSmartCallHomeGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support Smart Call Home messages."

    GROUP           ccmEventStatsGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which maintain statistical information Call Home
        events."

    GROUP           ccmEventNotifGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmCallhomeEventsGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmHttpProxyServerGroup
    DESCRIPTION
        "Implementation of this group is mandatory for the devices
        which implement HTTP proxy support for Call Home."

    GROUP           ccmHttpTransportVrfGroup
    DESCRIPTION
        "Implementation of this group is mandatory for the devices
        which implement VRF information for HTTP transport in 
        Call Home."

    GROUP           ccmCallHomeVrfGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which maintain VRF information for Call Home."

    GROUP           ccmSmtpServersVrfGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which maintain VRF information for Call Home."

    GROUP           ccmSingleSmtpServerGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        single SMTP server."

    GROUP           ccmMessageSourceGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which allow user to specify the source address
        for generation of Call Home messages."

    OBJECT          callHomeDestProfileTrnsprtMthd
    SYNTAX          INTEGER  {
                        email(1)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'email' needs to be supported."

    OBJECT          callHomeDestProfileMsgFormat
    SYNTAX          INTEGER  {
                        shortText(3)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'shortText' needs to be supported."

    OBJECT          callHomeDestProfileStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'active' needs to be supported."

    OBJECT          callHomeDestEmailAddress
    SYNTAX          SnmpAdminString (SIZE (1..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 1 to 63
        octets."

    OBJECT          callHomeDestEmailAddressStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          ccmSmtpServersPort
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmSmtpServersStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          callHomeEmailFrom
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          callHomeEmailReplyTo
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          callHomeEmailMsgDispNotification
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          ccmCallHomeVrfName
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmMsgSourceIpAddrType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmMsgSourceIpAddr
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmMsgSourceInterface
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { chMIBCompliances 9 }

chMIBCompliance9 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for entities which
        implement the Call Home feature.

        OBJECT ccmSmtpServersAddrType
        SYNTAX  INTEGER { ipv4(1) }
        DESCRIPTION
                An implementation is only required to
                support IPv4 addresses."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ccmConfigurationGroup3,
                        chStatisticsGroup
                    }

    GROUP           chSystemInformationGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chSystemServicePriorityGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chEmailMsgDispGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmAlertActionGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which generate test messages for all
        (and not any particular) of configured destination
        profiles which meet test message generation criteria
        determined by platform."

    GROUP           ccmProfileMessageLevelGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which allow user to filter Call Home
        messages based on their associated levels."

    GROUP           ccmProfileActivationGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which provide user control to enable or
        disable configured Call Home profiles."

    GROUP           ccmProfileTestGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which are capable of generating test
        messages specifically for a configured destination
        profile."

    GROUP           ccmProfileAlertGroupsGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which categorize various events that result
        in Call Home messages in different alert-groups and
        provide user control to associate different alert-groups
        to configured profiles."

    GROUP           ccmProfileAlertGroupControlGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for
        the platforms which implement ccmProfileAlertGroupsGroup
        and can enable or disable various alert-groups."

    GROUP           ccmThrottleConfigurationGroup
    DESCRIPTION
        "Implementation of this group is only for the systems
        which support such message throttling functionality."

    GROUP           chSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chPeriodicSwInventoryInfoGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmPeriodicSwInventoryInfoGroup1
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           chMultipleSmtpServersGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        multiple SMTP servers."

    GROUP           ccmSmtpServersPriorityGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        prioritization among multiple SMTP servers."

    GROUP           ccmSysLogSeverityGroup
    DESCRIPTION
        "This group is mandatory for devices that issue
        Call Home alerts based on  severity level of the
        syslog messages generated on the device."

    GROUP           ccmMIBNotificationsConfigGroup
    DESCRIPTION
        "The ccmMIBNotificationsConfigGroup is optional."

    GROUP           ccmMIBNotificationsGroup1
    DESCRIPTION
        "The ccmMIBNotificationsGroup1 is optional."

    GROUP           ccmHttpCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support http as a transport method to deliver
        Call Home messages."

    GROUP           ccmSeverityAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support severity based alert groups."

    GROUP           ccmPeriodicAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support periodic alert groups."

    GROUP           ccmPatternAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support pattern based alert groups."

    GROUP           ccmEventAlertGroupCfgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support event based alert groups."

    GROUP           ccmAlertGroupCapabilityGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support alert group capabilities."

    GROUP           ccmUserDefCmdGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmSmtpMsgSendFailNotifCtrlGroup
    DESCRIPTION
        "Implementation of ccmSmtpMsgSendFailNotifCtrlGroup
        is optional."

    GROUP           ccmSmtpMsgSendFailNotifGroup
    DESCRIPTION
        "Implementation of ccmSmtpMsgSendFailNotifGroup
        is optional."

    GROUP           ccmAlertHCStatisticsGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support 64 bit Call Home alert statistics."

    GROUP           ccmAlertRateLimitGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support Call Home alert rate limit feature."

    GROUP           ccmSmtpServerStatusGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support Call Home SMTP Server status
        check feature."

    GROUP           ccmProfileHiMessageSizeGroup
    DESCRIPTION
        "Implementation of this group mandatory only for the
        devices which support the maximum size of message
        greater than 1000,000 bytes."

    GROUP           ccmOnDemandMsgSendControlGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support on demand Call Home messages."

    GROUP           ccmOnDemandMsgStatusGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which do not support concurrent generation of
        on demand Call Home messages."

    GROUP           ccmSmartCallHomeGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support Smart Call Home messages."

    GROUP           ccmEventStatsGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which maintain statistical information Call Home
        events."

    GROUP           ccmEventNotifGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmCallhomeEventsGroup
    DESCRIPTION
        "Implementation of this group is optional."

    GROUP           ccmHttpProxyServerGroup
    DESCRIPTION
        "Implementation of this group is mandatory for the devices
        which implement HTTP proxy support for Call Home."

    GROUP           ccmHttpTransportVrfGroup
    DESCRIPTION
        "Implementation of this group is mandatory for the devices
        which implement VRF information for HTTP transport in 
        Call Home."

    GROUP           ccmCallHomeVrfGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which maintain VRF information for Call Home."

    GROUP           ccmSmtpServersVrfGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which maintain VRF information for Call Home."

    GROUP           ccmSingleSmtpServerGroup
    DESCRIPTION
        "This group is mandatory for devices which support
        single SMTP server."

    GROUP           ccmMessageSourceGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which allow user to specify the source address
        for generation of Call Home messages."

    GROUP           ccmCallHomePeriodicMinutesGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support periodic interval configuration in
        minutes."

    GROUP           ccmOnDemandCliMsgGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support on demand Call Home messages with CLI
        output."

    GROUP           ccmCallHomeDiagSignatureGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support Diagnostic Signature functionality of
        Call Home."

    GROUP           ccmCallHomeSecurityLevelGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support security level configuration for
        Call Home."

    GROUP           ccmCallHomeAnonymousReportingGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support reporting functionality of Call Home."

    GROUP           ccmCallHomeAaaGroup
    DESCRIPTION
        "Implementation of this group is mandatory only for the
        devices which support AAA configuration for Call Home."

    OBJECT          callHomeDestProfileTrnsprtMthd
    SYNTAX          INTEGER  {
                        email(1)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'email' needs to be supported."

    OBJECT          callHomeDestProfileMsgFormat
    SYNTAX          INTEGER  {
                        shortText(3)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'shortText' needs to be supported."

    OBJECT          callHomeDestProfileStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION
        "Only 'active' needs to be supported."

    OBJECT          callHomeDestEmailAddress
    SYNTAX          SnmpAdminString (SIZE (1..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 1 to 63
        octets."

    OBJECT          callHomeDestEmailAddressStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          ccmSmtpServersPort
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmSmtpServersStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "Only 'active', 'createAndGo' and 'destroy' needs
        to be supported."

    OBJECT          callHomeEmailFrom
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          callHomeEmailReplyTo
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          callHomeEmailMsgDispNotification
    SYNTAX          SnmpAdminString (SIZE (0..63))
    DESCRIPTION
        "An implementation is only required to
        support an address of size 0 to 63
        octets."

    OBJECT          ccmCallHomeVrfName
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmMsgSourceIpAddrType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmMsgSourceIpAddr
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmMsgSourceInterface
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmPeriodicAlertGroupIntervalMinutes
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmOnDemandCliMsgCliList
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmOnDemandCliMsgTransport
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmOnDemandCliMsgEmail
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmOnDemandCliMsgFormat
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmOnDemandCliMsgTacServiceReqId
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmOnDemandCliMsgTrigger
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmDiagSignatureActive
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmCallHomeSecurityLevel
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmAnonymousReportingEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmAaaAuthEnable
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          ccmAaaAuthUserName
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { chMIBCompliances 10 }

-- Units of Conformance

chSystemInformationGroup OBJECT-GROUP
    OBJECTS         {
                        sysContactPhoneNumber,
                        sysContactEmailAddress,
                        sysStreetAddress,
                        callHomeCustomerId,
                        callHomeContractId,
                        callHomeSiteId,
                        callHomeDeviceServicePriority
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects for displaying and
        configuring system information pertaining to
        Call Home."
    ::= { chMIBGroups 1 }

chConfigurationGroup OBJECT-GROUP
    OBJECTS         {
                        callHomeEnable,
                        callHomeAlertAction,
                        callHomeAlertActionStatus,
                        callHomeAlertActionFailureCause,
                        callHomeDestProfileMsgFormat,
                        callHomeDestProfileMaxMsgSize,
                        callHomeDestProfileTrnsprtMthd,
                        callHomeDestProfileStatus,
                        callHomeEmailAddrTblMaxEntries,
                        callHomeDestEmailAddress,
                        callHomeDestEmailAddressStatus,
                        callHomeEmailFrom,
                        callHomeEmailReplyTo
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects for displaying and
        configuring Call Home parameters."
    ::= { chMIBGroups 2 }

chEmailMsgDispGroup OBJECT-GROUP
    OBJECTS         { callHomeEmailMsgDispNotification }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) for displaying and
        configuring e-mail address to which the
        e-mail disposition notification should be sent."
    ::= { chMIBGroups 3 }

chSingleSmtpServerGroup OBJECT-GROUP
    OBJECTS         {
                        callHomeSmtpServerAddrType,
                        callHomeSmtpServerAddr,
                        callHomeSmtpServerPort
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects for displaying and
        configuring Call Home SMTP server on the devices which
        support only one SMTP server."
    ::= { chMIBGroups 4 }

chMultipleSmtpServersGroup OBJECT-GROUP
    OBJECTS         {
                        ccmSmtpServersTblMaxEntries,
                        ccmSmtpServersPort,
                        ccmSmtpServersStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects for displaying and
        configuring Call Home SMTP server on the devices which
        support on one SMTP server."
    ::= { chMIBGroups 5 }

chStatisticsGroup OBJECT-GROUP
    OBJECTS         {
                        callHomeLastAlertSent,
                        callHomeAlerts
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects for displaying
        Call Home statistics."
    ::= { chMIBGroups 6 }

ccmSysLogSeverityGroup OBJECT-GROUP
    OBJECTS         { ccmSysLogSeverity }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) for displaying and
        configuring Call Home syslog severity based on which
        Call Home alerts may be issued."
    ::= { chMIBGroups 7 }

ccmMIBNotificationsConfigGroup OBJECT-GROUP
    OBJECTS         { ccmEnableSmtpServerNotif }
    STATUS          current
    DESCRIPTION
        "A collection of objects for displaying and
        configuring Call Home notifications."
    ::= { chMIBGroups 8 }

ccmMIBNotificationsGroup NOTIFICATION-GROUP
   NOTIFICATIONS    { ccmSmtpServerFailNotif }
    STATUS          deprecated
    DESCRIPTION
        "A collection of notifications."
    ::= { chMIBGroups 9 }

chConfigurationGroup1 OBJECT-GROUP
    OBJECTS         {
                        callHomeEnable,
                        callHomeAlertAction,
                        callHomeAlertActionStatus,
                        callHomeAlertActionFailureCause,
                        callHomeDestProfileMsgFormat,
                        callHomeDestProfileMaxMsgSize,
                        callHomeDestProfileTrnsprtMthd,
                        callHomeDestProfileStatus,
                        callHomeDestProfileMsgLevel,
                        callHomeDestProfileAlertGroups,
                        callHomeEmailAddrTblMaxEntries,
                        callHomeDestEmailAddress,
                        callHomeDestEmailAddressStatus,
                        callHomeEmailFrom,
                        callHomeEmailReplyTo,
                        callHomeAlertGroupName
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects for displaying and
        configuring Call Home parameters."
    ::= { chMIBGroups 10 }

ccmMIBNotificationsGroup1 NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        ccmSmtpServerFailNotif,
                        ccmAlertGroupTypeAddedNotif,
                        ccmAlertGroupTypeDeletedNotif
                    }
    STATUS          current
    DESCRIPTION
        "A collection of notifications."
    ::= { chMIBGroups 11 }

chConfigurationGroup2 OBJECT-GROUP
    OBJECTS         {
                        callHomeEnable,
                        callHomeAlertAction,
                        callHomeAlertActionStatus,
                        callHomeAlertActionFailureCause,
                        callHomeDestProfileMsgFormat,
                        callHomeDestProfileMaxMsgSize,
                        callHomeDestProfileTrnsprtMthd,
                        callHomeDestProfileStatus,
                        callHomeDestProfileMsgLevel,
                        callHomeDestProfileAlertGroups,
                        callHomeEmailAddrTblMaxEntries,
                        callHomeDestEmailAddress,
                        callHomeDestEmailAddressStatus,
                        callHomeEmailFrom,
                        callHomeEmailReplyTo,
                        callHomeAlertGroupName,
                        ccmMsgThrottlingEnable
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects for displaying and
        configuring Call Home parameters."
    ::= { chMIBGroups 12 }

chSwInventoryInfoGroup OBJECT-GROUP
    OBJECTS         {
                        callHomeInventoryInfoName,
                        callHomeInventoryInfoValue,
                        ccmPeriodicSwInventoryMsgEnable,
                        ccmPeriodicSwInventoryTimeFrame
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects for displaying and
        configuring software inventory information."
    ::= { chMIBGroups 13 }

chPeriodicSwInventoryInfoGroup OBJECT-GROUP
    OBJECTS         {
                        ccmPeriodicSwInventoryMsgEnable,
                        ccmPeriodicSwInventoryTimeFrame
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects for configuring
        periodic software inventory information."
    ::= { chMIBGroups 14 }

chSwInventoryInfoGroup1 OBJECT-GROUP
    OBJECTS         {
                        callHomeInventoryInfoName,
                        callHomeInventoryInfoValue
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects for displaying
        software inventory information."
    ::= { chMIBGroups 15 }

ccmUserDefCmdGroup OBJECT-GROUP
    OBJECTS         {
                        callHomeUserDefMaxCmds,
                        callHomeUserDefCmdName,
                        callHomeUserDefCmdRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects for configuring user defined
        commands for the Call Home alert group types."
    ::= { chMIBGroups 16 }

ccmPeriodicSwInventoryInfoGroup1 OBJECT-GROUP
    OBJECTS         { ccmPeriodicSwInventoryTimeOfDay }
    STATUS          current
    DESCRIPTION
        "A collection of objects for configuring the
        additional information of periodic software
        inventory information."
    ::= { chMIBGroups 17 }

ccmConfigurationGroup3 OBJECT-GROUP
    OBJECTS         {
                        callHomeEnable,
                        callHomeDestProfileMsgFormat,
                        callHomeDestProfileTrnsprtMthd,
                        callHomeDestProfileStatus,
                        callHomeDestProfileMaxMsgSize,
                        callHomeEmailAddrTblMaxEntries,
                        callHomeDestEmailAddress,
                        callHomeDestEmailAddressStatus,
                        callHomeEmailFrom,
                        callHomeEmailReplyTo
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects for displaying and
        configuring Call Home parameters."
    ::= { chMIBGroups 18 }

ccmAlertActionGroup OBJECT-GROUP
    OBJECTS         {
                        callHomeAlertAction,
                        callHomeAlertActionStatus,
                        callHomeAlertActionFailureCause
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing control and status
        information for Call Home alert actions."
    ::= { chMIBGroups 19 }

ccmProfileMessageLevelGroup OBJECT-GROUP
    OBJECTS         { callHomeDestProfileMsgLevel }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing control over
        message filtering level for Call Home messages."
    ::= { chMIBGroups 20 }

ccmProfileActivationGroup OBJECT-GROUP
    OBJECTS         { callHomeDestProfileActive }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing control over
        activating and deactivating configured Call Home
        profiles."
    ::= { chMIBGroups 21 }

ccmProfileTestGroup OBJECT-GROUP
    OBJECTS         {
                        ccmDestProfileTestTrigger,
                        ccmDestProfileTestMessage,
                        ccmDestProfileTestStatus,
                        ccmDestProfileTestFailureCause
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing control over
        generation of test alert messages for a profile."
    ::= { chMIBGroups 22 }

ccmProfileAlertGroupsGroup OBJECT-GROUP
    OBJECTS         {
                        callHomeDestProfileAlertGroups,
                        callHomeAlertGroupName
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects that provide names to identify
        alert-groups supported by the system and ability to
        associate them with various profiles."
    ::= { chMIBGroups 23 }

ccmProfileAlertGroupControlGroup OBJECT-GROUP
    OBJECTS         { callHomeAlertGroupEnable }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing control over enabling
        and disabling various alert-groups supported by the
        system."
    ::= { chMIBGroups 24 }

ccmThrottleConfigurationGroup OBJECT-GROUP
    OBJECTS         { ccmMsgThrottlingEnable }
    STATUS          current
    DESCRIPTION
        "A collection of objects for controlling Call Home
        message throttling functionality."
    ::= { chMIBGroups 25 }

ccmSmtpServersPriorityGroup OBJECT-GROUP
    OBJECTS         { ccmSmtpServersPriority }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) providing priority related
        information for Call Home SMTP servers."
    ::= { chMIBGroups 26 }

ccmAlertGroupCapabilityGroup OBJECT-GROUP
    OBJECTS         { callHomeAlertGroupCapability }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) providing information about
        criteria used by system to issue message for the
        corresponding alert group."
    ::= { chMIBGroups 27 }

ccmHttpCfgGroup OBJECT-GROUP
    OBJECTS         {
                        callHomeDestType,
                        callHomeDestHttpUrl
                    }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) for configuring HTTP
        transport related information for delivering
        Call Home messages."
    ::= { chMIBGroups 28 }

ccmSeverityAlertGroupCfgGroup OBJECT-GROUP
    OBJECTS         { ccmAlertGroupSeverity }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing information of
        severity based alert groups."
    ::= { chMIBGroups 29 }

ccmPeriodicAlertGroupCfgGroup OBJECT-GROUP
    OBJECTS         {
                        ccmPeriodicAlertGroupInterval,
                        ccmPeriodicAlertGroupDayOfWeek,
                        ccmPeriodicAlertGroupDayOfMonth,
                        ccmPeriodicAlertGroupHour,
                        ccmPeriodicAlertGroupMinute,
                        ccmPeriodicAlertGroupEnable
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing information of
        periodic alert groups."
    ::= { chMIBGroups 30 }

ccmPatternAlertGroupCfgGroup OBJECT-GROUP
    OBJECTS         {
                        ccmMaxSyslogAlertGroupPatterns,
                        ccmPatternAlertGroupSeverity,
                        ccmPatternAlertGroupStorage,
                        ccmPatternAlertGroupStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing information of
        pattern based alert groups."
    ::= { chMIBGroups 31 }

ccmEventAlertGroupCfgGroup OBJECT-GROUP
    OBJECTS         {
                        ccmEventAlertGroupEnable,
                        ccmEventAlertGroupOperSeverity
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing information of
        event based alert groups."
    ::= { chMIBGroups 32 }

ccmSmtpMsgSendFailNotifCtrlGroup OBJECT-GROUP
    OBJECTS         { ccmSmtpMsgSendFailNotifEnable }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) to control SMTP message
        send failure related notification(s)."
    ::= { chMIBGroups 33 }

ccmSmtpMsgSendFailNotifGroup NOTIFICATION-GROUP
   NOTIFICATIONS    { ccmSmtpMsgSendFailNotif }
    STATUS          current
    DESCRIPTION
        "A collection of notification(s) for SMTP message
        send failures."
    ::= { chMIBGroups 34 }

ccmAlertHCStatisticsGroup OBJECT-GROUP
    OBJECTS         { callHomeHCAlerts }
    STATUS          current
    DESCRIPTION
        "A collection of objects for displaying
        Call Home 64 bit alert statistics."
    ::= { chMIBGroups 35 }

ccmAlertRateLimitGroup OBJECT-GROUP
    OBJECTS         {
                        ccmAlertsDropped,
                        ccmAlertRateLimit
                    }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) providing information regarding
        the Call Home rate limit mechanism."
    ::= { chMIBGroups 36 }

ccmSmtpServerStatusGroup OBJECT-GROUP
    OBJECTS         {
                        ccmSmtpServerStatusTimeStamp,
                        ccmSmtpServerStatusInitiate,
                        ccmSmtpServerStatusResult,
                        ccmSmtpServerStatusAvailability
                    }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) providing information
        regarding status availability of Call Home Smtp Servers."
    ::= { chMIBGroups 37 }

ccmProfileHiMessageSizeGroup OBJECT-GROUP
    OBJECTS         { callHomeDestProfileHiMaxMsgSize }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing information
        regarding to maximum size message to destination."
    ::= { chMIBGroups 38 }

chSystemInformationGroup1 OBJECT-GROUP
    OBJECTS         {
                        sysContactPhoneNumber,
                        sysContactEmailAddress,
                        sysStreetAddress,
                        callHomeCustomerId,
                        callHomeContractId,
                        callHomeSiteId
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects for displaying and
        configuring system information pertaining to
        Call Home."
    ::= { chMIBGroups 39 }

chSystemServicePriorityGroup OBJECT-GROUP
    OBJECTS         { callHomeDeviceServicePriority }
    STATUS          current
    DESCRIPTION
        "A collection of objects for configuring
        configuring system service priority pertaining to
        Call Home."
    ::= { chMIBGroups 40 }

ccmOnDemandMsgSendControlGroup OBJECT-GROUP
    OBJECTS         {
                        ccmOnDemandMsgSendAlertGroup,
                        ccmOnDemandMsgSendProfile,
                        ccmOnDemandMsgSendEntPhyIndex,
                        ccmOnDemandMsgSendTrigger
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects that enable sending on demand
        Call Home messages."
    ::= { chMIBGroups 41 }

ccmOnDemandMsgStatusGroup OBJECT-GROUP
    OBJECTS         { ccmOnDemandMsgServAvailable }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) to indicate status of
        on demand message service on the device."
    ::= { chMIBGroups 42 }

ccmSmartCallHomeGroup OBJECT-GROUP
    OBJECTS         {
                        ccmSmartCallHomeProfile,
                        ccmSmartCallHomeServiceType,
                        ccmSmartCallHomeAnalysisCmd,
                        ccmSmartCallHomeCcoId,
                        ccmSmartCallHomeTrigger
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects that enable issuing Smart Call Home
        messages."
    ::= { chMIBGroups 43 }

ccmEventStatsGroup OBJECT-GROUP
    OBJECTS         {
                        ccmEventStatsTotal,
                        ccmEventStatsConfiguration,
                        ccmEventStatsDiagnostic,
                        ccmEventStatsEnvironment,
                        ccmEventStatsInventory,
                        ccmEventStatsSystemLog,
                        ccmEventStatsTest,
                        ccmEventStatsRequest,
                        ccmEventStatsSendCliOutput
                    }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) indicating statistical information
        for the Call Home events."
    ::= { chMIBGroups 44 }

ccmEventNotifGroup NOTIFICATION-GROUP
   NOTIFICATIONS    { ccmEventNotif }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) indicating the Call Home events that
        occurred in the system."
    ::= { chMIBGroups 45 }

ccmCallhomeEventsGroup OBJECT-GROUP
    OBJECTS         {
                        ccmEventDescription,
                        ccmEventTime,
                        ccmEventUrgencyLevel
                    }
    STATUS          current
    DESCRIPTION
        "A collection of notification objects required for Call Home
        events that occurred in the system."
    ::= { chMIBGroups 46 }

ccmCallHomeVrfGroup OBJECT-GROUP
    OBJECTS         { ccmCallHomeVrfName }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) to manage VRF information for
        Call Home feature."
    ::= { chMIBGroups 47 }

ccmSmtpServersVrfGroup OBJECT-GROUP
    OBJECTS         { ccmSmtpServersUseVrf }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) to manage VRF information for
        SMTP Servers in Call Home feature."
    ::= { chMIBGroups 48 }

ccmHttpProxyServerGroup OBJECT-GROUP
    OBJECTS         {
                        ccmHttpProxyServerAddrType,
                        ccmHttpProxyServerAddr,
                        ccmHttpProxyServerPort,
                        ccmHttpProxyServerUseEnable
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects for displaying and
        configuring Call Home HTTP proxy server on the devices
        which support HTTP proxy server for Call Home feature"
    ::= { chMIBGroups 49 }

ccmHttpTransportVrfGroup OBJECT-GROUP
    OBJECTS         { ccmHttpTransportUseVrf }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) to manage VRF information for
        HTTP transport in Call Home feature."
    ::= { chMIBGroups 50 }

ccmSingleSmtpServerGroup OBJECT-GROUP
    OBJECTS         {
                        callHomeSmtpServerAddrType,
                        callHomeSmtpServerAddr,
                        callHomeSmtpServerPort,
                        callHomeSmtpServerUseVrf
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects for displaying and
        configuring Call Home SMTP server on the devices which
        support only one SMTP server."
    ::= { chMIBGroups 51 }

ccmMessageSourceGroup OBJECT-GROUP
    OBJECTS         {
                        ccmMsgSourceIpAddrType,
                        ccmMsgSourceIpAddr,
                        ccmMsgSourceInterface
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects to manage Call Home message
        source address."
    ::= { chMIBGroups 52 }

ccmCallHomePeriodicMinutesGroup OBJECT-GROUP
    OBJECTS         { ccmPeriodicAlertGroupIntervalMinutes }
    STATUS          current
    DESCRIPTION
        "A collection of objects to configure periodic interval
        in minutes."
    ::= { chMIBGroups 53 }

ccmOnDemandCliMsgGroup OBJECT-GROUP
    OBJECTS         {
                        ccmOnDemandCliMsgCliList,
                        ccmOnDemandCliMsgTransport,
                        ccmOnDemandCliMsgEmail,
                        ccmOnDemandCliMsgFormat,
                        ccmOnDemandCliMsgTacServiceReqId,
                        ccmOnDemandCliMsgTrigger
                    }
    STATUS          current
    DESCRIPTION
        "A collection of object(s) to manage on demand Call Home
        messages with CLI output."
    ::= { chMIBGroups 54 }

ccmCallHomeDiagSignatureGroup OBJECT-GROUP
    OBJECTS         {
                        ccmDiagSignatureActive,
                        ccmDiagSignatureProfileName,
                        ccmCallHomeDiagSignatureType,
                        ccmCallHomeDiagSignatureFuncDescr,
                        ccmCallHomeDiagSignatureRev,
                        ccmCallHomeDiagSignatureSigner,
                        ccmCallHomeDiagSignatureTriggerCount,
                        ccmCallHomeDiagSignatureAvgRuntime,
                        ccmCallHomeDiagSignatureMaxRuntime
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects to manage Call Home Diagnostic
        Signature functionality."
    ::= { chMIBGroups 55 }

ccmCallHomeSecurityLevelGroup OBJECT-GROUP
    OBJECTS         { ccmCallHomeSecurityLevel }
    STATUS          current
    DESCRIPTION
        "A collection of objects to manage security level of Call Home."
    ::= { chMIBGroups 56 }

ccmCallHomeAnonymousReportingGroup OBJECT-GROUP
    OBJECTS         { ccmAnonymousReportingEnable }
    STATUS          current
    DESCRIPTION
        "A collection of objects to manage reporting functionality of
        Call Home."
    ::= { chMIBGroups 57 }

ccmCallHomeAaaGroup OBJECT-GROUP
    OBJECTS         {
                        ccmAaaAuthEnable,
                        ccmAaaAuthUserName
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects to manage AAA functionality for
        Call Home."
    ::= { chMIBGroups 58 }

END










