HC-RMON-MIB DEFINITIONS ::= BEGIN
IMPORTS 
    MODULE-IDENTITY, OBJECT-TYPE, Counter32, Integer32, 
        Gauge32, Counter64 FROM SNMPv2-SMI 
    TEXTUAL-CONVENTION, RowStatus   FROM SNMPv2-TC 
    MODULE-COMPLIANCE, OBJECT-GROUP FROM SNMPv2-CONF 
    rmon, OwnerString, statistics, history, hosts, hostTopN, matrix, 
    etherStatsIndex, etherHistoryIndex, etherHistorySampleIndex, 
    hostIndex, hostAddress, hostTimeIndex, hostTimeCreationOrder, 
    hostTopNControlEntry, hostTopNReport, hostTopNIndex, 
    matrixSDIndex, matrixSDSourceAddress, matrixSDDestAddress, 
    matrixDSIndex, matrixDSDestAddress, matrixDSSourceAddress, 
    capture, captureBufferControlIndex, captureBufferIndex 
                                    FROM RMON-MIB 
    protocolDirLocalIndex, protocolDistControlIndex, 
    protocolDist, hlHostControlIndex, 
    nlHost, nlHostTimeMark, nlHostAddress, 
    hlMatrixControlIndex, nlMatrix, 
    nlMatrixSDTimeMark, nlMatrixSDSourceAddress, nlMatrixSDDestAddress, 
    nlMatrixDSTimeMark, nlMatrixDSDestAddress, nlMatrixDSSourceAddress, 
    nlMatrixTopNControlEntry, nlMatrixTopNControlIndex, nlMatrixTopNIndex, 
    alHost, alHostTimeMark, 
    alMatrix, alMatrixSDTimeMark, alMatrixDSTimeMark, 
    alMatrixTopNControlEntry, alMatrixTopNControlIndex, alMatrixTopNIndex, 
    usrHistory, usrHistoryControlIndex, 
    usrHistorySampleIndex, usrHistoryObjectIndex, 
    rmonConformance, ZeroBasedCounter32, probeConfig 
                                    FROM RMON2-MIB; 
--  Remote Network Monitoring MIB 
 
hcRMON MODULE-IDENTITY 
    LAST-UPDATED "9702120000Z" 
    ORGANIZATION "IETF RMON MIB Working Group" 
    CONTACT-INFO 
        "Steve Waldbusser 
        Postal: International Network Services 
        1213 Innsbruck Dr. 
        Sunnyvale, CA 94089 
        Phone:  +1 408 542 0251 
        Email:  waldbusser@ins.com" 
    DESCRIPTION 
        "The MIB module for managing remote monitoring 
        device implementations. This MIB module 
        augments the original RMON MIB as specified in 
        RFC 1757 and RFC 1513 and RMON2 MIB as specified in 
        RFC 2021." 
--    ::= { rmonConformance 3 } 
    ::= { rmonConformance 8 } 
 
-- { rmon 1 } through { rmon 20 } are defined in RMON [RFC 1757] and 
-- the Token Ring RMON MIB [RFC 1513] and the RMON2 MIB [RFC2021]. 
 
mediaIndependentStats  OBJECT IDENTIFIER ::= { rmon 21 } 
 
-- Textual Conventions 
 
ZeroBasedCounter64 ::= TEXTUAL-CONVENTION 
    STATUS current 
    DESCRIPTION 
        "This TC describes an object which counts events with the 
        following semantics: objects of this type will be set to 
        zero(0) on creation and will thereafter count appropriate 
        events, wrapping back to zero(0) when the value 2^64 is 
        reached. 
 
        Provided that an application discovers the new object within 
        the minimum time to wrap it can use the initial value as a 
 
 
 
 
 
 
 
 
 
 
 
        delta since it last polled the table of which this object is 
        part.  It is important for a management station to be aware of 
        this minimum time and the actual time between polls, and to 
        discard data if the actual time is too long or there is no 
        defined minimum time. 
 
        Typically this TC is used in tables where the INDEX space is 
        constantly changing and/or the TimeFilter mechanism is in use." 
    SYNTAX Counter64 
 
RmonGauge64 ::= TEXTUAL-CONVENTION 
    STATUS current 
    DESCRIPTION 
        "The RmonGauge64 type represents a non-negative integer, which 
        may increase or decrease, but shall never exceed a maximum value. 
        The maximum value can not be greater than 2^64-1. The value of a 
        Gauge has its maximum value whenever the information being modeled 
        is greater or equal to that maximum value; if the information 
        being modeled subsequently decreases below the maximum value, the 
        Gauge also decreases." 
    SYNTAX Counter64 
 
mediaIndependentTable OBJECT-TYPE 
    SYNTAX     SEQUENCE OF MediaIndependentEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Media independent statistics for promiscious monitoring of 
        any media. 
 
        The following table defines media independent statistics that 
        provides information for full and/or half-duplex links as well 
        as high capacity links. 
 
        For half-duplex links, the mediaIndependentOut* objects will 
        not be present. 
        For full-duplex links, the mediaIndependentOut* objects will be 
        present. Whenever possible, the probe should count packets 
        moving away from the closest terminating equipment as output 
        packets. Failing that, the probe should count packets moving 
        away from the DTE as output packets." 
    ::= { mediaIndependentStats 1 } 
 
mediaIndependentEntry OBJECT-TYPE 
    SYNTAX     MediaIndependentEntry 
 
 
 
 
 
 
 
 
 
 
 
    MAX-ACCESS not-accessible 
    STATUS      current 
    DESCRIPTION 
        "Media independent statistics for promiscious monitoring of 
        any media." 
    INDEX { mediaIndependentIndex } 
    ::= { mediaIndependentTable 1 } 
 
MediaIndependentEntry ::= SEQUENCE { 
    mediaIndependentIndex                       INTEGER (1..65535), 
    mediaIndependentDataSource                  OBJECT IDENTIFIER, 
    mediaIndependentDropEvents                  Counter32, 
    mediaIndependentDroppedFrames               Counter32, 
    mediaIndependentInPkts                      Counter32, 
    mediaIndependentInOverflowPkts              Counter32, 
    mediaIndependentInHighCapacityPkts          Counter64, 
    mediaIndependentOutPkts                     Counter32, 
    mediaIndependentOutOverflowPkts             Counter32, 
    mediaIndependentOutHighCapacityPkts         Counter64, 
    mediaIndependentInOctets                    Counter32, 
    mediaIndependentInOverflowOctets            Counter32, 
    mediaIndependentInHighCapacityOctets        Counter64, 
    mediaIndependentOutOctets                   Counter32, 
    mediaIndependentOutOverflowOctets           Counter32, 
    mediaIndependentOutHighCapacityOctets       Counter64, 
    mediaIndependentInNUCastPkts                Counter32, 
    mediaIndependentInNUCastOverflowPkts        Counter32, 
    mediaIndependentInNUCastHighCapacityPkts    Counter64, 
    mediaIndependentOutNUCastPkts               Counter32, 
    mediaIndependentOutNUCastOverflowPkts       Counter32, 
    mediaIndependentOutNUCastHighCapacityPkts   Counter64, 
    mediaIndependentInErrors                    Counter32, 
    mediaIndependentOutErrors                   Counter32, 
    mediaIndependentInputSpeed                  Gauge32, 
    mediaIndependentOutputSpeed                 Gauge32, 
    mediaIndependentOwner                       OwnerString, 
    mediaIndependentStatus                      RowStatus 
} 
 
mediaIndependentIndex OBJECT-TYPE 
    SYNTAX     INTEGER (1..65535) 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The value of this object uniquely identifies this 
 
 
 
 
 
 
 
 
 
 
 
        mediaIndependent entry." 
    ::= { mediaIndependentEntry 1 } 
 
mediaIndependentDataSource OBJECT-TYPE 
    SYNTAX     OBJECT IDENTIFIER 
    MAX-ACCESS read-create 
    STATUS     current 
    DESCRIPTION 
        "This object identifies the source of the data that 
        this mediaIndependent entry is configured to analyze.  This 
        source can be any interface on this device. 
        In order to identify a particular interface, this 
        object shall identify the instance of the ifIndex 
        object, defined in RFC 1213 and RFC 1573 [4,6], for 
        the desired interface.  For example, if an entry 
        were to receive data from interface #1, this object 
        would be set to ifIndex.1. 
 
        The statistics in this group reflect all packets 
        on the local network segment attached to the 
        identified interface. 
 
        An agent may or may not be able to tell if 
        fundamental changes to the media of the interface 
        have occurred and necessitate an invalidation of 
        this entry.  For example, a hot-pluggable ethernet 
        card could be pulled out and replaced by a 
        token-ring card.  In such a case, if the agent has 
        such knowledge of the change, it is recommended that 
        it invalidate this entry. 
 
        This object may not be modified if the associated 
        mediaIndependentStatus object is equal to valid(1)." 
    ::= { mediaIndependentEntry 2 } 
 
mediaIndependentDropEvents OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The total number of events in which packets 
        were dropped by the probe due to lack of resources. 
        Note that this number is not necessarily the number of 
        packets dropped; it is just the number of times this 
        condition has been detected." 
 
 
 
 
 
 
 
 
 
 
 
    ::= { mediaIndependentEntry 3 } 
 
mediaIndependentDroppedFrames OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
       "The total number of frames which were received by the probe 
        and therefore not accounted for in the 
        mediaIndependentDropEvents, but for which the probe chose not 
        to count for this entry for whatever reason.  Most often, this 
        event occurs when the probe is out of some resources and 
        decides to shed load from this collection. 
 
        This count does not include packets that were not counted 
        because they had MAC-layer errors. 
 
        Note that, unlike the dropEvents counter, this number is the 
        exact number of frames dropped." 
    ::= { mediaIndependentEntry 4 } 
 
mediaIndependentInPkts OBJECT-TYPE 
    SYNTAX      Counter32 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The total number of packets (including bad packets, 
        broadcast packets, and multicast packets) received 
        on a half-duplex link or on the inbound connection of a 
        full-duplex link." 
    ::= { mediaIndependentEntry 5 } 
 
mediaIndependentInOverflowPkts OBJECT-TYPE 
    SYNTAX      Counter32 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The number of times the associated 
        mediaIndependentInPkts counter has overflowed." 
    ::= { mediaIndependentEntry 6 } 
 
mediaIndependentInHighCapacityPkts OBJECT-TYPE 
    SYNTAX      Counter64 
    MAX-ACCESS  read-only 
    STATUS      current 
 
 
 
 
 
 
 
 
 
 
 
    DESCRIPTION 
        "The total number of packets (including bad packets, 
        broadcast packets, and multicast packets) received 
        on a half-duplex link or on the inbound connection of a 
        full-duplex link." 
    ::= { mediaIndependentEntry 7 } 
 
mediaIndependentOutPkts OBJECT-TYPE 
    SYNTAX      Counter32 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The total number of packets (including bad packets, 
        broadcast packets, and multicast packets) received on a 
        full-duplex link in the direction of the network." 
    ::= { mediaIndependentEntry 8 } 
 
mediaIndependentOutOverflowPkts OBJECT-TYPE 
    SYNTAX      Counter32 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The number of times the associated 
        mediaIndependentOutPkts counter has overflowed." 
    ::= { mediaIndependentEntry 9 } 
 
mediaIndependentOutHighCapacityPkts OBJECT-TYPE 
    SYNTAX      Counter64 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The total number of packets (including bad packets, 
        broadcast packets, and multicast packets) received on a 
        full-duplex link in the direction of the network." 
    ::= { mediaIndependentEntry 10 } 
 
mediaIndependentInOctets OBJECT-TYPE 
    SYNTAX      Counter32 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The total number of octets of data (including those in bad 
        packets) received (excluding framing bits but including FCS 
        octets) on a half-duplex link or on the inbound connection of 
        a full-duplex link." 
 
 
 
 
 
 
 
 
 
 
 
    ::= { mediaIndependentEntry 11 } 
 
mediaIndependentInOverflowOctets OBJECT-TYPE 
    SYNTAX      Counter32 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The number of times the associated 
        mediaIndependentInOctets counter has overflowed." 
    ::= { mediaIndependentEntry 12 } 
 
mediaIndependentInHighCapacityOctets OBJECT-TYPE 
    SYNTAX      Counter64 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The total number of octets of data (including those in bad 
        packets) received (excluding framing bits but 
        including FCS octets) on a half-duplex link or on the inbound 
        connection of a full-duplex link." 
    ::= { mediaIndependentEntry 13 } 
 
mediaIndependentOutOctets OBJECT-TYPE 
    SYNTAX      Counter32 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The total number of octets of data (including those in bad 
        packets) received on a full-duplex link in the direction of 
        the network (excluding framing bits but including FCS 
        octets)." 
    ::= { mediaIndependentEntry 14 } 
 
mediaIndependentOutOverflowOctets OBJECT-TYPE 
    SYNTAX      Counter32 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The number of times the associated 
        mediaIndependentOutOctets counter has overflowed." 
    ::= { mediaIndependentEntry 15 } 
 
mediaIndependentOutHighCapacityOctets OBJECT-TYPE 
    SYNTAX      Counter64 
    MAX-ACCESS  read-only 
 
 
 
 
 
 
 
 
 
 
 
    STATUS      current 
    DESCRIPTION 
        "The total number of packets (including bad packets, 
        broadcast packets, and multicast packets) received on a 
        full-duplex link in the direction of the network (excluding 
        framing bits but including FCS octets)." 
    ::= { mediaIndependentEntry 16 } 
 
mediaIndependentInNUCastPkts OBJECT-TYPE 
    SYNTAX      Counter32 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The total number of non-unicast packets (including bad 
        packets) received on a half-duplex link or on the inbound 
        connection of a full-duplex link." 
    ::= { mediaIndependentEntry 17 } 
 
mediaIndependentInNUCastOverflowPkts OBJECT-TYPE 
    SYNTAX      Counter32 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The number of times the associated 
        mediaIndependentInNUCastPkts counter has overflowed." 
    ::= { mediaIndependentEntry 18 } 
 
mediaIndependentInNUCastHighCapacityPkts OBJECT-TYPE 
    SYNTAX      Counter64 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The total number of non-unicast packets (including bad 
        packets) received on a half-duplex link or on the inbound 
        connection of a full-duplex link." 
    ::= { mediaIndependentEntry 19 } 
 
mediaIndependentOutNUCastPkts OBJECT-TYPE 
    SYNTAX      Counter32 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The total number of non-unicast packets (including bad 
        packets) received on a full-duplex link in the direction of 
        the network." 
 
 
 
 
 
 
 
 
 
 
 
    ::= { mediaIndependentEntry 20 } 
 
mediaIndependentOutNUCastOverflowPkts OBJECT-TYPE 
    SYNTAX      Counter32 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The number of times the associated 
        mediaIndependentOutNUCastPkts counter has overflowed." 
    ::= { mediaIndependentEntry 21 } 
 
mediaIndependentOutNUCastHighCapacityPkts OBJECT-TYPE 
    SYNTAX      Counter64 
    MAX-ACCESS  read-only 
    STATUS      current 
    DESCRIPTION 
        "The total number of packets (including bad packets) 
        received on a full-duplex link in the direction of the 
        network." 
    ::= { mediaIndependentEntry 22 } 
 
mediaIndependentInErrors OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The total number of bad packets received on a 
        half-duplex link or on the inbound connection of a 
        full-duplex link." 
    ::= { mediaIndependentEntry 23 } 
 
mediaIndependentOutErrors OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The total number of bad packets received on a full-duplex 
        link in the direction of the network." 
    ::= { mediaIndependentEntry 24 } 
 
mediaIndependentInputSpeed OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
 
 
 
 
 
 
 
 
 
 
 
        "The nominal maximum speed in kilobits per second of this 
        half-duplex link or on the inbound connection of this 
        full-duplex link. If the speed is unknown or there is no fixed 
        maximum (e.g. a compressed link), this value shall be zero." 
    ::= { mediaIndependentEntry 25 } 
 
mediaIndependentOutputSpeed OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The nominal maximum speed in kilobits per second of this 
        full-duplex link in the direction of the network. If the speed 
        is unknown or there is no fixed maximum (e.g. a compressed 
        link), this value shall be zero." 
    ::= { mediaIndependentEntry 26 } 
 
mediaIndependentOwner OBJECT-TYPE 
    SYNTAX     OwnerString 
    MAX-ACCESS read-create 
    STATUS     current 
    DESCRIPTION 
        "The entity that configured this entry and is 
        therefore using the resources assigned to it." 
    ::= { mediaIndependentEntry 27 } 
 
mediaIndependentStatus OBJECT-TYPE 
    SYNTAX      RowStatus 
    MAX-ACCESS  read-create 
    STATUS      current 
    DESCRIPTION 
        "The status of this media independent statistics entry." 
    ::= { mediaIndependentEntry 28 } 
 
 
 
-- High Capacity extensions for the etherStatsTable 
 
etherStatsHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF EtherStatsHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        etherStatsTable." 
 
 
 
 
 
 
 
 
 
 
 
    ::= { statistics 7 } 
 
etherStatsHighCapacityEntry  OBJECT-TYPE 
    SYNTAX     EtherStatsHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        etherStatsEntry. These objects will be created by the agent 
        for all etherStatsEntries it deems appropriate." 
    INDEX { etherStatsIndex } 
    ::= { etherStatsHighCapacityTable 1 } 
 
EtherStatsHighCapacityEntry ::= SEQUENCE { 
    etherStatsHighCapacityOverflowPkts                 Counter32, 
    etherStatsHighCapacityPkts                         Counter64, 
    etherStatsHighCapacityOverflowOctets               Counter32, 
    etherStatsHighCapacityOctets                       Counter64, 
    etherStatsHighCapacityOverflowPkts64Octets         Counter32, 
    etherStatsHighCapacityPkts64Octets                 Counter64, 
    etherStatsHighCapacityOverflowPkts65to127Octets    Counter32, 
    etherStatsHighCapacityPkts65to127Octets            Counter64, 
    etherStatsHighCapacityOverflowPkts128to255Octets   Counter32, 
    etherStatsHighCapacityPkts128to255Octets           Counter64, 
    etherStatsHighCapacityOverflowPkts256to511Octets   Counter32, 
    etherStatsHighCapacityPkts256to511Octets           Counter64, 
    etherStatsHighCapacityOverflowPkts512to1023Octets  Counter32, 
    etherStatsHighCapacityPkts512to1023Octets          Counter64, 
    etherStatsHighCapacityOverflowPkts1024to1518Octets Counter32, 
    etherStatsHighCapacityPkts1024to1518Octets         Counter64 
} 
 
etherStatsHighCapacityOverflowPkts OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated etherStatsPkts 
        counter has overflowed." 
    ::= { etherStatsHighCapacityEntry 1 } 
 
etherStatsHighCapacityPkts OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
 
 
 
 
 
 
 
 
 
 
 
    DESCRIPTION 
        "The total number of packets (including bad packets, 
        broadcast packets, and multicast packets) received." 
    ::= { etherStatsHighCapacityEntry 2 } 
 
etherStatsHighCapacityOverflowOctets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated etherStatsOctets 
        counter has overflowed." 
    ::= { etherStatsHighCapacityEntry 3 } 
 
etherStatsHighCapacityOctets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The total number of octets of data (including 
        those in bad packets) received on the 
        network (excluding framing bits but including 
        FCS octets). 
 
        If the network is half-duplex Fast Ethernet, this 
        object can be used as a reasonable estimate of 
        utilization. If greater precision is desired, the 
        etherStatsHighCapacityPkts and 
        etherStatsHighCapacityOctets objects should be sampled 
        before and after a common interval.  The differences 
        in the sampled values are Pkts and Octets, 
        respectively, and the number of seconds in the 
        interval is Interval.  These values 
        are used to calculate the Utilization as follows: 
 
                        Pkts * (.96 + .64) + (Octets * .08) 
        Utilization = ------------------------------------- 
                                Interval * 10,000 
 
        The result of this equation is the value Utilization 
        which is the percent utilization of the ethernet 
        segment on a scale of 0 to 100 percent. 
 
        This table is not appropriate for monitoring full-duplex 
        ethernets. If the network is a full-duplex ethernet and the 
 
 
 
 
 
 
 
 
 
 
 
        mediaIndependentTable is monitoring that network, the 
        utilization can be calculated as follows: 
 
        1) Determine the utilization of the inbound path by using 
           the appropriate equation (for ethernet or fast ethernet) 
           to determine the utilization, substituting 
           mediaIndependentInPkts for etherStatsHighCapacityPkts, and 
           mediaIndependentInOctets for etherStatsHighCapacityOctets. 
           Call the resulting utilization inUtilization. 
 
        2) Determine the utilization of the outbound path by using 
           the same equation to determine the utilization, substituting 
           mediaIndependentOutPkts for etherStatsHighCapacityPkts, and 
           mediaIndependentOutOctetss for etherStatsHighCapacityOctets. 
           Call the resulting utilization outUtilization. 
 
        3) The utilization is the maximum of inUtilization and 
           outUtilization. This metric shows the amount of percentage 
           of bandwidth that is left before congestion will be 
           experienced on the link." 
    ::= { etherStatsHighCapacityEntry 4 } 
 
etherStatsHighCapacityOverflowPkts64Octets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated etherStatsPkts64Octets 
        counter has overflowed." 
    ::= { etherStatsHighCapacityEntry 5 } 
 
etherStatsHighCapacityPkts64Octets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The total number of packets (including bad 
        packets) received that were 64 octets in length 
        (excluding framing bits but including FCS octets)." 
    ::= { etherStatsHighCapacityEntry 6 } 
 
etherStatsHighCapacityOverflowPkts65to127Octets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
 
 
 
 
 
 
 
 
 
 
 
    DESCRIPTION 
        "The number of times the associated etherStatsPkts65to127Octets 
        counter has overflowed." 
    ::= { etherStatsHighCapacityEntry 7 } 
 
etherStatsHighCapacityPkts65to127Octets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The total number of packets (including bad 
        packets) received that were between 
        65 and 127 octets in length inclusive 
        (excluding framing bits but including FCS octets)." 
    ::= { etherStatsHighCapacityEntry 8 } 
 
etherStatsHighCapacityOverflowPkts128to255Octets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated etherStatsPkts128to255Octets 
        counter has overflowed." 
    ::= { etherStatsHighCapacityEntry 9 } 
 
etherStatsHighCapacityPkts128to255Octets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The total number of packets (including bad 
        packets) received that were between 
        128 and 255 octets in length inclusive 
        (excluding framing bits but including FCS octets)." 
    ::= { etherStatsHighCapacityEntry 10 } 
 
etherStatsHighCapacityOverflowPkts256to511Octets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated etherStatsPkts256to511Octets 
        counter has overflowed." 
    ::= { etherStatsHighCapacityEntry 11 } 
 
 
 
 
 
 
 
 
 
 
 
 
etherStatsHighCapacityPkts256to511Octets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The total number of packets (including bad 
        packets) received that were between 
        256 and 511 octets in length inclusive 
        (excluding framing bits but including FCS octets)." 
    ::= { etherStatsHighCapacityEntry 12 } 
 
etherStatsHighCapacityOverflowPkts512to1023Octets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated etherStatsPkts512to1023Octets 
        counter has overflowed." 
    ::= { etherStatsHighCapacityEntry 13 } 
 
etherStatsHighCapacityPkts512to1023Octets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The total number of packets (including bad 
        packets) received that were between 
        512 and 1023 octets in length inclusive 
        (excluding framing bits but including FCS octets)." 
    ::= { etherStatsHighCapacityEntry 14 } 
 
etherStatsHighCapacityOverflowPkts1024to1518Octets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated etherStatsPkts1024to1518Octets 
        counter has overflowed." 
    ::= { etherStatsHighCapacityEntry 15 } 
 
etherStatsHighCapacityPkts1024to1518Octets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
 
 
 
 
 
 
 
 
 
 
 
        "The total number of packets (including bad 
        packets) received that were between 
        1024 and 1518 octets in length inclusive 
        (excluding framing bits but including FCS octets)." 
    ::= { etherStatsHighCapacityEntry 16 } 
 
-- High Capacity extensions for the etherHistoryTable 
 
etherHistoryHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF EtherHistoryHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        etherHistoryTable." 
    ::= { history 6 } 
 
etherHistoryHighCapacityEntry  OBJECT-TYPE 
    SYNTAX     EtherHistoryHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        etherHistoryEntry. These objects will be created by the agent 
        for all etherHistoryEntries associated with whichever 
        historyControlEntries it deems appropriate. (i.e., either all 
        etherHistoryHighCapacityEntries associated with a particular 
        historyControlEntry will be created, or none of them will 
        be.)" 
    INDEX { etherHistoryIndex, etherHistorySampleIndex } 
    ::= { etherHistoryHighCapacityTable 1 } 
 
EtherHistoryHighCapacityEntry ::= SEQUENCE { 
    etherHistoryHighCapacityOverflowPkts           Gauge32, 
    etherHistoryHighCapacityPkts                   RmonGauge64, 
    etherHistoryHighCapacityOverflowOctets         Gauge32, 
    etherHistoryHighCapacityOctets                 RmonGauge64 
} 
 
etherHistoryHighCapacityOverflowPkts OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated etherHistoryPkts 
 
 
 
 
 
 
 
 
 
 
 
        Gauge overflowed during this sampling interval." 
    ::= { etherHistoryHighCapacityEntry 1 } 
 
etherHistoryHighCapacityPkts OBJECT-TYPE 
    SYNTAX     RmonGauge64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The total number of packets (including bad packets, 
        broadcast packets, and multicast packets) received during 
        this sampling interval." 
    ::= { etherHistoryHighCapacityEntry 2 } 
 
etherHistoryHighCapacityOverflowOctets OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated etherHistoryOctets 
        counter has overflowed during this sampling interval." 
    ::= { etherHistoryHighCapacityEntry 3 } 
 
etherHistoryHighCapacityOctets OBJECT-TYPE 
    SYNTAX     RmonGauge64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The total number of octets of data (including 
        those in bad packets) received on the 
        network (excluding framing bits but including 
        FCS octets) during this sampling interval." 
    ::= { etherHistoryHighCapacityEntry 4 } 
 
-- High Capacity Extensions for the hostTable 
 
hostHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF HostHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        hostTable." 
    ::= { hosts 5 } 
 
hostHighCapacityEntry  OBJECT-TYPE 
 
 
 
 
 
 
 
 
 
 
 
    SYNTAX     HostHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        hostEntry. These objects will be created by the agent 
        for all hostEntries associated with whichever 
        hostControlEntries it deems appropriate. (i.e., either all 
        hostHighCapacityEntries associated with a particular 
        hostControlEntry will be created, or none of them will 
        be.)" 
    INDEX { hostIndex, hostAddress } 
    ::= { hostHighCapacityTable 1 } 
 
HostHighCapacityEntry ::= SEQUENCE { 
    hostHighCapacityInOverflowPkts    Counter32, 
    hostHighCapacityInPkts            Counter64, 
    hostHighCapacityOutOverflowPkts   Counter32, 
    hostHighCapacityOutPkts           Counter64, 
    hostHighCapacityInOverflowOctets  Counter32, 
    hostHighCapacityInOctets          Counter64, 
    hostHighCapacityOutOverflowOctets Counter32, 
    hostHighCapacityOutOctets         Counter64 
} 
 
hostHighCapacityInOverflowPkts OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated hostInPkts 
        counter has overflowed." 
    ::= { hostHighCapacityEntry 1 } 
 
hostHighCapacityInPkts OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of good packets transmitted to 
        this address since it was added to the 
        hostHighCapacityTable." 
    ::= { hostHighCapacityEntry 2 } 
 
hostHighCapacityOutOverflowPkts OBJECT-TYPE 
 
 
 
 
 
 
 
 
 
 
 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated hostOutPkts 
        counter has overflowed." 
    ::= { hostHighCapacityEntry 3 } 
 
hostHighCapacityOutPkts OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets, including bad packets, transmitted 
        by this address since it was added to the 
        hostHighCapacityTable." 
    ::= { hostHighCapacityEntry 4 } 
 
hostHighCapacityInOverflowOctets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated hostInOctets 
        counter has overflowed." 
    ::= { hostHighCapacityEntry 5 } 
 
hostHighCapacityInOctets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets transmitted to this address 
        since it was added to the hostHighCapacityTable (excluding 
        framing bits but including FCS octets), except for 
        those octets in bad packets." 
    ::= { hostHighCapacityEntry 6 } 
 
hostHighCapacityOutOverflowOctets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated hostOutOctets 
        counter has overflowed." 
 
 
 
 
 
 
 
 
 
 
 
    ::= { hostHighCapacityEntry 7 } 
 
hostHighCapacityOutOctets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets transmitted by this address 
        since it was added to the hostHighCapacityTable (excluding 
        framing bits but including FCS octets), including 
        those octets in bad packets." 
    ::= { hostHighCapacityEntry 8 } 
 
-- High Capacity extensions for the hostTimeTable 
 
hostTimeHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF HostTimeHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        hostTimeTable." 
    ::= { hosts 6 } 
 
hostTimeHighCapacityEntry  OBJECT-TYPE 
    SYNTAX     HostTimeHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        hostTimeEntry. These objects will be created by the agent 
        for all hostTimeEntries associated with whichever 
        hostControlEntries it deems appropriate. (i.e., either all 
        hostTimeHighCapacityEntries associated with a particular 
        hostControlEntry will be created, or none of them will 
        be.)" 
    INDEX { hostTimeIndex, hostTimeCreationOrder } 
    ::= { hostTimeHighCapacityTable 1 } 
 
HostTimeHighCapacityEntry ::= SEQUENCE { 
    hostTimeHighCapacityInOverflowPkts    Counter32, 
    hostTimeHighCapacityInPkts            Counter64, 
    hostTimeHighCapacityOutOverflowPkts   Counter32, 
    hostTimeHighCapacityOutPkts           Counter64, 
    hostTimeHighCapacityInOverflowOctets  Counter32, 
 
 
 
 
 
 
 
 
 
 
 
    hostTimeHighCapacityInOctets          Counter64, 
    hostTimeHighCapacityOutOverflowOctets Counter32, 
    hostTimeHighCapacityOutOctets         Counter64 
} 
 
hostTimeHighCapacityInOverflowPkts OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated hostTimeInPkts 
        counter has overflowed." 
    ::= { hostTimeHighCapacityEntry 1 } 
 
hostTimeHighCapacityInPkts OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of good packets transmitted to this address 
        since it was added to the hostTimeHighCapacityTable." 
    ::= { hostTimeHighCapacityEntry 2 } 
 
hostTimeHighCapacityOutOverflowPkts OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated hostTimeOutPkts 
        counter has overflowed." 
    ::= { hostTimeHighCapacityEntry 3 } 
 
hostTimeHighCapacityOutPkts OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets, including bad packets, transmitted 
        by this address since it was added to the 
        hostTimeHighCapacityTable." 
    ::= { hostTimeHighCapacityEntry 4 } 
 
hostTimeHighCapacityInOverflowOctets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
 
 
 
 
 
 
 
 
 
 
 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated hostTimeInOctets 
        counter has overflowed." 
    ::= { hostTimeHighCapacityEntry 5 } 
 
hostTimeHighCapacityInOctets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets transmitted to this address 
        since it was added to the hostTimeHighCapacityTable 
        (excluding framing bits but including FCS octets), 
        except for those octets in bad packets." 
    ::= { hostTimeHighCapacityEntry 6 } 
 
hostTimeHighCapacityOutOverflowOctets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated hostTimeOutOctets 
        counter has overflowed." 
    ::= { hostTimeHighCapacityEntry 7 } 
 
hostTimeHighCapacityOutOctets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets transmitted by this address since 
        it was added to the hostTimeTable (excluding framing 
        bits but including FCS octets), including those 
        octets in bad packets." 
    ::= { hostTimeHighCapacityEntry 8 } 
 
-- High Capacity Extensions for the hostTopNTable 
 
-- This definition extends the enumeration defined in [RFC 1757] 
hostTopNRateBase OBJECT-TYPE 
    SYNTAX INTEGER { 
            hostTopNInPkts(1), 
            hostTopNOutPkts(2), 
            hostTopNInOctets(3), 
 
 
 
 
 
 
 
 
 
 
 
            hostTopNOutOctets(4), 
            hostTopNOutErrors(5), 
            hostTopNOutBroadcastPkts(6), 
            hostTopNOutMulticastPkts(7), 
            hostTopNHCInPkts(8), 
            hostTopNHCOutPkts(9), 
            hostTopNHCInOctets(10), 
            hostTopNHCOutOctets(11) 
    } 
    MAX-ACCESS read-write 
    STATUS     current 
    DESCRIPTION 
        "The variable for each host that the hostTopNRate 
        variable is based upon, as well as a control 
        for the table that the results will be reported in. 
 
        This object may not be modified if the associated 
        hostTopNStatus [RFC 1757] object is equal to valid(1). 
 
        If this value is less than or equal to 7, when the report 
        is prepared, entries are created in the hostTopNTable 
        associated with this object. 
        If this value is greater than or equal to 8, when the report 
        is prepared, entries are created in the 
        hostTopNHighCapacityTable associated with this object." 
    ::= { hostTopNControlEntry 3 } 
 
hostTopNHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF HostTopNHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        hostTopNTable when hostTopNRateBase specifies a High Capacity 
    TopN Report." 
    ::= { hostTopN 3 } 
 
hostTopNHighCapacityEntry  OBJECT-TYPE 
    SYNTAX     HostTopNHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        hostTopNEntry when hostTopNRateBase specifies a High Capacity 
        TopN Report. These objects will be created by the agent 
 
 
 
 
 
 
 
 
 
 
 
        for all hostTopNEntries associated with whichever 
        hostTopNControlEntries have a hostTopNRateBase that specify 
        a high capacity report." 
    INDEX { hostTopNReport, hostTopNIndex } 
    ::= { hostTopNHighCapacityTable 1 } 
 
HostTopNHighCapacityEntry ::= SEQUENCE { 
     hostTopNHighCapacityBaseRate       Gauge32, 
     hostTopNHighCapacityOverflowRate   Gauge32, 
     hostTopNHighCapacityRate           RmonGauge64 
} 
 
hostTopNHighCapacityBaseRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
          "The amount of change in the selected variable 
          during this sampling interval, modulo 2^32.  The 
          selected variable is this host's instance of the 
          object selected by hostTopNRateBase." 
    ::= { hostTopNHighCapacityEntry 1 } 
 
hostTopNHighCapacityOverflowRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
          "The amount of change in the selected variable 
          during this sampling interval, divided by 2^32, truncating 
          fractions (i.e., X DIV 2^32).  The selected variable is 
          this host's instance of the object selected by 
          hostTopNRateBase." 
    ::= { hostTopNHighCapacityEntry 2 } 
 
hostTopNHighCapacityRate OBJECT-TYPE 
     SYNTAX     RmonGauge64 
     MAX-ACCESS read-only 
     STATUS     current 
     DESCRIPTION 
          "The amount of change in the selected variable 
          during this sampling interval.  The selected 
          variable is this host's instance of the object 
          selected by hostTopNRateBase." 
     ::= { hostTopNHighCapacityEntry 3 } 
 
 
 
 
 
 
 
 
 
 
 
-- High Capacity Extensions for the matrixSDTable 
 
matrixSDHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF MatrixSDHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        matrixSDTable." 
    ::= { matrix 5 } 
 
matrixSDHighCapacityEntry  OBJECT-TYPE 
    SYNTAX     MatrixSDHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        matrixSDEntry. These objects will be created by the agent 
        for all matrixSDEntries associated with whichever 
        matrixControlEntries it deems appropriate. (i.e., either all 
        matrixSDHighCapacityEntries associated with a particular 
        matrixControlEntry will be created, or none of them will 
        be.)" 
    INDEX { matrixSDIndex, 
            matrixSDSourceAddress, matrixSDDestAddress } 
    ::= { matrixSDHighCapacityTable 1 } 
 
MatrixSDHighCapacityEntry ::= SEQUENCE { 
    matrixSDHighCapacityOverflowPkts   Counter32, 
    matrixSDHighCapacityPkts           Counter64, 
    matrixSDHighCapacityOverflowOctets Counter32, 
    matrixSDHighCapacityOctets         Counter64 
} 
 
matrixSDHighCapacityOverflowPkts OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated matrixSDPkts 
        counter has overflowed." 
    ::= { matrixSDHighCapacityEntry 1 } 
 
matrixSDHighCapacityPkts OBJECT-TYPE 
    SYNTAX     Counter64 
 
 
 
 
 
 
 
 
 
 
 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets transmitted from the source 
        address to the destination address (this number 
        includes bad packets)." 
    ::= { matrixSDHighCapacityEntry 2 } 
 
matrixSDHighCapacityOverflowOctets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated matrixSDOctets 
        counter has overflowed." 
    ::= { matrixSDHighCapacityEntry 3 } 
 
matrixSDHighCapacityOctets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets (excluding framing bits but 
        including FCS octets) contained in all packets 
        transmitted from the source address to the 
        destination address." 
    ::= { matrixSDHighCapacityEntry 4 } 
 
-- High Capacity extensions for the matrixDSTable 
 
matrixDSHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF MatrixDSHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
        matrixDSTable." 
    ::= { matrix 6 } 
 
matrixDSHighCapacityEntry  OBJECT-TYPE 
    SYNTAX     MatrixDSHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-1 
 
 
 
 
 
 
 
 
 
 
 
        matrixDSEntry. These objects will be created by the agent 
        for all matrixDSEntries associated with whichever 
        matrixControlEntries it deems appropriate. (i.e., either all 
        matrixDSHighCapacityEntries associated with a particular 
        matrixControlEntry will be created, or none of them will 
        be.)" 
    INDEX { matrixDSIndex, 
            matrixDSDestAddress, matrixDSSourceAddress } 
    ::= { matrixDSHighCapacityTable 1 } 
 
MatrixDSHighCapacityEntry ::= SEQUENCE { 
    matrixDSHighCapacityOverflowPkts   Counter32, 
    matrixDSHighCapacityPkts           Counter64, 
    matrixDSHighCapacityOverflowOctets Counter32, 
    matrixDSHighCapacityOctets         Counter64 
} 
 
matrixDSHighCapacityOverflowPkts OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated matrixDSPkts 
        counter has overflowed." 
    ::= { matrixDSHighCapacityEntry 1 } 
 
matrixDSHighCapacityPkts OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets transmitted from the source 
        address to the destination address (this number 
        includes bad packets)." 
    ::= { matrixDSHighCapacityEntry 2 } 
 
matrixDSHighCapacityOverflowOctets OBJECT-TYPE 
    SYNTAX     Counter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated matrixDSOctets 
        counter has overflowed." 
    ::= { matrixDSHighCapacityEntry 3 } 
 
 
 
 
 
 
 
 
 
 
 
 
matrixDSHighCapacityOctets OBJECT-TYPE 
    SYNTAX     Counter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets (excluding framing bits 
        but including FCS octets) contained in all packets 
        transmitted from the source address to the 
        destination address." 
    ::= { matrixDSHighCapacityEntry 4 } 
 
-- High Capacity extensions for the captureBufferTable 
 
captureBufferHighCapacityTable OBJECT-TYPE 
    SYNTAX     SEQUENCE OF CaptureBufferHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON 
        captureBufferTable." 
    ::= { capture 3 } 
 
captureBufferHighCapacityEntry OBJECT-TYPE 
    SYNTAX     CaptureBufferHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON 
        captureBufferEntry. These objects will be created by the agent 
        for all captureBufferEntries associated with whichever 
        bufferControlEntries it deems appropriate. (i.e., either all 
        captureBufferHighCapacityEntries associated with a particular 
        bufferControlEntry will be created, or none of them will 
        be.)" 
    INDEX { captureBufferControlIndex, captureBufferIndex } 
    ::= { captureBufferHighCapacityTable 1 } 
 
CaptureBufferHighCapacityEntry ::= SEQUENCE { 
    captureBufferPacketHighCapacityTime     Integer32 
} 
 
captureBufferPacketHighCapacityTime  OBJECT-TYPE 
    SYNTAX      Integer32 (0..999999) 
    UNITS       "nanoseconds" 
    MAX-ACCESS  read-only 
 
 
 
 
 
 
 
 
 
 
 
    STATUS      current 
    DESCRIPTION 
        "The number of nanoseconds that had passed since this capture 
        buffer was first turned on when this packet was captured, 
        modulo 10^6. 
 
        This object is used in conjunction with existing timestamp 
        object. This object returns the number of nano-seconds to be 
        added to to number of milli-seconds obtained from the 
        captureBufferPacketTime object, to obtain more accurate 
        inter packet arrival time." 
  ::= { captureBufferHighCapacityEntry 1 } 
 
-- High Capacity extensions for the protocolDistStatsTable 
 
protocolDistStatsHighCapacityTable OBJECT-TYPE 
    SYNTAX     SEQUENCE OF ProtocolDistStatsHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        protocolDistStatsTable." 
    ::= { protocolDist 3 } 
 
protocolDistStatsHighCapacityEntry OBJECT-TYPE 
    SYNTAX     ProtocolDistStatsHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        protocolDistStatsTable. These objects will be created by the 
        agent for all protocolDistStatsEntries associated with 
        whichever protocolDistControlEntries it deems appropriate. 
        (i.e., either all protocolDistStatsHighCapacityEntries 
        associated with a particular protocolDistControlEntry will be 
        created, or none of them will be.)" 
    INDEX { protocolDistControlIndex, protocolDirLocalIndex } 
    ::= { protocolDistStatsHighCapacityTable 1 } 
 
ProtocolDistStatsHighCapacityEntry ::= SEQUENCE { 
    protocolDistStatsHighCapacityOverflowPkts   ZeroBasedCounter32, 
    protocolDistStatsHighCapacityPkts           ZeroBasedCounter64, 
    protocolDistStatsHighCapacityOverflowOctets ZeroBasedCounter32, 
    protocolDistStatsHighCapacityOctets         ZeroBasedCounter64 
} 
 
 
 
 
 
 
 
 
 
 
 
protocolDistStatsHighCapacityOverflowPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated protocolDistStatsPkts 
        counter has overflowed." 
    ::= { protocolDistStatsHighCapacityEntry 1 } 
 
protocolDistStatsHighCapacityPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets without errors received of this 
        protocol type.  Note that this is the number of link-layer 
        packets, so if a single network-layer packet is fragmented 
        into several link-layer frames, this counter is incremented 
        several times." 
    ::= { protocolDistStatsHighCapacityEntry 2 } 
 
protocolDistStatsHighCapacityOverflowOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated protocolDistStatsOctets 
        counter has overflowed." 
    ::= { protocolDistStatsHighCapacityEntry 3 } 
 
protocolDistStatsHighCapacityOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets in packets received of this protocol 
        type since it was added to the protocolDistStatsTable 
        (excluding framing bits but including FCS octets), except for 
        those octets in packets that contained errors. 
 
        Note this doesn't count just those octets in the particular 
        protocol frames, but includes the entire packet that contained 
        the protocol." 
    ::= { protocolDistStatsHighCapacityEntry 4 } 
 
 
 
 
 
 
 
 
 
 
 
 
-- High Capacity extensions for the nlHostTable. 
 
nlHostHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF NlHostHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        nlHostTable." 
    ::= { nlHost 3 } 
 
nlHostHighCapacityEntry  OBJECT-TYPE 
    SYNTAX     NlHostHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        nlHostEntry. These objects will be created by the agent 
        for all nlHostEntries associated with whichever 
        hlHostControlEntries it deems appropriate. (i.e., either all 
        nlHostHighCapacityEntries associated with a particular 
        hlHostControlEntry will be created, or none of them will 
        be.)" 
    INDEX { hlHostControlIndex, nlHostTimeMark, 
            protocolDirLocalIndex, nlHostAddress } 
    ::= { nlHostHighCapacityTable 1 } 
 
NlHostHighCapacityEntry ::= SEQUENCE { 
    nlHostHighCapacityInOverflowPkts    ZeroBasedCounter32, 
    nlHostHighCapacityInPkts            ZeroBasedCounter64, 
    nlHostHighCapacityOutOverflowPkts   ZeroBasedCounter32, 
    nlHostHighCapacityOutPkts           ZeroBasedCounter64, 
    nlHostHighCapacityInOverflowOctets  ZeroBasedCounter32, 
    nlHostHighCapacityInOctets          ZeroBasedCounter64, 
    nlHostHighCapacityOutOverflowOctets ZeroBasedCounter32, 
    nlHostHighCapacityOutOctets         ZeroBasedCounter64 
} 
 
nlHostHighCapacityInOverflowPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated nlHostInPkts 
        counter has overflowed." 
 
 
 
 
 
 
 
 
 
 
 
    ::= { nlHostHighCapacityEntry 1 } 
 
nlHostHighCapacityInPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets without errors transmitted to 
        this address since it was added to the nlHostHighCapacityTable. 
        Note that this is the number of link-layer packets, so if a 
        single network-layer packet is fragmented into several 
        link-layer frames, this counter is incremented several times." 
    ::= { nlHostHighCapacityEntry 2 } 
 
nlHostHighCapacityOutOverflowPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated nlHostOutPkts 
        counter has overflowed." 
    ::= { nlHostHighCapacityEntry 3 } 
 
nlHostHighCapacityOutPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets without errors transmitted by 
        this address since it was added to the nlHostHighCapacityTable. 
        Note that this is the number of link-layer packets, so if a 
        single network-layer packet is fragmented into several 
        link-layer frames, this counter is incremented several times." 
    ::= { nlHostHighCapacityEntry 4 } 
 
nlHostHighCapacityInOverflowOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated nlHostInOctets 
        counter has overflowed." 
    ::= { nlHostHighCapacityEntry 5 } 
 
nlHostHighCapacityInOctets OBJECT-TYPE 
 
 
 
 
 
 
 
 
 
 
 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets transmitted to this address 
        since it was added to the nlHostHighCapacityTable 
        (excluding framing bits but including FCS octets), 
        excluding those octets in packets that contained 
        errors. 
 
        Note this doesn't count just those octets in the 
        particular protocol frames, but includes the entire 
        packet that contained the protocol." 
    ::= { nlHostHighCapacityEntry 6 } 
 
nlHostHighCapacityOutOverflowOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated nlHostOutOctets 
        counter has overflowed." 
    ::= { nlHostHighCapacityEntry 7 } 
 
nlHostHighCapacityOutOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets transmitted by this address 
        since it was added to the nlHostHighCapacityTable 
        (excluding framing bits but including FCS octets), 
        excluding those octets in packets that contained 
        errors. 
 
        Note this doesn't count just those octets in the 
        particular protocol frames, but includes the entire 
        packet that contained the protocol." 
    ::= { nlHostHighCapacityEntry 8 } 
 
-- High Capacity extensions for the nlMatrixTable 
 
nlMatrixSDHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF NlMatrixSDHighCapacityEntry 
    MAX-ACCESS not-accessible 
 
 
 
 
 
 
 
 
 
 
 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        nlMatrixTable." 
    ::= { nlMatrix 6 } 
 
nlMatrixSDHighCapacityEntry  OBJECT-TYPE 
    SYNTAX     NlMatrixSDHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        nlMatrixEntry. These objects will be created by the agent 
        for all nlMatrixSDEntries associated with whichever 
        hlMatrixControlEntries it deems appropriate. (i.e., either all 
        nlMatrixSDHighCapacityEntries associated with a particular 
        hlMatrixControlEntry will be created, or none of them will 
        be.)" 
    INDEX { hlMatrixControlIndex, nlMatrixSDTimeMark, 
            protocolDirLocalIndex, 
            nlMatrixSDSourceAddress, nlMatrixSDDestAddress } 
    ::= { nlMatrixSDHighCapacityTable 1 } 
 
NlMatrixSDHighCapacityEntry ::= SEQUENCE { 
    nlMatrixSDHighCapacityOverflowPkts   ZeroBasedCounter32, 
    nlMatrixSDHighCapacityPkts           ZeroBasedCounter64, 
    nlMatrixSDHighCapacityOverflowOctets ZeroBasedCounter32, 
    nlMatrixSDHighCapacityOctets         ZeroBasedCounter64 
} 
 
nlMatrixSDHighCapacityOverflowPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated nlMatrixSDPkts 
        counter has overflowed." 
    ::= { nlMatrixSDHighCapacityEntry 1 } 
 
nlMatrixSDHighCapacityPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets without errors transmitted from the 
 
 
 
 
 
 
 
 
 
 
 
        source address to the destination address since this entry was 
        added to the nlMatrixSDHighCapacityTable.  Note that this is 
        the number of link-layer packets, so if a single network-layer 
        packet is fragmented into several link-layer frames, this 
        counter is incremented several times." 
    ::= { nlMatrixSDHighCapacityEntry 2 } 
 
nlMatrixSDHighCapacityOverflowOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated nlMatrixSDOctets 
        counter has overflowed." 
    ::= { nlMatrixSDHighCapacityEntry 3 } 
 
nlMatrixSDHighCapacityOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets transmitted from the source address to 
        the destination address since this entry was added to the 
        nlMatrixSDHighCapacityTable (excluding framing bits but 
        including FCS octets), excluding those octets in packets that 
        contained errors. 
 
        Note this doesn't count just those octets in the particular 
        protocol frames, but includes the entire packet that contained 
        the protocol." 
    ::= { nlMatrixSDHighCapacityEntry 4 } 
 
-- High Capacity extensions for the nlMatrixDSTable 
 
nlMatrixDSHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF NlMatrixDSHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        nlMatrixDSTable." 
    ::= { nlMatrix 7 } 
 
nlMatrixDSHighCapacityEntry  OBJECT-TYPE 
    SYNTAX     NlMatrixDSHighCapacityEntry 
 
 
 
 
 
 
 
 
 
 
 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        nlMatrixDSEntry. These objects will be created by the agent 
        for all nlMatrixDSEntries associated with whichever 
        hlmatrixControlEntries it deems appropriate. (i.e., either all 
        nlMatrixDSHighCapacityEntries associated with a particular 
        hlMatrixControlEntry will be created, or none of them will 
        be.)" 
    INDEX { hlMatrixControlIndex, nlMatrixDSTimeMark, 
            protocolDirLocalIndex, 
            nlMatrixDSDestAddress, nlMatrixDSSourceAddress } 
    ::= { nlMatrixDSHighCapacityTable 1 } 
 
NlMatrixDSHighCapacityEntry ::= SEQUENCE { 
    nlMatrixDSHighCapacityOverflowPkts   ZeroBasedCounter32, 
    nlMatrixDSHighCapacityPkts           ZeroBasedCounter64, 
    nlMatrixDSHighCapacityOverflowOctets ZeroBasedCounter32, 
    nlMatrixDSHighCapacityOctets         ZeroBasedCounter64 
} 
 
nlMatrixDSHighCapacityOverflowPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated nlMatrixDSPkts 
        counter has overflowed." 
    ::= { nlMatrixDSHighCapacityEntry 1 } 
 
nlMatrixDSHighCapacityPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets without errors transmitted from the 
        source address to the destination address since this entry was 
        added to the nlMatrixHighCapacityDSTable.  Note that this is 
        the number of link-layer packets, so if a single network-layer 
        packet is fragmented into several link-layer frames, this 
        counter is incremented several times." 
    ::= { nlMatrixDSHighCapacityEntry 2 } 
 
nlMatrixDSHighCapacityOverflowOctets OBJECT-TYPE 
 
 
 
 
 
 
 
 
 
 
 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated nlMatrixDSOctets 
        counter has overflowed." 
    ::= { nlMatrixDSHighCapacityEntry 3 } 
 
nlMatrixDSHighCapacityOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets transmitted from the source address 
        to the destination address since this entry was added to the 
        nlMatrixDSHighCapacityTable (excluding framing bits but 
        including FCS octets), excluding those octets in packets that 
        contained errors. 
 
        Note this doesn't count just those octets in the particular 
        protocol frames, but includes the entire packet that contained 
        the protocol." 
    ::= { nlMatrixDSHighCapacityEntry 4 } 
 
-- High Capacity extensions for the nlMatrixTopNTable 
 
-- This definition extends the enumeration defined in [RFC 2021] 
nlMatrixTopNControlRateBase OBJECT-TYPE 
    SYNTAX      INTEGER { 
                    nlMatrixTopNPkts(1), 
                    nlMatrixTopNOctets(2), 
                    nlMatrixTopNHighCapacityPkts(3), 
                    nlMatrixTopNHighCapacityOctets(4) 
                } 
    MAX-ACCESS read-create 
    STATUS     current 
    DESCRIPTION 
        "The variable for each nlMatrix[SD/DS] entry that the 
        nlMatrixTopNEntries are sorted by, as well as a control 
        for the table that the results will be reported in. 
 
        This object may not be modified if the associated 
        nlMatrixTopNControlStatus object is equal to active(1). 
 
        If this value is less than or equal to 2, when the report 
 
 
 
 
 
 
 
 
 
 
 
        is prepared, entries are created in the nlMatrixTopNTable 
        associated with this object. 
        If this value is greater than or equal to 3, when the report 
        is prepared, entries are created in the 
        nlMatrixTopNHighCapacityTable associated with this object." 
    ::= { nlMatrixTopNControlEntry 3 } 
 
nlMatrixTopNHighCapacityTable OBJECT-TYPE 
    SYNTAX     SEQUENCE OF NlMatrixTopNHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        nlMatrixTopNTable when nlMatrixTopNControlRateBase specifies 
        a High Capacity TopN Report." 
    ::= { nlMatrix 8 } 
 
nlMatrixTopNHighCapacityEntry OBJECT-TYPE 
    SYNTAX     NlMatrixTopNHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        nlMatrixTopNEntry when nlMatrixTopNControlRateBase specifies 
        a High Capacity TopN Report. These objects will be created by 
        the agent for all nlMatrixTopNEntries associated with whichever 
        nlMatrixTopNControlEntries have a nlMatrixTopNControlRateBase 
        that specify a high capacity report." 
    INDEX { nlMatrixTopNControlIndex, nlMatrixTopNIndex } 
    ::= { nlMatrixTopNHighCapacityTable 1 } 
 
NlMatrixTopNHighCapacityEntry ::= SEQUENCE { 
    nlMatrixTopNHighCapacityBasePktRate               Gauge32, 
    nlMatrixTopNHighCapacityOverflowPktRate           Gauge32, 
    nlMatrixTopNHighCapacityPktRate                   RmonGauge64, 
    nlMatrixTopNHighCapacityReverseBasePktRate        Gauge32, 
    nlMatrixTopNHighCapacityReverseOverflowPktRate    Gauge32, 
    nlMatrixTopNHighCapacityReversePktRate            RmonGauge64, 
    nlMatrixTopNHighCapacityBaseOctetRate             Gauge32, 
    nlMatrixTopNHighCapacityOverflowOctetRate         Gauge32, 
    nlMatrixTopNHighCapacityOctetRate                 RmonGauge64, 
    nlMatrixTopNHighCapacityReverseBaseOctetRate      Gauge32, 
    nlMatrixTopNHighCapacityReverseOverflowOctetRate  Gauge32, 
    nlMatrixTopNHighCapacityReverseOctetRate          RmonGauge64 
} 
 
 
 
 
 
 
 
 
 
 
 
nlMatrixTopNHighCapacityBasePktRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets seen from the source host 
        to the destination host during this sampling interval, 
        modulo 2^32, counted using the rules for counting the 
        nlMatrixSDPkts object." 
    ::= { nlMatrixTopNHighCapacityEntry 1 } 
 
nlMatrixTopNHighCapacityOverflowPktRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets seen from the source host 
        to the destination host during this sampling interval, 
        divided by 2^32, truncating fractions (i.e., X DIV 2^32), 
        and counted using the rules for counting the 
        nlMatrixSDPkts object." 
    ::= { nlMatrixTopNHighCapacityEntry 2 } 
 
nlMatrixTopNHighCapacityPktRate OBJECT-TYPE 
    SYNTAX     RmonGauge64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets seen from the source host 
        to the destination host during this sampling interval, 
    counted using the rules for counting the 
        nlMatrixSDPkts object. 
        If the value of nlMatrixTopNControlRateBase is 
        nlMatrixTopNHighCapacityPkts, this variable will be used 
        to sort this report." 
    ::= { nlMatrixTopNHighCapacityEntry 3 } 
 
nlMatrixTopNHighCapacityReverseBasePktRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets seen from the destination host to the 
        source host during this sampling interval, modulo 2^32, counted 
        using the rules for counting the nlMatrixSDPkts object (note 
 
 
 
 
 
 
 
 
 
 
 
        that the corresponding nlMatrixSDPkts object selected is the 
        one whose source address is equal to nlMatrixTopNDestAddress 
        and whose destination address is equal to 
        nlMatrixTopNSourceAddress.) 
 
        Note that if the value of nlMatrixTopNControlRateBase is equal 
        to nlMatrixTopNHighCapacityPkts, the sort of topN entries is 
        based entirely on nlMatrixTopNHighCapacityPktRate, and not on 
        the value of this object." 
    ::= { nlMatrixTopNHighCapacityEntry 4 } 
 
nlMatrixTopNHighCapacityReverseOverflowPktRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets seen from the destination host to the 
        source host during this sampling interval, divided by 2^32, 
    truncating fractions (i.e., X DIV 2^32), and counted 
        using the rules for counting the nlMatrixSDPkts object (note 
        that the corresponding nlMatrixSDPkts object selected is the 
        one whose source address is equal to nlMatrixTopNDestAddress 
        and whose destination address is equal to 
        nlMatrixTopNSourceAddress.) 
 
        Note that if the value of nlMatrixTopNControlRateBase is equal 
        to nlMatrixTopNHighCapacityPkts, the sort of topN entries is 
        based entirely on nlMatrixTopNHighCapacityPktRate, and not on 
        the value of this object." 
    ::= { nlMatrixTopNHighCapacityEntry 5 } 
 
nlMatrixTopNHighCapacityReversePktRate OBJECT-TYPE 
    SYNTAX     RmonGauge64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets seen from the destination host to the 
        source host during this sampling interval, counted 
        using the rules for counting the nlMatrixSDPkts object (note 
        that the corresponding nlMatrixSDPkts object selected is the 
        one whose source address is equal to nlMatrixTopNDestAddress 
        and whose destination address is equal to 
        nlMatrixTopNSourceAddress.) 
 
        Note that if the value of nlMatrixTopNControlRateBase is equal 
 
 
 
 
 
 
 
 
 
 
 
        to nlMatrixTopNHighCapacityPkts, the sort of topN entries is 
        based entirely on nlMatrixTopNHighCapacityPktRate, and not on 
        the value of this object." 
    ::= { nlMatrixTopNHighCapacityEntry 6 } 
 
nlMatrixTopNHighCapacityBaseOctetRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets seen from the source host 
        to the destination host during this sampling interval, 
        modulo 2^32, counted using the rules for counting the 
        nlMatrixSDOctets object." 
    ::= { nlMatrixTopNHighCapacityEntry 7 } 
 
nlMatrixTopNHighCapacityOverflowOctetRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets seen from the source host 
        to the destination host during this sampling interval, 
        divided by 2^32, truncating fractions (i.e., X DIV 2^32), 
        and counted using the rules for counting the 
        nlMatrixSDOctets object." 
    ::= { nlMatrixTopNHighCapacityEntry 8 } 
 
nlMatrixTopNHighCapacityOctetRate OBJECT-TYPE 
    SYNTAX     RmonGauge64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets seen from the source host 
        to the destination host during this sampling interval, 
    counted using the rules for counting the 
        nlMatrixSDOctets object. 
        If the value of nlMatrixTopNControlRateBase is 
        nlMatrixTopNHighCapacityOctets, this variable will be used 
        to sort this report." 
    ::= { nlMatrixTopNHighCapacityEntry 9 } 
 
nlMatrixTopNHighCapacityReverseBaseOctetRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
 
 
 
 
 
 
 
 
 
 
 
    STATUS     current 
    DESCRIPTION 
        "The number of octets seen from the destination host to the 
        source host during this sampling interval, modulo 2^32, counted 
        using the rules for counting the nlMatrixSDOctets object (note 
        that the corresponding nlMatrixSDOctets object selected is the 
        one whose source address is equal to nlMatrixTopNDestAddress 
        and whose destination address is equal to 
        nlMatrixTopNSourceAddress.) 
 
        Note that if the value of nlMatrixTopNControlRateBase is equal 
        to nlMatrixTopNHighCapacityOctets, the sort of topN entries is 
        based entirely on nlMatrixTopNHighCapacityOctetRate, and not on 
        the value of this object." 
    ::= { nlMatrixTopNHighCapacityEntry 10 } 
 
nlMatrixTopNHighCapacityReverseOverflowOctetRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets seen from the destination host to the 
        source host during this sampling interval, divided by 2^32, 
        truncating fractions (i.e., X DIV 2^32), and counted 
        using the rules for counting the nlMatrixSDOctets object (note 
        that the corresponding nlMatrixSDOctets object selected is the 
        one whose source address is equal to nlMatrixTopNDestAddress 
        and whose destination address is equal to 
        nlMatrixTopNSourceAddress.) 
 
        Note that if the value of nlMatrixTopNControlRateBase is equal 
        to nlMatrixTopNHighCapacityOctets, the sort of topN entries is 
        based entirely on nlMatrixTopNHighCapacityOctetRate, and not on 
        the value of this object." 
    ::= { nlMatrixTopNHighCapacityEntry 11 } 
 
nlMatrixTopNHighCapacityReverseOctetRate OBJECT-TYPE 
    SYNTAX     RmonGauge64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets seen from the destination host to the 
        source host during this sampling interval, counted 
        using the rules for counting the nlMatrixSDOctets object (note 
        that the corresponding nlMatrixSDOctets object selected is the 
 
 
 
 
 
 
 
 
 
 
 
        one whose source address is equal to nlMatrixTopNDestAddress 
        and whose destination address is equal to 
        nlMatrixTopNSourceAddress.) 
 
        Note that if the value of nlMatrixTopNControlRateBase is equal 
        to nlMatrixTopNHighCapacityOctets, the sort of topN entries is 
        based entirely on nlMatrixTopNHighCapacityOctetRate, and not on 
        the value of this object." 
    ::= { nlMatrixTopNHighCapacityEntry 12 } 
 
-- High Capacity extensions for the alHostTable 
 
alHostHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF AlHostHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        alHostTable." 
    ::= { alHost 2 } 
 
alHostHighCapacityEntry  OBJECT-TYPE 
    SYNTAX     AlHostHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        alHostEntry. These objects will be created by the agent 
        for all alHostEntries associated with whichever 
        hlHostControlEntries it deems appropriate. (i.e., either all 
        alHostHighCapacityEntries associated with a particular 
        hlHostControlEntry will be created, or none of them will 
        be.)" 
    INDEX { hlHostControlIndex, alHostTimeMark, 
            protocolDirLocalIndex, nlHostAddress, 
            protocolDirLocalIndex } 
    ::= { alHostHighCapacityTable 1 } 
 
AlHostHighCapacityEntry ::= SEQUENCE { 
    alHostHighCapacityInOverflowPkts    ZeroBasedCounter32, 
    alHostHighCapacityInPkts            ZeroBasedCounter64, 
    alHostHighCapacityOutOverflowPkts   ZeroBasedCounter32, 
    alHostHighCapacityOutPkts           ZeroBasedCounter64, 
    alHostHighCapacityInOverflowOctets  ZeroBasedCounter32, 
    alHostHighCapacityInOctets          ZeroBasedCounter64, 
 
 
 
 
 
 
 
 
 
 
 
    alHostHighCapacityOutOverflowOctets ZeroBasedCounter32, 
    alHostHighCapacityOutOctets         ZeroBasedCounter64 
} 
 
alHostHighCapacityInOverflowPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated alHostInPkts 
        counter has overflowed." 
    ::= { alHostHighCapacityEntry 1 } 
 
alHostHighCapacityInPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets of this protocol type without errors 
        transmitted to this address since it was added to the 
        alHostHighCapacityTable.  Note that this is the number of 
        link-layer packets, so if a single network-layer packet 
        is fragmented into several link-layer frames, this counter 
        is incremented several times." 
    ::= { alHostHighCapacityEntry 2 } 
 
alHostHighCapacityOutOverflowPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated alHostOutPkts 
        counter has overflowed." 
    ::= { alHostHighCapacityEntry 3 } 
 
alHostHighCapacityOutPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets of this protocol type without errors 
        transmitted by this address since it was added to the 
        alHostHighCapacityTable.  Note that this is the number of 
        link-layer packets, so if a single network-layer packet 
        is fragmented into several link-layer frames, this counter 
 
 
 
 
 
 
 
 
 
 
 
        is incremented several times." 
    ::= { alHostHighCapacityEntry 4 } 
 
alHostHighCapacityInOverflowOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated alHostInOctets 
        counter has overflowed." 
    ::= { alHostHighCapacityEntry 5 } 
 
alHostHighCapacityInOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets transmitted to this address 
        of this protocol type since it was added to the 
        alHostHighCapacityTable (excluding framing bits but 
        including FCS octets), excluding those octets in 
        packets that contained errors. 
 
        Note this doesn't count just those octets in the particular 
        protocol frames, but includes the entire packet that contained 
        the protocol." 
    ::= { alHostHighCapacityEntry 6 } 
 
alHostHighCapacityOutOverflowOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated alHostOutOctets 
        counter has overflowed." 
    ::= { alHostHighCapacityEntry 7 } 
 
alHostHighCapacityOutOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets transmitted by this address 
        of this protocol type since it was added to the 
        alHostHighCapacityTable (excluding framing bits but 
 
 
 
 
 
 
 
 
 
 
 
        including FCS octets), excluding those octets in 
        packets that contained errors. 
 
        Note this doesn't count just those octets in the particular 
        protocol frames, but includes the entire packet that contained 
        the protocol." 
    ::= { alHostHighCapacityEntry 8 } 
 
-- High Capacity extensions for the alMatrixSDTable 
 
alMatrixSDHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF AlMatrixSDHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        alMatrixSDTable." 
    ::= { alMatrix 5 } 
 
alMatrixSDHighCapacityEntry  OBJECT-TYPE 
    SYNTAX     AlMatrixSDHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        alMatrixSDEntry. These objects will be created by the agent 
        for all alMatrixSDEntries associated with whichever 
        hlMatrixControlEntries it deems appropriate. (i.e., either all 
        alMatrixSDHighCapacityEntries associated with a particular 
        hlMatrixControlEntry will be created, or none of them will 
        be.)" 
    INDEX { hlMatrixControlIndex, alMatrixSDTimeMark, 
            protocolDirLocalIndex, 
            nlMatrixSDSourceAddress, nlMatrixSDDestAddress, 
            protocolDirLocalIndex } 
    ::= { alMatrixSDHighCapacityTable 1 } 
 
AlMatrixSDHighCapacityEntry ::= SEQUENCE { 
    alMatrixSDHighCapacityOverflowPkts   ZeroBasedCounter32, 
    alMatrixSDHighCapacityPkts           ZeroBasedCounter64, 
    alMatrixSDHighCapacityOverflowOctets ZeroBasedCounter32, 
    alMatrixSDHighCapacityOctets         ZeroBasedCounter64 
} 
 
alMatrixSDHighCapacityOverflowPkts OBJECT-TYPE 
 
 
 
 
 
 
 
 
 
 
 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated alMatrixSDPkts 
        counter has overflowed." 
    ::= { alMatrixSDHighCapacityEntry 1 } 
 
alMatrixSDHighCapacityPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets of this protocol type without errors 
        transmitted from the source address to the destination address 
        since this entry was added to the alMatrixSDHighCapacityTable. 
        Note that this is the number of link-layer packets, so if a 
        single network-layer packet is fragmented into several 
        link-layer frames, this counter is incremented several times." 
    ::= { alMatrixSDHighCapacityEntry 2 } 
 
alMatrixSDHighCapacityOverflowOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated alMatrixSDOctets 
        counter has overflowed." 
    ::= { alMatrixSDHighCapacityEntry 3 } 
 
alMatrixSDHighCapacityOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets in packets of this protocol type 
        transmitted from the source address to the destination address 
        since this entry was added to the alMatrixSDHighCapacityTable 
        (excluding framing bits but including FCS octets), excluding 
        those octets in packets that contained errors. 
 
        Note this doesn't count just those octets in the particular 
        protocol frames, but includes the entire packet that contained 
        the protocol." 
    ::= { alMatrixSDHighCapacityEntry 4 } 
 
 
 
 
 
 
 
 
 
 
 
-- High Capacity extensions for the alMatrixDSTable 
 
alMatrixDSHighCapacityTable  OBJECT-TYPE 
    SYNTAX     SEQUENCE OF AlMatrixDSHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        alMatrixDSTable." 
    ::= { alMatrix 6 } 
 
alMatrixDSHighCapacityEntry  OBJECT-TYPE 
    SYNTAX     AlMatrixDSHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        alMatrixSDTable. These objects will be created by the agent 
        for all alMatrixDSEntries associated with whichever 
        hlMatrixControlEntries it deems appropriate. (i.e., either all 
        alMatrixDSHighCapacityEntries associated with a particular 
        hlMatrixControlEntry will be created, or none of them will 
        be.)" 
    INDEX { hlMatrixControlIndex, alMatrixDSTimeMark, 
            protocolDirLocalIndex, 
            nlMatrixDSDestAddress, nlMatrixDSSourceAddress, 
            protocolDirLocalIndex } 
    ::= { alMatrixDSHighCapacityTable 1 } 
 
AlMatrixDSHighCapacityEntry ::= SEQUENCE { 
    alMatrixDSHighCapacityOverflowPkts   ZeroBasedCounter32, 
    alMatrixDSHighCapacityPkts           ZeroBasedCounter64, 
    alMatrixDSHighCapacityOverflowOctets ZeroBasedCounter32, 
    alMatrixDSHighCapacityOctets         ZeroBasedCounter64 
} 
 
alMatrixDSHighCapacityOverflowPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated alMatrixDSPkts 
        counter has overflowed." 
    ::= { alMatrixDSHighCapacityEntry 1 } 
 
 
 
 
 
 
 
 
 
 
 
 
alMatrixDSHighCapacityPkts OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets of this protocol type without errors 
        transmitted from the source address to the destination address 
        since this entry was added to the alMatrixDSHighCapacityTable. 
        Note that this is the number of link-layer packets, so if a 
        single network-layer packet is fragmented into several 
        link-layer frames, this counter is incremented several times." 
    ::= { alMatrixDSHighCapacityEntry 2 } 
 
alMatrixDSHighCapacityOverflowOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of times the associated alMatrixDSOctets 
        counter has overflowed." 
    ::= { alMatrixDSHighCapacityEntry 3 } 
 
alMatrixDSHighCapacityOctets OBJECT-TYPE 
    SYNTAX     ZeroBasedCounter64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets in packets of this protocol type 
        transmitted from the source address to the destination address 
        since this entry was added to the alMatrixDSHighCapacityTable 
        (excluding framing bits but including FCS octets), excluding 
        those octets in packets that contained errors. 
 
        Note this doesn't count just those octets in the particular 
        protocol frames, but includes the entire packet that contained 
        the protocol." 
    ::= { alMatrixDSHighCapacityEntry 4 } 
 
-- This definition extends the enumeration defined in [RFC 2021] 
alMatrixTopNControlRateBase OBJECT-TYPE 
    SYNTAX     INTEGER { 
                  alMatrixTopNTerminalsPkts(1), 
                  alMatrixTopNTerminalsOctets(2), 
                  alMatrixTopNAllPkts(3), 
                  alMatrixTopNAllOctets(4), 
 
 
 
 
 
 
 
 
 
 
 
                  alMatrixTopNTerminalsHighCapacityPkts(5), 
                  alMatrixTopNTerminalsHighCapacityOctets(6), 
                  alMatrixTopNAllHighCapacityPkts(7), 
                  alMatrixTopNAllHighCapacityOctets(8) 
               } 
    MAX-ACCESS read-create 
    STATUS     current 
    DESCRIPTION 
        "The variable for each alMatrix[SD/DS] entry that the 
        alMatrixTopNEntries are sorted by, as well as the 
        selector of the view of the matrix table that will be 
        used, as well as a control for the table that the results 
        will be reported in. 
 
        The values alMatrixTopNTerminalsPkts, 
        alMatrixTopNTerminalsOctets, 
        alMatrixTopNTerminalsHighCapacityPkts, and 
        alMatrixTopNTerminalsHighCapacityOctets cause collection 
        only from protocols that have no child protocols that are 
        counted. The values alMatrixTopNAllPkts, 
        alMatrixTopNAllOctets, alMatrixTopNAllHighCapacityPkts, and 
        alMatrixTopNAllHighCapacityOctets cause collection from all 
        alMatrix entries. 
 
        This object may not be modified if the associated 
        alMatrixTopNControlStatus object is equal to active(1)." 
    ::= { alMatrixTopNControlEntry 3 } 
 
alMatrixTopNHighCapacityTable OBJECT-TYPE 
    SYNTAX     SEQUENCE OF AlMatrixTopNHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        alMatrixTopNTable when alMatrixTopNControlRateBase specifies 
        a High Capacity TopN Report." 
    ::= { alMatrix 7 } 
 
alMatrixTopNHighCapacityEntry OBJECT-TYPE 
    SYNTAX     AlMatrixTopNHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        alMatrixTopNEntry when alMatrixTopNControlRateBase specifies 
 
 
 
 
 
 
 
 
 
 
 
        a High Capacity TopN Report. These objects will be created by 
        the agent for all alMatrixTopNEntries associated with whichever 
        alMatrixTopNControlEntries have a alMatrixTopNControlRateBase 
        that specify a high capacity report." 
     INDEX { alMatrixTopNControlIndex, alMatrixTopNIndex } 
    ::= { alMatrixTopNHighCapacityTable 1 } 
 
AlMatrixTopNHighCapacityEntry ::= SEQUENCE { 
    alMatrixTopNHighCapacityBasePktRate               Gauge32, 
    alMatrixTopNHighCapacityOverflowPktRate           Gauge32, 
    alMatrixTopNHighCapacityPktRate                   RmonGauge64, 
    alMatrixTopNHighCapacityReverseBasePktRate        Gauge32, 
    alMatrixTopNHighCapacityReverseOverflowPktRate    Gauge32, 
    alMatrixTopNHighCapacityReversePktRate            RmonGauge64, 
    alMatrixTopNHighCapacityBaseOctetRate             Gauge32, 
    alMatrixTopNHighCapacityOverflowOctetRate         Gauge32, 
    alMatrixTopNHighCapacityOctetRate                 RmonGauge64, 
    alMatrixTopNHighCapacityReverseBaseOctetRate      Gauge32, 
    alMatrixTopNHighCapacityReverseOverflowOctetRate  Gauge32, 
    alMatrixTopNHighCapacityReverseOctetRate          RmonGauge64 
} 
 
alMatrixTopNHighCapacityBasePktRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets seen of this protocol from the source 
        host to the destination host during this sampling interval, 
        modulo 2^32, counted using the rules for counting the 
        alMatrixSDPkts object." 
    ::= { alMatrixTopNHighCapacityEntry 1 } 
 
alMatrixTopNHighCapacityOverflowPktRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets seen of this protocol from the source host 
        to the destination host during this sampling interval, 
        divided by 2^32, truncating fractions (i.e., X DIV 2^32), 
        and counted using the rules for counting the 
        alMatrixSDPkts object." 
    ::= { alMatrixTopNHighCapacityEntry 2 } 
 
 
 
 
 
 
 
 
 
 
 
 
alMatrixTopNHighCapacityPktRate OBJECT-TYPE 
    SYNTAX     RmonGauge64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets seen of this protocol from the source 
        host to the destination host during this sampling interval, 
        counted using the rules for counting the 
        alMatrixSDPkts object. 
        If the value of alMatrixTopNControlRateBase is 
        alMatrixTopNTerminalsPkts, alMatrixTopNAllPkts, 
        alMatrixTopNTerminalsHighCapacityPkts, or 
        alMatrixTopNAllHighCapacityPkts, this variable will be used 
        to sort this report." 
    ::= { alMatrixTopNHighCapacityEntry 3 } 
 
alMatrixTopNHighCapacityReverseBasePktRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets seen of this protocol from the 
        destination host to the source host during this sampling 
        interval, modulo 2^32, counted using the rules for counting 
        the alMatrixSDPkts object (note that the corresponding 
        alMatrixSDPkts object selected is the one whose source address 
        is equal to alMatrixTopNDestAddress and whose destination 
        address is equal to alMatrixTopNSourceAddress.)" 
    ::= { alMatrixTopNHighCapacityEntry 4 } 
 
alMatrixTopNHighCapacityReverseOverflowPktRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets seen of this protocol from the 
        destination host to the source host during this sampling 
        interval, divided by 2^32, truncating fractions 
        (i.e., X DIV 2^32), and counted using the rules for 
        counting the alMatrixSDPkts object (note that the 
        corresponding alMatrixSDPkts object selected is the 
        one whose source address is equal to alMatrixTopNDestAddress 
        and whose destination address is equal to 
        alMatrixTopNSourceAddress.)" 
    ::= { alMatrixTopNHighCapacityEntry 5 } 
 
 
 
 
 
 
 
 
 
 
 
alMatrixTopNHighCapacityReversePktRate OBJECT-TYPE 
    SYNTAX     RmonGauge64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of packets seen of this protocol from the 
        destination host to the source host during this sampling 
        interval, counted using the rules for counting the 
        alMatrixSDPkts object (note that the corresponding 
        alMatrixSDPkts object selected is the one whose source address 
        is equal to alMatrixTopNDestAddress and whose destination 
        address is equal to alMatrixTopNSourceAddress.)" 
    ::= { alMatrixTopNHighCapacityEntry 6 } 
 
alMatrixTopNHighCapacityBaseOctetRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets seen of this protocol from the source host 
        to the destination host during this sampling interval, 
        modulo 2^32, counted using the rules for counting the 
        alMatrixSDOctets object." 
    ::= { alMatrixTopNHighCapacityEntry 7 } 
 
alMatrixTopNHighCapacityOverflowOctetRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets seen of this protocol from the source host 
        to the destination host during this sampling interval, 
        divided by 2^32, truncating fractions (i.e., X DIV 2^32), 
        and counted using the rules for counting the 
        alMatrixSDOctets object." 
    ::= { alMatrixTopNHighCapacityEntry 8 } 
 
alMatrixTopNHighCapacityOctetRate OBJECT-TYPE 
    SYNTAX     RmonGauge64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets seen of this protocol from the source host 
        to the destination host during this sampling interval, 
        counted using the rules for counting the 
 
 
 
 
 
 
 
 
 
 
 
        alMatrixSDOctets object. 
        If the value of alMatrixTopNControlRateBase is 
        alMatrixTopNTerminalsOctets, alMatrixTopNAllOctets, 
        alMatrixTopNTerminalsHighCapacityOctets, or 
        alMatrixTopNAllHighCapacityOctets, this variable will be used 
        to sort this report." 
    ::= { alMatrixTopNHighCapacityEntry 9 } 
 
alMatrixTopNHighCapacityReverseBaseOctetRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets seen of this protocol from the 
        destination host to the source host during this sampling 
        interval, modulo 2^32, counted using the rules for counting 
        the alMatrixSDOctets object (note that the corresponding 
        alMatrixSDOctets object selected is the one whose source 
        address is equal to alMatrixTopNDestAddress and whose 
        destination address is equal to alMatrixTopNSourceAddress.)" 
    ::= { alMatrixTopNHighCapacityEntry 10 } 
 
alMatrixTopNHighCapacityReverseOverflowOctetRate OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets seen of this protocol from the 
        destination host to the source host during this sampling 
        interval, divided by 2^32, truncating fractions (i.e., X DIV 
        2^32), and counted using the rules for counting the 
        alMatrixSDOctets object (note that the corresponding 
        alMatrixSDOctets object selected is the one whose source 
        address is equal to alMatrixTopNDestAddress and whose 
        destination address is equal to alMatrixTopNSourceAddress.)" 
    ::= { alMatrixTopNHighCapacityEntry 11 } 
 
alMatrixTopNHighCapacityReverseOctetRate OBJECT-TYPE 
    SYNTAX     RmonGauge64 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The number of octets seen of this protocol from the 
        destination host to the source host during this sampling 
        interval, counted using the rules for counting the 
 
 
 
 
 
 
 
 
 
 
 
        alMatrixSDOctets object (note that the corresponding 
        alMatrixSDOctets object selected is the one whose source 
        address is equal to alMatrixTopNDestAddress and whose 
        destination address is equal to alMatrixTopNSourceAddress.)" 
    ::= { alMatrixTopNHighCapacityEntry 12 } 
 
usrHistoryHighCapacityTable OBJECT-TYPE 
    SYNTAX SEQUENCE OF UsrHistoryHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS     current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        usrHistoryTable." 
        ::= { usrHistory 4 } 
 
usrHistoryHighCapacityEntry OBJECT-TYPE 
    SYNTAX UsrHistoryHighCapacityEntry 
    MAX-ACCESS not-accessible 
    STATUS  current 
    DESCRIPTION 
        "Contains the High Capacity RMON extensions to the RMON-2 
        usrHistoryEntry. These objects will be created by the agent 
        for all usrHistoryEntries associated with whichever 
        usrHistoryControlEntries it deems appropriate. (i.e., either all 
        usrHistoryHighCapacityEntries associated with a particular 
        usrHistoryControlEntry will be created, or none of them will 
        be.)" 
    INDEX { usrHistoryControlIndex, usrHistorySampleIndex, 
            usrHistoryObjectIndex } 
    ::= { usrHistoryHighCapacityTable 1 } 
 
UsrHistoryHighCapacityEntry ::= SEQUENCE { 
    usrHistoryHighCapacityOverflowAbsValue     Gauge32, 
    usrHistoryHighCapacityAbsValue             RmonGauge64 
} 
 
usrHistoryHighCapacityOverflowAbsValue OBJECT-TYPE 
    SYNTAX     Gauge32 
    MAX-ACCESS read-only 
    STATUS     current 
    DESCRIPTION 
        "The absolute value (i.e. unsigned value) of the 
        user-specified statistic during the last sampling period, 
        divided by 2^32, truncating fractions (i.e., X DIV 2^32). 
        The value during the current sampling period is not made 
 
 
 
 
 
 
 
 
 
 
 
        available until the period is completed. 
 
        To obtain the true value for this sampling interval, the 
        associated instance of usrHistoryValStatus must be checked, 
        and usrHistoryAbsValue adjusted as necessary. 
 
        If the MIB instance could not be accessed during the sampling 
        interval, then this object will have a value of zero and the 
        associated instance of usrHistoryValStatus will be set to 
        'valueNotAvailable(1)'." 
    ::= { usrHistoryHighCapacityEntry 1 } 
 
usrHistoryHighCapacityAbsValue OBJECT-TYPE 
    SYNTAX RmonGauge64 
    MAX-ACCESS read-only 
    STATUS current 
    DESCRIPTION 
        "The absolute value (i.e. unsigned value) of the 
        user-specified statistic during the last sampling period. The 
        value during the current sampling period is not made available 
        until the period is completed. 
 
        To obtain the true value for this sampling interval, the 
        associated instance of usrHistoryValStatus must be checked, 
        and usrHistoryHighCapacityAbsValue adjusted as necessary. 
 
        If the MIB instance could not be accessed during the sampling 
        interval, then this object will have a value of zero and the 
        associated instance of usrHistoryValStatus will be set to 
        'valueNotAvailable(1)'." 
    ::= { usrHistoryHighCapacityEntry 2 } 
 
-- 
-- High Capacity RMON Probe Capabilities 
-- 
hcRMONCapabilities OBJECT-TYPE 
    SYNTAX BITS { 
        mediaIndependentGroup(0), 
        etherStatsHighCapacityGroup(1), 
        etherHistoryHighCapacityGroup(2), 
        hostHighCapacityGroup(3), 
        hostTopNHighCapacityGroup(4), 
        matrixHighCapacityGroup(5), 
        captureBufferHighCapacityGroup(6), 
        protocolDistributionHighCapacityGroup(7), 
 
 
 
 
 
 
 
 
 
 
 
        nlHostHighCapacityGroup(8), 
        nlMatrixHighCapacityGroup(9), 
        nlMatrixTopNHighCapacityGroup(10), 
        alHostHighCapacityGroup(11), 
        alMatrixHighCapacityGroup(12), 
        alMatrixTopNHighCapacityGroup(13), 
        usrHistoryHighCapacityGroup(14) 
    } 
    MAX-ACCESS read-only 
    STATUS current 
    DESCRIPTION 
        "An indication of the High Capacity RMON MIB groups supported 
        on at least one interface by this probe." 
    ::= { probeConfig 16 } 
 
 
-- Conformance Macros 
 
--hcRmonMIBCompliances OBJECT IDENTIFIER ::= { rmonConformance 4 } 
hcRmonMIBCompliances OBJECT IDENTIFIER ::= { rmonConformance 6 } 
--hcRmonMIBGroups      OBJECT IDENTIFIER ::= { rmonConformance 5 } 
hcRmonMIBGroups      OBJECT IDENTIFIER ::= { rmonConformance 7 } 
 
hcRmonMIBCompliance MODULE-COMPLIANCE 
    STATUS  current 
    DESCRIPTION 
        "Describes the minimum requirements for conformance to the 
        high capacity RMON MIB." 
    MODULE  -- this module 
    MANDATORY-GROUPS { mediaIndependentGroup, hcRMONInformationGroup } 
    ::= { hcRmonMIBCompliances 1 } 
 
hcRmon2MIBCompliance MODULE-COMPLIANCE 
    STATUS  current 
    DESCRIPTION 
        "Describes the requirements for conformance to 
        the High Capacity RMON 2 MIB" 
    MODULE  -- this module 
        MANDATORY-GROUPS { mediaIndependentGroup, 
                           protocolDistributionHighCapacityGroup, 
                           nlHostHighCapacityGroup, 
                           nlMatrixHighCapacityGroup, 
                           nlMatrixTopNHighCapacityGroup, 
                           usrHistoryHighCapacityGroup, 
                           hcRMONInformationGroup } 
    ::= { hcRmonMIBCompliances 2 } 
 
 
 
 
 
 
 
 
 
 
 
 
hcRmon2MIBApplicationLayerCompliance MODULE-COMPLIANCE 
    STATUS  current 
    DESCRIPTION 
        "Describes the requirements for conformance to 
        the High Capacity RMON2 MIB with Application Layer Enhancements." 
    MODULE  -- this module 
        MANDATORY-GROUPS { mediaIndependentGroup, 
                           protocolDistributionHighCapacityGroup, 
                           nlHostHighCapacityGroup, 
                           nlMatrixHighCapacityGroup, 
                           nlMatrixTopNHighCapacityGroup, 
                           alHostHighCapacityGroup, 
                           alMatrixHighCapacityGroup, 
                           alMatrixTopNHighCapacityGroup, 
                           usrHistoryHighCapacityGroup, 
                           hcRMONInformationGroup } 
 
    ::= { hcRmonMIBCompliances 3 } 
 
mediaIndependentGroup OBJECT-GROUP 
    OBJECTS {mediaIndependentIndex, 
        mediaIndependentDataSource, 
        mediaIndependentDropEvents, 
        mediaIndependentDroppedFrames, 
        mediaIndependentInPkts, 
        mediaIndependentInOverflowPkts, 
        mediaIndependentInHighCapacityPkts, 
        mediaIndependentOutPkts, 
        mediaIndependentOutOverflowPkts, 
        mediaIndependentOutHighCapacityPkts, 
        mediaIndependentInOctets, 
        mediaIndependentInOverflowOctets, 
        mediaIndependentInHighCapacityOctets, 
        mediaIndependentOutOctets, 
        mediaIndependentOutOverflowOctets, 
        mediaIndependentOutHighCapacityOctets, 
        mediaIndependentInNUCastPkts, 
        mediaIndependentInNUCastOverflowPkts, 
        mediaIndependentInNUCastHighCapacityPkts, 
        mediaIndependentOutNUCastPkts, 
        mediaIndependentOutNUCastOverflowPkts, 
        mediaIndependentOutNUCastHighCapacityPkts, 
        mediaIndependentInErrors, 
        mediaIndependentOutErrors, 
        mediaIndependentInputSpeed, 
 
 
 
 
 
 
 
 
 
 
 
        mediaIndependentOutputSpeed, 
        mediaIndependentOwner, 
        mediaIndependentStatus } 
    STATUS current 
    DESCRIPTION 
        "Collects utilization statistics for any type of network." 
    ::= { hcRmonMIBGroups 1 } 
 
etherStatsHighCapacityGroup OBJECT-GROUP 
    OBJECTS { etherStatsHighCapacityOverflowPkts, 
              etherStatsHighCapacityPkts, 
              etherStatsHighCapacityOverflowOctets, 
              etherStatsHighCapacityOctets, 
              etherStatsHighCapacityOverflowPkts64Octets, 
              etherStatsHighCapacityPkts64Octets, 
              etherStatsHighCapacityOverflowPkts65to127Octets, 
              etherStatsHighCapacityPkts65to127Octets, 
              etherStatsHighCapacityOverflowPkts128to255Octets, 
              etherStatsHighCapacityPkts128to255Octets, 
              etherStatsHighCapacityOverflowPkts256to511Octets, 
              etherStatsHighCapacityPkts256to511Octets, 
              etherStatsHighCapacityOverflowPkts512to1023Octets, 
              etherStatsHighCapacityPkts512to1023Octets, 
              etherStatsHighCapacityOverflowPkts1024to1518Octets, 
              etherStatsHighCapacityPkts1024to1518Octets } 
    STATUS  current 
    DESCRIPTION 
        "Collects utilization statistics for ethernet networks." 
    ::= { hcRmonMIBGroups 2 } 
 
etherHistoryHighCapacityGroup OBJECT-GROUP 
    OBJECTS { etherHistoryHighCapacityOverflowPkts, 
              etherHistoryHighCapacityPkts, 
              etherHistoryHighCapacityOverflowOctets, 
              etherHistoryHighCapacityOctets } 
    STATUS  current 
    DESCRIPTION 
        "Collects utilization statistics for ethernet networks." 
    ::= { hcRmonMIBGroups 3 } 
 
hostHighCapacityGroup OBJECT-GROUP 
    OBJECTS { hostHighCapacityInOverflowPkts, 
              hostHighCapacityInPkts, 
              hostHighCapacityOutOverflowPkts, 
              hostHighCapacityOutPkts, 
 
 
 
 
 
 
 
 
 
 
 
              hostHighCapacityInOverflowOctets, 
              hostHighCapacityInOctets, 
              hostHighCapacityOutOverflowOctets, 
              hostHighCapacityOutOctets, 
              hostTimeHighCapacityInOverflowPkts, 
              hostTimeHighCapacityInPkts, 
              hostTimeHighCapacityOutOverflowPkts, 
              hostTimeHighCapacityOutPkts, 
              hostTimeHighCapacityInOverflowOctets, 
              hostTimeHighCapacityInOctets, 
              hostTimeHighCapacityOutOverflowOctets, 
              hostTimeHighCapacityOutOctets } 
    STATUS  current 
    DESCRIPTION 
        "Collects utilization and error statistics per host." 
    ::= { hcRmonMIBGroups 4 } 
 
hostTopNHighCapacityGroup OBJECT-GROUP 
    OBJECTS { hostTopNHighCapacityBaseRate, 
        hostTopNHighCapacityOverflowRate, 
        hostTopNHighCapacityRate } 
    STATUS  current 
    DESCRIPTION 
        "Prepares sorted reports of utilization and error statistics 
        per host." 
    ::= { hcRmonMIBGroups 5 } 
 
 
matrixHighCapacityGroup OBJECT-GROUP 
    OBJECTS { matrixSDHighCapacityOverflowPkts, 
              matrixSDHighCapacityPkts, 
              matrixSDHighCapacityOverflowOctets, 
              matrixSDHighCapacityOctets, 
              matrixDSHighCapacityOverflowPkts, 
              matrixDSHighCapacityPkts, 
              matrixDSHighCapacityOverflowOctets, 
              matrixDSHighCapacityOctets } 
    STATUS  current 
    DESCRIPTION 
        "Collects utilization statistics per conversation." 
    ::= { hcRmonMIBGroups 6 } 
 
captureBufferHighCapacityGroup OBJECT-GROUP 
    OBJECTS { captureBufferPacketHighCapacityTime } 
    STATUS  current 
 
 
 
 
 
 
 
 
 
 
 
    DESCRIPTION 
        "Provides finer granularity timestamps." 
    ::= { hcRmonMIBGroups 7 } 
 
protocolDistributionHighCapacityGroup OBJECT-GROUP 
    OBJECTS { protocolDistStatsHighCapacityOverflowPkts, 
              protocolDistStatsHighCapacityPkts, 
              protocolDistStatsHighCapacityOverflowOctets, 
              protocolDistStatsHighCapacityOctets } 
    STATUS  current 
    DESCRIPTION 
        "Collects the relative amounts of octets and packets for the 
        different protocols detected on a network segment." 
    ::= { hcRmonMIBGroups 8 } 
 
nlHostHighCapacityGroup OBJECT-GROUP 
    OBJECTS { nlHostHighCapacityInOverflowPkts, 
              nlHostHighCapacityInPkts, 
              nlHostHighCapacityOutOverflowPkts, 
              nlHostHighCapacityOutPkts, 
              nlHostHighCapacityInOverflowOctets, 
              nlHostHighCapacityInOctets, 
              nlHostHighCapacityOutOverflowOctets, 
              nlHostHighCapacityOutOctets } 
    STATUS  current 
    DESCRIPTION 
        "Counts the amount of traffic sent from and to each network 
        address discovered by the probe." 
    ::= { hcRmonMIBGroups 9 } 
 
nlMatrixHighCapacityGroup OBJECT-GROUP 
    OBJECTS { nlMatrixSDHighCapacityOverflowPkts, 
              nlMatrixSDHighCapacityPkts, 
              nlMatrixSDHighCapacityOverflowOctets, 
              nlMatrixSDHighCapacityOctets, 
              nlMatrixDSHighCapacityOverflowPkts, 
              nlMatrixDSHighCapacityPkts, 
              nlMatrixDSHighCapacityOverflowOctets, 
              nlMatrixDSHighCapacityOctets } 
    STATUS  current 
    DESCRIPTION 
        "Counts the amount of traffic sent between each pair of 
        network addresses discovered by the probe." 
    ::= { hcRmonMIBGroups 10 } 
 
 
 
 
 
 
 
 
 
 
 
 
nlMatrixTopNHighCapacityGroup OBJECT-GROUP 
    OBJECTS { nlMatrixTopNHighCapacityBasePktRate, 
        nlMatrixTopNHighCapacityOverflowPktRate, 
        nlMatrixTopNHighCapacityPktRate, 
        nlMatrixTopNHighCapacityReverseBasePktRate, 
        nlMatrixTopNHighCapacityReverseOverflowPktRate, 
        nlMatrixTopNHighCapacityReversePktRate, 
        nlMatrixTopNHighCapacityBaseOctetRate, 
        nlMatrixTopNHighCapacityOverflowOctetRate, 
        nlMatrixTopNHighCapacityOctetRate, 
        nlMatrixTopNHighCapacityReverseBaseOctetRate, 
        nlMatrixTopNHighCapacityReverseOverflowOctetRate, 
        nlMatrixTopNHighCapacityReverseOctetRate } 
    STATUS  current 
    DESCRIPTION 
        "Prepares sorted reports of the amount of traffic sent between 
        each pair of network addresses discovered by the probe." 
    ::= { hcRmonMIBGroups 11 } 
 
alHostHighCapacityGroup OBJECT-GROUP 
    OBJECTS { alHostHighCapacityInOverflowPkts, 
              alHostHighCapacityInPkts, 
              alHostHighCapacityOutOverflowPkts, 
              alHostHighCapacityOutPkts, 
              alHostHighCapacityInOverflowOctets, 
              alHostHighCapacityInOctets, 
              alHostHighCapacityOutOverflowOctets, 
              alHostHighCapacityOutOctets } 
    STATUS  current 
    DESCRIPTION 
        "Counts the amount of traffic, by protocol, sent from and to 
        each network address discovered by the probe." 
    ::= { hcRmonMIBGroups 12 } 
 
alMatrixHighCapacityGroup OBJECT-GROUP 
    OBJECTS { alMatrixSDHighCapacityOverflowPkts, 
              alMatrixSDHighCapacityPkts, 
              alMatrixSDHighCapacityOverflowOctets, 
              alMatrixSDHighCapacityOctets, 
              alMatrixDSHighCapacityOverflowPkts, 
              alMatrixDSHighCapacityPkts, 
              alMatrixDSHighCapacityOverflowOctets, 
              alMatrixDSHighCapacityOctets } 
    STATUS  current 
    DESCRIPTION 
 
 
 
 
 
 
 
 
 
 
 
        "Counts the amount of traffic, by protocol, sent between each 
        pair of network addresses discovered by the 
        probe." 
    ::= { hcRmonMIBGroups 13 } 
 
alMatrixTopNHighCapacityGroup OBJECT-GROUP 
    OBJECTS { alMatrixTopNHighCapacityBasePktRate, 
        alMatrixTopNHighCapacityOverflowPktRate, 
        alMatrixTopNHighCapacityPktRate, 
        alMatrixTopNHighCapacityReverseBasePktRate, 
        alMatrixTopNHighCapacityReverseOverflowPktRate, 
        alMatrixTopNHighCapacityReversePktRate, 
        alMatrixTopNHighCapacityBaseOctetRate, 
        alMatrixTopNHighCapacityOverflowOctetRate, 
        alMatrixTopNHighCapacityOctetRate, 
        alMatrixTopNHighCapacityReverseBaseOctetRate, 
        alMatrixTopNHighCapacityReverseOverflowOctetRate, 
        alMatrixTopNHighCapacityReverseOctetRate } 
    STATUS  current 
    DESCRIPTION 
        "Prepares sorted reports of the amount of traffic per protocol 
        sent between each pair of network addresses discovered by the 
        probe." 
    ::= { hcRmonMIBGroups 14 } 
 
usrHistoryHighCapacityGroup OBJECT-GROUP 
    OBJECTS { usrHistoryHighCapacityOverflowAbsValue, 
        usrHistoryHighCapacityAbsValue } 
    STATUS  current 
    DESCRIPTION 
        "Provides user-defined collection of historical information 
        from MIB objects on the probe with scalability to statistics 
        from high-capacity networks." 
    ::= { hcRmonMIBGroups 15 } 
 
hcRMONInformationGroup OBJECT-GROUP 
    OBJECTS { hcRMONCapabilities } 
    STATUS  current 
    DESCRIPTION 
        "An indication of the high capacity RMON groups supported on 
        at least one interface by this probe." 
    ::= { hcRmonMIBGroups 16 } 
END 
 
 
 
 
 
 
 
 
 
 
 
 
 

 
 
 
 
 
 
 
 
 
 
 
 
 

