
-- $Id: CISCO-CONFIG-MAN-MIB.my,v 3.3.52.1 1996/06/11 19:38:20 snyder
-- Exp $
-- $Source: /release/112/cvs/Xsys/MIBS/CISCO-CONFIG-MAN-MIB.my,v $
-- *****************************************************************
-- CISCO-CONFIG-MAN-MIB.my:  Configuration Management MIB
--   
-- January 2002, A S Kiran Koushik
--   
-- Copyright (c) 1995-1996, 2002, 2004-2006, 2014 by cisco Systems, Inc.
-- All rights reserved.
--   
-- *****************************************************************
-- $Log: CISCO-CONFIG-MAN-MIB.my,v $
-- Revision 3.3.52.1  1996/06/11  19:38:20  snyder
-- CSCdi60118:  MIB doc spellink errors
-- Branch: California_branch
--   
-- Revision 3.3  1995/11/28  22:18:48  bstewart
-- CSCdi43134:  Configuration Management MIB needs a ciscoMgmt arc
-- assigned
-- Got a proper number.
--   
-- Revision 3.2  1995/11/17  08:33:54  hampton
-- Remove old entries from the RCS header logs.
--   
-- Revision 3.1  1995/11/09  10:49:43  shaker
-- Bump version numbers from 2.x to 3.x.
--   
-- Revision 2.2  1995/11/08  20:48:22  shaker
-- Merge Arkansas_branch into 11.1 mainline.
--   
-- Revision 2.1  1995/09/15  22:38:24  thille
-- Add placeholders for Bob's config history feature and MIB.
--   

-- *****************************************************************
-- $Endlog

CISCO-CONFIG-MAN-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
    TimeTicks,
    Integer32,
    Counter32,
    IpAddress,
    Gauge32,
    Unsigned32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    DisplayString,
    TruthValue,
    DateAndTime,
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    InetAddressType,
    InetAddress
        FROM INET-ADDRESS-MIB
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    Unsigned64
        FROM CISCO-TC
    ciscoMgmt
        FROM CISCO-SMI;


ciscoConfigManMIB MODULE-IDENTITY
    LAST-UPDATED    "200608220000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service


            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-snmp@cisco.com"
    DESCRIPTION
            "Configuration management MIB.

            The MIB represents a model of configuration data that
            exists in various locations:

            running        in use by the running system
            terminal    operator's mind or attached hardware
            local        saved locally in NVRAM or flash
            remote        saved to some server on the network

            Although some of the system functions that relate here
            can be used for general file storage and transfer, this
            MIB intends to include only such operations as clearly
            relate to configuration.  Its primary emphasis is to
            track changes and saves of the running configuration.

            As saved data moves further from startup use, such as
            into different local flash files or onto the network,
            tracking becomes difficult to impossible, so the MIB's
            interest and functions are confined in that area.

            Information from ccmCLIHistoryCommandTable can be used
            to track the exact configuration changes that took
            place within a particular Configuration History
            event. NMS' can use this information to update 
            the related components. 
            For example:
                If commands related only to MPLS are entered
                then the NMS need to update only the MPLS related
                management information rather than updating
                all of its management information.
                Acronyms and terms:

                CLI   Command Line Interface."
    REVISION        "201903110000Z"
    DESCRIPTION
            "Added new varbind ccmHistoryEventTerminalUser to 
            ciscoConfigManEvent and ccmCLIRunningConfigChanged 
            notifications"
    REVISION        "200608170000Z"
    DESCRIPTION
            "Added a new group of objects to store the information
            related to the Config Change Tracking ID (CTID) feature. 

            CTID will provide a version number that is unique for 
            version-incrementing changes to the IOS
            running-configuration. It will also provide information
            about when CTID last changed.

            Added scalars: 
            * ccmCTID
            * ccmCTIDLastChangeTime
            * ccmCTIDWhoChanged
            * ccmCTIDRolledOverNotifEnable

            Added Notification:
            * ccmCTIDRolledOver

            Added Object Group:
            * ciscoConfigManCTIDObjectGroup

            Added Notification Group:
            * ciscoConfigManCTIDNotifyGroup

            Added Compliance:
            ciscoConfigManMIBComplianceRev4"
    REVISION        "200406180000Z"
    DESCRIPTION
            "The Objects ccmHistoryEventCommandSourceAddress and
            ccmHistoryEventServerAddress are deprecated since
            they support only IPv4 address. These objects have
            been replaced by two new objects 
            ccmHistoryEventCommandSourceAddrRev1 and 
            ccmHistoryEventServerAddrRev1. In addition to these
            objects two more new objects are defined
            ccmHistoryEventCommandSourceAddrType and
            ccmHistoryEventServerAddrType"
    REVISION        "200206070000Z"
    DESCRIPTION
            "Added new enumerations networkFtp(8) and
            networkScp(9) to HistoryEventMedium."
    REVISION        "200203120000Z"
    DESCRIPTION
            "Added ccmCLIHistoryCommandTable for
            storing the CLI commands that took effect during
            a configuration event.

            Added scalars ccmCLIHistoryMaxCmdEntries
            ccmCLIHistoryCmdEntries and 
            ccmCLIHistoryCmdEntriesAllowed.

            Added ccmHistoryCLICmdEntriesBumped to 
            ccmHistoryEventTable to store the number of
            corresponding bumped entries in the 
            ccmCLIHistoryCommandTable.

            Added the ccmCLIRunningConfigChanged notification.
            Added ccmCLICfgRunConfNotifEnable to control the
            ccmCLIRunningConfigChanged notification.

            Added notification group 
            ciscoConfigManHistNotifyGroup.

            Updated the MIB description to indicate the use of
            the above additions."
    REVISION        "9511280000Z"
    DESCRIPTION
            "Initial version of this MIB module."
          ::= { ciscoMgmt 43 }


ciscoConfigManMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoConfigManMIB 1 }

ccmHistory  OBJECT IDENTIFIER
    ::= { ciscoConfigManMIBObjects 1 }

ccmCLIHistory  OBJECT IDENTIFIER
    ::= { ciscoConfigManMIBObjects 2 }

ccmCLICfg  OBJECT IDENTIFIER
    ::= { ciscoConfigManMIBObjects 3 }

ccmCTIDObjects  OBJECT IDENTIFIER
    ::= { ciscoConfigManMIBObjects 4 }

-- Textual Conventions

HistoryEventMedium ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
            "The source or destination of a configuration change,
            save, or copy.

            erase        erasing destination (source only)
            running        live operational data
            commandSource    the command source itself
            startup        what the system will use next reboot
            local        local NVRAM or flash
            networkTftp    network host via Trivial File Transfer
            networkRcp    network host via Remote Copy
            networkFtp       network host via File transfer
            networkScp       network host via Secure Copy
            "
    SYNTAX          INTEGER  {
                        erase(1),
                        commandSource(2),
                        running(3),
                        startup(4),
                        local(5),
                        networkTftp(6),
                        networkRcp(7),
                        networkFtp(8),
                        networkScp(9)
                    }

-- Configuration History
ccmHistoryRunningLastChanged OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "The value of sysUpTime when the running configuration
            was last changed.

                    If the value of ccmHistoryRunningLastChanged is
                    greater than ccmHistoryRunningLastSaved, the 
                    configuration has been changed but not saved." 
    ::= { ccmHistory 1 }

ccmHistoryRunningLastSaved OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "The value of sysUpTime when the running configuration
            was last saved (written).

            If the value of ccmHistoryRunningLastChanged is 
            greater than ccmHistoryRunningLastSaved, the 
            configuration has been changed but not saved.

            What constitutes a safe saving of the running
            configuration is a management policy issue beyond the
            scope of this MIB.  For some installations, writing the
            running configuration to a terminal may be a way of
            capturing and saving it.  Others may use local or
            remote storage.  Thus ANY write is considered saving
            for the purposes of the MIB." 
    ::= { ccmHistory 2 }

ccmHistoryStartupLastChanged OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "The value of sysUpTime when the startup configuration
            was last written to.  In general this is the
            default configuration used when cold starting the
            system.  It may have been changed by a save of the
            running configuration or by a copy from elsewhere." 
    ::= { ccmHistory 3 }

ccmHistoryMaxEventEntries OBJECT-TYPE
    SYNTAX          Integer32 (0..2147483647 )
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "The maximum number of entries that can be held in
            ccmHistoryEventTable.

            The recommended value for implementations is 10." 
    ::= { ccmHistory 4 }

ccmHistoryEventEntriesBumped OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "The number of times the oldest entry in
            ccmHistoryEventTable was deleted to make room 
            for a new entry." 
    ::= { ccmHistory 5 }

ccmHistoryEventTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CcmHistoryEventEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "A table of configuration events on this router."
    ::= { ccmHistory 6 }

ccmHistoryEventEntry OBJECT-TYPE
    SYNTAX          CcmHistoryEventEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
            "Information about a configuration event on this
            router."
    INDEX           { ccmHistoryEventIndex } 
    ::= { ccmHistoryEventTable 1 }

CcmHistoryEventEntry ::= SEQUENCE {
        ccmHistoryEventIndex                 Integer32,
        ccmHistoryEventTime                  TimeTicks,
        ccmHistoryEventCommandSource         INTEGER ,
        ccmHistoryEventConfigSource          HistoryEventMedium,
        ccmHistoryEventConfigDestination     HistoryEventMedium,
        ccmHistoryEventTerminalType          INTEGER ,
        ccmHistoryEventTerminalNumber        Integer32,
        ccmHistoryEventTerminalUser          DisplayString,
        ccmHistoryEventTerminalLocation      DisplayString,
        ccmHistoryEventCommandSourceAddress  IpAddress,
        ccmHistoryEventVirtualHostName       DisplayString,
        ccmHistoryEventServerAddress         IpAddress,
        ccmHistoryEventFile                  DisplayString,
        ccmHistoryEventRcpUser               DisplayString,
        ccmHistoryCLICmdEntriesBumped        Counter32,
        ccmHistoryEventCommandSourceAddrType InetAddressType,
        ccmHistoryEventCommandSourceAddrRev1 InetAddress,
        ccmHistoryEventServerAddrType        InetAddressType,
        ccmHistoryEventServerAddrRev1        InetAddress
}

ccmHistoryEventIndex OBJECT-TYPE
    SYNTAX          Integer32 (1..2147483647 )
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
            "A monotonically increasing integer for the sole
            purpose of indexing events.  When it reaches the 
            maximum value, an extremely unlikely event, the agent 
            wraps the value back to 1 and may flush existing 
            entries." 
    ::= { ccmHistoryEventEntry 1 }

ccmHistoryEventTime OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION     "The value of sysUpTime when the event occurred." 
    ::= { ccmHistoryEventEntry 2 }

ccmHistoryEventCommandSource OBJECT-TYPE
    SYNTAX          INTEGER  {
                        commandLine(1),
                        snmp(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "The source of the command that instigated the event." 
    ::= { ccmHistoryEventEntry 3 }

ccmHistoryEventConfigSource OBJECT-TYPE
    SYNTAX          HistoryEventMedium
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION     "The configuration data source for the event." 
    ::= { ccmHistoryEventEntry 4 }

ccmHistoryEventConfigDestination OBJECT-TYPE
    SYNTAX          HistoryEventMedium
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION     "The configuration data destination for the event." 
    ::= { ccmHistoryEventEntry 5 }

ccmHistoryEventTerminalType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        notApplicable(1),
                        unknown(2),
                        console(3),
                        terminal(4),
                        virtual(5),
                        auxiliary(6)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "If ccmHistoryEventCommandSource is 'commandLine',
            the terminal type, otherwise 'notApplicable'." 
    ::= { ccmHistoryEventEntry 6 }

ccmHistoryEventTerminalNumber OBJECT-TYPE
    SYNTAX          Integer32 (-2147483648..2147483647 )
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "If ccmHistoryEventCommandSource is 'commandLine',
            the terminal number.  The value is -1 if not available
            or not applicable." 
    ::= { ccmHistoryEventEntry 7 }

ccmHistoryEventTerminalUser OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..64))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "If ccmHistoryEventCommandSource is 'commandLine',
            the name of the logged in user.  The length is zero if
            not available or not applicable." 
    ::= { ccmHistoryEventEntry 8 }

ccmHistoryEventTerminalLocation OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..64))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "If ccmHistoryEventCommandSource is 'commandLine',
            the hard-wired location of the terminal or the remote 
            host for an incoming connection.  The length is zero 
            if not available or not applicable." 
    ::= { ccmHistoryEventEntry 9 }

ccmHistoryEventCommandSourceAddress OBJECT-TYPE
    SYNTAX          IpAddress
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
            "If ccmHistoryEventTerminalType is 'virtual', the
            internet address of the connected system.

            If ccmHistoryEventCommandSource is 'snmp', the internet
            address of the requester.

            The value is 0.0.0.0 if not available or not 
            applicable.

            This object is deprecated by
            ccmHistoryEventCommandSourceAddrRev1" 
    ::= { ccmHistoryEventEntry 10 }

ccmHistoryEventVirtualHostName OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..64))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "If ccmHistoryEventTerminalType is 'virtual', the host
            name of the connected system.  The length is zero if
            not available or not applicable." 
    ::= { ccmHistoryEventEntry 11 }

ccmHistoryEventServerAddress OBJECT-TYPE
    SYNTAX          IpAddress
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
            "If ccmHistoryEventConfigSource or
            ccmHistoryEventConfigDestination is 'networkTftp' or
            'networkRcp', the internet address of the storage file
            server.  The value is 0.0.0.0 if not applicable or not
                    available.
                    This object is deprecated by
                    ccmHistoryEventServerAddrRev1" 
    ::= { ccmHistoryEventEntry 12 }

ccmHistoryEventFile OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..64))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "If ccmHistoryEventConfigSource or
            ccmHistoryEventConfigDestination is 'networkTftp' or
            'networkRcp', the configuration file name at the
            storage file server.  The length is zero if not
            available or not applicable." 
    ::= { ccmHistoryEventEntry 13 }

ccmHistoryEventRcpUser OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..64))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "If ccmHistoryEventConfigSource or
            ccmHistoryEventConfigDestination is 'networkRcp', the
            remote user name.  The length is zero if not applicable
            or not available." 
    ::= { ccmHistoryEventEntry 14 }

ccmHistoryCLICmdEntriesBumped OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "The number of times the oldest entry in
            ccmCLIHistoryCommandTable with first index as 
            ccmHistoryEventIndex was deleted to make 
            room for a new entry.

            This object is applicable only if 
            ccmHistoryEventCommandSource has a value 
            of 'commandLine'." 
    ::= { ccmHistoryEventEntry 15 }

ccmHistoryEventCommandSourceAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "This object indicates the transport type of the
            address contained in
            ccmHistoryEventCommandSourceAddrRev1.

            The value will be zero if not available or not
            applicable." 
    ::= { ccmHistoryEventEntry 16 }

ccmHistoryEventCommandSourceAddrRev1 OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "If ccmHistoryEventTerminalType is 'virtual', the
            internet address of the connected system.

            If ccmHistoryEventCommandSource is 'snmp', the
            internet address of the requester.

            The value of all bit's is zero  if not available or
            not applicable.

            The Format of this address depends on the value of the
            ccmHistoryEventCommandSourceAddrType object.

            This object deprecates
            ccmHistoryEventCommandSourceAddress" 
    ::= { ccmHistoryEventEntry 17 }

ccmHistoryEventServerAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "This object indicates the transport type of the
            address contained in ccmHistoryEventServerAddrRev1.

            The value will be zero if not available or not
            aplicable." 
    ::= { ccmHistoryEventEntry 18 }

ccmHistoryEventServerAddrRev1 OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "If ccmHistoryEventConfigSource or
            ccmHistoryEventConfigDestination is 'networkTftp' or
            'networkRcp', the internet address of the storage file
            server. 

            The value of all bits is 0s if not applicable or not
            available.

            The Format of this address depends on the value of the
            ccmHistoryEventServerAddrType object.

            This object deprecates ccmHistoryEventServerAddress." 
    ::= { ccmHistoryEventEntry 19 }
 


-- ccmCLIHistory
ccmCLIHistoryMaxCmdEntries OBJECT-TYPE
    SYNTAX          Unsigned32 (0..4294967295 )
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
            "The maximum number of entries that can be held in
            ccmCLIHistoryCommandTable.

            The recommended value for implementations is 100.

            If the number of entries in ccmCLIHistoryCommandTable 
            exceeds the value of this object, old entries will be 
            bumped to make room for new entries.

            The ccmCLIHistoryCommandTable will not be populated
            if the value of this object is 0." 
    ::= { ccmCLIHistory 1 }

ccmCLIHistoryCmdEntries OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "The current number of entries in
            ccmCLIHistoryCommandTable." 
    ::= { ccmCLIHistory 2 }

ccmCLIHistoryCmdEntriesAllowed OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "This object indicates the upper limit on the
            number of entries allowed in 
            ccmCLIHistoryCommandTable by the managed system." 
    ::= { ccmCLIHistory 3 }

ccmCLIHistoryCommandTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CcmCLIHistoryCommandEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
            "A table of CLI commands that took effect during
            configuration events."
    ::= { ccmCLIHistory 4 }

ccmCLIHistoryCommandEntry OBJECT-TYPE
    SYNTAX          CcmCLIHistoryCommandEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
            "Information about the CLI commands that took effect
            during the configuration event pointed by 
            ccmCLIHistoryEventIndex.

            A set of rows in this table having the first
            index as ccmHistoryEventIndex will store the
            CLI commands entered during the corresponding 
            configuration event in ccmHistoryEventTable.

            An entry will be created in this table only if 
            the corresponding entry in ccmHistoryEventTable has 
            a value of 'commandLine' for 
            ccmHistoryEventCommandSource."
    INDEX           {
                        ccmHistoryEventIndex,
                        ccmCLIHistoryCommandIndex
                    } 
    ::= { ccmCLIHistoryCommandTable 1 }

CcmCLIHistoryCommandEntry ::= SEQUENCE {
        ccmCLIHistoryCommandIndex Unsigned32,
        ccmCLIHistoryCommand      DisplayString
}

ccmCLIHistoryCommandIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4294967295 )
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
            "A monotonically increasing integer for the
            purpose of indexing CLI commands which took effect
            during a configuration event." 
    ::= { ccmCLIHistoryCommandEntry 1 }

ccmCLIHistoryCommand OBJECT-TYPE
    SYNTAX          DisplayString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "The CLI command entered which took effect
            during the configuration event pointed by 
            ccmHistoryEventIndex." 
    ::= { ccmCLIHistoryCommandEntry 2 }
 


ccmCLICfgRunConfNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
            "This variable indicates whether the system produces
            the ccmCLIRunningConfigChanged notification. A false 
            value will prevent notifications from being generated 
            by this system."
    DEFVAL          { false } 
    ::= { ccmCLICfg 1 }

ccmCTID OBJECT-TYPE
    SYNTAX          Unsigned64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "This object indicates the Config Change Tracking ID which
            uniquely represents version-incrementing changes to the IOS 
            running configuration." 
    ::= { ccmCTIDObjects 1 }

ccmCTIDLastChangeTime OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "This object indicates the time when the Config Change Tracking
            ID last changed." 
    ::= { ccmCTIDObjects 2 }

ccmCTIDWhoChanged OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
            "This object indicates the user who last reset the Config Change
            Tracking ID." 
    ::= { ccmCTIDObjects 3 }

ccmCTIDRolledOverNotifEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
            "This variable indicates whether the system produces the
            ccmCTIDRolledOver notification. A false value will prevent
            notifications from being generated by this system."
    DEFVAL          { false } 
    ::= { ccmCTIDObjects 4 }
-- Notifications
ciscoConfigManMIBNotificationPrefix  OBJECT IDENTIFIER
    ::= { ciscoConfigManMIB 2 }

ciscoConfigManMIBNotifications  OBJECT IDENTIFIER
    ::= { ciscoConfigManMIBNotificationPrefix 0 }



ciscoConfigManEvent NOTIFICATION-TYPE
    OBJECTS         {
                        ccmHistoryEventCommandSource,
                        ccmHistoryEventConfigSource,
                        ccmHistoryEventConfigDestination,
                        ccmHistoryEventTerminalUser
                    }
    STATUS          current
    DESCRIPTION
            "Notification of a configuration management event as
            recorded in ccmHistoryEventTable."
   ::= { ciscoConfigManMIBNotifications 1 }


ccmCLIRunningConfigChanged NOTIFICATION-TYPE
    OBJECTS         {
                        ccmHistoryRunningLastChanged,
                        ccmHistoryEventTerminalType,
                        ccmHistoryEventTerminalUser
                    }
    STATUS          current
    DESCRIPTION
            "This notification indicates that the running
            configuration of the managed system has changed
            from the CLI.

            If the managed system supports a separate 
            configuration mode(where the configuration commands 
            are entered under a  configuration session which 
            affects the running configuration of the system), 
            then this notification is sent when the configuration 
            mode is exited.
            During this configuration session there can be 
            one or more running configuration changes."
   ::= { ciscoConfigManMIBNotifications 2 }


ccmCTIDRolledOver NOTIFICATION-TYPE
    STATUS          current
    DESCRIPTION
            "This notification indicates that the Config Change Tracking
            ID has rolled over and will be reset."
   ::= { ciscoConfigManMIBNotifications 3 }
-- Conformance
ciscoConfigManMIBConformance  OBJECT IDENTIFIER
    ::= { ciscoConfigManMIB 3 }

ciscoConfigManMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoConfigManMIBConformance 1 }

ciscoConfigManMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoConfigManMIBConformance 2 }


-- Compliance
ciscoConfigManMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
            "The compliance statement for entities which implement
            the Cisco Configuration Management MIB"
    MODULE          -- this module
    MANDATORY-GROUPS { ciscoConfigManHistoryGroup }
    ::= { ciscoConfigManMIBCompliances 1 }

ciscoConfigManMIBComplianceRev2 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
            "The compliance statement for entities which implement
            the Cisco Configuration Management MIB"
    MODULE          -- this module
    MANDATORY-GROUPS { ciscoConfigManHistoryGroupRev1 }

    GROUP           ciscoConfigManCLIHistCmdGroup
    DESCRIPTION
            "This Optional group contains information about
            the CLI commands entered during a particular
            configuration event. Implementation of this 
            group is mandatory if the system can be 
            configured via CLI."

    GROUP           ciscoConfigManHistNotifyGroup
    DESCRIPTION
            "This optional group contains the
            notifications which represent various
            configuration events on the system.
            Implementation of this group is mandatory 
            if the system can be configured via CLI."
    ::= { ciscoConfigManMIBCompliances 2 }

ciscoConfigManMIBComplianceRev3 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
            "The compliance statement for entities which implement
            the Cisco Configuration Management MIB.

            This compliance module deprecates
            ciscoConfigManMIBCompliance."
    MODULE          -- this module
    MANDATORY-GROUPS { ciscoConfigManHistoryGroupRev2 }

    GROUP           ciscoConfigManCLIHistCmdGroup
    DESCRIPTION
            "This Optional group contains information about
            the CLI commands entered during a particular
            configuration event. Implementation of this 
            group is mandatory if the system can be 
            configured via CLI."

    GROUP           ciscoConfigManHistNotifyGroup
    DESCRIPTION
            "This optional group contains the
            notifications which represent various
            configuration events on the system.
            Implementation of this group is mandatory 
            if the system can be configured via CLI."
    ::= { ciscoConfigManMIBCompliances 3 }

ciscoConfigManMIBComplianceRev4 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
            "The compliance statement for entities which implement
            the Cisco Configuration Management MIB.

            This compliance module deprecates
            ciscoConfigManMIBCompliance."
    MODULE          -- this module
    MANDATORY-GROUPS { ciscoConfigManHistoryGroupRev2 }

    GROUP           ciscoConfigManCLIHistCmdGroup
    DESCRIPTION
            "This Optional group contains information about
            the CLI commands entered during a particular
            configuration event. Implementation of this 
            group is mandatory if the system can be 
            configured via CLI."

    GROUP           ciscoConfigManHistNotifyGroup
    DESCRIPTION
            "This optional group contains the
            notifications which represent various
            configuration events on the system.
            Implementation of this group is mandatory 
            if the system can be configured via CLI."

    GROUP           ciscoConfigManCTIDNotifyGroup
    DESCRIPTION
            "This optional group contains the
            notifications which represent the various
            Config Change Tracking ID events on the system."

    GROUP           ciscoConfigManCTIDObjectGroup
    DESCRIPTION
            "This optional group contains objects that expose
            Config Change Tracking ID and the associated 
            information.  This group is mandatory when the 
            device implements the Config Change Tracking ID
            feature."
    ::= { ciscoConfigManMIBCompliances 4 }

-- Units of Conformance
ciscoConfigManHistoryGroup OBJECT-GROUP
    OBJECTS         {
                        ccmHistoryRunningLastChanged,
                        ccmHistoryRunningLastSaved,
                        ccmHistoryStartupLastChanged,
                        ccmHistoryMaxEventEntries,
                        ccmHistoryEventEntriesBumped,
                        ccmHistoryEventTime,
                        ccmHistoryEventCommandSource,
                        ccmHistoryEventConfigSource,
                        ccmHistoryEventConfigDestination,
                        ccmHistoryEventTerminalType,
                        ccmHistoryEventTerminalNumber,
                        ccmHistoryEventTerminalUser,
                        ccmHistoryEventTerminalLocation,
                        ccmHistoryEventCommandSourceAddress,
                        ccmHistoryEventVirtualHostName,
                        ccmHistoryEventServerAddress,
                        ccmHistoryEventFile,
                        ccmHistoryEventRcpUser
                    }
    STATUS          deprecated
    DESCRIPTION     "Configuration history."
    ::= { ciscoConfigManMIBGroups 1 }

ciscoConfigManHistoryGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        ccmHistoryRunningLastChanged,
                        ccmHistoryRunningLastSaved,
                        ccmHistoryStartupLastChanged,
                        ccmHistoryMaxEventEntries,
                        ccmHistoryEventEntriesBumped,
                        ccmHistoryEventTime,
                        ccmHistoryEventCommandSource,
                        ccmHistoryEventConfigSource,
                        ccmHistoryEventConfigDestination,
                        ccmHistoryEventTerminalType,
                        ccmHistoryEventTerminalNumber,
                        ccmHistoryEventTerminalUser,
                        ccmHistoryEventTerminalLocation,
                        ccmHistoryEventCommandSourceAddress,
                        ccmHistoryEventVirtualHostName,
                        ccmHistoryEventServerAddress,
                        ccmHistoryEventFile,
                        ccmHistoryEventRcpUser,
                        ccmHistoryCLICmdEntriesBumped
                    }
    STATUS          deprecated
    DESCRIPTION     "Configuration history."
    ::= { ciscoConfigManMIBGroups 2 }

ciscoConfigManHistNotifyGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        ciscoConfigManEvent,
                        ccmCLIRunningConfigChanged
                    }
    STATUS          current
    DESCRIPTION
            "Notifications of a configuration management event."
    ::= { ciscoConfigManMIBGroups 3 }

ciscoConfigManHistoryGroupRev2 OBJECT-GROUP
    OBJECTS         {
                        ccmHistoryRunningLastChanged,
                        ccmHistoryRunningLastSaved,
                        ccmHistoryStartupLastChanged,
                        ccmHistoryMaxEventEntries,
                        ccmHistoryEventEntriesBumped,
                        ccmHistoryEventTime,
                        ccmHistoryEventCommandSource,
                        ccmHistoryEventConfigSource,
                        ccmHistoryEventConfigDestination,
                        ccmHistoryEventTerminalType,
                        ccmHistoryEventTerminalNumber,
                        ccmHistoryEventTerminalUser,
                        ccmHistoryEventTerminalLocation,
                        ccmHistoryEventVirtualHostName,
                        ccmHistoryEventFile,
                        ccmHistoryEventRcpUser,
                        ccmHistoryCLICmdEntriesBumped,
                        ccmHistoryEventCommandSourceAddrType,
                        ccmHistoryEventCommandSourceAddrRev1,
                        ccmHistoryEventServerAddrType,
                        ccmHistoryEventServerAddrRev1
                    }
    STATUS          current
    DESCRIPTION
            "Configuration history.

            This group deprecates the old group
            ciscoConfigManHistoryGroupRev1"
    ::= { ciscoConfigManMIBGroups 5 }

ciscoConfigManCLIHistCmdGroup OBJECT-GROUP
    OBJECTS         {
                        ccmCLIHistoryMaxCmdEntries,
                        ccmCLIHistoryCmdEntries,
                        ccmCLIHistoryCmdEntriesAllowed,
                        ccmCLIHistoryCommand,
                        ccmCLICfgRunConfNotifEnable
                    }
    STATUS          current
    DESCRIPTION
            "CLI commands entered during a configuration history
            event."
    ::= { ciscoConfigManMIBGroups 4 }

ciscoConfigManCTIDNotifyGroup NOTIFICATION-GROUP
   NOTIFICATIONS    { ccmCTIDRolledOver }
    STATUS          current
    DESCRIPTION
            "Notifications of a Config Change Tracking ID event."
    ::= { ciscoConfigManMIBGroups 6 }

ciscoConfigManCTIDObjectGroup OBJECT-GROUP
    OBJECTS         {
                        ccmCTID,
                        ccmCTIDLastChangeTime,
                        ccmCTIDWhoChanged,
                        ccmCTIDRolledOverNotifEnable
                    }
    STATUS          current
    DESCRIPTION
            "Information about the current CTID value, when CTID last
            changed, and who last changed the CTID."
    ::= { ciscoConfigManMIBGroups 7 }

END


