-- *****************************************************************
-- IP-FORWARD-MIB.my:  (IP version independent) IP Forwarding Table MIB
--   
-- Nov 2006, Tim Gleeson
--   
-- Copyright (c) 2006 by Cisco Systems, Inc.
-- All rights reserved.
--   
-- *****************************************************************
--   
-- This mib was extracted from RFC4293
-- XXX Changed inetCidrRouteStatus compliance syntax:
-- RowStatus -> INTEGER

IP-FORWARD-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    IpAddress,
    Integer32,
    Gauge32,
    Counter32
        FROM SNMPv2-SMI
    RowStatus
        FROM SNMPv2-TC
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    InterfaceIndexOrZero
        FROM IF-MIB
    ip
        FROM IP-MIB
    IANAipRouteProtocol
        FROM IANA-RTPROTO-MIB
    InetAddress,
    InetAddressType,
    InetAddressPrefixLength,
    InetAutonomousSystemNumber
        FROM INET-ADDRESS-MIB;


ipForward MODULE-IDENTITY
    LAST-UPDATED    "200602010000Z"
    ORGANIZATION    "IETF IPv6 Working Group
            http://www.ietf.org/html.charters/ipv6-charter.html"
    CONTACT-INFO
            "Editor:
            Brian Haberman
            Johns Hopkins University - Applied Physics Laboratory
            Mailstop 17-S442
            11100 Johns Hopkins Road
            Laurel MD,  20723-6099  USA

            Phone: +1-443-778-1319
            Email: brian@innovationslab.net

            Send comments to <ipv6@ietf.org>"
    DESCRIPTION
        "The MIB module for the management of CIDR multipath IP
        Routes.

        Copyright (C) The Internet Society (2006).  This version
        of this MIB module is a part of RFC 4292; see the RFC
        itself for full legal notices."
    REVISION        "200602010000Z"
    DESCRIPTION
        "IPv4/v6 version-independent revision.  Minimal changes
        were made to the original RFC 2096 MIB to allow easy
        upgrade of existing IPv4 implementations to the
        version-independent MIB.  These changes include:

        Adding inetCidrRouteDiscards as a replacement for the
        deprecated ipRoutingDiscards and ipv6DiscardedRoutes
        objects.

        Adding a new conformance statement to support the
        implementation of the IP Forwarding MIB in a
        read-only mode.

        The inetCidrRouteTable replaces the IPv4-specific
        ipCidrRouteTable, its related objects, and related
        conformance statements.

        Published as RFC 4292."
    REVISION        "199609190000Z"
    DESCRIPTION
        "Revised to support CIDR routes.
        Published as RFC 2096."
    REVISION        "199207022156Z"
    DESCRIPTION
        "Initial version, published as RFC 1354."
          ::= { ip 24 }



inetCidrRouteNumber OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of current inetCidrRouteTable entries that
        are not invalid." 
    ::= { ipForward 6 }

inetCidrRouteDiscards OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of valid route entries discarded from the
        inetCidrRouteTable.  Discarded route entries do not
        appear in the inetCidrRouteTable.  One possible reason
        for discarding an entry would be to free-up buffer space
        for other route table entries." 
    ::= { ipForward 8 }
-- Inet CIDR Route Table
--   
-- The Inet CIDR Route Table deprecates and replaces the
-- ipCidrRoute Table currently in the IP Forwarding Table MIB.
-- It adds IP protocol independence.

inetCidrRouteTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF InetCidrRouteEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "This entity's IP Routing table."
    REFERENCE       "RFC 1213 Section 6.6, The IP Group"
    ::= { ipForward 7 }

inetCidrRouteEntry OBJECT-TYPE
    SYNTAX          InetCidrRouteEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A particular route to a particular destination, under a
        particular policy (as reflected in the
        inetCidrRoutePolicy object).

        Dynamically created rows will survive an agent reboot.

        Implementers need to be aware that if the total number
        of elements (octets or sub-identifiers) in
        inetCidrRouteDest, inetCidrRoutePolicy, and
        inetCidrRouteNextHop exceeds 111, then OIDs of column
        instances in this table will have more than 128 sub-
        identifiers and cannot be accessed using SNMPv1,
        SNMPv2c, or SNMPv3."
    INDEX           {
                        inetCidrRouteDestType,
                        inetCidrRouteDest,
                        inetCidrRoutePfxLen,
                        inetCidrRoutePolicy,
                        inetCidrRouteNextHopType,
                        inetCidrRouteNextHop
                    } 
    ::= { inetCidrRouteTable 1 }

InetCidrRouteEntry ::= SEQUENCE {
        inetCidrRouteDestType    InetAddressType,
        inetCidrRouteDest        InetAddress,
        inetCidrRoutePfxLen      InetAddressPrefixLength,
        inetCidrRoutePolicy      OBJECT IDENTIFIER,
        inetCidrRouteNextHopType InetAddressType,
        inetCidrRouteNextHop     InetAddress,
        inetCidrRouteIfIndex     InterfaceIndexOrZero,
        inetCidrRouteType        INTEGER ,
        inetCidrRouteProto       IANAipRouteProtocol,
        inetCidrRouteAge         Gauge32,
        inetCidrRouteNextHopAS   InetAutonomousSystemNumber,
        inetCidrRouteMetric1     Integer32,
        inetCidrRouteMetric2     Integer32,
        inetCidrRouteMetric3     Integer32,
        inetCidrRouteMetric4     Integer32,
        inetCidrRouteMetric5     Integer32,
        inetCidrRouteStatus      RowStatus
}

inetCidrRouteDestType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The type of the inetCidrRouteDest address, as defined
        in the InetAddress MIB.

        Only those address types that may appear in an actual
        routing table are allowed as values of this object."
    REFERENCE       "RFC 4001" 
    ::= { inetCidrRouteEntry 1 }

inetCidrRouteDest OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The destination IP address of this route.

        The type of this address is determined by the value of
        the inetCidrRouteDestType object.

        The values for the index objects inetCidrRouteDest and
        inetCidrRoutePfxLen must be consistent.  When the value
        of inetCidrRouteDest (excluding the zone index, if one
        is present) is x, then the bitwise logical-AND
        of x with the value of the mask formed from the
        corresponding index object inetCidrRoutePfxLen MUST be
        equal to x.  If not, then the index pair is not
        consistent and an inconsistentName error must be
        returned on SET or CREATE requests." 
    ::= { inetCidrRouteEntry 2 }

inetCidrRoutePfxLen OBJECT-TYPE
    SYNTAX          InetAddressPrefixLength
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Indicates the number of leading one bits that form the
        mask to be logical-ANDed with the destination address
        before being compared to the value in the
        inetCidrRouteDest field.

        The values for the index objects inetCidrRouteDest and
        inetCidrRoutePfxLen must be consistent.  When the value
        of inetCidrRouteDest (excluding the zone index, if one
        is present) is x, then the bitwise logical-AND
        of x with the value of the mask formed from the
        corresponding index object inetCidrRoutePfxLen MUST be
        equal to x.  If not, then the index pair is not
        consistent and an inconsistentName error must be
        returned on SET or CREATE requests." 
    ::= { inetCidrRouteEntry 3 }

inetCidrRoutePolicy OBJECT-TYPE
    SYNTAX          OBJECT IDENTIFIER
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object is an opaque object without any defined
        semantics.  Its purpose is to serve as an additional
        index that may delineate between multiple entries to
        the same destination.  The value { 0 0 } shall be used
        as the default value for this object." 
    ::= { inetCidrRouteEntry 4 }

inetCidrRouteNextHopType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The type of the inetCidrRouteNextHop address, as
        defined in the InetAddress MIB.

        Value should be set to unknown(0) for non-remote
        routes.

        Only those address types that may appear in an actual
        routing table are allowed as values of this object."
    REFERENCE       "RFC 4001" 
    ::= { inetCidrRouteEntry 5 }

inetCidrRouteNextHop OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "On remote routes, the address of the next system en
        route.  For non-remote routes, a zero length string.

        The type of this address is determined by the value of
        the inetCidrRouteNextHopType object." 
    ::= { inetCidrRouteEntry 6 }

inetCidrRouteIfIndex OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The ifIndex value that identifies the local interface
        through which the next hop of this route should be
        reached.  A value of 0 is valid and represents the
        scenario where no interface is specified." 
    ::= { inetCidrRouteEntry 7 }

inetCidrRouteType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        reject(2),
                        local(3),
                        remote(4),
                        blackhole(5)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The type of route.  Note that local(3) refers to a
        route for which the next hop is the final destination;
        remote(4) refers to a route for which the next hop is
        not the final destination.

        Routes that do not result in traffic forwarding or
        rejection should not be displayed, even if the
        implementation keeps them stored internally.

        reject(2) refers to a route that, if matched, discards
        the message as unreachable and returns a notification
        (e.g., ICMP error) to the message sender.  This is used
        in some protocols as a means of correctly aggregating
        routes.

        blackhole(5) refers to a route that, if matched,
        discards the message silently." 
    ::= { inetCidrRouteEntry 8 }

inetCidrRouteProto OBJECT-TYPE
    SYNTAX          IANAipRouteProtocol
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The routing mechanism via which this route was learned.
        Inclusion of values for gateway routing protocols is
        not intended to imply that hosts should support those
        protocols." 
    ::= { inetCidrRouteEntry 9 }

inetCidrRouteAge OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of seconds since this route was last updated
        or otherwise determined to be correct.  Note that no
        semantics of 'too old' can be implied, except through
        knowledge of the routing protocol by which the route
        was learned." 
    ::= { inetCidrRouteEntry 10 }

inetCidrRouteNextHopAS OBJECT-TYPE
    SYNTAX          InetAutonomousSystemNumber
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The Autonomous System Number of the Next Hop.  The
        semantics of this object are determined by the routing-
        protocol specified in the route's inetCidrRouteProto
        value.  When this object is unknown or not relevant, its
        value should be set to zero."
    DEFVAL          { 0 } 
    ::= { inetCidrRouteEntry 11 }

inetCidrRouteMetric1 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The primary routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's inetCidrRouteProto
        value.  If this metric is not used, its value should be
        set to -1."
    DEFVAL          { -1 } 
    ::= { inetCidrRouteEntry 12 }

inetCidrRouteMetric2 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "An alternate routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's inetCidrRouteProto
        value.  If this metric is not used, its value should be
        set to -1."
    DEFVAL          { -1 } 
    ::= { inetCidrRouteEntry 13 }

inetCidrRouteMetric3 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "An alternate routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's inetCidrRouteProto
        value.  If this metric is not used, its value should be
        set to -1."
    DEFVAL          { -1 } 
    ::= { inetCidrRouteEntry 14 }

inetCidrRouteMetric4 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "An alternate routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's inetCidrRouteProto
        value.  If this metric is not used, its value should be
        set to -1."
    DEFVAL          { -1 } 
    ::= { inetCidrRouteEntry 15 }

inetCidrRouteMetric5 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "An alternate routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's inetCidrRouteProto
        value.  If this metric is not used, its value should be
        set to -1."
    DEFVAL          { -1 } 
    ::= { inetCidrRouteEntry 16 }

inetCidrRouteStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The row status variable, used according to row
        installation and removal conventions.

        A row entry cannot be modified when the status is
        marked as active(1)." 
    ::= { inetCidrRouteEntry 17 }
 

-- Conformance information
ipForwardConformance  OBJECT IDENTIFIER
    ::= { ipForward 5 }

ipForwardGroups  OBJECT IDENTIFIER
    ::= { ipForwardConformance 1 }

ipForwardCompliances  OBJECT IDENTIFIER
    ::= { ipForwardConformance 2 }


-- Compliance statements
ipForwardFullCompliance MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "When this MIB is implemented for read-create, the
        implementation can claim full compliance.

        There are a number of INDEX objects that cannot be
        represented in the form of OBJECT clauses in SMIv2,
        but for which there are compliance requirements,
        expressed in OBJECT clause form in this description:

        -- OBJECT      inetCidrRouteDestType
        -- SYNTAX      InetAddressType (ipv4(1), ipv6(2),
        --                              ipv4z(3), ipv6z(4))
        -- DESCRIPTION
        --     This MIB requires support for global and
        --     non-global ipv4 and ipv6 addresses.
        --
        -- OBJECT      inetCidrRouteDest
        -- SYNTAX      InetAddress (SIZE (4 | 8 | 16 | 20))
        -- DESCRIPTION
        --     This MIB requires support for global and
        --     non-global IPv4 and IPv6 addresses.
        --
        -- OBJECT      inetCidrRouteNextHopType
        -- SYNTAX      InetAddressType (unknown(0), ipv4(1),
        --                              ipv6(2), ipv4z(3)
        --                              ipv6z(4))
        -- DESCRIPTION
        --     This MIB requires support for global and
        --     non-global ipv4 and ipv6 addresses.
        --
        -- OBJECT      inetCidrRouteNextHop
        -- SYNTAX      InetAddress (SIZE (0 | 4 | 8 | 16 | 20))
        -- DESCRIPTION
        --     This MIB requires support for global and
        --     non-global IPv4 and IPv6 addresses.
        "
    MODULE          -- this module
    MANDATORY-GROUPS { inetForwardCidrRouteGroup }

    OBJECT          inetCidrRouteStatus
    SYNTAX          INTEGER  {
                        active(1),
                        notInService(2)
                    }
    WRITE-SYNTAX    INTEGER  {
                        active(1),
                        notInService(2),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION     "Support for createAndWait is not required."
    ::= { ipForwardCompliances 3 }

ipForwardReadOnlyCompliance MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "When this MIB is implemented without support for read-
        create (i.e., in read-only mode), the implementation can
        claim read-only compliance."
    MODULE          -- this module
    MANDATORY-GROUPS { inetForwardCidrRouteGroup }

    OBJECT          inetCidrRouteIfIndex
    MIN-ACCESS      read-only
    DESCRIPTION     "Write access is not required."

    OBJECT          inetCidrRouteType
    MIN-ACCESS      read-only
    DESCRIPTION     "Write access is not required."

    OBJECT          inetCidrRouteNextHopAS
    MIN-ACCESS      read-only
    DESCRIPTION     "Write access is not required."

    OBJECT          inetCidrRouteMetric1
    MIN-ACCESS      read-only
    DESCRIPTION     "Write access is not required."

    OBJECT          inetCidrRouteMetric2
    MIN-ACCESS      read-only
    DESCRIPTION     "Write access is not required."

    OBJECT          inetCidrRouteMetric3
    MIN-ACCESS      read-only
    DESCRIPTION     "Write access is not required."

    OBJECT          inetCidrRouteMetric4
    MIN-ACCESS      read-only
    DESCRIPTION     "Write access is not required."

    OBJECT          inetCidrRouteMetric5
    MIN-ACCESS      read-only
    DESCRIPTION     "Write access is not required."

    OBJECT          inetCidrRouteStatus
    SYNTAX          INTEGER  {
                        active(1)
                    }
    MIN-ACCESS      read-only
    DESCRIPTION     "Write access is not required."
    ::= { ipForwardCompliances 4 }

-- units of conformance
inetForwardCidrRouteGroup OBJECT-GROUP
    OBJECTS         {
                        inetCidrRouteDiscards,
                        inetCidrRouteIfIndex,
                        inetCidrRouteType,
                        inetCidrRouteProto,
                        inetCidrRouteAge,
                        inetCidrRouteNextHopAS,
                        inetCidrRouteMetric1,
                        inetCidrRouteMetric2,
                        inetCidrRouteMetric3,
                        inetCidrRouteMetric4,
                        inetCidrRouteMetric5,
                        inetCidrRouteStatus,
                        inetCidrRouteNumber
                    }
    STATUS          current
    DESCRIPTION     "The IP version-independent CIDR Route Table."
    ::= { ipForwardGroups 4 }

-- Deprecated Objects
ipCidrRouteNumber OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of current ipCidrRouteTable entries that are
        not invalid.  This object is deprecated in favor of
        inetCidrRouteNumber and the inetCidrRouteTable." 
    ::= { ipForward 3 }
-- IP CIDR Route Table
--   
-- The IP CIDR Route Table obsoletes and replaces the ipRoute
-- Table current in MIB-I and MIB-II and the IP Forwarding Table.
-- It adds knowledge of the autonomous system of the next hop,
-- multiple next hops, policy routing, and Classless
-- Inter-Domain Routing.

ipCidrRouteTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IpCidrRouteEntry 
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "This entity's IP Routing table.  This table has been
        deprecated in favor of the IP version neutral
        inetCidrRouteTable."
    REFERENCE       "RFC 1213 Section 6.6, The IP Group"
    ::= { ipForward 4 }

ipCidrRouteEntry OBJECT-TYPE
    SYNTAX          IpCidrRouteEntry
    MAX-ACCESS      not-accessible
    STATUS          deprecated
    DESCRIPTION
        "A particular route to a particular destination, under a
        particular policy."
    INDEX           {
                        ipCidrRouteDest,
                        ipCidrRouteMask,
                        ipCidrRouteTos,
                        ipCidrRouteNextHop
                    } 
    ::= { ipCidrRouteTable 1 }

IpCidrRouteEntry ::= SEQUENCE {
        ipCidrRouteDest      IpAddress,
        ipCidrRouteMask      IpAddress,
        ipCidrRouteTos       Integer32,
        ipCidrRouteNextHop   IpAddress,
        ipCidrRouteIfIndex   Integer32,
        ipCidrRouteType      INTEGER ,
        ipCidrRouteProto     INTEGER ,
        ipCidrRouteAge       Integer32,
        ipCidrRouteInfo      OBJECT IDENTIFIER,
        ipCidrRouteNextHopAS Integer32,
        ipCidrRouteMetric1   Integer32,
        ipCidrRouteMetric2   Integer32,
        ipCidrRouteMetric3   Integer32,
        ipCidrRouteMetric4   Integer32,
        ipCidrRouteMetric5   Integer32,
        ipCidrRouteStatus    RowStatus
}

ipCidrRouteDest OBJECT-TYPE
    SYNTAX          IpAddress
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The destination IP address of this route.

        This object may not take a Multicast (Class D) address
        value.

        Any assignment (implicit or otherwise) of an instance
        of this object to a value x must be rejected if the
        bitwise logical-AND of x with the value of the
        corresponding instance of the ipCidrRouteMask object is
        not equal to x." 
    ::= { ipCidrRouteEntry 1 }

ipCidrRouteMask OBJECT-TYPE
    SYNTAX          IpAddress
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "Indicate the mask to be logical-ANDed with the
        destination address before being compared to the value
        in the ipCidrRouteDest field.  For those systems that
        do not support arbitrary subnet masks, an agent
        constructs the value of the ipCidrRouteMask by
        reference to the IP Address Class.

        Any assignment (implicit or otherwise) of an instance
        of this object to a value x must be rejected if the
        bitwise logical-AND of x with the value of the
        corresponding instance of the ipCidrRouteDest object is
        not equal to ipCidrRouteDest." 
    ::= { ipCidrRouteEntry 2 }

-- The following convention is included for specification
-- of TOS Field contents.  At this time, the Host Requirements
-- and the Router Requirements documents disagree on the width
-- of the TOS field.  This mapping describes the Router
-- Requirements mapping, and leaves room to widen the TOS field
-- without impact to fielded systems.
ipCidrRouteTos OBJECT-TYPE
    SYNTAX          Integer32 (0..2147483647 )
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The policy specifier is the IP TOS Field.  The encoding
        of IP TOS is as specified by the following convention.
        Zero indicates the default path if no more specific
        policy applies.

        +-----+-----+-----+-----+-----+-----+-----+-----+
        |                 |                       |     |
        |   PRECEDENCE    |    TYPE OF SERVICE    |  0  |
        |                 |                       |     |
        +-----+-----+-----+-----+-----+-----+-----+-----+

                     IP TOS                IP TOS
           Field     Policy      Field     Policy
           Contents    Code      Contents    Code
           0 0 0 0  ==>   0      0 0 0 1  ==>   2
           0 0 1 0  ==>   4      0 0 1 1  ==>   6
           0 1 0 0  ==>   8      0 1 0 1  ==>  10
           0 1 1 0  ==>  12      0 1 1 1  ==>  14
           1 0 0 0  ==>  16      1 0 0 1  ==>  18
           1 0 1 0  ==>  20      1 0 1 1  ==>  22
           1 1 0 0  ==>  24      1 1 0 1  ==>  26
           1 1 1 0  ==>  28      1 1 1 1  ==>  30" 
    ::= { ipCidrRouteEntry 3 }

ipCidrRouteNextHop OBJECT-TYPE
    SYNTAX          IpAddress
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "On remote routes, the address of the next system en
        route; Otherwise, 0.0.0.0." 
    ::= { ipCidrRouteEntry 4 }

ipCidrRouteIfIndex OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "The ifIndex value that identifies the local interface
        through which the next hop of this route should be
        reached."
    DEFVAL          { 0 } 
    ::= { ipCidrRouteEntry 5 }

ipCidrRouteType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        reject(2),
                        local(3),
                        remote(4)
                    }
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "The type of route.  Note that local(3) refers to a
        route for which the next hop is the final destination;
        remote(4) refers to a route for which the next hop is
        not the final destination.

        Routes that do not result in traffic forwarding or
        rejection should not be displayed, even if the
        implementation keeps them stored internally.

        reject (2) refers to a route that, if matched,
        discards the message as unreachable.  This is used in
        some protocols as a means of correctly aggregating
        routes." 
    ::= { ipCidrRouteEntry 6 }

ipCidrRouteProto OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        local(2),
                        netmgmt(3),
                        icmp(4),
                        egp(5),
                        ggp(6),
                        hello(7),
                        rip(8),
                        isIs(9),
                        esIs(10),
                        ciscoIgrp(11),
                        bbnSpfIgp(12),
                        ospf(13),
                        bgp(14),
                        idpr(15),
                        ciscoEigrp(16)
                    }
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The routing mechanism via which this route was learned.
        Inclusion of values for gateway routing protocols is
        not intended to imply that hosts should support those
        protocols." 
    ::= { ipCidrRouteEntry 7 }

ipCidrRouteAge OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "The number of seconds since this route was last updated
        or otherwise determined to be correct.  Note that no
        semantics of `too old' can be implied, except through
        knowledge of the routing protocol by which the route
        was learned."
    DEFVAL          { 0 } 
    ::= { ipCidrRouteEntry 8 }

ipCidrRouteInfo OBJECT-TYPE
    SYNTAX          OBJECT IDENTIFIER
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "A reference to MIB definitions specific to the
        particular routing protocol that is responsible for
        this route, as determined by the value specified in the
        route's ipCidrRouteProto value.  If this information is
        not present, its value should be set to the OBJECT
        IDENTIFIER { 0 0 }, which is a syntactically valid
        object identifier, and any implementation conforming to
        ASN.1 and the Basic Encoding Rules must be able to
        generate and recognize this value." 
    ::= { ipCidrRouteEntry 9 }

ipCidrRouteNextHopAS OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "The Autonomous System Number of the Next Hop.  The
        semantics of this object are determined by the routing-
        protocol specified in the route's ipCidrRouteProto
        value.  When this object is unknown or not relevant, its
        value should be set to zero."
    DEFVAL          { 0 } 
    ::= { ipCidrRouteEntry 10 }

ipCidrRouteMetric1 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "The primary routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's ipCidrRouteProto
        value.  If this metric is not used, its value should be
        set to -1."
    DEFVAL          { -1 } 
    ::= { ipCidrRouteEntry 11 }

ipCidrRouteMetric2 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "An alternate routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's ipCidrRouteProto
        value.  If this metric is not used, its value should be
        set to -1."
    DEFVAL          { -1 } 
    ::= { ipCidrRouteEntry 12 }

ipCidrRouteMetric3 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "An alternate routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's ipCidrRouteProto
        value.  If this metric is not used, its value should be
        set to -1."
    DEFVAL          { -1 } 
    ::= { ipCidrRouteEntry 13 }

ipCidrRouteMetric4 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "An alternate routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's ipCidrRouteProto
        value.  If this metric is not used, its value should be
        set to -1."
    DEFVAL          { -1 } 
    ::= { ipCidrRouteEntry 14 }

ipCidrRouteMetric5 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "An alternate routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's ipCidrRouteProto
        value.  If this metric is not used, its value should be
        set to -1."
    DEFVAL          { -1 } 
    ::= { ipCidrRouteEntry 15 }

ipCidrRouteStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "The row status variable, used according to row
        installation and removal conventions." 
    ::= { ipCidrRouteEntry 16 }
 


-- compliance statements
ipForwardCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for SNMPv2 entities that
        implement the ipForward MIB.

        This compliance statement has been deprecated and
        replaced with ipForwardFullCompliance and
        ipForwardReadOnlyCompliance."
    MODULE          -- this module
    MANDATORY-GROUPS { ipForwardCidrRouteGroup }
    ::= { ipForwardCompliances 1 }

-- units of conformance
ipForwardCidrRouteGroup OBJECT-GROUP
    OBJECTS         {
                        ipCidrRouteNumber,
                        ipCidrRouteDest,
                        ipCidrRouteMask,
                        ipCidrRouteTos,
                        ipCidrRouteNextHop,
                        ipCidrRouteIfIndex,
                        ipCidrRouteType,
                        ipCidrRouteProto,
                        ipCidrRouteAge,
                        ipCidrRouteInfo,
                        ipCidrRouteNextHopAS,
                        ipCidrRouteMetric1,
                        ipCidrRouteMetric2,
                        ipCidrRouteMetric3,
                        ipCidrRouteMetric4,
                        ipCidrRouteMetric5,
                        ipCidrRouteStatus
                    }
    STATUS          deprecated
    DESCRIPTION
        "The CIDR Route Table.

        This group has been deprecated and replaced with
        inetForwardCidrRouteGroup."
    ::= { ipForwardGroups 3 }

-- Obsoleted Definitions - Objects
ipForwardNumber OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The number of current ipForwardTable entries that are
        not invalid." 
    ::= { ipForward 1 }
-- IP Forwarding Table
--   
-- The IP Forwarding Table obsoletes and replaces the ipRoute
-- Table current in MIB-I and MIB-II.  It adds knowledge of
-- the autonomous system of the next hop, multiple next hop
-- support, and policy routing support.

ipForwardTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IpForwardEntry 
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION     "This entity's IP Routing table."
    REFERENCE       "RFC 1213 Section 6.6, The IP Group"
    ::= { ipForward 2 }

ipForwardEntry OBJECT-TYPE
    SYNTAX          IpForwardEntry
    MAX-ACCESS      not-accessible
    STATUS          obsolete
    DESCRIPTION
        "A particular route to a particular destination, under a
        particular policy."
    INDEX           {
                        ipForwardDest,
                        ipForwardProto,
                        ipForwardPolicy,
                        ipForwardNextHop
                    } 
    ::= { ipForwardTable 1 }

IpForwardEntry ::= SEQUENCE {
        ipForwardDest      IpAddress,
        ipForwardMask      IpAddress,
        ipForwardPolicy    Integer32,
        ipForwardNextHop   IpAddress,
        ipForwardIfIndex   Integer32,
        ipForwardType      INTEGER ,
        ipForwardProto     INTEGER ,
        ipForwardAge       Integer32,
        ipForwardInfo      OBJECT IDENTIFIER,
        ipForwardNextHopAS Integer32,
        ipForwardMetric1   Integer32,
        ipForwardMetric2   Integer32,
        ipForwardMetric3   Integer32,
        ipForwardMetric4   Integer32,
        ipForwardMetric5   Integer32
}

ipForwardDest OBJECT-TYPE
    SYNTAX          IpAddress
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The destination IP address of this route.  An entry
        with a value of 0.0.0.0 is considered a default route.

        This object may not take a Multicast (Class D) address
        value.

        Any assignment (implicit or otherwise) of an instance
        of this object to a value x must be rejected if the
        bitwise logical-AND of x with the value of the
        corresponding instance of the ipForwardMask object is
        not equal to x." 
    ::= { ipForwardEntry 1 }

ipForwardMask OBJECT-TYPE
    SYNTAX          IpAddress
    MAX-ACCESS      read-create
    STATUS          obsolete
    DESCRIPTION
        "Indicate the mask to be logical-ANDed with the
        destination address before being compared to the value
        in the ipForwardDest field.  For those systems that do
        not support arbitrary subnet masks, an agent constructs
        the value of the ipForwardMask by reference to the IP
        Address Class.

        Any assignment (implicit or otherwise) of an instance
        of this object to a value x must be rejected if the
        bitwise logical-AND of x with the value of the
        corresponding instance of the ipForwardDest object is
        not equal to ipForwardDest."
    DEFVAL          { '00000000'H } 
    ::= { ipForwardEntry 2 }

-- The following convention is included for specification
-- of TOS Field contents.  At this time, the Host Requirements
-- and the Router Requirements documents disagree on the width
-- of the TOS field.  This mapping describes the Router
-- Requirements mapping, and leaves room to widen the TOS field
-- without impact to fielded systems.
ipForwardPolicy OBJECT-TYPE
    SYNTAX          Integer32 (0..2147483647 )
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The general set of conditions that would cause
        the selection of one multipath route (set of
        next hops for a given destination) is referred
        to as 'policy'.

        Unless the mechanism indicated by ipForwardProto
        specifies otherwise, the policy specifier is
        the IP TOS Field.  The encoding of IP TOS is as
        specified by the following convention.  Zero
        indicates the default path if no more specific
        policy applies.

        +-----+-----+-----+-----+-----+-----+-----+-----+
        |                 |                       |     |
        |   PRECEDENCE    |    TYPE OF SERVICE    |  0  |
        |                 |                       |     |
        +-----+-----+-----+-----+-----+-----+-----+-----+



                     IP TOS                IP TOS
           Field     Policy      Field     Policy
           Contents    Code      Contents    Code
           0 0 0 0  ==>   0      0 0 0 1  ==>   2
           0 0 1 0  ==>   4      0 0 1 1  ==>   6
           0 1 0 0  ==>   8      0 1 0 1  ==>  10
           0 1 1 0  ==>  12      0 1 1 1  ==>  14
           1 0 0 0  ==>  16      1 0 0 1  ==>  18
           1 0 1 0  ==>  20      1 0 1 1  ==>  22
           1 1 0 0  ==>  24      1 1 0 1  ==>  26
           1 1 1 0  ==>  28      1 1 1 1  ==>  30

        Protocols defining 'policy' otherwise must either
        define a set of values that are valid for
        this object or must implement an integer-instanced
        policy table for which this object's
        value acts as an index." 
    ::= { ipForwardEntry 3 }

ipForwardNextHop OBJECT-TYPE
    SYNTAX          IpAddress
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "On remote routes, the address of the next system en
        route; otherwise, 0.0.0.0." 
    ::= { ipForwardEntry 4 }

ipForwardIfIndex OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          obsolete
    DESCRIPTION
        "The ifIndex value that identifies the local interface
        through which the next hop of this route should be
        reached."
    DEFVAL          { 0 } 
    ::= { ipForwardEntry 5 }

ipForwardType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        invalid(2),
                        local(3),
                        remote(4)
                    }
    MAX-ACCESS      read-create
    STATUS          obsolete
    DESCRIPTION
        "The type of route.  Note that local(3) refers to a
        route for which the next hop is the final destination;
        remote(4) refers to a route for which the next hop is
        not the final destination.

        Setting this object to the value invalid(2) has the
        effect of invalidating the corresponding entry in the
        ipForwardTable object.  That is, it effectively
        disassociates the destination identified with said
        entry from the route identified with said entry.  It is
        an implementation-specific matter as to whether the
        agent removes an invalidated entry from the table.
        Accordingly, management stations must be prepared to
        receive tabular information from agents that
        corresponds to entries not currently in use.  Proper
        interpretation of such entries requires examination of
        the relevant ipForwardType object."
    DEFVAL          { invalid } 
    ::= { ipForwardEntry 6 }

ipForwardProto OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        local(2),
                        netmgmt(3),
                        icmp(4),
                        egp(5),
                        ggp(6),
                        hello(7),
                        rip(8),
                        is-is(9),
                        es-is(10),
                        ciscoIgrp(11),
                        bbnSpfIgp(12),
                        ospf(13),
                        bgp(14),
                        idpr(15)
                    }
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The routing mechanism via which this route was learned.
        Inclusion of values for gateway routing protocols is
        not intended to imply that hosts should support those
        protocols." 
    ::= { ipForwardEntry 7 }

ipForwardAge OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-only
    STATUS          obsolete
    DESCRIPTION
        "The number of seconds since this route was last updated
        or otherwise determined to be correct.  Note that no
        semantics of `too old' can be implied except through
        knowledge of the routing protocol by which the route
        was learned."
    DEFVAL          { 0 } 
    ::= { ipForwardEntry 8 }

ipForwardInfo OBJECT-TYPE
    SYNTAX          OBJECT IDENTIFIER
    MAX-ACCESS      read-create
    STATUS          obsolete
    DESCRIPTION
        "A reference to MIB definitions specific to the
        particular routing protocol that is responsible for
        this route, as determined by the value specified in the
        route's ipForwardProto value.  If this information is
        not present, its value should be set to the OBJECT
        IDENTIFIER { 0 0 }, which is a syntactically valid
        object identifier, and any implementation conforming to
        ASN.1 and the Basic Encoding Rules must be able to
        generate and recognize this value." 
    ::= { ipForwardEntry 9 }

ipForwardNextHopAS OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          obsolete
    DESCRIPTION
        "The Autonomous System Number of the Next Hop.  When
        this is unknown or not relevant to the protocol
        indicated by ipForwardProto, zero."
    DEFVAL          { 0 } 
    ::= { ipForwardEntry 10 }

ipForwardMetric1 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          obsolete
    DESCRIPTION
        "The primary routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's ipForwardProto value.
        If this metric is not used, its value should be set to
        -1."
    DEFVAL          { -1 } 
    ::= { ipForwardEntry 11 }

ipForwardMetric2 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          obsolete
    DESCRIPTION
        "An alternate routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's ipForwardProto value.
        If this metric is not used, its value should be set to
        -1."
    DEFVAL          { -1 } 
    ::= { ipForwardEntry 12 }

ipForwardMetric3 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          obsolete
    DESCRIPTION
        "An alternate routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's ipForwardProto value.
        If this metric is not used, its value should be set to
        -1."
    DEFVAL          { -1 } 
    ::= { ipForwardEntry 13 }

ipForwardMetric4 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          obsolete
    DESCRIPTION
        "An alternate routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's ipForwardProto value.
        If this metric is not used, its value should be set to
        -1."
    DEFVAL          { -1 } 
    ::= { ipForwardEntry 14 }

ipForwardMetric5 OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-create
    STATUS          obsolete
    DESCRIPTION
        "An alternate routing metric for this route.  The
        semantics of this metric are determined by the routing-
        protocol specified in the route's ipForwardProto value.
        If this metric is not used, its value should be set to
        -1."
    DEFVAL          { -1 } 
    ::= { ipForwardEntry 15 }
 


-- Obsoleted Definitions - Groups
-- compliance statements
ipForwardOldCompliance MODULE-COMPLIANCE
    STATUS          obsolete
    DESCRIPTION
        "The compliance statement for SNMP entities that
        implement the ipForward MIB."
    MODULE          -- this module
    MANDATORY-GROUPS { ipForwardMultiPathGroup }
    ::= { ipForwardCompliances 2 }

ipForwardMultiPathGroup OBJECT-GROUP
    OBJECTS         {
                        ipForwardNumber,
                        ipForwardDest,
                        ipForwardMask,
                        ipForwardPolicy,
                        ipForwardNextHop,
                        ipForwardIfIndex,
                        ipForwardType,
                        ipForwardProto,
                        ipForwardAge,
                        ipForwardInfo,
                        ipForwardNextHopAS,
                        ipForwardMetric1,
                        ipForwardMetric2,
                        ipForwardMetric3,
                        ipForwardMetric4,
                        ipForwardMetric5
                    }
    STATUS          obsolete
    DESCRIPTION     "IP Multipath Route Table."
    ::= { ipForwardGroups 2 }

END


-- %DNP%  MLC -Compiled MLC

