-- ****************************************************
-- HDSL2-SHDSL-LINE-MIB.my:  HDSL2 SHDSL LINE MIB file
--   
-- January 2011.
--   
-- Copyright (c) 2010-2011 by cisco Systems, Inc.
-- All rights reserved.
--   
-- ****************************************************
-- This mib was extracted from RFC 4319.

HDSL2-SHDSL-LINE-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Counter32,
    Unsigned32,
    Gauge32,
    NOTIFICATION-TYPE,
    Integer32,
    transmission
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    RowStatus,
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    ifIndex
        FROM IF-MIB
    PerfCurrentCount,
    PerfIntervalCount
        FROM PerfHist-TC-MIB
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB;


hdsl2ShdslMIB MODULE-IDENTITY
    LAST-UPDATED    "201112210000Z"
    ORGANIZATION    "ADSLMIB Working Group"
    CONTACT-INFO
            "WG-email:  adslmib@ietf.org
            WG-URL:
               http://www.ietf.org/html.charters/adslmib-charter.html
            Info:       https://www1.ietf.org/mailman/listinfo/adslmib
            Chair:      Mike Sneed
                        Sand Channel Systems
            Postal:     1210-203 Westview Ln
                        Raleigh NC 27605  USA
            Email:      sneedmike@hotmail.com
            Phone:     +1 206 600 7022

            Co-Chair    Bob Ray
                        PESA Switching Systems, Inc.

            Postal      330-A Wynn Drive
                        Huntsville, AL 35805 USA
            Phone       +1 256 726 9200 ext. 142

            Co-editor:  Clay Sikes
                        Zhone Technologies, Inc.
            Postal:     8545 126th Ave. N.
                        Largo, FL 33772 USA
            Email:      csikes@zhone.com
            Phone:      +1 727 530 8257

            Co-editor:  Bob Ray
                        PESA Switching Systems, Inc.
            Postal:     330-A Wynn Drive
                        Huntsville, AL 35805 USA
            Email:      rray@pesa.com
            Phone:      +1 256 726 9200 ext. 142

            Co-editor:  Rajesh Abbi
                        Alcatel USA
            Postal:     2301 Sugar Bush Road
                        Raleigh, NC 27612-3339 USA

            Email:      Rajesh.Abbi@alcatel.com
            Phone:      +1 919 850 6194"
    DESCRIPTION
        "This MIB module defines a collection of objects for managing
        HDSL2/SHDSL lines.  An agent may reside at either end of the
        line; however, the MIB module is designed to require no
        management communication between the modems beyond that
        inherent in the low-level EOC line protocol as defined in
        ANSI T1E1.4/2000-006 (for HDSL2 lines) or in ITU G.991.2
        (for SHDSL lines).

        Copyright (C) The Internet Society (2005).  This version of
        this MIB module is part of RFC 4319; see the RFC itself for
        full legal notices."
    REVISION        "201112210000Z"
    DESCRIPTION
        "addressed comment: defval missing, added region1 as def val as
        per RFC"
    REVISION        "200512070000Z"
    DESCRIPTION
        "This version, published as RFC 4319.
        The following changes have been made in this version:
          1.  Added a 3rd and 4th wire pair.
          2.  Modified all rates such that their rates are only
              constrained by an unsigned 32-bit value and not by
              what today's perceived technology limitations are.
          3.  Clarified that the rates from RFC 3276 include
              payload and any applicable framing and added
              objects for payload-only rates.
          4.  Added an object to indicate whether the
              tip and ring are reversed on a wire pair.
          5.  Added an object to display the activation state
              of a wire pair.
          6.  Added references as necessary for clarification.
          7.  Added display hints to textual conventions as
              necessary.
          8.  Updated conformance statements as necessary.
          9.  Some changes were due to IETF requirements and
              RFC generation tools."
    REVISION        "200205090000Z"
    DESCRIPTION
        "Initial version, published as RFC 3276."
    ::= { transmission 48 }


hdsl2ShdslMibObjects  OBJECT IDENTIFIER
    ::= { hdsl2ShdslMIB 1 }


-- Textual Conventions used in this MIB module

Hdsl2ShdslPerfCurrDayCount ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION
        "A gauge associated with interface performance measurements in
        a current 1-day (24 hour) measurement interval.

        The value of this gauge starts at zero at the beginning of an
        interval and is increased when associated events occur, until
        the end of the 1-day interval.  At that time, the value of the
        gauge is stored in the previous 1-day history interval, as
        defined in a companion object of type
        Hdsl2Shdsl1DayIntevalCount, and the current interval gauge
        is restarted at zero.

        In the case where the agent has no valid data available for
        this interval, the corresponding object instance is not
        available, and upon a retrieval request, a corresponding error
        message shall be returned to indicate that this instance does
        not exist.  Please note that zero is a valid value."
    SYNTAX          Gauge32

Hdsl2Shdsl1DayIntervalCount ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION
        "A counter associated with interface performance measurements
        during the most previous 1-day (24 hour) measurement interval.
        The value of this gauge is equal to the value of the current
        day gauge, as defined in a companion object of type
        Hdsl2ShdslPerfCurrDayCount, at the end of its most recent
        interval.

        In the case where the agent has no valid data available for
        this interval, the corresponding object instance is not
        available, and upon a retrieval request, a corresponding error
        message shall be returned to indicate that this instance does
        not exist."
    SYNTAX          Gauge32

Hdsl2ShdslPerfTimeElapsed ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION
        "The number of seconds that have elapsed since the beginning of
        the current measurement period.  If, for some reason, such as
        an adjustment in the system's time-of-day clock or the addition
        of a leap second, the current interval exceeds the maximum
        value, the agent will return the maximum value.

        For 15-minute intervals, the range is limited to (0..899).
        For 24-hour intervals, the range is limited to (0..86399)."
    SYNTAX          Unsigned32 (0..86399)

Hdsl2ShdslPerfIntervalThreshold ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "d"
    STATUS          current
    DESCRIPTION
        "This convention defines a range of values that may be set in
        a fault threshold alarm control.  As the number of seconds in
        a 15-minute interval numbers at most 900, objects of this type
        may have a range of 0...900, where the value of 0 disables the
        alarm."
    SYNTAX          Unsigned32 (0..900)

Hdsl2ShdslUnitId ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is the unique identification for all units in an
        HDSL2/SHDSL span.  It is based on the EOC unit addressing
        scheme with reference to the xtuC."
    SYNTAX          INTEGER  {
                        xtuC(1),
                        xtuR(2),
                        xru1(3),
                        xru2(4),
                        xru3(5),
                        xru4(6),
                        xru5(7),
                        xru6(8),
                        xru7(9),
                        xru8(10)
                    }

Hdsl2ShdslUnitSide ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is the referenced side of an HDSL2/SHDSL unit - Network
        or Customer side.  The side facing the Network is the Network
        side, while the side facing the Customer is the Customer side."
    SYNTAX          INTEGER  {
                        networkSide(1),
                        customerSide(2)
                    }

Hdsl2ShdslWirePair ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This is the referenced pair of wires in an HDSL2/SHDSL segment.
        HDSL2 only supports a single pair (wirePair1 or two wire),
        SHDSL lines support an optional second pair (wirePair2 or four
        wire), and G.shdsl.bis support an optional third pair
        (wirePair3 or six wire) and an optional fourth pair
        (wirePair4 or eight wire)."
    SYNTAX          INTEGER  {
                        wirePair1(1), -- two wire
                        wirePair2(2), -- four wire
                        wirePair3(3), -- six wire
                        wirePair4(4) -- eight wire                        
                    }

Hdsl2ShdslTransmissionModeType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Contains the regional setting of the HDSL2/SHDSL span,
        represented as a bit-map of possible settings.  The various
        bit positions are as follows:
        Bit   Meaning      Description
        1     region 1     Indicates ITU-T G.991.2 Annex A.
        2     region 2     Indicates ITU-T G.991.2 Annex B."
    SYNTAX          BITS {
                        region1(0),
                        region2(1)
                    }

Hdsl2ShdslClockReferenceType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "The various STU-C symbol clock references for the
        HDSL2/SHDSL span, represented as an enumeration."
    SYNTAX          INTEGER  {
                        localClk(1), -- Mode-1 per G991.2
                        networkClk(2), -- Mode-2 per G991.2
                        dataOrNetworkClk(3), -- Mode-3a per G991.2
                        dataClk(4) -- Mode-3b per G991.2                        
                    }
-- Span Configuration Group

hdsl2ShdslSpanConfTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Hdsl2ShdslSpanConfEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table supports overall configuration of HDSL2/SHDSL
        spans.  Entries in this table MUST be maintained in a
        persistent manner."
    ::= { hdsl2ShdslMibObjects 1 }

hdsl2ShdslSpanConfEntry OBJECT-TYPE
    SYNTAX          Hdsl2ShdslSpanConfEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in the hdsl2ShdslSpanConfTable.  Each entry
        represents the complete span in a single HDSL2/SHDSL line.
        It is indexed by the ifIndex of the associated HDSL2/SHDSL
        line."
    INDEX           { ifIndex } 
    ::= { hdsl2ShdslSpanConfTable 1 }

Hdsl2ShdslSpanConfEntry ::= SEQUENCE {
        hdsl2ShdslSpanConfNumRepeaters Unsigned32,
        hdsl2ShdslSpanConfProfile      SnmpAdminString,
        hdsl2ShdslSpanConfAlarmProfile SnmpAdminString
}

hdsl2ShdslSpanConfNumRepeaters OBJECT-TYPE
    SYNTAX          Unsigned32 (0..8)
    UNITS           "repeaters"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object provisions the number of repeaters/regenerators
        in this HDSL2/SHDSL span." 
    ::= { hdsl2ShdslSpanConfEntry 1 }

hdsl2ShdslSpanConfProfile OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is a pointer to a span configuration profile in
        the hdsl2ShdslSpanConfProfileTable, which applies to this
        span.  The value of this object is the index of the referenced
        profile in the hdsl2ShdslSpanConfProfileTable.  Note that span
        configuration profiles are only applicable to SHDSL lines.

        HDSL2 lines MUST reference the default profile, 'DEFVAL'.
        By default, this object will have the value 'DEFVAL'
        (the index of the default profile).

        Any attempt to set this object to a value that is not the value
        of the index for an active entry in the profile table,
        hdsl2ShdslSpanConfProfileTable, MUST be rejected." 
    ::= { hdsl2ShdslSpanConfEntry 2 }

hdsl2ShdslSpanConfAlarmProfile OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is a pointer to an alarm configuration profile in
        the hdsl2ShdslEndpointAlarmConfProfileTable.  The value of
        this object is the index of the referenced profile in the
        hdsl2ShdslEndpointAlarmConfProfileTable.  The alarm
        threshold configuration in the referenced profile will be
        used by default for all segment endpoints in this span.
        Individual endpoints may override this profile by explicitly
        specifying some other profile in the
        hdsl2ShdslEndpointConfTable.  By default, this object will
        have the value 'DEFVAL' (the index of the default
        profile).

        Any attempt to set this object to a value that is not the value
        of the index for an active entry in the profile table,
        hdsl2ShdslEndpointAlarmConfProfileTable, MUST be rejected." 
    ::= { hdsl2ShdslSpanConfEntry 3 }
 

-- Span Status Group

hdsl2ShdslSpanStatusTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Hdsl2ShdslSpanStatusEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides overall status information of
        HDSL2/SHDSL spans.  This table contains live data from
        equipment.  As such, it is NOT persistent."
    ::= { hdsl2ShdslMibObjects 2 }

hdsl2ShdslSpanStatusEntry OBJECT-TYPE
    SYNTAX          Hdsl2ShdslSpanStatusEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in the hdsl2ShdslSpanStatusTable.  Each entry
        represents the complete span in a single HDSL2/SHDSL line.
        It is indexed by the ifIndex of the associated HDSL2/SHDSL
        line."
    INDEX           { ifIndex } 
    ::= { hdsl2ShdslSpanStatusTable 1 }

Hdsl2ShdslSpanStatusEntry ::= SEQUENCE {
        hdsl2ShdslStatusNumAvailRepeaters        Unsigned32,
        hdsl2ShdslStatusMaxAttainableLineRate    Unsigned32,
        hdsl2ShdslStatusActualLineRate           Unsigned32,
        hdsl2ShdslStatusTransmissionModeCurrent  Hdsl2ShdslTransmissionModeType,
        hdsl2ShdslStatusMaxAttainablePayloadRate Unsigned32,
        hdsl2ShdslStatusActualPayloadRate        Unsigned32
}

hdsl2ShdslStatusNumAvailRepeaters OBJECT-TYPE
    SYNTAX          Unsigned32 (0..8)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Contains the actual number of repeaters/regenerators
        discovered in this HDSL2/SHDSL span." 
    ::= { hdsl2ShdslSpanStatusEntry 1 }

hdsl2ShdslStatusMaxAttainableLineRate OBJECT-TYPE
    SYNTAX          Unsigned32 (0..4294967295)
    UNITS           "bps"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Contains the maximum attainable line rate in this HDSL2/SHDSL
        span.  This object provides the maximum rate the line is
        capable of achieving.  This is based upon measurements made
        during line probing.  This rate includes payload (user data)
        and any applicable framing overhead." 
    ::= { hdsl2ShdslSpanStatusEntry 2 }

hdsl2ShdslStatusActualLineRate OBJECT-TYPE
    SYNTAX          Unsigned32 (0..4294967295)
    UNITS           "bps"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Contains the actual line rate in this HDSL2/SHDSL span.  This
        SHOULD equal ifSpeed.  This rate includes payload (user data)
        and any applicable framing overhead" 
    ::= { hdsl2ShdslSpanStatusEntry 3 }

hdsl2ShdslStatusTransmissionModeCurrent OBJECT-TYPE
    SYNTAX          Hdsl2ShdslTransmissionModeType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Contains the current Power Spectral Density (PSD) regional
        setting of the HDSL2/SHDSL span." 
    ::= { hdsl2ShdslSpanStatusEntry 4 }

hdsl2ShdslStatusMaxAttainablePayloadRate OBJECT-TYPE
    SYNTAX          Unsigned32 (0..4294967295)
    UNITS           "bps"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Contains the maximum attainable payload (user data)
        line rate in this HDSL2/SHDSL span.  This object provides
        the maximum rate the line is capable of achieving.  This
        is based upon measurements made during line probing.  Any
        framing overhead is not included." 
    ::= { hdsl2ShdslSpanStatusEntry 5 }

hdsl2ShdslStatusActualPayloadRate OBJECT-TYPE
    SYNTAX          Unsigned32 (0..4294967295)
    UNITS           "bps"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Contains the actual line rate in this HDSL2/SHDSL span.  Any
        framing overhead is not included." 
    ::= { hdsl2ShdslSpanStatusEntry 6 }
 

-- Unit Inventory Group

hdsl2ShdslInventoryTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Hdsl2ShdslInventoryEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table supports retrieval of unit inventory information
        available via the EOC from units in an HDSL2/SHDSL line.

        Entries in this table are dynamically created during the
        line discovery process.  The life cycle for these entries
        is as follows:

           - xtu discovers a device, either a far-end xtu or an xru
           - an inventory table entry is created for the device
           - the line goes down for whatever reason
           - inventory table entries for unreachable devices are
             destroyed

        As these entries are created/destroyed dynamically, they
        are NOT persistent."
    ::= { hdsl2ShdslMibObjects 3 }

hdsl2ShdslInventoryEntry OBJECT-TYPE
    SYNTAX          Hdsl2ShdslInventoryEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in the hdsl2ShdslInventoryTable.  Each entry
        represents inventory information for a single unit in an
        HDSL2/SHDSL line.  It is indexed by the ifIndex of the
        HDSL2/SHDSL line and the Hdsl2ShdslUnitId of the
        associated unit."
    INDEX           {
                        ifIndex,
                        hdsl2ShdslInvIndex
                    } 
    ::= { hdsl2ShdslInventoryTable 1 }

Hdsl2ShdslInventoryEntry ::= SEQUENCE {
        hdsl2ShdslInvIndex                      Hdsl2ShdslUnitId,
        hdsl2ShdslInvVendorID                   OCTET STRING,
        hdsl2ShdslInvVendorModelNumber          OCTET STRING,
        hdsl2ShdslInvVendorSerialNumber         OCTET STRING,
        hdsl2ShdslInvVendorEOCSoftwareVersion   Integer32,
        hdsl2ShdslInvStandardVersion            Integer32,
        hdsl2ShdslInvVendorListNumber           OCTET STRING,
        hdsl2ShdslInvVendorIssueNumber          OCTET STRING,
        hdsl2ShdslInvVendorSoftwareVersion      OCTET STRING,
        hdsl2ShdslInvEquipmentCode              OCTET STRING,
        hdsl2ShdslInvVendorOther                OCTET STRING,
        hdsl2ShdslInvTransmissionModeCapability Hdsl2ShdslTransmissionModeType
}

hdsl2ShdslInvIndex OBJECT-TYPE
    SYNTAX          Hdsl2ShdslUnitId
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table corresponds to a physical element
        in an HDSL2/SHDSL span.  It is based on the EOC unit addressing
        scheme with reference to the xtuC." 
    ::= { hdsl2ShdslInventoryEntry 1 }

hdsl2ShdslInvVendorID OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (8))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Vendor ID as reported in an Inventory Response message."
    REFERENCE
        "G.991.2, Section 9.5.5.7.4, Inventory response - Message ID
         130, Octets 25-32." 
    ::= { hdsl2ShdslInventoryEntry 2 }

hdsl2ShdslInvVendorModelNumber OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (12))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Vendor model number as reported in an Inventory Response
        message."
    REFERENCE
        "G.991.2, Section 9.5.5.7.4, Inventory response - Message ID
         130, Octets 33-44." 
    ::= { hdsl2ShdslInventoryEntry 3 }

hdsl2ShdslInvVendorSerialNumber OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (12))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Vendor serial number as reported in an Inventory Response
        message."
    REFERENCE
        "G.991.2, Section 9.5.5.7.4, Inventory response - Message ID
         130, Octets 45-56." 
    ::= { hdsl2ShdslInventoryEntry 4 }

hdsl2ShdslInvVendorEOCSoftwareVersion OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Vendor EOC version as reported in a Discovery Response
        message."
    REFERENCE
        "G.991.2, Section 9.5.5.7.2, Discovery response - Message ID
         129, Octet 12." 
    ::= { hdsl2ShdslInventoryEntry 5 }

hdsl2ShdslInvStandardVersion OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Version of the HDSL2/SHDSL standard implemented, as reported
        in an Inventory Response message."
    REFERENCE
        "G.991.2, Section 9.5.5.7.4, Inventory response - Message ID
         130, Octet 2." 
    ::= { hdsl2ShdslInventoryEntry 6 }

hdsl2ShdslInvVendorListNumber OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (3))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Vendor list number as reported in an Inventory Response
        message."
    REFERENCE
        "G.991.2, Section 9.5.5.7.4, Inventory response - Message ID
         130, Octets 3-5." 
    ::= { hdsl2ShdslInventoryEntry 7 }

hdsl2ShdslInvVendorIssueNumber OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (2))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Vendor issue number as reported in an Inventory Response
        message."
    REFERENCE
        "G.991.2, Section 9.5.5.7.4, Inventory response - Message ID
         130, Octets 6-7." 
    ::= { hdsl2ShdslInventoryEntry 8 }

hdsl2ShdslInvVendorSoftwareVersion OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (6))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Vendor software version as reported in an Inventory Response
        message."
    REFERENCE
        "G.991.2, Section 9.5.5.7.4, Inventory response - Message ID
         130, Octets 8-13." 
    ::= { hdsl2ShdslInventoryEntry 9 }

hdsl2ShdslInvEquipmentCode OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (10))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Equipment code conforming to ANSI T1.213, Coded Identification
        of Equipment Entities."
    REFERENCE
        "G.991.2, Section 9.5.5.7.4, Inventory response - Message ID
         130, Octets 14-23." 
    ::= { hdsl2ShdslInventoryEntry 10 }

hdsl2ShdslInvVendorOther OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (12))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Other vendor information as reported in an Inventory Response
        message."
    REFERENCE
        "G.991.2, Section 9.5.5.7.4, Inventory response - Message ID
         130, Octets 57-68." 
    ::= { hdsl2ShdslInventoryEntry 11 }

hdsl2ShdslInvTransmissionModeCapability OBJECT-TYPE
    SYNTAX          Hdsl2ShdslTransmissionModeType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Contains the transmission mode capability of the SHDSL unit." 
    ::= { hdsl2ShdslInventoryEntry 12 }
 

-- Segment Endpoint Configuration Group

hdsl2ShdslEndpointConfTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Hdsl2ShdslEndpointConfEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table supports configuration parameters for segment
        endpoints in an HDSL2/SHDSL line.  As this table is indexed
        by ifIndex, it MUST be maintained in a persistent manner."
    ::= { hdsl2ShdslMibObjects 4 }

hdsl2ShdslEndpointConfEntry OBJECT-TYPE
    SYNTAX          Hdsl2ShdslEndpointConfEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in the hdsl2ShdslEndpointConfTable.  Each entry
        represents a single segment endpoint in an HDSL2/SHDSL line.
        It is indexed by the ifIndex of the HDSL2/SHDSL line, the
        UnitId of the associated unit, the side of the unit, and the
        wire pair of the associated modem."
    INDEX           {
                        ifIndex,
                        hdsl2ShdslInvIndex,
                        hdsl2ShdslEndpointSide,
                        hdsl2ShdslEndpointWirePair
                    } 
    ::= { hdsl2ShdslEndpointConfTable 1 }

Hdsl2ShdslEndpointConfEntry ::= SEQUENCE {
        hdsl2ShdslEndpointSide             Hdsl2ShdslUnitSide,
        hdsl2ShdslEndpointWirePair         Hdsl2ShdslWirePair,
        hdsl2ShdslEndpointAlarmConfProfile SnmpAdminString
}

hdsl2ShdslEndpointSide OBJECT-TYPE
    SYNTAX          Hdsl2ShdslUnitSide
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The side of the unit associated with this segment endpoint --
        Network/Customer side -- as per the Hdsl2ShdslUnitSide textual
        convention." 
    ::= { hdsl2ShdslEndpointConfEntry 1 }

hdsl2ShdslEndpointWirePair OBJECT-TYPE
    SYNTAX          Hdsl2ShdslWirePair
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The wire pair of the modem associated with this segment
        endpoint as per the Hdsl2ShdslWirePair textual convention." 
    ::= { hdsl2ShdslEndpointConfEntry 2 }

hdsl2ShdslEndpointAlarmConfProfile OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..32))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object configures the alarm threshold values to be used
        for this segment endpoint.  The values are obtained from the
        alarm configuration profile referenced by this object.  The
        value of this object is the index of the referenced profile in
        the hdsl2ShdslEndpointAlarmConfProfileTable, or NULL (a
        zero-length SnmpAdminString).  If the value is a zero-length
        SnmpAdminString, the endpoint uses the default Alarm
        Configuration Profile for the associated span as per the
        hdsl2ShdslSpanConfAlarmProfile object in the
        hdsl2ShdslSpanConfTable.  The default value of this object is
        a zero-length SnmpAdminString.

        Any attempt to set this object to a value that is not the value
        of the index for an active entry in the profile table,
        hdsl2ShdslEndpointAlarmConfProfileTable, MUST be rejected." 
    ::= { hdsl2ShdslEndpointConfEntry 3 }
 

-- Segment Endpoint Current Status/Performance Group

hdsl2ShdslEndpointCurrTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Hdsl2ShdslEndpointCurrEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains current status and performance information
        for segment endpoints in HDSL2/SHDSL lines.  As with other
        tables in this MIB module indexed by ifIndex, entries in this
        table MUST be maintained in a persistent manner."
    ::= { hdsl2ShdslMibObjects 5 }

hdsl2ShdslEndpointCurrEntry OBJECT-TYPE
    SYNTAX          Hdsl2ShdslEndpointCurrEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in the hdsl2ShdslEndpointCurrTable.  Each entry
        contains status and performance information relating to a
        single segment endpoint.  It is indexed by the ifIndex of the
        HDSL2/SHDSL line, the UnitId of the associated unit, the side
        of the unit, and the wire pair of the associated modem."
    INDEX           {
                        ifIndex,
                        hdsl2ShdslInvIndex,
                        hdsl2ShdslEndpointSide,
                        hdsl2ShdslEndpointWirePair
                    } 
    ::= { hdsl2ShdslEndpointCurrTable 1 }

Hdsl2ShdslEndpointCurrEntry ::= SEQUENCE {
        hdsl2ShdslEndpointCurrAtn               Integer32,
        hdsl2ShdslEndpointCurrSnrMgn            Integer32,
        hdsl2ShdslEndpointCurrStatus            BITS,
        hdsl2ShdslEndpointES                    Counter32,
        hdsl2ShdslEndpointSES                   Counter32,
        hdsl2ShdslEndpointCRCanomalies          Counter32,
        hdsl2ShdslEndpointLOSWS                 Counter32,
        hdsl2ShdslEndpointUAS                   Counter32,
        hdsl2ShdslEndpointCurr15MinTimeElapsed  Hdsl2ShdslPerfTimeElapsed,
        hdsl2ShdslEndpointCurr15MinES           PerfCurrentCount,
        hdsl2ShdslEndpointCurr15MinSES          PerfCurrentCount,
        hdsl2ShdslEndpointCurr15MinCRCanomalies PerfCurrentCount,
        hdsl2ShdslEndpointCurr15MinLOSWS        PerfCurrentCount,
        hdsl2ShdslEndpointCurr15MinUAS          PerfCurrentCount,
        hdsl2ShdslEndpointCurr1DayTimeElapsed   Hdsl2ShdslPerfTimeElapsed,
        hdsl2ShdslEndpointCurr1DayES            Hdsl2ShdslPerfCurrDayCount,
        hdsl2ShdslEndpointCurr1DaySES           Hdsl2ShdslPerfCurrDayCount,
        hdsl2ShdslEndpointCurr1DayCRCanomalies  Hdsl2ShdslPerfCurrDayCount,
        hdsl2ShdslEndpointCurr1DayLOSWS         Hdsl2ShdslPerfCurrDayCount,
        hdsl2ShdslEndpointCurr1DayUAS           Hdsl2ShdslPerfCurrDayCount,
        hdsl2ShdslEndpointCurrTipRingReversal   INTEGER,
        hdsl2ShdslEndpointCurrActivationState   INTEGER
}

hdsl2ShdslEndpointCurrAtn OBJECT-TYPE
    SYNTAX          Integer32 (-127..128)
    UNITS           "dB"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The current loop attenuation for this endpoint as reported in
        a Network or Customer Side Performance Status message."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 1 }

hdsl2ShdslEndpointCurrSnrMgn OBJECT-TYPE
    SYNTAX          Integer32 (-127..128)
    UNITS           "dB"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The current SNR margin for this endpoint as reported in a
        Status Response/SNR message."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 2 }

hdsl2ShdslEndpointCurrStatus OBJECT-TYPE
    SYNTAX          BITS {
                        noDefect(0),
                        powerBackoff(1),
                        deviceFault(2),
                        dcContinuityFault(3),
                        snrMarginAlarm(4),
                        loopAttenuationAlarm(5),
                        loswFailureAlarm(6),
                        configInitFailure(7),
                        protocolInitFailure(8),
                        noNeighborPresent(9),
                        loopbackActive(10)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Contains the current state of the endpoint.  This is a
        bit-map of possible conditions.  The various bit positions
        are as follows:

        noDefect               There are no defects on the line.

        powerBackoff           Indicates enhanced Power Backoff.

        deviceFault            Indicates that a vendor-dependent
                               diagnostic or self-test fault
                               has been detected.

        dcContinuityFault      Indicates vendor-dependent
                               conditions that interfere with
                               span powering such as short and
                               open circuits.

        snrMarginAlarm         Indicates that the SNR margin
                               has dropped below the alarm threshold.

        loopAttenuationAlarm   Indicates that the loop attenuation
                               exceeds the alarm threshold.

        loswFailureAlarm       Indicates a forward LOSW alarm.

        configInitFailure      Endpoint failure during initialization
                               due to paired endpoint not able to
                               support requested configuration.

        protocolInitFailure    Endpoint failure during initialization
                               due to incompatible protocol used by
                               the paired endpoint.

        noNeighborPresent      Endpoint failure during initialization
                               due to no activation sequence detected
                               from paired endpoint.

        loopbackActive         A loopback is currently active at this
                               segment endpoint.

        This is intended to supplement ifOperStatus.  Note that there
        is a 1:1 relationship between the status bits defined in this
        object and the notification thresholds defined elsewhere in
        this MIB module."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 3 }

hdsl2ShdslEndpointES OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Errored Seconds (ES) on this endpoint since the xU
        was last restarted."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 4 }

hdsl2ShdslEndpointSES OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Severely Errored Seconds (SES) on this endpoint
        since the xU was last restarted."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 5 }

hdsl2ShdslEndpointCRCanomalies OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "detected CRC Anomalies"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of CRC anomalies on this endpoint since the xU was
        last restarted."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 6 }

hdsl2ShdslEndpointLOSWS OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Loss of Sync Word (LOSW) Seconds on this endpoint
        since the xU was last restarted."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 7 }

hdsl2ShdslEndpointUAS OBJECT-TYPE
    SYNTAX          Counter32
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Unavailable Seconds (UAS) on this endpoint since
        the xU was last restarted."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 8 }

hdsl2ShdslEndpointCurr15MinTimeElapsed OBJECT-TYPE
    SYNTAX          Hdsl2ShdslPerfTimeElapsed
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Total elapsed seconds in the current 15-minute interval." 
    ::= { hdsl2ShdslEndpointCurrEntry 9 }

hdsl2ShdslEndpointCurr15MinES OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Errored Seconds (ES) in the current 15-minute
        interval."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 10 }

hdsl2ShdslEndpointCurr15MinSES OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Severely Errored Seconds (SES) in the current
        15-minute interval."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 11 }

hdsl2ShdslEndpointCurr15MinCRCanomalies OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "detected CRC Anomalies"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of CRC anomalies in the current 15-minute interval."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 12 }

hdsl2ShdslEndpointCurr15MinLOSWS OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Loss of Sync Word (LOSW) Seconds in the current
        15-minute interval."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 13 }

hdsl2ShdslEndpointCurr15MinUAS OBJECT-TYPE
    SYNTAX          PerfCurrentCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Unavailable Seconds (UAS) in the current 15-minute
        interval."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 14 }

hdsl2ShdslEndpointCurr1DayTimeElapsed OBJECT-TYPE
    SYNTAX          Hdsl2ShdslPerfTimeElapsed
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Number of seconds that have elapsed since the beginning of
        the current 1-day interval." 
    ::= { hdsl2ShdslEndpointCurrEntry 15 }

hdsl2ShdslEndpointCurr1DayES OBJECT-TYPE
    SYNTAX          Hdsl2ShdslPerfCurrDayCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Errored Seconds (ES) during the current day as
        measured by hdsl2ShdslEndpointCurr1DayTimeElapsed."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 16 }

hdsl2ShdslEndpointCurr1DaySES OBJECT-TYPE
    SYNTAX          Hdsl2ShdslPerfCurrDayCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Severely Errored Seconds (SES) during the current
        day as measured by hdsl2ShdslEndpointCurr1DayTimeElapsed."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 17 }

hdsl2ShdslEndpointCurr1DayCRCanomalies OBJECT-TYPE
    SYNTAX          Hdsl2ShdslPerfCurrDayCount
    UNITS           "detected CRC Anomalies"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of CRC anomalies during the current day as measured
        by hdsl2ShdslEndpointCurr1DayTimeElapsed."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 18 }

hdsl2ShdslEndpointCurr1DayLOSWS OBJECT-TYPE
    SYNTAX          Hdsl2ShdslPerfCurrDayCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Loss of Sync Word (LOSW) Seconds during the current
        day as measured by hdsl2ShdslEndpointCurr1DayTimeElapsed."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 19 }

hdsl2ShdslEndpointCurr1DayUAS OBJECT-TYPE
    SYNTAX          Hdsl2ShdslPerfCurrDayCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Unavailable Seconds (UAS) during the current day as
        measured by hdsl2ShdslEndpointCurr1DayTimeElapsed."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2ShdslEndpointCurrEntry 20 }

hdsl2ShdslEndpointCurrTipRingReversal OBJECT-TYPE
    SYNTAX          INTEGER  {
                        normal(1),
                        reversed(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the state of the tip/ring for the
        wire pair." 
    ::= { hdsl2ShdslEndpointCurrEntry 21 }

hdsl2ShdslEndpointCurrActivationState OBJECT-TYPE
    SYNTAX          INTEGER  {
                        preActivation(1), -- PreTrain
                        activation(2), -- Training
                        data(3) -- Trained                        
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the activation or training state of
        the wire pair."
    REFERENCE
        "ITU-T G.991.2, Section 6.2 PMD Activation Sequence" 
    ::= { hdsl2ShdslEndpointCurrEntry 22 }
 

-- Segment Endpoint 15-Minute Interval Status/Performance Group

hdsl2Shdsl15MinIntervalTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Hdsl2Shdsl15MinIntervalEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides one row for each HDSL2/SHDSL endpoint
        performance data collection interval.  This table contains
        live data from equipment.  As such, it is NOT persistent."
    ::= { hdsl2ShdslMibObjects 6 }

hdsl2Shdsl15MinIntervalEntry OBJECT-TYPE
    SYNTAX          Hdsl2Shdsl15MinIntervalEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in the hdsl2Shdsl15MinIntervalTable."
    INDEX           {
                        ifIndex,
                        hdsl2ShdslInvIndex,
                        hdsl2ShdslEndpointSide,
                        hdsl2ShdslEndpointWirePair,
                        hdsl2Shdsl15MinIntervalNumber
                    } 
    ::= { hdsl2Shdsl15MinIntervalTable 1 }

Hdsl2Shdsl15MinIntervalEntry ::= SEQUENCE {
        hdsl2Shdsl15MinIntervalNumber       Unsigned32,
        hdsl2Shdsl15MinIntervalES           PerfIntervalCount,
        hdsl2Shdsl15MinIntervalSES          PerfIntervalCount,
        hdsl2Shdsl15MinIntervalCRCanomalies PerfIntervalCount,
        hdsl2Shdsl15MinIntervalLOSWS        PerfIntervalCount,
        hdsl2Shdsl15MinIntervalUAS          PerfIntervalCount
}

hdsl2Shdsl15MinIntervalNumber OBJECT-TYPE
    SYNTAX          Unsigned32 (1..96)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Performance Data Interval number.  Interval 1 is the most
        recent previous interval; interval 96 is 24 hours ago.
        Intervals 2..96 are optional." 
    ::= { hdsl2Shdsl15MinIntervalEntry 1 }

hdsl2Shdsl15MinIntervalES OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Errored Seconds (ES) during the interval."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2Shdsl15MinIntervalEntry 2 }

hdsl2Shdsl15MinIntervalSES OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Severely Errored Seconds (SES) during the interval."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2Shdsl15MinIntervalEntry 3 }

hdsl2Shdsl15MinIntervalCRCanomalies OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "detected CRC Anomalies"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of CRC anomalies during the interval."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2Shdsl15MinIntervalEntry 4 }

hdsl2Shdsl15MinIntervalLOSWS OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Loss of Sync Word (LOSW) Seconds during the
        interval."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2Shdsl15MinIntervalEntry 5 }

hdsl2Shdsl15MinIntervalUAS OBJECT-TYPE
    SYNTAX          PerfIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Unavailable Seconds (UAS) during the interval."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2Shdsl15MinIntervalEntry 6 }
 

-- Segment Endpoint 1-Day Interval Status/Performance Group

hdsl2Shdsl1DayIntervalTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Hdsl2Shdsl1DayIntervalEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides one row for each HDSL2/SHDSL endpoint
        performance data collection interval.  This table contains
        live data from equipment.  As such, it is NOT persistent."
    ::= { hdsl2ShdslMibObjects 7 }

hdsl2Shdsl1DayIntervalEntry OBJECT-TYPE
    SYNTAX          Hdsl2Shdsl1DayIntervalEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in the hdsl2Shdsl1DayIntervalTable."
    INDEX           {
                        ifIndex,
                        hdsl2ShdslInvIndex,
                        hdsl2ShdslEndpointSide,
                        hdsl2ShdslEndpointWirePair,
                        hdsl2Shdsl1DayIntervalNumber
                    } 
    ::= { hdsl2Shdsl1DayIntervalTable 1 }

Hdsl2Shdsl1DayIntervalEntry ::= SEQUENCE {
        hdsl2Shdsl1DayIntervalNumber       Unsigned32,
        hdsl2Shdsl1DayIntervalMoniSecs     Hdsl2ShdslPerfTimeElapsed,
        hdsl2Shdsl1DayIntervalES           Hdsl2Shdsl1DayIntervalCount,
        hdsl2Shdsl1DayIntervalSES          Hdsl2Shdsl1DayIntervalCount,
        hdsl2Shdsl1DayIntervalCRCanomalies Hdsl2Shdsl1DayIntervalCount,
        hdsl2Shdsl1DayIntervalLOSWS        Hdsl2Shdsl1DayIntervalCount,
        hdsl2Shdsl1DayIntervalUAS          Hdsl2Shdsl1DayIntervalCount
}

hdsl2Shdsl1DayIntervalNumber OBJECT-TYPE
    SYNTAX          Unsigned32 (1..30)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "History Data Interval number.  Interval 1 is the most
        recent previous day; interval 30 is 30 days ago.  Intervals
        2..30 are optional." 
    ::= { hdsl2Shdsl1DayIntervalEntry 1 }

hdsl2Shdsl1DayIntervalMoniSecs OBJECT-TYPE
    SYNTAX          Hdsl2ShdslPerfTimeElapsed
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The amount of time in the 1-day interval over which the
        performance monitoring information is actually counted.
        This value will be the same as the interval duration except
        in a situation where performance monitoring data could not
        be collected for any reason." 
    ::= { hdsl2Shdsl1DayIntervalEntry 2 }

hdsl2Shdsl1DayIntervalES OBJECT-TYPE
    SYNTAX          Hdsl2Shdsl1DayIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Errored Seconds (ES) during the 1-day interval as
        measured by hdsl2Shdsl1DayIntervalMoniSecs."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2Shdsl1DayIntervalEntry 3 }

hdsl2Shdsl1DayIntervalSES OBJECT-TYPE
    SYNTAX          Hdsl2Shdsl1DayIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Severely Errored Seconds (SES) during the 1-day
        interval as measured by hdsl2Shdsl1DayIntervalMoniSecs."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2Shdsl1DayIntervalEntry 4 }

hdsl2Shdsl1DayIntervalCRCanomalies OBJECT-TYPE
    SYNTAX          Hdsl2Shdsl1DayIntervalCount
    UNITS           "detected CRC Anomalies"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of CRC anomalies during the 1-day interval as
        measured by hdsl2Shdsl1DayIntervalMoniSecs."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2Shdsl1DayIntervalEntry 5 }

hdsl2Shdsl1DayIntervalLOSWS OBJECT-TYPE
    SYNTAX          Hdsl2Shdsl1DayIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Loss of Sync Word (LOSW) Seconds during the 1-day
        interval as measured by hdsl2Shdsl1DayIntervalMoniSecs."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2Shdsl1DayIntervalEntry 6 }

hdsl2Shdsl1DayIntervalUAS OBJECT-TYPE
    SYNTAX          Hdsl2Shdsl1DayIntervalCount
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Count of Unavailable Seconds (UAS) during the 1-day interval
        as measured by hdsl2Shdsl1DayIntervalMoniSecs."
    REFERENCE       "HDSL2 Section 7.5.3.7; SHDSL Section 9.5.5.7" 
    ::= { hdsl2Shdsl1DayIntervalEntry 7 }
 

-- Maintenance Group

hdsl2ShdslEndpointMaintTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Hdsl2ShdslEndpointMaintEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table supports maintenance operations (e.g., loopbacks)
        to be performed on HDSL2/SHDSL segment endpoints.  This table
        contains live data from equipment.  As such, it is NOT
        persistent."
    ::= { hdsl2ShdslMibObjects 8 }

hdsl2ShdslEndpointMaintEntry OBJECT-TYPE
    SYNTAX          Hdsl2ShdslEndpointMaintEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in the hdsl2ShdslEndpointMaintTable.  Each entry
        corresponds to a single segment endpoint and is indexed by the
        ifIndex of the HDSL2/SHDSL line, the UnitId of the associated
        unit, and the side of the unit."
    INDEX           {
                        ifIndex,
                        hdsl2ShdslInvIndex,
                        hdsl2ShdslEndpointSide
                    } 
    ::= { hdsl2ShdslEndpointMaintTable 1 }

Hdsl2ShdslEndpointMaintEntry ::= SEQUENCE {
        hdsl2ShdslMaintLoopbackConfig  INTEGER,
        hdsl2ShdslMaintTipRingReversal INTEGER,
        hdsl2ShdslMaintPowerBackOff    INTEGER,
        hdsl2ShdslMaintSoftRestart     INTEGER
}

hdsl2ShdslMaintLoopbackConfig OBJECT-TYPE
    SYNTAX          INTEGER  {
                        noLoopback(1),
                        normalLoopback(2),
                        specialLoopback(3)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object controls configuration of loopbacks for the
        associated segment endpoint.  The status of the loopback
        is obtained via the hdsl2ShdslEndpointCurrStatus object." 
    ::= { hdsl2ShdslEndpointMaintEntry 1 }

hdsl2ShdslMaintTipRingReversal OBJECT-TYPE
    SYNTAX          INTEGER  {
                        normal(1),
                        reversed(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the state of the tip/ring pair at the
        associated segment endpoint." 
    ::= { hdsl2ShdslEndpointMaintEntry 2 }

hdsl2ShdslMaintPowerBackOff OBJECT-TYPE
    SYNTAX          INTEGER  {
                        default(1),
                        enhanced(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object configures the receiver at the associated
        segment endpoint to operate in default or enhanced power
        backoff mode." 
    ::= { hdsl2ShdslEndpointMaintEntry 3 }

hdsl2ShdslMaintSoftRestart OBJECT-TYPE
    SYNTAX          INTEGER  {
                        ready(1),
                        restart(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object enables the manager to trigger a soft restart
        of the modem at the associated segment endpoint.  The
        manager may only set this object to the 'restart(2)'
        value, which initiates a restart.  The agent will perform a
        restart after approximately 5 seconds.  Following the 5 second
        period, the agent will restore the object to the 'ready(1)'
        state." 
    ::= { hdsl2ShdslEndpointMaintEntry 4 }
 


hdsl2ShdslUnitMaintTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Hdsl2ShdslUnitMaintEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table supports maintenance operations for units in a
        HDSL2/SHDSL line.  Entries in this table MUST be maintained
        in a persistent manner."
    ::= { hdsl2ShdslMibObjects 9 }

hdsl2ShdslUnitMaintEntry OBJECT-TYPE
    SYNTAX          Hdsl2ShdslUnitMaintEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in the hdsl2ShdslUnitMaintTable.  Each entry
        corresponds to a single unit and is indexed by the
        ifIndex of the HDSL2/SHDSL line and the UnitId of the
        associated unit."
    INDEX           {
                        ifIndex,
                        hdsl2ShdslInvIndex
                    } 
    ::= { hdsl2ShdslUnitMaintTable 1 }

Hdsl2ShdslUnitMaintEntry ::= SEQUENCE {
        hdsl2ShdslMaintLoopbackTimeout Integer32,
        hdsl2ShdslMaintUnitPowerSource INTEGER
}

hdsl2ShdslMaintLoopbackTimeout OBJECT-TYPE
    SYNTAX          Integer32 (0..4095)
    UNITS           "minutes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object configures the timeout value for loopbacks
        initiated at segments endpoints contained in the associated
        unit.  A value of 0 disables the timeout." 
    ::= { hdsl2ShdslUnitMaintEntry 1 }

hdsl2ShdslMaintUnitPowerSource OBJECT-TYPE
    SYNTAX          INTEGER  {
                        local(1),
                        span(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the DC power source being used by the
        associated unit." 
    ::= { hdsl2ShdslUnitMaintEntry 2 }
 

-- Span Configuration Profile Group

hdsl2ShdslSpanConfProfileTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Hdsl2ShdslSpanConfProfileEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table supports definitions of span configuration
        profiles for SHDSL lines.  HDSL2 does not support these
        configuration options.  This table MUST be maintained
        in a persistent manner."
    ::= { hdsl2ShdslMibObjects 10 }

hdsl2ShdslSpanConfProfileEntry OBJECT-TYPE
    SYNTAX          Hdsl2ShdslSpanConfProfileEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry corresponds to a single span configuration
        profile.  Each profile contains a set of span configuration
        parameters.  The configuration parameters in a profile are
        applied to those lines referencing that profile (see the
        hdsl2ShdslSpanConfProfile object).  Profiles may be
        created/deleted using the row creation/deletion mechanism
        via hdsl2ShdslSpanConfProfileRowStatus.  If an active
        entry is referenced in hdsl2ShdslSpanConfProfile, the
        entry MUST remain active until all references are removed."
    INDEX           { IMPLIED hdsl2ShdslSpanConfProfileName } 
    ::= { hdsl2ShdslSpanConfProfileTable 1 }

Hdsl2ShdslSpanConfProfileEntry ::= SEQUENCE {
        hdsl2ShdslSpanConfProfileName               SnmpAdminString,
        hdsl2ShdslSpanConfWireInterface             INTEGER,
        hdsl2ShdslSpanConfMinLineRate               Unsigned32,
        hdsl2ShdslSpanConfMaxLineRate               Unsigned32,
        hdsl2ShdslSpanConfPSD                       INTEGER,
        hdsl2ShdslSpanConfTransmissionMode          Hdsl2ShdslTransmissionModeType,
        hdsl2ShdslSpanConfRemoteEnabled             INTEGER,
        hdsl2ShdslSpanConfPowerFeeding              INTEGER,
        hdsl2ShdslSpanConfCurrCondTargetMarginDown  Integer32,
        hdsl2ShdslSpanConfWorstCaseTargetMarginDown Integer32,
        hdsl2ShdslSpanConfCurrCondTargetMarginUp    Integer32,
        hdsl2ShdslSpanConfWorstCaseTargetMarginUp   Integer32,
        hdsl2ShdslSpanConfUsedTargetMargins         BITS,
        hdsl2ShdslSpanConfReferenceClock            Hdsl2ShdslClockReferenceType,
        hdsl2ShdslSpanConfLineProbeEnable           INTEGER,
        hdsl2ShdslSpanConfProfileRowStatus          RowStatus
}

hdsl2ShdslSpanConfProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object is the unique index associated with this profile.
        Entries in this table are referenced via the object
        hdsl2ShdslSpanConfProfile in Hdsl2ShdslSpanConfEntry." 
    ::= { hdsl2ShdslSpanConfProfileEntry 1 }

hdsl2ShdslSpanConfWireInterface OBJECT-TYPE
    SYNTAX          INTEGER  {
                        twoWire(1),
                        fourWire(2),
                        sixWire(3),
                        eightWire(4)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object configures the two-wire or optional four-wire,
        six-wire, or eight-wire operation for SHDSL lines."
    DEFVAL          { twoWire } 
    ::= { hdsl2ShdslSpanConfProfileEntry 2 }

hdsl2ShdslSpanConfMinLineRate OBJECT-TYPE
    SYNTAX          Unsigned32 (0..4294967295)
    UNITS           "bps"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object configures the minimum transmission rate for
        the associated SHDSL Line in bits-per-second (bps) and includes
        both payload (user data) and any applicable framing overhead.
        If the minimum line rate equals the maximum line rate
        (hdsl2ShdslSpanMaxLineRate), the line rate is considered
        'fixed'.  If the minimum line rate is less than the
        maximum line rate, the line rate is considered
        'rate-adaptive'."
    DEFVAL          { 1552000 } 
    ::= { hdsl2ShdslSpanConfProfileEntry 3 }

hdsl2ShdslSpanConfMaxLineRate OBJECT-TYPE
    SYNTAX          Unsigned32 (0..4294967295)
    UNITS           "bps"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object configures the maximum transmission rate for
        the associated SHDSL Line in bits-per-second (bps) and includes
        both payload (user data) and any applicable framing overhead.
        If the minimum line rate equals the maximum line rate
        (hdsl2ShdslSpanMaxLineRate), the line rate is considered
        'fixed'.  If the minimum line rate is less than the
        maximum line rate, the line rate is considered
        'rate-adaptive'."
    DEFVAL          { 1552000 } 
    ::= { hdsl2ShdslSpanConfProfileEntry 4 }

hdsl2ShdslSpanConfPSD OBJECT-TYPE
    SYNTAX          INTEGER  {
                        symmetric(1),
                        asymmetric(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object configures use of symmetric/asymmetric PSD (Power
        Spectral Density) Mask for the associated SHDSL Line.  Support
        for symmetric PSD is mandatory for all supported data rates.
        Support for asymmetric PSD is optional."
    DEFVAL          { symmetric } 
    ::= { hdsl2ShdslSpanConfProfileEntry 5 }

hdsl2ShdslSpanConfTransmissionMode OBJECT-TYPE
    SYNTAX          Hdsl2ShdslTransmissionModeType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the regional setting for the SHDSL
        line."
    DEFVAL          { {region1} } 
    ::= { hdsl2ShdslSpanConfProfileEntry 6 }

hdsl2ShdslSpanConfRemoteEnabled OBJECT-TYPE
    SYNTAX          INTEGER  {
                        enabled(1),
                        disabled(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object enables/disables support for remote management
        of the units in an SHDSL line from the STU-R via the EOC."
    DEFVAL          { enabled } 
    ::= { hdsl2ShdslSpanConfProfileEntry 7 }

hdsl2ShdslSpanConfPowerFeeding OBJECT-TYPE
    SYNTAX          INTEGER  {
                        noPower(1),
                        powerFeed(2),
                        wettingCurrent(3)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object enables/disables support for optional power
        feeding in an SHDSL line."
    DEFVAL          { noPower } 
    ::= { hdsl2ShdslSpanConfProfileEntry 8 }

hdsl2ShdslSpanConfCurrCondTargetMarginDown OBJECT-TYPE
    SYNTAX          Integer32 (-10..21)
    UNITS           "dB"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the downstream current condition target
        SNR margin for an SHDSL line.  The SNR margin is the difference
        between the desired SNR and the actual SNR.  Target SNR margin
        is the desired SNR margin for a unit."
    DEFVAL          { 0 } 
    ::= { hdsl2ShdslSpanConfProfileEntry 9 }

hdsl2ShdslSpanConfWorstCaseTargetMarginDown OBJECT-TYPE
    SYNTAX          Integer32 (-10..21)
    UNITS           "dB"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the downstream worst-case target SNR
        margin for an SHDSL line.  The SNR margin is the difference
        between the desired SNR and the actual SNR.  Target SNR
        margin is the desired SNR margin for a unit."
    DEFVAL          { 0 } 
    ::= { hdsl2ShdslSpanConfProfileEntry 10 }

hdsl2ShdslSpanConfCurrCondTargetMarginUp OBJECT-TYPE
    SYNTAX          Integer32 (-10..21)
    UNITS           "dB"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the upstream current-condition target
        SNR margin for an SHDSL line.  The SNR margin is the difference
        between the desired SNR and the actual SNR.  Target SNR margin
        is the desired SNR margin for a unit."
    DEFVAL          { 0 } 
    ::= { hdsl2ShdslSpanConfProfileEntry 11 }

hdsl2ShdslSpanConfWorstCaseTargetMarginUp OBJECT-TYPE
    SYNTAX          Integer32 (-10..21)
    UNITS           "dB"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the upstream worst-case target SNR
        margin for an SHDSL line.  The SNR margin is the difference
        between the desired SNR and the actual SNR.  Target SNR margin
        is the desired SNR margin for a unit."
    DEFVAL          { 0 } 
    ::= { hdsl2ShdslSpanConfProfileEntry 12 }

hdsl2ShdslSpanConfUsedTargetMargins OBJECT-TYPE
    SYNTAX          BITS {
                        currCondDown(0),
                        worstCaseDown(1),
                        currCondUp(2),
                        worstCaseUp(3)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Indicates whether a target SNR margin is enabled or
        disabled.  This is a bit-map of possible settings.  The
        various bit positions are as follows:

        currCondDown   - current-condition downstream target SNR
                         margin enabled

        worstCaseDown  - worst-case downstream target SNR margin
                         enabled

        currCondUp     - current-condition upstream target SNR
                         margin enabled

        worstCaseUp    - worst-case upstream target SNR margin
                         enabled."
    DEFVAL          { { currCondDown } } 
    ::= { hdsl2ShdslSpanConfProfileEntry 13 }

hdsl2ShdslSpanConfReferenceClock OBJECT-TYPE
    SYNTAX          Hdsl2ShdslClockReferenceType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object configures the clock reference for the STU-C
        in an SHDSL Line."
    DEFVAL          { localClk } 
    ::= { hdsl2ShdslSpanConfProfileEntry 14 }

hdsl2ShdslSpanConfLineProbeEnable OBJECT-TYPE
    SYNTAX          INTEGER  {
                        disable(1),
                        enable(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object enables/disables support for Line Probe of
        the units in an SHDSL line.  When Line Probe is enabled, the
        system performs Line Probing to find the best possible
        rate.  If Line Probe is disabled, the rate adaptation phase
        is skipped to shorten set up time."
    DEFVAL          { disable } 
    ::= { hdsl2ShdslSpanConfProfileEntry 15 }

hdsl2ShdslSpanConfProfileRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object controls creation/deletion of the associated
        entry in this table per the semantics of RowStatus.  If an
        active entry is referenced in hdsl2ShdslSpanConfProfile, the
        entry MUST remain active until all references are removed." 
    ::= { hdsl2ShdslSpanConfProfileEntry 16 }
 

-- Segment Endpoint Alarm Configuration Profile group

hdsl2ShdslEndpointAlarmConfProfileTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF Hdsl2ShdslEndpointAlarmConfProfileEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table supports definitions of alarm configuration
        profiles for HDSL2/SHDSL segment endpoints.  This table
        MUST be maintained in a persistent manner."
    ::= { hdsl2ShdslMibObjects 11 }

hdsl2ShdslEndpointAlarmConfProfileEntry OBJECT-TYPE
    SYNTAX          Hdsl2ShdslEndpointAlarmConfProfileEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry corresponds to a single alarm configuration profile.
        Each profile contains a set of parameters for setting alarm
        thresholds for various performance attributes monitored at
        HDSL2/SHDSL segment endpoints.  Profiles may be created/deleted
        using the row creation/deletion mechanism via
        hdsl2ShdslEndpointAlarmConfProfileRowStatus.  If an active
        entry is referenced in either hdsl2ShdslSpanConfAlarmProfile
        or hdsl2ShdslEndpointAlarmConfProfile, the entry MUST remain
        active until all references are removed."
    INDEX           { IMPLIED hdsl2ShdslEndpointAlarmConfProfileName } 
    ::= { hdsl2ShdslEndpointAlarmConfProfileTable 1 }

Hdsl2ShdslEndpointAlarmConfProfileEntry ::= SEQUENCE {
        hdsl2ShdslEndpointAlarmConfProfileName      SnmpAdminString,
        hdsl2ShdslEndpointThreshLoopAttenuation     Integer32,
        hdsl2ShdslEndpointThreshSNRMargin           Integer32,
        hdsl2ShdslEndpointThreshES                  Hdsl2ShdslPerfIntervalThreshold,
        hdsl2ShdslEndpointThreshSES                 Hdsl2ShdslPerfIntervalThreshold,
        hdsl2ShdslEndpointThreshCRCanomalies        Integer32,
        hdsl2ShdslEndpointThreshLOSWS               Hdsl2ShdslPerfIntervalThreshold,
        hdsl2ShdslEndpointThreshUAS                 Hdsl2ShdslPerfIntervalThreshold,
        hdsl2ShdslEndpointAlarmConfProfileRowStatus RowStatus
}

hdsl2ShdslEndpointAlarmConfProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object is the unique index associated with this profile." 
    ::= { hdsl2ShdslEndpointAlarmConfProfileEntry 1 }

hdsl2ShdslEndpointThreshLoopAttenuation OBJECT-TYPE
    SYNTAX          Integer32 (-127..128)
    UNITS           "dB"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object configures the loop attenuation alarm threshold.
        When the current value of hdsl2ShdslEndpointCurrAtn reaches
        or exceeds this threshold, an hdsl2ShdslLoopAttenCrossing
        MAY be generated."
    DEFVAL          { 0 } 
    ::= { hdsl2ShdslEndpointAlarmConfProfileEntry 2 }

hdsl2ShdslEndpointThreshSNRMargin OBJECT-TYPE
    SYNTAX          Integer32 (-127..128)
    UNITS           "dB"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object configures the SNR margin alarm threshold.
        When the current value of hdsl2ShdslEndpointCurrSnrMgn
        reaches or drops below this threshold, a
        hdsl2ShdslSNRMarginCrossing MAY be generated."
    DEFVAL          { 0 } 
    ::= { hdsl2ShdslEndpointAlarmConfProfileEntry 3 }

hdsl2ShdslEndpointThreshES OBJECT-TYPE
    SYNTAX          Hdsl2ShdslPerfIntervalThreshold
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object configures the threshold for the number of
        Errored Seconds (ES) within any given 15-minute performance
        data collection interval.  If the value of Errored Seconds
        in a particular 15-minute collection interval reaches/
        exceeds this value, an hdsl2ShdslPerfESThresh MAY be
        generated.  At most, one notification will be sent per
        interval per endpoint."
    DEFVAL          { 0 } 
    ::= { hdsl2ShdslEndpointAlarmConfProfileEntry 4 }

hdsl2ShdslEndpointThreshSES OBJECT-TYPE
    SYNTAX          Hdsl2ShdslPerfIntervalThreshold
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object configures the threshold for the number of
        Severely Errored Seconds (SES) within any given 15-minute
        performance data collection interval.  If the value of
        Severely Errored Seconds in a particular 15-minute collection
        interval reaches/exceeds this value, an hdsl2ShdslPerfSESThresh
        MAY be generated.  At most, one notification will be sent per
        interval per endpoint."
    DEFVAL          { 0 } 
    ::= { hdsl2ShdslEndpointAlarmConfProfileEntry 5 }

hdsl2ShdslEndpointThreshCRCanomalies OBJECT-TYPE
    SYNTAX          Integer32
    UNITS           "detected CRC Anomalies"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object configures the threshold for the number of
        CRC anomalies within any given 15-minute performance data
        collection interval.  If the value of CRC anomalies in a
        particular 15-minute collection interval reaches/exceeds
        this value, an hdsl2ShdslPerfCRCanomaliesThresh MAY be
        generated.  At most, one notification will be sent per
        interval per endpoint."
    DEFVAL          { 0 } 
    ::= { hdsl2ShdslEndpointAlarmConfProfileEntry 6 }

hdsl2ShdslEndpointThreshLOSWS OBJECT-TYPE
    SYNTAX          Hdsl2ShdslPerfIntervalThreshold
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object configures the threshold for the number of
        Loss of Sync Word (LOSW) Seconds within any given 15-minute
        performance data collection interval.  If the value of LOSW
        in a particular 15-minute collection interval reaches/exceeds
        this value, an hdsl2ShdslPerfLOSWSThresh MAY be generated.
        At most, one notification will be sent per interval per
        endpoint."
    DEFVAL          { 0 } 
    ::= { hdsl2ShdslEndpointAlarmConfProfileEntry 7 }

hdsl2ShdslEndpointThreshUAS OBJECT-TYPE
    SYNTAX          Hdsl2ShdslPerfIntervalThreshold
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object configures the threshold for the number of
        Unavailable Seconds (UAS) within any given 15-minute
        performance data collection interval.  If the value of UAS
        in a particular 15-minute collection interval reaches/exceeds
        this value, an hdsl2ShdslPerfUASThresh MAY be generated.
        At most, one notification will be sent per interval per
        endpoint."
    DEFVAL          { 0 } 
    ::= { hdsl2ShdslEndpointAlarmConfProfileEntry 8 }

hdsl2ShdslEndpointAlarmConfProfileRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object controls creation/deletion of the associated
        entry in this table as per the semantics of RowStatus.
        If an active entry is referenced in either
        hdsl2ShdslSpanConfAlarmProfile or
        hdsl2ShdslEndpointAlarmConfProfile, the entry MUST remain
        active until all references are removed." 
    ::= { hdsl2ShdslEndpointAlarmConfProfileEntry 9 }
 

-- Notifications Group

hdsl2ShdslNotifications  OBJECT IDENTIFIER
    ::= { hdsl2ShdslMIB 0 }


hdsl2ShdslLoopAttenCrossing NOTIFICATION-TYPE
    OBJECTS         {
                        hdsl2ShdslEndpointCurrAtn,
                        hdsl2ShdslEndpointThreshLoopAttenuation
                    }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the loop attenuation
        threshold (as per the hdsl2ShdslEndpointThreshLoopAttenuation
        value) has been reached/exceeded for the HDSL2/SHDSL segment
        endpoint."
   ::= { hdsl2ShdslNotifications 1 }

hdsl2ShdslSNRMarginCrossing NOTIFICATION-TYPE
    OBJECTS         {
                        hdsl2ShdslEndpointCurrSnrMgn,
                        hdsl2ShdslEndpointThreshSNRMargin
                    }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the SNR margin threshold (as
        per the hdsl2ShdslEndpointThreshSNRMargin value) has been
        reached/exceeded for the HDSL2/SHDSL segment endpoint."
   ::= { hdsl2ShdslNotifications 2 }

hdsl2ShdslPerfESThresh NOTIFICATION-TYPE
    OBJECTS         {
                        hdsl2ShdslEndpointCurr15MinES,
                        hdsl2ShdslEndpointThreshES
                    }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the errored seconds
        threshold (as per the hdsl2ShdslEndpointThreshES value)
        has been reached/exceeded for the HDSL2/SHDSL segment
        endpoint."
   ::= { hdsl2ShdslNotifications 3 }

hdsl2ShdslPerfSESThresh NOTIFICATION-TYPE
    OBJECTS         {
                        hdsl2ShdslEndpointCurr15MinSES,
                        hdsl2ShdslEndpointThreshSES
                    }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the severely errored seconds
        threshold (as per the hdsl2ShdslEndpointThreshSES value) has
        been reached/exceeded for the HDSL2/SHDSL segment endpoint."
   ::= { hdsl2ShdslNotifications 4 }

hdsl2ShdslPerfCRCanomaliesThresh NOTIFICATION-TYPE
    OBJECTS         {
                        hdsl2ShdslEndpointCurr15MinCRCanomalies,
                        hdsl2ShdslEndpointThreshCRCanomalies
                    }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the CRC anomalies threshold
        (as per the hdsl2ShdslEndpointThreshCRCanomalies value) has
        been reached/exceeded for the HDSL2/SHDSL segment endpoint."
   ::= { hdsl2ShdslNotifications 5 }

hdsl2ShdslPerfLOSWSThresh NOTIFICATION-TYPE
    OBJECTS         {
                        hdsl2ShdslEndpointCurr15MinLOSWS,
                        hdsl2ShdslEndpointThreshLOSWS
                    }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the LOSW Seconds threshold
        (as per the hdsl2ShdslEndpointThreshLOSWS value) has been
        reached/exceeded for the HDSL2/SHDSL segment endpoint."
   ::= { hdsl2ShdslNotifications 6 }

hdsl2ShdslPerfUASThresh NOTIFICATION-TYPE
    OBJECTS         {
                        hdsl2ShdslEndpointCurr15MinUAS,
                        hdsl2ShdslEndpointThreshUAS
                    }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the unavailable seconds
        threshold (as per the hdsl2ShdslEndpointThreshUAS value) has
        been reached/exceeded for the HDSL2/SHDSL segment endpoint."
   ::= { hdsl2ShdslNotifications 7 }

hdsl2ShdslSpanInvalidNumRepeaters NOTIFICATION-TYPE
    OBJECTS         { hdsl2ShdslSpanConfNumRepeaters }
    STATUS          current
    DESCRIPTION
        "This notification indicates that a mismatch has been detected
        between the number of repeater/regenerator units configured
        for an HDSL2/SHDSL line via the hdsl2ShdslSpanConfNumRepeaters
        object and the actual number of repeater/regenerator units
        discovered via the EOC."
   ::= { hdsl2ShdslNotifications 8 }

hdsl2ShdslLoopbackFailure NOTIFICATION-TYPE
    OBJECTS         { hdsl2ShdslMaintLoopbackConfig }
    STATUS          current
    DESCRIPTION
        "This notification indicates that an endpoint maintenance
        loopback command failed for an HDSL2/SHDSL segment."
   ::= { hdsl2ShdslNotifications 9 }

hdsl2ShdslpowerBackoff NOTIFICATION-TYPE
    OBJECTS         { hdsl2ShdslEndpointCurrStatus }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the bit setting for
        powerBackoff in the hdsl2ShdslEndpointCurrStatus object for
        this endpoint has changed."
   ::= { hdsl2ShdslNotifications 10 }

hdsl2ShdsldeviceFault NOTIFICATION-TYPE
    OBJECTS         { hdsl2ShdslEndpointCurrStatus }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the bit setting for
        deviceFault in the hdsl2ShdslEndpointCurrStatus object for
        this endpoint has changed."
   ::= { hdsl2ShdslNotifications 11 }

hdsl2ShdsldcContinuityFault NOTIFICATION-TYPE
    OBJECTS         { hdsl2ShdslEndpointCurrStatus }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the bit setting for
        dcContinuityFault in the hdsl2ShdslEndpointCurrStatus object
        for this endpoint has changed."
   ::= { hdsl2ShdslNotifications 12 }

hdsl2ShdslconfigInitFailure NOTIFICATION-TYPE
    OBJECTS         { hdsl2ShdslEndpointCurrStatus }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the bit setting for
        configInitFailure in the hdsl2ShdslEndpointCurrStatus object
        for this endpoint has changed."
   ::= { hdsl2ShdslNotifications 13 }

hdsl2ShdslprotocolInitFailure NOTIFICATION-TYPE
    OBJECTS         { hdsl2ShdslEndpointCurrStatus }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the bit setting for
        protocolInitFailure in the hdsl2ShdslEndpointCurrStatus
        object for this endpoint has changed."
   ::= { hdsl2ShdslNotifications 14 }

hdsl2ShdslnoNeighborPresent NOTIFICATION-TYPE
    OBJECTS         { hdsl2ShdslEndpointCurrStatus }
    STATUS          current
    DESCRIPTION
        "This notification indicates that the bit setting for
        noNeighborPresent in the hdsl2ShdslEndpointCurrStatus object
        for this endpoint has changed."
   ::= { hdsl2ShdslNotifications 15 }

hdsl2ShdslLocalPowerLoss NOTIFICATION-TYPE
    OBJECTS         { hdsl2ShdslInvVendorID }
    STATUS          current
    DESCRIPTION
        "This notification indicates impending unit failure due to
        loss of local power (last gasp)."
   ::= { hdsl2ShdslNotifications 16 }
-- conformance information

hdsl2ShdslConformance  OBJECT IDENTIFIER
    ::= { hdsl2ShdslMIB 3 }

hdsl2ShdslGroups  OBJECT IDENTIFIER
    ::= { hdsl2ShdslConformance 1 }

hdsl2ShdslCompliances  OBJECT IDENTIFIER
    ::= { hdsl2ShdslConformance 2 }


-- agent compliance statements

hdsl2ShdslLineMibCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for SNMP entities that implement
        HDSL2 and SHDSL.  The version of SHDSL supported in this
        compliance statement is g.shdsl.

        **** This compliance statement is deprecated. ****"
    MODULE          -- this module
    MANDATORY-GROUPS {
                        hdsl2ShdslSpanConfGroup,
                        hdsl2ShdslSpanStatusGroup,
                        hdsl2ShdslInventoryGroup,
                        hdsl2ShdslEndpointConfGroup,
                        hdsl2ShdslEndpointCurrGroup,
                        hdsl2Shdsl15MinIntervalGroup,
                        hdsl2Shdsl1DayIntervalGroup,
                        hdsl2ShdslMaintenanceGroup,
                        hdsl2ShdslEndpointAlarmConfGroup,
                        hdsl2ShdslNotificationGroup
                    }

    GROUP           hdsl2ShdslInventoryShdslGroup
    DESCRIPTION
        "Support for this group is only required for implementations
        supporting SHDSL lines."

    GROUP           hdsl2ShdslSpanShdslStatusGroup
    DESCRIPTION
        "Support for this group is only required for implementations
        supporting SHDSL lines."

    GROUP           hdsl2ShdslSpanConfProfileGroup
    DESCRIPTION
        "Support for this group is only required for implementations
        supporting SHDSL lines."

    OBJECT          hdsl2ShdslSpanConfWireInterface
    SYNTAX          INTEGER  {
                        twoWire(1),
                        fourWire(2)
                    }
    DESCRIPTION
        "An implementation only has to support the range as
        applicable for the original g.shdsl specification defined
        in RFC 3276."

    OBJECT          hdsl2ShdslStatusMaxAttainableLineRate
    SYNTAX          Unsigned32 (0..4112000)
    DESCRIPTION
        "An implementation only has to support the range as
        applicable for the original g.shdsl specification defined
        in RFC 3276."

    OBJECT          hdsl2ShdslStatusActualLineRate
    SYNTAX          Unsigned32 (0..4112000)
    DESCRIPTION
        "An implementation only has to support the range as
        applicable for the original g.shdsl specification defined
        in RFC 3276."

    OBJECT          hdsl2ShdslSpanConfMinLineRate
    SYNTAX          Unsigned32 (0..4112000)
    DESCRIPTION
        "An implementation only has to support the range as
        applicable for the original g.shdsl specification defined
        in RFC 3276."

    OBJECT          hdsl2ShdslSpanConfMaxLineRate
    SYNTAX          Unsigned32 (0..4112000)
    DESCRIPTION
        "An implementation only has to support the range as
        applicable for the original g.shdsl specification defined
        in RFC 3276."
    ::= { hdsl2ShdslCompliances 1 }

hdsl2GshdslbisLineMibCompliance MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for SNMP entities that implement
        HDSL2 and SHDSL.  The version of SHDSL supported in this
        compliance statement is g.shdsl.bis."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        hdsl2ShdslSpanConfGroup,
                        hdsl2ShdslSpanStatusGroup,
                        hdsl2ShdslInventoryGroup,
                        hdsl2ShdslEndpointConfGroup,
                        hdsl2ShdslEndpointCurrGroup,
                        hdsl2Shdsl15MinIntervalGroup,
                        hdsl2Shdsl1DayIntervalGroup,
                        hdsl2ShdslMaintenanceGroup,
                        hdsl2ShdslEndpointAlarmConfGroup,
                        hdsl2ShdslNotificationGroup
                    }

    GROUP           hdsl2ShdslInventoryShdslGroup
    DESCRIPTION
        "Support for this group is only required for implementations
        supporting SHDSL lines."

    GROUP           hdsl2ShdslSpanShdslStatusGroup
    DESCRIPTION
        "Support for this group is only required for implementations
        supporting SHDSL lines."

    GROUP           hdsl2ShdslSpanConfProfileGroup
    DESCRIPTION
        "Support for this group is only required for implementations
        supporting SHDSL lines."

    GROUP           hdsl2ShdslWirePairGroup
    DESCRIPTION
        "Support for this group is only required for implementations
        supporting SHDSL lines."

    GROUP           hdsl2ShdslPayloadRateGroup
    DESCRIPTION
        "Support for this group is only required for implementations
        supporting SHDSL lines."
    ::= { hdsl2ShdslCompliances 2 }

-- units of conformance

hdsl2ShdslSpanConfGroup OBJECT-GROUP
    OBJECTS         {
                        hdsl2ShdslSpanConfNumRepeaters,
                        hdsl2ShdslSpanConfProfile,
                        hdsl2ShdslSpanConfAlarmProfile
                    }
    STATUS          current
    DESCRIPTION
        "This group supports objects for configuring span-related
        parameters for HDSL2/SHDSL lines."
    ::= { hdsl2ShdslGroups 1 }

hdsl2ShdslSpanStatusGroup OBJECT-GROUP
    OBJECTS         { hdsl2ShdslStatusNumAvailRepeaters }
    STATUS          current
    DESCRIPTION
        "This group supports objects for retrieving span-related
        status for HDSL2/SHDSL lines."
    ::= { hdsl2ShdslGroups 2 }

hdsl2ShdslInventoryShdslGroup OBJECT-GROUP
    OBJECTS         { hdsl2ShdslInvTransmissionModeCapability }
    STATUS          current
    DESCRIPTION
        "This group supports objects for retrieving SHDSL-specific
        inventory information."
    ::= { hdsl2ShdslGroups 3 }

hdsl2ShdslSpanShdslStatusGroup OBJECT-GROUP
    OBJECTS         {
                        hdsl2ShdslStatusMaxAttainableLineRate,
                        hdsl2ShdslStatusActualLineRate,
                        hdsl2ShdslStatusTransmissionModeCurrent
                    }
    STATUS          current
    DESCRIPTION
        "This group supports objects for retrieving SHDSL-specific
        span-related status."
    ::= { hdsl2ShdslGroups 4 }

hdsl2ShdslInventoryGroup OBJECT-GROUP
    OBJECTS         {
                        hdsl2ShdslInvVendorID,
                        hdsl2ShdslInvVendorModelNumber,
                        hdsl2ShdslInvVendorSerialNumber,
                        hdsl2ShdslInvVendorEOCSoftwareVersion,
                        hdsl2ShdslInvStandardVersion,
                        hdsl2ShdslInvVendorListNumber,
                        hdsl2ShdslInvVendorIssueNumber,
                        hdsl2ShdslInvVendorSoftwareVersion,
                        hdsl2ShdslInvEquipmentCode,
                        hdsl2ShdslInvVendorOther
                    }
    STATUS          current
    DESCRIPTION
        "This group supports objects that provide unit inventory
        information about the units in HDSL2/SHDSL lines."
    ::= { hdsl2ShdslGroups 5 }

hdsl2ShdslEndpointConfGroup OBJECT-GROUP
    OBJECTS         { hdsl2ShdslEndpointCurrAtn }
    STATUS          current
    DESCRIPTION
        "This group supports objects for configuring parameters for
        segment endpoints in HDSL2/SHDSL lines."
    ::= { hdsl2ShdslGroups 6 }

hdsl2ShdslEndpointCurrGroup OBJECT-GROUP
    OBJECTS         {
                        hdsl2ShdslEndpointCurrAtn,
                        hdsl2ShdslEndpointCurrSnrMgn,
                        hdsl2ShdslEndpointCurrStatus,
                        hdsl2ShdslEndpointES,
                        hdsl2ShdslEndpointSES,
                        hdsl2ShdslEndpointCRCanomalies,
                        hdsl2ShdslEndpointLOSWS,
                        hdsl2ShdslEndpointUAS,
                        hdsl2ShdslEndpointCurr15MinTimeElapsed,
                        hdsl2ShdslEndpointCurr15MinES,
                        hdsl2ShdslEndpointCurr15MinSES,
                        hdsl2ShdslEndpointCurr15MinCRCanomalies,
                        hdsl2ShdslEndpointCurr15MinLOSWS,
                        hdsl2ShdslEndpointCurr15MinUAS,
                        hdsl2ShdslEndpointCurr1DayTimeElapsed,
                        hdsl2ShdslEndpointCurr1DayES,
                        hdsl2ShdslEndpointCurr1DaySES,
                        hdsl2ShdslEndpointCurr1DayCRCanomalies,
                        hdsl2ShdslEndpointCurr1DayLOSWS,
                        hdsl2ShdslEndpointCurr1DayUAS
                    }
    STATUS          current
    DESCRIPTION
        "This group supports objects that provide current status and
        performance measurements relating to segment endpoints in
        HDSL2/SHDSL lines."
    ::= { hdsl2ShdslGroups 7 }

hdsl2Shdsl15MinIntervalGroup OBJECT-GROUP
    OBJECTS         {
                        hdsl2Shdsl15MinIntervalES,
                        hdsl2Shdsl15MinIntervalSES,
                        hdsl2Shdsl15MinIntervalCRCanomalies,
                        hdsl2Shdsl15MinIntervalLOSWS,
                        hdsl2Shdsl15MinIntervalUAS
                    }
    STATUS          current
    DESCRIPTION
        "This group supports objects that maintain historic
        performance measurements relating to segment endpoints in
        HDSL2/SHDSL lines in 15-minute intervals."
    ::= { hdsl2ShdslGroups 8 }

hdsl2Shdsl1DayIntervalGroup OBJECT-GROUP
    OBJECTS         {
                        hdsl2Shdsl1DayIntervalMoniSecs,
                        hdsl2Shdsl1DayIntervalES,
                        hdsl2Shdsl1DayIntervalSES,
                        hdsl2Shdsl1DayIntervalCRCanomalies,
                        hdsl2Shdsl1DayIntervalLOSWS,
                        hdsl2Shdsl1DayIntervalUAS
                    }
    STATUS          current
    DESCRIPTION
        "This group supports objects that maintain historic
        performance measurements relating to segment endpoints in
        HDSL2/SHDSL lines in 1-day intervals."
    ::= { hdsl2ShdslGroups 9 }

hdsl2ShdslMaintenanceGroup OBJECT-GROUP
    OBJECTS         {
                        hdsl2ShdslMaintLoopbackConfig,
                        hdsl2ShdslMaintTipRingReversal,
                        hdsl2ShdslMaintPowerBackOff,
                        hdsl2ShdslMaintSoftRestart,
                        hdsl2ShdslMaintLoopbackTimeout,
                        hdsl2ShdslMaintUnitPowerSource
                    }
    STATUS          current
    DESCRIPTION
        "This group supports objects that provide support for
        maintenance actions for HDSL2/SHDSL lines."
    ::= { hdsl2ShdslGroups 10 }

hdsl2ShdslEndpointAlarmConfGroup OBJECT-GROUP
    OBJECTS         {
                        hdsl2ShdslEndpointAlarmConfProfile,
                        hdsl2ShdslEndpointThreshLoopAttenuation,
                        hdsl2ShdslEndpointThreshSNRMargin,
                        hdsl2ShdslEndpointThreshES,
                        hdsl2ShdslEndpointThreshSES,
                        hdsl2ShdslEndpointThreshCRCanomalies,
                        hdsl2ShdslEndpointThreshLOSWS,
                        hdsl2ShdslEndpointThreshUAS,
                        hdsl2ShdslEndpointAlarmConfProfileRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "This group supports objects that allow configuration of alarm
        thresholds for various performance parameters for HDSL2/SHDSL
        lines."
    ::= { hdsl2ShdslGroups 11 }

hdsl2ShdslNotificationGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        hdsl2ShdslLoopAttenCrossing,
                        hdsl2ShdslSNRMarginCrossing,
                        hdsl2ShdslPerfESThresh,
                        hdsl2ShdslPerfSESThresh,
                        hdsl2ShdslPerfCRCanomaliesThresh,
                        hdsl2ShdslPerfLOSWSThresh,
                        hdsl2ShdslPerfUASThresh,
                        hdsl2ShdslSpanInvalidNumRepeaters,
                        hdsl2ShdslLoopbackFailure,
                        hdsl2ShdslpowerBackoff,
                        hdsl2ShdsldeviceFault,
                        hdsl2ShdsldcContinuityFault,
                        hdsl2ShdslconfigInitFailure,
                        hdsl2ShdslprotocolInitFailure,
                        hdsl2ShdslnoNeighborPresent,
                        hdsl2ShdslLocalPowerLoss
                    }
    STATUS          current
    DESCRIPTION
        "This group supports notifications of significant conditions
        associated with HDSL2/SHDSL lines."
    ::= { hdsl2ShdslGroups 12 }

hdsl2ShdslSpanConfProfileGroup OBJECT-GROUP
    OBJECTS         {
                        hdsl2ShdslSpanConfWireInterface,
                        hdsl2ShdslSpanConfMinLineRate,
                        hdsl2ShdslSpanConfMaxLineRate,
                        hdsl2ShdslSpanConfPSD,
                        hdsl2ShdslSpanConfTransmissionMode,
                        hdsl2ShdslSpanConfRemoteEnabled,
                        hdsl2ShdslSpanConfPowerFeeding,
                        hdsl2ShdslSpanConfCurrCondTargetMarginDown,
                        hdsl2ShdslSpanConfWorstCaseTargetMarginDown,
                        hdsl2ShdslSpanConfCurrCondTargetMarginUp,
                        hdsl2ShdslSpanConfWorstCaseTargetMarginUp,
                        hdsl2ShdslSpanConfUsedTargetMargins,
                        hdsl2ShdslSpanConfReferenceClock,
                        hdsl2ShdslSpanConfLineProbeEnable,
                        hdsl2ShdslSpanConfProfileRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "This group supports objects that constitute configuration
        profiles for configuring span-related parameters in SHDSL
        lines."
    ::= { hdsl2ShdslGroups 13 }

hdsl2ShdslWirePairGroup OBJECT-GROUP
    OBJECTS         {
                        hdsl2ShdslEndpointCurrTipRingReversal,
                        hdsl2ShdslEndpointCurrActivationState
                    }
    STATUS          current
    DESCRIPTION
        "This group supports objects that provide the status
        of SHDSL-specific wire pairs."
    ::= { hdsl2ShdslGroups 14 }

hdsl2ShdslPayloadRateGroup OBJECT-GROUP
    OBJECTS         {
                        hdsl2ShdslStatusMaxAttainablePayloadRate,
                        hdsl2ShdslStatusActualPayloadRate
                    }
    STATUS          current
    DESCRIPTION
        "This group supports objects for retrieving payload rates
        that exclude any framing overhead."
    ::= { hdsl2ShdslGroups 15 }

END


