-- *****************************************************************
-- CISCO-EIGRP-MIB.my:  Cisco Enterprise EIGRP MIB file
--   
-- November 2004, Wayne Bond
--   
-- Copyright (c) 2004, 2011 by cisco Systems Inc.
-- All rights reserved.
--   
-- *****************************************************************

CISCO-EIGRP-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
    Unsigned32,
    Gauge32,
    Counter32,
    Counter64
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    TruthValue,
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    InterfaceIndexOrZero,
    ifIndex
        FROM IF-MIB
    InetAddressType,
    InetAddress,
    InetAddressPrefixLength
        FROM INET-ADDRESS-MIB
    ciscoMgmt
        FROM CISCO-SMI;


ciscoEigrpMIB MODULE-IDENTITY
    LAST-UPDATED    "201111240000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
                    San Jose, CA  95134
                    USA

            Tel: +1 800 553-NETS

            E-mail: cs-eigrp@cisco.com"
    DESCRIPTION
        "Enhanced Interior Gateway Protocol (EIGRP) is a Cisco
        proprietary distance vector routing protocol.   It is based on
        the Diffusing Update Algorithm (DUAL), which is a method of
        finding loop-free paths through a network.   Directly
        connected routers running EIGRP form neighbor adjacencies in
        order to propagate best-path and alternate-path routing
        information for configured and learned routes.

        The tables defined within the MIB are closely aligned with how
        the router command-line interface for EIGRP displays
        information on EIGRP configurations, i.e., the topology table
        contains objects associated with the EIGRP topology commands,
        and the peer table contains objects associated withe EIGRP
        neighbor commands, etc.

        There are five main tables within this mib:

           EIGRP VPN table
              Contains information regarding which virtual private
              networks (VPN) are configured with EIGRP.

           EIGRP traffic statistics table
              Contains counter & statistcs regarding specific types of
              EIGRP packets sent and related collective information
              per VPN and per autonomous system (AS).

           EIGRP topology table
              Contains information regarding EIGRP routes received in
              updates and originated locally.   EIGRP sends and
              receives routing updates from adjacent routers running
              EIGRP with which it formed a peer relationship.

           EIGRP peer (neighbor) table
              Contains information about neighbor EIGRP routers with
              which peer adjacencies have been established.   EIGRP
              uses a Hello protocol to form neighbor relationships
              with directly connected routers also running EIGRP.

           EIGRP interfaces table
              Contains information and statistics on each of the 
              configured to run.

        RIB-scale 
        ========== 
        The Wide-Metrics feature calculates all metrics in 64-bit 
        under named mode EIGRP. Since the RIB can only hold 32-bit, 
        we divide the wide metrics by RIB-scale (range 1-255, 
        default value 128) to convert it to a 32-bit value 
        before assiging it to RIB metrics."
    REVISION        "201111240000Z"
    DESCRIPTION
        "Added new notification cEigrpNbrDownEvent.

        Added the following new objects to cEigrpTopoEntry:
        cEigrpFdistanceWide, cEigrpDistanceWide and
        cEigrpReportDistanceWide.

        Added the following new groups:
        cEigrpNotificationGroupSupR01 and cEigrpTopoDataGroupSupR01.

        Added new compliance cEigrpMIBComplianceRev1, which deprecates
        cEigrpMIBCompliance."
    REVISION        "200411160000Z"
    DESCRIPTION
        "Initial version of the MIB module."
    ::= { ciscoMgmt 449 }



-- Textual Conventions

EigrpUpTimeString ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "8a"
    STATUS          current
    DESCRIPTION
        "Specifies a timer value in days, hours, minutes,
        and seconds in ASCII format.

        If the up time is less than 24 hours, the number
        of days will not be reflected and the string will
        be formatted like this: 'hh:mm:ss', reflecting
        hours, minutes, and seconds.

        If the up time is greater than 24 hours, EIGRP is
        less precise and the minutes and seconds are not
        reflected.  Instead only the days and hours are shown
        and the string will be formatted like this: 'xxxdxxh'."
    SYNTAX          OCTET STRING (SIZE (0..8))

EigrpVersionString ::= TEXTUAL-CONVENTION
    DISPLAY-HINT    "1d.1d/1d.1d"
    STATUS          current
    DESCRIPTION
        "Specifies an ASCII string representing the IOS major
        and minor version followed by the EIGRP major and minor
        version."
    SYNTAX          OCTET STRING (SIZE (0..9))
-- Objects

cEigrpMIBNotifications  OBJECT IDENTIFIER
    ::= { ciscoEigrpMIB 0 }

cEigrpMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoEigrpMIB 1 }

cEigrpMIBConformance  OBJECT IDENTIFIER
    ::= { ciscoEigrpMIB 2 }

cEigrpVpnInfo  OBJECT IDENTIFIER
    ::= { cEigrpMIBObjects 1 }

cEigrpAsInfo  OBJECT IDENTIFIER
    ::= { cEigrpMIBObjects 2 }

cEigrpTopologyInfo  OBJECT IDENTIFIER
    ::= { cEigrpMIBObjects 3 }

cEigrpPeerInfo  OBJECT IDENTIFIER
    ::= { cEigrpMIBObjects 4 }

cEigrpInterfaceInfo  OBJECT IDENTIFIER
    ::= { cEigrpMIBObjects 5 }

-- EIGRP VPN Base Table definition

cEigrpVpnTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CEigrpVpnEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains information on those VPN's configured
        to run EIGRP.  The VPN creation on a router is independent
        of the routing protocol to be used over it.   A VPN is
        given a name and has a dedicated routing table associated
        with it.  This routing table is identified internally
        by a unique integer value."
    ::= { cEigrpVpnInfo 1 }

cEigrpVpnEntry OBJECT-TYPE
    SYNTAX          CEigrpVpnEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Information relating to a single VPN which is configured
        to run EIGRP."
    INDEX           { cEigrpVpnId } 
    ::= { cEigrpVpnTable 1 }

CEigrpVpnEntry ::= SEQUENCE {
        cEigrpVpnId   Unsigned32,
        cEigrpVpnName SnmpAdminString
}

cEigrpVpnId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The unique VPN identifier.  This is a unique integer
        relative to all other VPN's defined on the router.  It
        also identifies internally the routing table instance." 
    ::= { cEigrpVpnEntry 1 }

cEigrpVpnName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The name given to the VPN." 
    ::= { cEigrpVpnEntry 2 }
 

-- EIGRP Traffic Stats table definition

cEigrpTraffStatsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CEigrpTraffStatsEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Table of EIGRP traffic statistics and information
        associated with all EIGRP autonomous systems."
    ::= { cEigrpAsInfo 1 }

cEigrpTraffStatsEntry OBJECT-TYPE
    SYNTAX          CEigrpTraffStatsEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The set of statistics and information for a single EIGRP
        Autonomous System."
    INDEX           {
                        cEigrpVpnId,
                        cEigrpAsNumber
                    } 
    ::= { cEigrpTraffStatsTable 1 }

CEigrpTraffStatsEntry ::= SEQUENCE {
        cEigrpAsNumber        Unsigned32,
        cEigrpNbrCount        Unsigned32,
        cEigrpHellosSent      Counter32,
        cEigrpHellosRcvd      Counter32,
        cEigrpUpdatesSent     Counter32,
        cEigrpUpdatesRcvd     Counter32,
        cEigrpQueriesSent     Counter32,
        cEigrpQueriesRcvd     Counter32,
        cEigrpRepliesSent     Counter32,
        cEigrpRepliesRcvd     Counter32,
        cEigrpAcksSent        Counter32,
        cEigrpAcksRcvd        Counter32,
        cEigrpInputQHighMark  Unsigned32,
        cEigrpInputQDrops     Counter32,
        cEigrpSiaQueriesSent  Counter32,
        cEigrpSiaQueriesRcvd  Counter32,
        cEigrpAsRouterIdType  InetAddressType,
        cEigrpAsRouterId      InetAddress,
        cEigrpTopoRoutes      Counter32,
        cEigrpHeadSerial      Counter64,
        cEigrpNextSerial      Counter64,
        cEigrpXmitPendReplies Unsigned32,
        cEigrpXmitDummies     Unsigned32
}

cEigrpAsNumber OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The Autonomous System number which is unique integer
        per VPN." 
    ::= { cEigrpTraffStatsEntry 1 }

cEigrpNbrCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of live EIGRP neighbors formed on all
        interfaces whose IP addresses fall under networks configured
        in the EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 2 }

cEigrpHellosSent OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number Hello packets that have been sent to all
        EIGRP neighbors formed on all interfaces whose IP addresses
        fall under networks configured for the EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 3 }

cEigrpHellosRcvd OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number Hello packets that have been received
        from all EIGRP neighbors formed on all interfaces whose IP
        addresses fall under networks configured for the
        EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 4 }

cEigrpUpdatesSent OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number routing update packets that have been
        sent to all EIGRP neighbors formed on all interfaces whose
        IP addresses fall under networks configured for the
        EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 5 }

cEigrpUpdatesRcvd OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number routing update packets that have been
        received from all EIGRP neighbors formed on all interfaces
        whose IP addresses fall under networks configured for the
        EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 6 }

cEigrpQueriesSent OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number alternate route query packets that have
        been sent to all EIGRP neighbors formed on all interfaces
        whose IP addresses fall under networks configured for the
        EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 7 }

cEigrpQueriesRcvd OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number alternate route query packets that
        have been received from all EIGRP neighbors formed on
        all interfaces whose IP addresses fall under networks
        configured for the EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 8 }

cEigrpRepliesSent OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number query reply packets that have been sent
        to all EIGRP neighbors formed on all interfaces whose IP
        addresses fall under networks configured for the
        EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 9 }

cEigrpRepliesRcvd OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number query reply packets that have been
        received from all EIGRP neighbors formed on all interfaces
        whose IP addresses fall under networks configured for the
        EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 10 }

cEigrpAcksSent OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number packet acknowledgements that have been
        sent to all EIGRP neighbors formed on all interfaces whose
        IP addresses fall under networks configured for the
        EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 11 }

cEigrpAcksRcvd OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number packet acknowledgements that have been
        received from all EIGRP neighbors formed on all interfaces
        whose IP addresses fall under networks configured for the
        EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 12 }

cEigrpInputQHighMark OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The highest number of EIGRP packets in the input queue
        waiting to be processed internally addressed to this
        AS." 
    ::= { cEigrpTraffStatsEntry 13 }

cEigrpInputQDrops OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of EIGRP packets dropped from the input
        queue due to it being full within the AS." 
    ::= { cEigrpTraffStatsEntry 14 }

cEigrpSiaQueriesSent OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of Stuck-In-Active (SIA) query packets
        sent to all EIGRP neighbors formed on all interfaces whose
        IP addresses fall under networks configured for the
        EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 15 }

cEigrpSiaQueriesRcvd OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of Stuck-In-Active (SIA) query packets
        received from all EIGRP neighbors formed on all interfaces
        whose IP addresses fall under networks configured for the
        EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 16 }

cEigrpAsRouterIdType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The format of the router-id configured or automatically
        selected for the EIGRP AS." 
    ::= { cEigrpTraffStatsEntry 17 }

cEigrpAsRouterId OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The router-id configured or automatically selected for the
        EIGRP AS.   Each EIGRP routing process has a unique
        router-id selected from each autonomous system configured.
        The format is governed by object cEigrpAsRouterIdType." 
    ::= { cEigrpTraffStatsEntry 18 }

cEigrpTopoRoutes OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of EIGRP derived routes currently existing
        in the topology table for the AS." 
    ::= { cEigrpTraffStatsEntry 19 }

cEigrpHeadSerial OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Routes in a topology table for an AS are assigned serial
        numbers and are sequenced internally as they are inserted
        and deleted.   The serial number of the first route in
        that internal sequence is called the head serial number.
        Each AS has its own topology table, and its own serial
        number space, each of which begins with the value 1.
        A serial number of zero implies that there are no routes
        in the topology." 
    ::= { cEigrpTraffStatsEntry 20 }

cEigrpNextSerial OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The serial number that would be assigned to the next new
        or changed route in the topology table for the AS." 
    ::= { cEigrpTraffStatsEntry 21 }

cEigrpXmitPendReplies OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "When alternate route query packets are sent to adjacent
        EIGRP peers in an AS, replies are expected.   This object
        is the total number of outstanding replies expected to
        queries that have been sent to peers in the current AS.
        It remains at zero most of the time until an EIGRP route
        becomes active." 
    ::= { cEigrpTraffStatsEntry 22 }

cEigrpXmitDummies OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "A dummy is a temporary internal entity used as a place
        holder in the topology table for an AS. They are not
        transmitted in routing updates.  This is the total
        number currently in existence associated with the AS." 
    ::= { cEigrpTraffStatsEntry 23 }
 

-- EIGRP topology table definition

cEigrpTopoTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CEigrpTopoEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table of EIGRP routes and their associated
        attributes for an Autonomous System (AS) configured
        in a VPN is called a topology table.  All route entries in
        the topology table will be indexed by IP network type,
        IP network number and network mask (prefix) size."
    ::= { cEigrpTopologyInfo 1 }

cEigrpTopoEntry OBJECT-TYPE
    SYNTAX          CEigrpTopoEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The entry for a single EIGRP topology table in the given
        AS."
    INDEX           {
                        cEigrpVpnId,
                        cEigrpAsNumber,
                        cEigrpDestNetType,
                        cEigrpDestNet,
                        cEigrpDestNetPrefixLen
                    } 
    ::= { cEigrpTopoTable 1 }

CEigrpTopoEntry ::= SEQUENCE {
        cEigrpDestNetType         InetAddressType,
        cEigrpDestNet             InetAddress,
        cEigrpDestNetPrefixLen    InetAddressPrefixLength,
        cEigrpActive              TruthValue,
        cEigrpStuckInActive       TruthValue,
        cEigrpDestSuccessors      Unsigned32,
        cEigrpFdistance           Unsigned32,
        cEigrpRouteOriginType     SnmpAdminString,
        cEigrpRouteOriginAddrType InetAddressType,
        cEigrpRouteOriginAddr     InetAddress,
        cEigrpNextHopAddressType  InetAddressType,
        cEigrpNextHopAddress      InetAddress,
        cEigrpNextHopInterface    SnmpAdminString,
        cEigrpDistance            Unsigned32,
        cEigrpReportDistance      Unsigned32,
        cEigrpFdistanceWide       Counter64,
        cEigrpDistanceWide        Counter64,
        cEigrpReportDistanceWide  Counter64
}

cEigrpDestNetType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The format of the destination IP network number for
        a single route in the topology table in the AS specified
        in cEigrpDestNet." 
    ::= { cEigrpTopoEntry 1 }

cEigrpDestNet OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The destination IP network number for a single route in
        the topology table in the AS.  The format is governed
        by object cEigrpDestNetType." 
    ::= { cEigrpTopoEntry 2 }

cEigrpDestNetPrefixLen OBJECT-TYPE
    SYNTAX          InetAddressPrefixLength
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The prefix length associated with the destination IP
        network address for a single route in the topology
        table in the AS.  The format is governed by the object
        cEigrpDestNetType." 
    ::= { cEigrpTopoEntry 4 }

cEigrpActive OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "A value of true(1) indicates the route to the
        destination network has failed and an active (query)
        search for an alternative path is in progress.  A value
        of false(2) indicates the route is stable (passive)." 
    ::= { cEigrpTopoEntry 5 }

cEigrpStuckInActive OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "A value of true(1) indicates that that this route which is
        in active state (cEigrpActive = true(1)) has not received
        any replies to queries for alternate paths, and a second
        EIGRP route query, called a stuck-in-active query, has
        now been sent." 
    ::= { cEigrpTopoEntry 6 }

cEigrpDestSuccessors OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "A successor is the next routing hop for a path to the
        destination IP network number for a single route in the
        topology table in the AS.  There can be several
        potential successors if there are multiple paths to the
        destination.   This is the total number of successors for
        a topology entry." 
    ::= { cEigrpTopoEntry 7 }

cEigrpFdistance OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The feasibility (best) distance is the minimum distance
        from this router to the destination IP network in
        this topology entry.  The feasibility distance is
        used in determining the best successor for a path to the
        destination network." 
    ::= { cEigrpTopoEntry 8 }

cEigrpRouteOriginType OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This is a text string describing the internal origin
        of the EIGRP route represented by the topology entry." 
    ::= { cEigrpTopoEntry 9 }

cEigrpRouteOriginAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The format of the IP address defined as the origin of
        this topology route entry." 
    ::= { cEigrpTopoEntry 10 }

cEigrpRouteOriginAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "If the origin of the topology route entry is external
        to this router, then this object is the IP address
        of the router from which it originated.  The format 
        is governed by object cEigrpRouteOriginAddrType." 
    ::= { cEigrpTopoEntry 11 }

cEigrpNextHopAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The format of the next hop IP address for the route
        represented by the topology entry." 
    ::= { cEigrpTopoEntry 12 }

cEigrpNextHopAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This is the next hop IP address for the route represented
        by the topology entry.   The next hop is where
        network traffic will be routed to in order to reach
        the destination network for this topology entry.  The
        format is governed by cEigrpNextHopAddressType." 
    ::= { cEigrpTopoEntry 13 }

cEigrpNextHopInterface OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The interface through which the next hop IP address
        is reached to send network traffic to the destination
        network represented by the topology entry." 
    ::= { cEigrpTopoEntry 14 }

cEigrpDistance OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The computed distance to the destination network entry
        from this router." 
    ::= { cEigrpTopoEntry 15 }

cEigrpReportDistance OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The computed distance to the destination network in the
        topology entry reported to this router by the originator
        of this route." 
    ::= { cEigrpTopoEntry 16 }

cEigrpFdistanceWide OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The feasibility (best) distance is the minimum distance
        from this router to the destination IP network in
        this topology entry.  The feasibility distance is
        used in determining the best successor for a path to the
        destination network. This is the Wide Metric 64-bit value and
        not the RIB-scaled 32-bit value." 
    ::= { cEigrpTopoEntry 17 }

cEigrpDistanceWide OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The computed distance to the destination network entry
        from this router. This is the Wide Metric 64-bit value and not
        the RIB-scaled 32-bit value." 
    ::= { cEigrpTopoEntry 18 }

cEigrpReportDistanceWide OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The computed distance to the destination network in the
        topology entry reported to this router by the originator
        of this route. This is the Wide Metric 64-bit value and not the
        RIB-scaled 32-bit value." 
    ::= { cEigrpTopoEntry 19 }
 

-- EIGRP Peer table per VPN and AS (expansion table)

cEigrpPeerTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CEigrpPeerEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table of established EIGRP peers (neighbors) in the
        selected autonomous system.   Peers are indexed by their
        unique internal handle id, as well as the AS number and
        VPN id.   The peer entry is removed from the table if
        the peer is declared down."
    ::= { cEigrpPeerInfo 1 }

cEigrpPeerEntry OBJECT-TYPE
    SYNTAX          CEigrpPeerEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Statistics and operational parameters for a single peer
        in the AS."
    INDEX           {
                        cEigrpVpnId,
                        cEigrpAsNumber,
                        cEigrpHandle
                    } 
    ::= { cEigrpPeerTable 1 }

CEigrpPeerEntry ::= SEQUENCE {
        cEigrpHandle       Unsigned32,
        cEigrpPeerAddrType InetAddressType,
        cEigrpPeerAddr     InetAddress,
        cEigrpPeerIfIndex  InterfaceIndexOrZero,
        cEigrpHoldTime     Unsigned32,
        cEigrpUpTime       EigrpUpTimeString,
        cEigrpSrtt         Unsigned32,
        cEigrpRto          Unsigned32,
        cEigrpPktsEnqueued Unsigned32,
        cEigrpLastSeq      Unsigned32,
        cEigrpVersion      EigrpVersionString,
        cEigrpRetrans      Counter32,
        cEigrpRetries      Unsigned32
}

cEigrpHandle OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The unique internal identifier for the peer in the AS.
        This is a unique value among peer entries in a selected
        table." 
    ::= { cEigrpPeerEntry 1 }

cEigrpPeerAddrType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The format of the remote source IP address used by the
        peer to establish the EIGRP adjacency with this router." 
    ::= { cEigrpPeerEntry 2 }

cEigrpPeerAddr OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The source IP address used by the peer to establish the
        EIGRP adjacency with this router.  The format is
        governed by object cEigrpPeerAddrType." 
    ::= { cEigrpPeerEntry 3 }

cEigrpPeerIfIndex OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The ifIndex of the interface on this router through
        which this peer can be reached." 
    ::= { cEigrpPeerEntry 4 }

cEigrpHoldTime OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The count-down timer indicating how much time must
        pass without receiving a hello packet from this
        EIGRP peer before this router declares the peer down.
        A peer declared as down is removed from the table and
        is no longer visible." 
    ::= { cEigrpPeerEntry 5 }

cEigrpUpTime OBJECT-TYPE
    SYNTAX          EigrpUpTimeString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The elapsed time since the EIGRP adjacency was first
        established with the peer." 
    ::= { cEigrpPeerEntry 6 }

cEigrpSrtt OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The computed smooth round trip time for packets to and
        from the peer." 
    ::= { cEigrpPeerEntry 7 }

cEigrpRto OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The computed retransmission timeout for the peer.
        This value is computed over time as packets are sent to
        the peer and acknowledgements are received from it,
        and is the amount of time to wait before resending
        a packet from the retransmission queue to the peer
        when an expected acknowledgement has not been received." 
    ::= { cEigrpPeerEntry 8 }

cEigrpPktsEnqueued OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of any EIGRP packets currently enqueued
        waiting to be sent to this peer." 
    ::= { cEigrpPeerEntry 9 }

cEigrpLastSeq OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "All transmitted EIGRP packets have a sequence number
        assigned. This is the sequence number of the last EIGRP
        packet sent to this peer." 
    ::= { cEigrpPeerEntry 10 }

cEigrpVersion OBJECT-TYPE
    SYNTAX          EigrpVersionString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The EIGRP version information reported by the remote
        peer." 
    ::= { cEigrpPeerEntry 11 }

cEigrpRetrans OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The cumulative number of retransmissions to this peer
        during the period that the peer adjacency has remained
        up." 
    ::= { cEigrpPeerEntry 12 }

cEigrpRetries OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of times the current unacknowledged packet
        has been retried, i.e. resent to this peer to be
        acknowledged." 
    ::= { cEigrpPeerEntry 13 }
 

-- EIGRP Interfaces table per VPN and AS

cEigrpInterfaceTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CEigrpInterfaceEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table of interfaces over which EIGRP is running, and
        their associated statistics.   This table is independent
        of whether any peer adjacencies have been formed over
        the interfaces or not.   Interfaces running EIGRP are
        determined by whether their assigned IP addresses fall
        within configured EIGRP network statements."
    ::= { cEigrpInterfaceInfo 1 }

cEigrpInterfaceEntry OBJECT-TYPE
    SYNTAX          CEigrpInterfaceEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Information for a single interface running EIGRP in the
        AS and VPN."
    INDEX           {
                        cEigrpVpnId,
                        cEigrpAsNumber,
                        ifIndex
                    } 
    ::= { cEigrpInterfaceTable 1 }

CEigrpInterfaceEntry ::= SEQUENCE {
        cEigrpPeerCount        Gauge32,
        cEigrpXmitReliableQ    Gauge32,
        cEigrpXmitUnreliableQ  Gauge32,
        cEigrpMeanSrtt         Unsigned32,
        cEigrpPacingReliable   Unsigned32,
        cEigrpPacingUnreliable Unsigned32,
        cEigrpMFlowTimer       Unsigned32,
        cEigrpPendingRoutes    Gauge32,
        cEigrpHelloInterval    Unsigned32,
        cEigrpXmitNextSerial   Counter64,
        cEigrpUMcasts          Counter32,
        cEigrpRMcasts          Counter32,
        cEigrpUUcasts          Counter32,
        cEigrpRUcasts          Counter32,
        cEigrpMcastExcepts     Counter32,
        cEigrpCRpkts           Counter32,
        cEigrpAcksSuppressed   Counter32,
        cEigrpRetransSent      Counter32,
        cEigrpOOSrvcd          Counter32,
        cEigrpAuthMode         INTEGER,
        cEigrpAuthKeyChain     SnmpAdminString
}

cEigrpPeerCount OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of EIGRP adjacencies currently formed with
        peers reached through this interface." 
    ::= { cEigrpInterfaceEntry 3 }

cEigrpXmitReliableQ OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of EIGRP packets currently waiting in the
        reliable transport (acknowledgement-required) 
        transmission queue to be sent to a peer." 
    ::= { cEigrpInterfaceEntry 4 }

cEigrpXmitUnreliableQ OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number EIGRP of packets currently waiting in
        the unreliable transport (no acknowledgement required)
        transmission queue." 
    ::= { cEigrpInterfaceEntry 5 }

cEigrpMeanSrtt OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The average of all the computed smooth round trip time
        values for a packet to and from all peers established on
        this interface." 
    ::= { cEigrpInterfaceEntry 6 }

cEigrpPacingReliable OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The configured time interval between EIGRP packet
        transmissions on the interface when the reliable transport
        method is used." 
    ::= { cEigrpInterfaceEntry 7 }

cEigrpPacingUnreliable OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The configured time interval between EIGRP packet
        transmissions on the interface when the unreliable
        transport method is used." 
    ::= { cEigrpInterfaceEntry 8 }

cEigrpMFlowTimer OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "milliseconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The configured multicast flow control timer value for
        this interface." 
    ::= { cEigrpInterfaceEntry 9 }

cEigrpPendingRoutes OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The number of queued EIGRP routing updates awaiting
        transmission on this interface." 
    ::= { cEigrpInterfaceEntry 10 }

cEigrpHelloInterval OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The configured time interval between Hello packet
        transmissions for this interface." 
    ::= { cEigrpInterfaceEntry 11 }

cEigrpXmitNextSerial OBJECT-TYPE
    SYNTAX          Counter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The serial number of the next EIGRP packet that is to
        be queued for transmission on this interface." 
    ::= { cEigrpInterfaceEntry 12 }

cEigrpUMcasts OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of unreliable (no acknowledgement
        required) EIGRP multicast packets sent on this
        interface." 
    ::= { cEigrpInterfaceEntry 13 }

cEigrpRMcasts OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of reliable (acknowledgement required)
        EIGRP multicast packets sent on this interface." 
    ::= { cEigrpInterfaceEntry 14 }

cEigrpUUcasts OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of unreliable (no acknowledgement
        required) EIGRP unicast packets sent on this
        interface." 
    ::= { cEigrpInterfaceEntry 15 }

cEigrpRUcasts OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of reliable (acknowledgement required)
        unicast packets sent on this interface." 
    ::= { cEigrpInterfaceEntry 16 }

cEigrpMcastExcepts OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of EIGRP multicast exception
        transmissions that have occurred on this interface." 
    ::= { cEigrpInterfaceEntry 17 }

cEigrpCRpkts OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number EIGRP Conditional-Receive packets sent on
        this interface." 
    ::= { cEigrpInterfaceEntry 18 }

cEigrpAcksSuppressed OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of individual EIGRP acknowledgement
        packets that have been suppressed and combined in
        an already enqueued outbound reliable packet on this
        interface." 
    ::= { cEigrpInterfaceEntry 19 }

cEigrpRetransSent OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number EIGRP packet retransmissions sent on
        the interface." 
    ::= { cEigrpInterfaceEntry 20 }

cEigrpOOSrvcd OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The total number of out-of-sequence EIGRP packets
        received." 
    ::= { cEigrpInterfaceEntry 21 }

cEigrpAuthMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        none(1),
                        md5(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The EIGRP authentication mode of the interface.
        none  :  no authentication enabled on the interface
        md5   :  MD5 authentication enabled on the interface" 
    ::= { cEigrpInterfaceEntry 22 }

cEigrpAuthKeyChain OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The name of the authentication key-chain configured
        on this interface.   The key-chain is a reference to
        which set of secret keys are to be accessed in order
        to determine which secret key string to use.  The key
        chain name is not the secret key string password and
        can also be used in other routing protocols, such
        as RIP and ISIS." 
    ::= { cEigrpInterfaceEntry 23 }
 


-- Notifications

cEigrpAuthFailureEvent NOTIFICATION-TYPE
    OBJECTS         {
                        cEigrpPeerAddrType,
                        cEigrpPeerAddr
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent when EIGRP MD5 authentication
        is enabled on any interface and peer adjacencies are
        formed, and any adjacencies go down as a result of an
        authentication failure."
   ::= { cEigrpMIBNotifications 1 }

cEigrpRouteStuckInActive NOTIFICATION-TYPE
    OBJECTS         {
                        cEigrpPeerAddrType,
                        cEigrpPeerAddr,
                        cEigrpStuckInActive
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent when a route in the topology
        table is stuck in an active state.  During the query
        phase for a new route to a destination network, a route
        is described as being in the active state if when an
        alternate path is actively being sought, no replies are
        received to normal queries or stuck-in-active queries."
   ::= { cEigrpMIBNotifications 2 }

cEigrpNbrDownEvent NOTIFICATION-TYPE
    OBJECTS         {
                        cEigrpPeerAddrType,
                        cEigrpPeerAddr
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent when any EIGRP peer adjacency goes
        down."
   ::= { cEigrpMIBNotifications 3 }
-- Conformance

cEigrpMIBCompliances  OBJECT IDENTIFIER
    ::= { cEigrpMIBConformance 1 }

cEigrpMIBGroups  OBJECT IDENTIFIER
    ::= { cEigrpMIBConformance 2 }


-- Compliance

cEigrpMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which implement
        the Cisco EIGRP Management MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cEigrpVpnDataGroup,
                        cEigrpTrafficStatsGroup,
                        cEigrpInterfaceDataGroup,
                        cEigrpPeerDataGroup,
                        cEigrpTopoDataGroup,
                        cEigrpNotificationsGroup
                    }

    OBJECT          cEigrpAsRouterIdType
    SYNTAX          INTEGER  {
                        ipv4(1)
                    }
    DESCRIPTION
        "An implementation is only required to support
        IPv4 address type."

    OBJECT          cEigrpRouteOriginAddrType
    SYNTAX          INTEGER  {
                        ipv4(1)
                    }
    DESCRIPTION
        "An implementation is only required to support
        IPv4 address type."

    OBJECT          cEigrpNextHopAddressType
    SYNTAX          INTEGER  {
                        ipv4(1)
                    }
    DESCRIPTION
        "An implementation is only required to support
        IPv4 address type."

    OBJECT          cEigrpPeerAddrType
    SYNTAX          INTEGER  {
                        ipv4(1)
                    }
    DESCRIPTION
        "An implementation is only required to support
        IPv4 address type."
    ::= { cEigrpMIBCompliances 1 }

cEigrpMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The Revison1 compliance statement for entities which 
        implement the Cisco EIGRP Management MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cEigrpVpnDataGroup,
                        cEigrpTrafficStatsGroup,
                        cEigrpInterfaceDataGroup,
                        cEigrpPeerDataGroup,
                        cEigrpTopoDataGroup,
                        cEigrpNotificationsGroup,
                        cEigrpNotificationsGroupSupR01,
                        cEigrpTopoDataGroupSupR01
                    }
    ::= { cEigrpMIBCompliances 2 }

-- Units of Conformance

cEigrpVpnDataGroup OBJECT-GROUP
    OBJECTS         { cEigrpVpnName }
    STATUS          current
    DESCRIPTION
        "The collection of VPN names which have been configured
        with one or more EIGRP autonmous systems."
    ::= { cEigrpMIBGroups 1 }

cEigrpTrafficStatsGroup OBJECT-GROUP
    OBJECTS         {
                        cEigrpHellosSent,
                        cEigrpHellosRcvd,
                        cEigrpUpdatesSent,
                        cEigrpUpdatesRcvd,
                        cEigrpQueriesSent,
                        cEigrpQueriesRcvd,
                        cEigrpRepliesSent,
                        cEigrpRepliesRcvd,
                        cEigrpAcksSent,
                        cEigrpAcksRcvd,
                        cEigrpInputQHighMark,
                        cEigrpInputQDrops,
                        cEigrpSiaQueriesSent,
                        cEigrpSiaQueriesRcvd
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing management information
        regarding collective EIGRP packet statistics for all EIGRP
        autonomous systems configured."
    ::= { cEigrpMIBGroups 2 }

cEigrpInterfaceDataGroup OBJECT-GROUP
    OBJECTS         {
                        cEigrpPeerCount,
                        cEigrpXmitReliableQ,
                        cEigrpXmitUnreliableQ,
                        cEigrpMeanSrtt,
                        cEigrpPacingReliable,
                        cEigrpPacingUnreliable,
                        cEigrpMFlowTimer,
                        cEigrpPendingRoutes,
                        cEigrpHelloInterval,
                        cEigrpXmitNextSerial,
                        cEigrpUMcasts,
                        cEigrpRMcasts,
                        cEigrpUUcasts,
                        cEigrpRUcasts,
                        cEigrpMcastExcepts,
                        cEigrpCRpkts,
                        cEigrpAcksSuppressed,
                        cEigrpRetransSent,
                        cEigrpOOSrvcd,
                        cEigrpAuthMode,
                        cEigrpAuthKeyChain
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing management information
        for interfaces over which EIGRP is configured and
        running."
    ::= { cEigrpMIBGroups 3 }

cEigrpPeerDataGroup OBJECT-GROUP
    OBJECTS         {
                        cEigrpNbrCount,
                        cEigrpPeerAddrType,
                        cEigrpPeerAddr,
                        cEigrpPeerIfIndex,
                        cEigrpHoldTime,
                        cEigrpUpTime,
                        cEigrpSrtt,
                        cEigrpRto,
                        cEigrpPktsEnqueued,
                        cEigrpLastSeq,
                        cEigrpVersion,
                        cEigrpRetrans,
                        cEigrpRetries
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing management information
        for EIGRP peer adjacencies formed in the EIGRP
        autonoumous systems."
    ::= { cEigrpMIBGroups 4 }

cEigrpTopoDataGroup OBJECT-GROUP
    OBJECTS         {
                        cEigrpAsRouterId,
                        cEigrpAsRouterIdType,
                        cEigrpTopoRoutes,
                        cEigrpHeadSerial,
                        cEigrpNextSerial,
                        cEigrpXmitPendReplies,
                        cEigrpXmitDummies,
                        cEigrpActive,
                        cEigrpStuckInActive,
                        cEigrpDestSuccessors,
                        cEigrpFdistance,
                        cEigrpRouteOriginType,
                        cEigrpRouteOriginAddrType,
                        cEigrpRouteOriginAddr,
                        cEigrpNextHopAddressType,
                        cEigrpNextHopAddress,
                        cEigrpNextHopInterface,
                        cEigrpDistance,
                        cEigrpReportDistance
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing management information
        for EIGRP topology routes derived within autonomous
        systems and received in updates from EIGRP neighbors."
    ::= { cEigrpMIBGroups 5 }

cEigrpNotificationsGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        cEigrpAuthFailureEvent,
                        cEigrpRouteStuckInActive
                    }
    STATUS          current
    DESCRIPTION
        "Group of notifications on EIGRP routers."
    ::= { cEigrpMIBGroups 6 }

cEigrpNotificationsGroupSupR01 NOTIFICATION-GROUP
   NOTIFICATIONS    { cEigrpNbrDownEvent }
    STATUS          current
    DESCRIPTION
        "Additional Notifications that supplement
        cEigrpNotificationsGroup."
    ::= { cEigrpMIBGroups 7 }

cEigrpTopoDataGroupSupR01 OBJECT-GROUP
    OBJECTS         {
                        cEigrpFdistanceWide,
                        cEigrpDistanceWide,
                        cEigrpReportDistanceWide
                    }
    STATUS          current
    DESCRIPTION
        "Collection of objects providing wide metric management
        information for EIGRP topology routes that supplement the
        cEIGRPTopoDataGroup."
    ::= { cEigrpMIBGroups 8 }

END




























