-- *****************************************************************
-- CISCO-VOICE-COMMON-DIAL-CONTROL-MIB.my:
-- Voice Common Dial Control MIB file
--   
-- June 1999, Chris White
--   
-- Copyright (c) 1999, 2001, 2003, 2005-2010 by cisco Systems Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-VOICE-COMMON-DIAL-CONTROL-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Unsigned32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    TruthValue,
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    callActiveSetupTime,
    callActiveIndex
        FROM DIAL-CONTROL-MIB
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    cCallHistoryIndex
        FROM CISCO-DIAL-CONTROL-MIB
    ciscoExperiment
        FROM CISCO-SMI;


ciscoVoiceCommonDialControlMIB MODULE-IDENTITY
    LAST-UPDATED    "201006300000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W. Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-voice@cisco.com"
    DESCRIPTION
        "This MIB module contains voice related objects that
        are common across more than one network
        encapsulation i.e VoIP, VoATM and VoFR.

        *** ABBREVIATIONS, ACRONYMS AND SYMBOLS ***

        GSM    - Global System for Mobile Communication

        AMR-NB - Adaptive Multi Rate - Narrow Band

        iLBC   - internet Low Bitrate Codec

        iSAC   - internet Speech Audio Codec"
    REVISION        "201006300000Z"
    DESCRIPTION
        "Added CvcCallReferenceIdOrZero textual convention.
        Added aaclc and aacld enum to CvcCoderTypeRate and
        CvcSpeechCoderRate textual conventions."
    REVISION        "200903180000Z"
    DESCRIPTION
        "[1] Added acronym for iSAC codec
        [2] Added iSAC enum to CvcSpeechCoderRate and CvcCoderTypeRate  
            textual conventions."
    REVISION        "200807020000Z"
    DESCRIPTION
        "[1] Added '-- obsolete' to description of 'g722'
        enum from CvcCoderTypeRate.
        [2] Added new enum values 'g722r4800', 'g722r5600'
        and 'g722r6400' to CvcCoderTypeRate.
        [3] Added new enum values 'g722r4800', 'g722r5600'
        and 'g722r6400' to CvcSpeechCoderRate."
    REVISION        "200706260000Z"
    DESCRIPTION
        "[1] Imported TEXTUAL-CONVENTION from SNMPv2-TC.
        [2] Added acronyms for GSM AMR-NB and iLBC codecs
        [3] Added llcc, gsmAmrNb, iLBC, iLBCr15200 and iLBCr13330
            enums to CvcSpeechCoderRate textual conventions.
        [4] Added llcc, gsmAmrNb, g722, iLBC, iLBCr15200 and iLBCr13330 
            enums to CvcCoderTypeRate textual conventions.
        [5] Added REFERENCE clause to CvcSpeechCoderRate and
            CvcCoderTypeRate textual conventions for GSM AMR-NB and
            iLBC codecs."
    REVISION        "200508160000Z"
    DESCRIPTION
        "Added CvcH320CallType and CvcVideoCoderRate objects.
        Added g722 enum to CvcCoderTypeRate textual conventions."
    REVISION        "200503060000Z"
    DESCRIPTION
        "Added gsmAmrNb enum to CvcSpeechCoderRate and CvcCoderTypeRate
        textual conventions."
    REVISION        "200303110000Z"
    DESCRIPTION
        "Added new enum value 'llcc', to CvcSpeechCoderRate
        and CvcCoderTypeRate textual-conventions."
    REVISION        "200110060000Z"
    DESCRIPTION
        "[1] Added new enum value 'g726r40000',to CvcSpeechCoderRate's
        and CvcCoderTypeRate's textual-conventions.
        [2] Replaced 'clearch' enum with 'clearChannel' enum.
        [3] Replaced 'codec is disabled' comment for clearChannel enum
        with 'CLEAR channel codec'."
    REVISION        "200109050000Z"
    DESCRIPTION
        "[1] Added new enum value, 'clearch,' to CvcSpeechCoderRate's
        and CvcCoderTypeRate's textual-conventions. 
        [2] Added new enum value, 'gr303,' to CvcInBandSignaling's
        textual-conventions
        [3] Modified cvCommonDcCallActiveInBandSignaling's and
        cvCommonDcCallHistoryInBandSignaling's description
        to indicate value is valid only for Connection Trunk calls."
    REVISION        "200007220000Z"
    DESCRIPTION
        "Add new objects for handling the following features:
        [1] Calling Name display for call active and history table.
        [2] Caller ID Block, which indicates whether the Caller ID
            feature is in using,  for call active and history table."
    ::= { ciscoExperiment 55 }


-- Voice Common Dial Control MIB objects definitions

cvCommonDcMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoVoiceCommonDialControlMIB 1 }

-- The Voice Common Dial Control MIB consists of the following groups
-- [1] Voice Common Call Active Group (cvCommonDcCallActive)
-- [2] Voice Common Call History Group (cvCommonDcCallHistory)

cvCommonDcCallActive  OBJECT IDENTIFIER
    ::= { cvCommonDcMIBObjects 1 }

cvCommonDcCallHistory  OBJECT IDENTIFIER
    ::= { cvCommonDcMIBObjects 2 }


-- Textual Conventions
--   

--   

-- Speech Coder Rate Textual Conventions

CvcSpeechCoderRate ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This object specifies the most desirable codec of
        speech for the VoIP, VoATM or VoFR peer.
        g729r8000      - pre-IETF G.729 8000  bps
        g729Ar8000     - G.729 ANNEX-A 8000  bps
        g726r16000     - G.726 16000 bps
        g726r24000     - G.726 24000 bps
        g726r32000     - G.726 32000 bps
        g711ulawr64000 - G.711 u-Law 64000 bps
        g711Alawr64000 - G.711 A-Law 64000 bps
        g728r16000     - G.728 16000 bps
        g723r6300      - G.723.1 6300 bps
        g723r5300      - G.723.1 5300 bps
        gsmr13200      - GSM Full rate 13200 bps
        g729Br8000     - G.729 ANNEX-B 8000  bps
        g729ABr8000    - G.729 ANNEX-A & B 8000 bps
        g723Ar6300     - G723.1 Annex A 6300 bps              
        g723Ar5300     - G723.1 Annex A 5300 bps               
        g729IETFr8000  - IETF G.729 8000  bps
        gsmeEr12200    - GSM Enhanced Full Rate 12200 bps
        clearChannel   - CLEAR Channel codec
        g726r40000     - G.726 40000 bps
        llcc           - Lossless compression codec
        gsmAmrNb       - GSM AMR-NB 4750 - 12200 bps
        iLBC           - iILBC 13330 or 15200 bps
        iLBCr15200     - iLBC 15200 bps
        iLBCr13330     - iLBC 13330 bps
        g722r4800      - G.722 (modes 1, 2, 3)
        g722r5600      - G.722 (modes 1, 2)
        g722r6400      - G.722 (mode 1)
        iSAC           - iSAC (10 to 32 kbps)
        aaclc          - AAC-LC Advanced Audio Coding Low Complexity
        aacld          - AAC-LD MPEG-4 Low Delay Audio Coder"

    REFERENCE
        "[1] RFC 3267: For introduction about GSM AMR-NB codec,
         section 3.1
             [2] RFC 3952: For introduction about iLBC codec,
         section 2"
    SYNTAX          INTEGER  {
                        g729r8000(1),
                        g729Ar8000(2),
                        g726r16000(3),
                        g726r24000(4),
                        g726r32000(5),
                        g711ulawr64000(6),
                        g711Alawr64000(7),
                        g728r16000(8),
                        g723r6300(9),
                        g723r5300(10),
                        gsmr13200(11),
                        g729Br8000(12),
                        g729ABr8000(13),
                        g723Ar6300(14),
                        g723Ar5300(15),
                        g729IETFr8000(16),
                        gsmeEr12200(17),
                        clearChannel(18),
                        g726r40000(19),
                        llcc(20),
                        gsmAmrNb(21),
                        iLBC(22),
                        iLBCr15200(23),
                        iLBCr13330(24),
                        g722r4800(25),
                        g722r5600(26),
                        g722r6400(27),
                        iSAC(28),
                        aaclc(29),
                        aacld(30)
                    }

-- Fax Transmit Rate Textual Convention

CvcFaxTransmitRate ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This object specifies the default transmit rate of FAX
        for the VoIP, VoATM or VOFR peer. If the value of this
        object is 'none', then the Fax relay feature is disabled         
        ; otherwise the Fax relay feature is enabled.

        none      - Fax relay is disabled.
        voiceRate - the fastest possible fax rate not exceed
                    the configured voice rate.
        fax2400   - 2400  bps FAX transmit rate.
        fax4800   - 4800  bps FAX transmit rate.
        fax7200   - 7200  bps FAX transmit rate.
        fax9600   - 9600  bps FAX transmit rate.
        fax14400  - 14400 bps FAX transmit rate.
        fax12000  - 12000 bps FAX transmit rate."
    SYNTAX          INTEGER  {
                        none(1),
                        voiceRate(2),
                        fax2400(3),
                        fax4800(4),
                        fax7200(5),
                        fax9600(6),
                        fax14400(7),
                        fax12000(8)
                    }

-- Voice/FAX Call Coder Type-Rate textual convention

CvcCoderTypeRate ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents the coder type-rate for voice/fax compression
        used during a call.

        *** ABBREVIATIONS, ACRONYMS AND SYMBOLS ***

        GSM    - Global System for Mobile Communication

        AMR-NB - Adaptive Multi Rate - Narrow Band

        iLBC   - internet Low Bitrate Codec

        iSAC   - internet Speech Audio Codec

        other          - none of the following.
        fax2400        - FAX   2400  bps 
        fax4800        - FAX   4800  bps 
        fax7200        - FAX   7200  bps 
        fax9600        - FAX   9600  bps
        fax14400       - FAX   14400 bps  
        fax12000       - FAX   12000 bps  
        g729r8000      - G.729 8000  bps (pre-IETF bit ordering)
        g729Ar8000     - G.729 ANNEX-A 8000  bps
        g726r16000     - G.726 16000 bps
        g726r24000     - G.726 24000 bps
        g726r32000     - G.726 32000 bps
        g711ulawr64000 - G.711 u-Law 64000 bps
        g711Alawr64000 - G.711 A-Law 64000 bps
        g728r16000     - G.728 16000 bps
        g723r6300      - G.723.1 6300 bps
        g723r5300      - G.723.1 5300 bps
        gsmr13200      - GSM full rate 13200 bps
        g729Br8000     - G.729 ANNEX-B 8000  bps
        g729ABr8000    - G.729 ANNEX-A & B 8000 bps
        g723Ar6300     - G723.1 Annex A 6300 bps              
        g723Ar5300     - G723.1 Annex A 5300 bps               
        ietfg729r8000  - G.729 8000 bps (IETF bit ordering)
        gsmeEr12200    - GSM Enhanced Full Rate 12200 bps
        clearChannel   - CLEAR channel codec
        g726r40000     - G.726 40000 bps 
        llcc           - Lossless compression codec
        gsmAmrNb       - GSM AMR-NB 4750 - 12200 bps
        g722           - G.722 2400 - 6400 bps
        iLBC           - iILBC 13330 or 15200 bps
        iLBCr15200     - iLBC 15200 bps
        iLBCr13330     - iLBC 13330 bps
        g722r4800      - G.722 (modes 1, 2, 3)
        g722r5600      - G.722 (modes 1, 2)
        g722r6400      - G.722 (mode 1)
        iSAC           - iSAC (10 to 32 kbps)
        aaclc          - AAC-LC Advanced Audio Coding Low Complexity
        aacld          - AAC-LD MPEG-4 Low Delay Audio Coder"

    REFERENCE
        "[1] RFC 3267: For introduction about GSM AMR-NB codec,
         section 3.1
             [2] RFC 3952: For introduction about iLBC codec,
         section 2"
    SYNTAX          INTEGER  {
                        other(1),
                        fax2400(2),
                        fax4800(3),
                        fax7200(4),
                        fax9600(5),
                        fax14400(6),
                        fax12000(7),
                        g729r8000(10),
                        g729Ar8000(11),
                        g726r16000(12),
                        g726r24000(13),
                        g726r32000(14),
                        g711ulawr64000(15),
                        g711Alawr64000(16),
                        g728r16000(17),
                        g723r6300(18),
                        g723r5300(19),
                        gsmr13200(20),
                        g729Br8000(21),
                        g729ABr8000(22),
                        g723Ar6300(23),
                        g723Ar5300(24),
                        ietfg729r8000(25),
                        gsmeEr12200(26),
                        clearChannel(27),
                        g726r40000(28),
                        llcc(29),
                        gsmAmrNb(30),
                        g722(31),
                        iLBC(32),
                        iLBCr15200(33),
                        iLBCr13330(34),
                        g722r4800(35),
                        g722r5600(36),
                        g722r6400(37),
                        iSAC(38),
                        aaclc(39),
                        aacld(40)
                    }

-- Global Call Identifier textual convention

CvcGUid ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents a Global Call Identifier.
        The global call identifier is used as an unique identifier
        for an end-to-end call.
        A zero length CvcGUid indicates no value for the global call
        identifier."
    SYNTAX          OCTET STRING (SIZE (0..16))

-- InBand Signaling textual conventions

CvcInBandSignaling ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Represents the type of in-band signaling used between
        the two end points of the call and is used to inform the
        router how interpret the ABCD signaling data bits passed
        as part of the voice payload data.

        cas         - specifies interpret the signaling bits as
                      North American Channel Associated signaling.        
        none        - specifies no in-band signaling or signaling
                      is being done via an external method (e.g
                      CCS).
        cept        - specifies interpret the signaling bits as
                      MELCAS
        transparent - specifies do not interpret or translate the
                      signaling bits.
        gr303       - specifies interpret the signaling bits as
                      GR303"
    SYNTAX          INTEGER  {
                        cas(1),
                        none(2),
                        cept(3),
                        transparent(4),
                        gr303(5)
                    }

-- Call Reference Identifier textual convention

CvcCallReferenceIdOrZero ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "A call reference ID correlates the video and audio call entries
        that belong to the same endpoint.  In other words, if an audio
        call entry and a video call entry have the same call reference
        ID, these entries belong to the same endpoint.  
        Because an audio-only endpoint creates only one call entry, call
        reference ID is not necessary and is set to zero.
        A call reference ID with value greater than zero signifies a
        video call, the value zero is object-specific and must therefore
        be defined as part of the description of any object which uses
        this syntax.  Examples of the usage of zero include audio calls."
    SYNTAX          Unsigned32

-- Voice Call H.320 Call Type textual convention

CvcH320CallType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This object specifies the H320 call type of a voice call."
    SYNTAX          INTEGER  {
                        none(0), -- none of the following
                        primary(1), -- h320 primary call
                        secondary(2) -- h320 secondary call                        
                    }

-- Voice Call Coder Type-Rate textual convention

CvcVideoCoderRate ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This object specifies the encoding type used to compress
        the video data of the voice call."
    SYNTAX          INTEGER  {
                        none(0), -- none of the following
                        h261(1),
                        h263(2),
                        h263plus(3),
                        h264(4)
                    }
-- **********************************************************************
-- Voice Common Call Active Group
-- **********************************************************************
--   

-- Voice Common Call Active Table

cvCommonDcCallActiveTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CvCommonDcCallActiveEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table is a common extension to the call active
        table of IETF Dial Control MIB. It contains common call 
        leg information about a network call leg."
    ::= { cvCommonDcCallActive 1 }

cvCommonDcCallActiveEntry OBJECT-TYPE
    SYNTAX          CvCommonDcCallActiveEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The common information regarding a single network call
        leg. The call leg entry is identified by using the same 
        index objects that are used by Call Active table of IETF 
        Dial Control MIB to identify the call.
        An entry of this table is created when its associated 
        call active entry in the IETF Dial Control MIB is created
        and the call active entry contains information for the 
        call establishment to a network dialpeer.             
        The entry is deleted when its associated call active entry 
        in the IETF Dial Control MIB is deleted."
    INDEX           {
                        callActiveSetupTime,
                        callActiveIndex
                    } 
    ::= { cvCommonDcCallActiveTable 1 }

CvCommonDcCallActiveEntry ::= SEQUENCE {
        cvCommonDcCallActiveConnectionId    CvcGUid,
        cvCommonDcCallActiveVADEnable       TruthValue,
        cvCommonDcCallActiveCoderTypeRate   CvcCoderTypeRate,
        cvCommonDcCallActiveCodecBytes      INTEGER,
        cvCommonDcCallActiveInBandSignaling CvcInBandSignaling,
        cvCommonDcCallActiveCallingName     SnmpAdminString,
        cvCommonDcCallActiveCallerIDBlock   TruthValue
}

cvCommonDcCallActiveConnectionId OBJECT-TYPE
    SYNTAX          CvcGUid
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The global call identifier for the network call." 
    ::= { cvCommonDcCallActiveEntry 1 }

cvCommonDcCallActiveVADEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The object indicates whether or not the VAD (Voice
        Activity Detection) is enabled for the voice call." 
    ::= { cvCommonDcCallActiveEntry 2 }

cvCommonDcCallActiveCoderTypeRate OBJECT-TYPE
    SYNTAX          CvcCoderTypeRate
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The negotiated coder rate. It specifies the transmit
        rate of voice/fax compression to its associated call leg 
        for the call.
        This rate is different from the configuration rate 
        because of rate negotiation during the call." 
    ::= { cvCommonDcCallActiveEntry 3 }

cvCommonDcCallActiveCodecBytes OBJECT-TYPE
    SYNTAX          INTEGER (10..255)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Specifies the payload size of the voice packet." 
    ::= { cvCommonDcCallActiveEntry 4 }

cvCommonDcCallActiveInBandSignaling OBJECT-TYPE
    SYNTAX          CvcInBandSignaling
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Specifies the type of in-band signaling being used on
        the call.  This object is instantiated only for 
        Connection Trunk calls." 
    ::= { cvCommonDcCallActiveEntry 5 }

cvCommonDcCallActiveCallingName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The calling party name this call is connected to. If the
        name is not available, then it will have a length of zero." 
    ::= { cvCommonDcCallActiveEntry 6 }

cvCommonDcCallActiveCallerIDBlock OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The object indicates whether or not the caller ID feature
        is blocked for this voice call." 
    ::= { cvCommonDcCallActiveEntry 7 }
 

-- ****************************************************************************
-- Voice Common Call History Group
-- ****************************************************************************
--   

-- Voice Common Call History Table

cvCommonDcCallHistoryTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CvCommonDcCallHistoryEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table is the Common extension to the call history
        table of IETF Dial Control MIB. It contains Common call 
        leg information about a network call leg."
    ::= { cvCommonDcCallHistory 1 }

cvCommonDcCallHistoryEntry OBJECT-TYPE
    SYNTAX          CvCommonDcCallHistoryEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The common information regarding a single network call
        leg. The call leg entry is identified by using the same 
        index objects that are used by Call Active table of IETF 
        Dial Control MIB to identify the call.
        An entry of this table is created when its associated 
        call history entry in the IETF Dial Control MIB is 
        created and the call history entry contains information 
        for the call establishment to a network dialpeer.
        The entry is deleted when its associated call history 
        entry in the IETF Dial Control MIB is deleted."
    INDEX           { cCallHistoryIndex } 
    ::= { cvCommonDcCallHistoryTable 1 }

CvCommonDcCallHistoryEntry ::= SEQUENCE {
        cvCommonDcCallHistoryConnectionId    CvcGUid,
        cvCommonDcCallHistoryVADEnable       TruthValue,
        cvCommonDcCallHistoryCoderTypeRate   CvcCoderTypeRate,
        cvCommonDcCallHistoryCodecBytes      INTEGER,
        cvCommonDcCallHistoryInBandSignaling CvcInBandSignaling,
        cvCommonDcCallHistoryCallingName     SnmpAdminString,
        cvCommonDcCallHistoryCallerIDBlock   TruthValue
}

cvCommonDcCallHistoryConnectionId OBJECT-TYPE
    SYNTAX          CvcGUid
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The global call identifier for the gateway call." 
    ::= { cvCommonDcCallHistoryEntry 1 }

cvCommonDcCallHistoryVADEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The object indicates whether or not the VAD (Voice
        Activity Detection) was enabled for the voice call." 
    ::= { cvCommonDcCallHistoryEntry 2 }

cvCommonDcCallHistoryCoderTypeRate OBJECT-TYPE
    SYNTAX          CvcCoderTypeRate
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The negotiated coder rate. It specifies the transmit rate
        of voice/fax compression to its associated call leg for 
        the call.
        This rate is different from the configuration rate 
        because of rate negotiation during the call." 
    ::= { cvCommonDcCallHistoryEntry 3 }

cvCommonDcCallHistoryCodecBytes OBJECT-TYPE
    SYNTAX          INTEGER (10..255)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Specifies the payload size of the voice packet." 
    ::= { cvCommonDcCallHistoryEntry 4 }

cvCommonDcCallHistoryInBandSignaling OBJECT-TYPE
    SYNTAX          CvcInBandSignaling
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "Specifies the type of in-band signaling used on the
        call.  This object is instantiated only for 
        Connection Trunk calls." 
    ::= { cvCommonDcCallHistoryEntry 5 }

cvCommonDcCallHistoryCallingName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The calling party name this call is connected to. If
        the name is not available, then it will have a length 
        of zero." 
    ::= { cvCommonDcCallHistoryEntry 6 }

cvCommonDcCallHistoryCallerIDBlock OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The object indicates whether or not the caller ID
        feature is blocked for this voice call." 
    ::= { cvCommonDcCallHistoryEntry 7 }
 

-- **********************************************************************
-- Notifications
-- **********************************************************************

cvCommonDcMIBNotificationPrefix  OBJECT IDENTIFIER
    ::= { ciscoVoiceCommonDialControlMIB 2 }

cvCommonDcMIBNotifications  OBJECT IDENTIFIER
    ::= { cvCommonDcMIBNotificationPrefix 0 }

cvCommonDcMIBConformance  OBJECT IDENTIFIER
    ::= { ciscoVoiceCommonDialControlMIB 3 }

cvCommonDcMIBCompliances  OBJECT IDENTIFIER
    ::= { cvCommonDcMIBConformance 1 }

cvCommonDcMIBGroups  OBJECT IDENTIFIER
    ::= { cvCommonDcMIBConformance 2 }


-- **********************************************************************
-- Compliance statements
-- **********************************************************************

cvCommonDcMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which
        implement the CISCO VOICE COMMON MIB"
    MODULE          -- this module
    MANDATORY-GROUPS { cvCommonDcCallGroup }
    ::= { cvCommonDcMIBCompliances 1 }

cvCommonDcMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for entities which
        implement the CISCO VOICE COMMON MIB"
    MODULE          -- this module
    MANDATORY-GROUPS { cvCommonDcCallGroup1 }

    OBJECT          cvCommonDcCallActiveCallingName
    SYNTAX          SnmpAdminString (SIZE (0..64))
    DESCRIPTION
        "Support is required only for the subset of
        SnmpAdminString values which contain ASCII characters.  
        In effect, a minimal implementation implements this 
        object as a DisplayString."

    OBJECT          cvCommonDcCallHistoryCallingName
    SYNTAX          SnmpAdminString (SIZE (0..64))
    DESCRIPTION
        "Support is required only for the subset of
        SnmpAdminString values which contain ASCII characters.  
        In effect, a minimal implementation implements this 
        object as a DisplayString."
    ::= { cvCommonDcMIBCompliances 2 }

-- units of conformance

cvCommonDcCallGroup OBJECT-GROUP
    OBJECTS         {
                        cvCommonDcCallActiveConnectionId,
                        cvCommonDcCallActiveVADEnable,
                        cvCommonDcCallActiveCoderTypeRate,
                        cvCommonDcCallActiveCodecBytes,
                        cvCommonDcCallActiveInBandSignaling,
                        cvCommonDcCallHistoryConnectionId,
                        cvCommonDcCallHistoryVADEnable,
                        cvCommonDcCallHistoryCoderTypeRate,
                        cvCommonDcCallHistoryCodecBytes,
                        cvCommonDcCallHistoryInBandSignaling
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects providing the common network
        call leg information."
    ::= { cvCommonDcMIBGroups 1 }

cvCommonDcCallGroup1 OBJECT-GROUP
    OBJECTS         {
                        cvCommonDcCallActiveConnectionId,
                        cvCommonDcCallActiveVADEnable,
                        cvCommonDcCallActiveCoderTypeRate,
                        cvCommonDcCallActiveCodecBytes,
                        cvCommonDcCallActiveInBandSignaling,
                        cvCommonDcCallActiveCallingName,
                        cvCommonDcCallActiveCallerIDBlock,
                        cvCommonDcCallHistoryConnectionId,
                        cvCommonDcCallHistoryVADEnable,
                        cvCommonDcCallHistoryCoderTypeRate,
                        cvCommonDcCallHistoryCodecBytes,
                        cvCommonDcCallHistoryInBandSignaling,
                        cvCommonDcCallHistoryCallingName,
                        cvCommonDcCallHistoryCallerIDBlock
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing the common network
        call leg information."
    ::= { cvCommonDcMIBGroups 2 }

END










