-- *******************************************************************
-- CISCO-LWAPP-MOBILITY-MIB.my
-- June 2006, Bharat Biswal,Arun Kumar A
--   
-- Copyright (c) 2005-2019 by Cisco Systems Inc.
-- All rights reserved.
-- *******************************************************************

CISCO-LWAPP-MOBILITY-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
    Integer32,
    IpAddress,
    Unsigned32,
    Counter32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    TruthValue,
    RowStatus,
    MacAddress
        FROM SNMPv2-TC
    InetAddressType,
    InetAddress
        FROM INET-ADDRESS-MIB
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    ciscoMgmt
        FROM CISCO-SMI;


-- ********************************************************************
-- *  MODULE IDENTITY
-- ********************************************************************

ciscoLwappMobilityMIB MODULE-IDENTITY
    LAST-UPDATED    "201904250000Z"
    ORGANIZATION    "Cisco Systems Inc."
    CONTACT-INFO
            "Cisco Systems,
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            Email: cs-snmp@cisco.com"
    DESCRIPTION
        "This MIB is intended to be implemented on all those
        devices operating as Central Controllers (CC) that
        terminate the Light Weight Access Point Protocol
        tunnel from Light-weight LWAPP Access Points.

        This MIB provides configuration and status information
        about the 802.11 WLAN mobility.                 

        The relationship between CC and the LWAPP APs
        can be depicted as follows:

        +......+     +......+     +......+           +......+
        +      +     +      +     +      +           +      +
        +  CC  +     +  CC  +     +  CC  +           +  CC  +
        +      +     +      +     +      +           +      +
        +......+     +......+     +......+           +......+
        ..            .             .                 .
        ..            .             .                 .
        .  .            .             .                 .
        .    .            .             .                 .
        .      .            .             .                 .
        .        .            .             .                 .
        +......+ +......+     +......+      +......+          +......+
        +      + +      +     +      +      +      +          +      +
        +  AP  + +  AP  +     +  AP  +      +  AP  +          +  AP  +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+
         .              .             .                 .
        .  .              .             .                 .
        .    .              .             .                 .
        .      .              .             .                 .
        .        .              .             .                 .
        +......+ +......+     +......+      +......+          +......+
        +      + +      +     +      +      +      +          +      +
        +  MN  + +  MN  +     +  MN  +      +  MN  +          +  MN  +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+


        The LWAPP tunnel exists between the controller and
        the APs.  The MNs communicate with the APs through
        the protocol defined by the 802.11 standard.

        LWAPP APs, upon bootup, discover and join one of the
        controllers and the controller pushes the configuration,
        that includes the WLAN parameters, to the LWAPP APs.
        The APs then encapsulate all the 802.11 frames from
        wireless clients inside LWAPP frames and forward
        the LWAPP frames to the controller.

                          GLOSSARY

        Access Point ( AP )

        An entity that contains an 802.11 medium access
        control ( MAC ) and physical layer ( PHY ) interface
        and provides access to the distribution services via
        the wireless medium for associated clients.  

        LWAPP APs encapsulate all the 802.11 frames in
        LWAPP frames and sends it to the controller to which
        it is logically connected.

        Basic Service Set Identifier (BSSID)

        The identifier for the service set comprising of
        all the 802.11 stations under the control of
        one coordinating Access Point.  This identifier
        happens to be the MAC address of the dot11 radio
        interface of the Access Point.  The wireless
        clients that associate with the Access Point
        get the wired uplink through this particular 
        dot11 interface. 

        Central Controller ( CC )

        The central entity that terminates the LWAPP protocol
        tunnel from the LWAPP APs.  Throughout this MIB,
        this entity also referred to as 'controller'. 

        Light Weight Access Point Protocol ( LWAPP ) 

        This is a generic protocol that defines the 
        communication between the Access Points and the
        Central Controller. 

        Mobile Node ( MN )

        A roaming 802.11 wireless device in a wireless
        network associated with an access point. 

        Mobility 

        Concept by which a Mobile Node can roam from one 
        Access Point to another Access Point, across multiple
        Central Controllers, without need for repeated 
        authentication. 

        Mobility Group

        A set of Central Controllers which exchange Mobile 
        Node's authentication information, so that the Mobile
        Node upon roaming need not re-authenticate.  

        Mobility Anchor

        When a Central Controller in the Mobility Group is 
        designated as Mobility Anchor, then all the Mobile 
        Node's traffic is tunneled to it by other
        Controllers in the Mobility Group.

        Guest Tunneling (GT)

        The concept of designating a Central Controller in 
        the Mobility Group as Mobility Anchor, so that all
        the Mobile Node's traffic is tunneled to it by other
        Controllers in the Mobility Group.              

        Station Management (SMT)

        This term refers to the internal management of the
        802.11 protocol operations by the AP to work
        cooperatively with the other APs and 802.11
        devices in the network.

        Ethernet over Internet Protocol (EoIP)

        Ethernet over IP (EoIP) is a protocol that creates 
        an Ethernet tunnel between two routers on top of an
        IP connection. The EoIP interface appears as an 
        Ethernet interface.

        Reverse path filtering (RPF) 

        Reverse path filtering (RPF) is a feature provided
        by most modern Internet Protocol routers, which may
        be used to reduce the risk of customers attacking
        other internet hosts. One of the problems network
        service providers face today is hackers generating
        packets with fake source IP addresses, a technique
        known as spoofing. This is often done in order to
        initiate a denial-of-service attack against another
        internet host or network.
        Since the source IP addresses of the incoming packets
        change, often randomly, and for every packet, the
        target of such an attack can't easily filter out the
        attacking packets. However, the source of the attack,
        i.e. the network service provider of the attacking 
        host, has a simple way to stop such packets from ever
        leaving its network. A router always knows which 
        networks are reachable via any of its interfaces. 
        By checking the source IP address of all packets 
        coming in via an interface against the networks known
        to be behind that interface, the router can simply 
        drop packets that aren't supposed to come from there.
        Hence, reverse path filtering filters packets 
        according to the 'reverse path' to their source 
        address. If the path back to the source address 
        does not match the path the packet is coming from,
        it is dropped.

        REFERENCE

        [1] Part 11 Wireless LAN Medium Access Control ( MAC )
        and Physical Layer ( PHY ) Specifications.

        [2] Draft-obara-capwap-lwapp-00.txt, IETF Light 
        Weight Access Point Protocol."
    REVISION        "201904250000Z"
    DESCRIPTION
        "Added following table
        - cLMobilityGroupMembersOperTable
        - ciscoLwappMobilityMCGlobalObjects
        Added following compliance group
        - ciscoLwappMobilityMIBComplianceRev03
        Added following conformance group.
        - cLMobilityGroupMemberGlobalParametersGroup"
    REVISION        "201805280000Z"
    DESCRIPTION
        "Added cLMobilityGroupMemberRev02ConfigGroup."
    REVISION        "201804240000Z"
    DESCRIPTION
        "Added cLMobilityGroupMemberDataDtls in table
        cLMobilityGroupMembersTable."
    REVISION        "201704270000Z"
    DESCRIPTION
        "Added ciscoLwappMobilityMIBComplianceRev02 that deprecates
        ciscoLwappMobilityMIBComplianceRev01.
        Added cLMobilityGroupMemberRev02ConfigGroup and 
        cLMobilityGroupMemberRev02StatusGroup."
    REVISION        "201404010000Z"
    DESCRIPTION
        "Added IPV6 support for Initial version of this MIB
        module."
    REVISION        "201008230000Z"
    DESCRIPTION
        "Added ciscoLwappMobilityMIBComplianceRev01 that deprecates
        ciscoLwappMobilityMIBCompliance.
        Added cLMobilityGroupRev01ConfigGroup object group.
        cLMobilityGroupRev01ConfigGroup object group has  been 
        deprecated."
    REVISION        "200607190000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 576 }


ciscoLwappMobilityMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityMIB 0 }

ciscoLwappMobilityMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityMIB 1 }

ciscoLwappMobilityMIBConform  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityMIB 2 }

cLMobilityAnchorGlobalDot11Config  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityMIBObjects 2 }

cLMobilityTrapVariables  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityMIBObjects 3 }

cLMobilityMulticastGroupConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityMIBObjects 4 }

cLMobilityStats  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityMIBObjects 7 }

ciscoLwappMobilityMCGlobalObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityMIBObjects 8 }

-- *******************************************************************
-- Per WLAN, anchors table
-- *******************************************************************

cLMobilityAnchorTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityAnchorEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the information about the
        802.11 LWAPP Mobility Anchors on individual WLANs.  


           +...............+   
           +               +   
           +    ROUTER     +   
           +   10.16.1.1   +   
           +...............+   
                  .. 
                .    .
              .        .
            .            .
          .                .
        .                    .
        10.16.109.112        10.16.105.39
        +......+   <<-------->>   +......+    
        +      +  [3]CC2 tunnels  +      +    
        +  CC1 +   MN1's traffic  +  CC2 +    
        +      +   to Anchor CC1  +      +    
        +......+   using EoIP     +......+    
        .                        .
        . Anchor        Foreign  .
        .                        .
        +......+                  +......+          
        +      +                  +      +          
        +  AP1 +                  +  AP2 +          
        +      +                  +      +          
        +......+                  +......+          
        'typhoon'   .                      ^'typhoon'
        .                          |
        .           [2] associates  |
        .              with AP2/CC2  |
        .                             |
        +......+   [1]              +......+
        +      +  moves to region   +      +
        +  MN1 +  ---------->>>     +  MN1 +
        +      +  serviced by AP2   +      +
        +......+                    +......+
        10.16.109.199               10.16.109.199

        In the above diagram, Central Controllers CC1 and CC2 have
        been configured in a Mobility Group.

        Currently the Mobile Node 'MN1' obtains its IP from the 
        Central Controller 'CC1' with which it first associates 
        via WLAN 'typhoon' through Access Point 'AP1'. 'CC1' 
        obtains DHCP address, say 10.16.109.199 for client 'MN1'.
        Now the client 'MN1' is identified by 10.16.109.199 for 
        further communication with the network and the 
        communication happens via 'CC1'. 

        Since, 'CC1' and 'CC2' are in same mobility group, 'CC1' 
        sends the authentication block of 'MN1' to 'CC2'.


        Central Controller 'CC2' has an associated Access Point 
        'AP2' which beams WLAN 'typhoon' and uses 10.16.105.0 / 
        255.255.255.0 subnet instead.         

        Next, the Mobile Node 'MN1' moves out of range of 'AP1'
        and gets in to proximity with 'AP2' and continues to use
        WLAN 'typhoon'. 'CC2' locally authenticates 'MN1' against
        authentication block shared from 'CC1'. 'CC2' forwards all
        traffic from 'MN1' to router. This is called WLAN mobility.

        But hold on, 'CC2' uses 10.16.105.0 / 255.255.255.0 subnet 
        for WLAN 'typhoon'. So we have two problems here :    

        a> Traffic of 10.16.109.0 / 255.255.255.0 subnet has to be
        accessible from 10.16.105.0 / 255.255.255.0 subnet.

        b> Unnecessary overloading of 10.16.105.0 / 255.255.255.0 
        subnet by traffic from 10.16.109.0 / 255.255.255.0 subnet.

        How do we address these issues ??           

        If an EoIP tunnel can be established between 'CC1' and 'CC2'
        and 'CC1' sends all traffic bound to 'MN1', 10.16.109.199,
        on this tunnel to 'CC2', which in turn forwards it to 'MN1',
        then, above two subnet-problems are resolved. This is called
        Mobility Anchoring. 'CC1' is the Mobility Anchor and 'CC2' is
        the 'Foreign' for WLAN 'typhoon'.

        As per the configuration, user creates a MobilityAnchor entry
        in 'CC2' for WLAN 'typhoon' with IP address as 'CC1', i.e. 
        10.16.109.112. So, when 'MN1' connects to WLAN 'typhoon' via 
        'AP2', then 'CC2' establishes EoIP tunnel with 10.16.109.112
        and forwards the packets to 'MN1'.

        Given the above example, the cLMobilityAnchorEntry on 'CC2'
        looks like :    

        ------------------------------------------------------------------
        |      MIB - ATTRIBUTES           |       ROW#1        |  ROW#2  |
        ------------------------------------------------------------------
        | cLMobilityAnchorWlanProfileName |     typhoon        |         |
        ------------------------------------------------------------------
        | cLMobilityAnchorSwitchIPAddress |    10.16.109.112   |         |
        ------------------------------------------------------------------
        | cLMobilityAnchorStatus          |        up(4)       |         |
        ------------------------------------------------------------------
        | cLMobilityAnchorRowStatus       |      active(1)     |         |
        ------------------------------------------------------------------

        This feature has advantages for both security and load 
        balancing.  It can be used to restrict a WLAN to a single
        subnet, regardless of the MN's entry point into the network.
        A 'public' or guest WLAN can thus be accessed throughout an
        enterprise, but still is restricted to a specific subnet.  
        It can also be used to provide some geographic load balancing,
        since the WLANs can represent a particular section of a 
        building (i.e., engineering, marketing).  Those groups can be 
        'anchored' on a particular subnet/switch rather than on the 
        CC of first occurrence (i.e., the switch controlling the APs 
        by the front door)."
    ::= { ciscoLwappMobilityMIBObjects 1 }

cLMobilityAnchorEntry OBJECT-TYPE
    SYNTAX          CLMobilityAnchorEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table provides information about
        one 802.11 LWAPP mobility anchor configured on a WLAN
        on this controller."
    INDEX           {
                        cLMobilityAnchorWlanProfileName,
                        cLMobilityAnchorSwitchIPAddress
                    } 
    ::= { cLMobilityAnchorTable 1 }

CLMobilityAnchorEntry ::= SEQUENCE {
        cLMobilityAnchorWlanProfileName OCTET STRING,
        cLMobilityAnchorSwitchIPAddress IpAddress,
        cLMobilityAnchorStatus          BITS,
        cLMobilityAnchorRowStatus       RowStatus
}

cLMobilityAnchorWlanProfileName OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (1..32))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represenst local WLAN-profile name to connect
        to guest/anchor switch." 
    ::= { cLMobilityAnchorEntry 1 }

cLMobilityAnchorSwitchIPAddress OBJECT-TYPE
    SYNTAX          IpAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the guest/anchor switch IP
        address." 
    ::= { cLMobilityAnchorEntry 2 }

cLMobilityAnchorStatus OBJECT-TYPE
    SYNTAX          BITS {
                        controlpath(0),
                        datapath(1)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents operational and connectivity
        status of the mobility anchor.            

        controlpath:
                When bit is set to '0', this means successive
                ICMP pings to the anchor have failed. 
                When bit is set to '1', this means anchor is
                reachable and responding to ICMP pings.

        datapath:
                When bit is set to '0', this means successive 
                EoIP pings to the anchor have failed.
                When bit is set to '1', this means anchor is 
                reachable and responding to EoIP pings." 
    ::= { cLMobilityAnchorEntry 3 }

cLMobilityAnchorRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and is used to
        create and delete specific instances of rows in this 
        table." 
    ::= { cLMobilityAnchorEntry 4 }
 


-- *******************************************************************
-- Mobility Controller (MC) global parameters
-- *******************************************************************

cLMobilityMCMOEnableStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object  represents the current status of the
        Mobility Oracle (MO).
        A value of 'true' indicates Mobility Oracle is enabled. 
        A value of 'false' indicates Mobility Oracle (MO) 
        is disabled."
    DEFVAL          { false } 
    ::= { ciscoLwappMobilityMCGlobalObjects 1 }

cLMobilityMCMOAdminEnableStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object allows the user to enable or disable
        MO mode.  
        A value of 'true' indicates both Mobility 
        Oracle (MO) is enabled. 
        A value of 'false' indicates Mobility Oracle (MO)
        is disabled.
        Please note that cLMobilityMOEnableStatus (operational value)
        can be false even if cLMobilityMOAdminEnableStatus is true."
    DEFVAL          { false } 
    ::= { ciscoLwappMobilityMCGlobalObjects 2 }

cLMobilityMCEnableStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the current status of
        Mobility Controller (MC).  The controller can 
        operate either in MC/MA or MA only mode. 
        A value of 'true' indicates both Mobility 
        Controller (MC) is enabled. 
        A value of 'false' indicates Mobility Controller (MC)
        is disabled."
    DEFVAL          { false } 
    ::= { ciscoLwappMobilityMCGlobalObjects 3 }

cLMobilityMCAdminEnableStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object allows the user to enable or disable
        MC mode.  The controller can operate 
        either in MC/MA or MA only mode. 
        A value of 'true' indicates both Mobility 
        Controller (MC) is enabled. 
        A value of 'false' indicates Mobility Controller (MC)
        is disabled.
        Please note that cLMobilityMCEnableStatus (operational value)
        can be false even if cLMobilityMCAdminEnableStatus is true."
    DEFVAL          { false } 
    ::= { ciscoLwappMobilityMCGlobalObjects 4 }

cLMobilityMCMulticastMode OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object allows the user to enable or disable
        multicast  mode.
        A value of 'true' indicates Multicast mode 
        is enabled.
        A value of 'false' indicates Multicast mode 
        is disabled."
    DEFVAL          { false } 
    ::= { ciscoLwappMobilityMCGlobalObjects 5 }

cLMobilityMCKeepAliveCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the keep alive count.
        If keep alive response is not received consecutively
        for N (keep alive count) times, the mobility link is
        declared as down. Valid value ranges from 3 to 20."
    DEFVAL          { 3 } 
    ::= { ciscoLwappMobilityMCGlobalObjects 6 }

cLMobilityMCKeepAliveInterval OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Each MC sends periodically keep alive packet to other
        mobility devices (MA or MC). This object represents the keep
        alive interval. This object is valid for MC, not MA.
        Valid value ranges from 1 to 30."
    DEFVAL          { 10 } 
    ::= { ciscoLwappMobilityMCGlobalObjects 7 }

cLMobilityMCDscpValue OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the Differentiated Services Code Point
        (DSCP) value. Here it is used for classifying and managing 
        mobility control packets and providing quality of service (QoS)
        on IP networks. Valid value ranges from 0 to 63."
    DEFVAL          { 0 } 
    ::= { ciscoLwappMobilityMCGlobalObjects 8 }

cLMobilityMCMOPublicAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the MO's public IP address type." 
    ::= { ciscoLwappMobilityMCGlobalObjects 9 }

cLMobilityMCMOPublicAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the MO's public IP address." 
    ::= { ciscoLwappMobilityMCGlobalObjects 10 }

cLMobilityMCApCountLicensesInUse OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total APs directly associated with
        this MC and its MAs." 
    ::= { ciscoLwappMobilityMCGlobalObjects 11 }

cLMobilityMCOwnGroupMulticastAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the multicast IP address type of its own
        mobility group." 
    ::= { ciscoLwappMobilityMCGlobalObjects 12 }

cLMobilityMCOwnGroupMulticastAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the multicast IPv4 address of its own
        mobility group." 
    ::= { ciscoLwappMobilityMCGlobalObjects 13 }

cLMobilityMCMobilityGroupName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the name for this mobility group." 
    ::= { ciscoLwappMobilityMCGlobalObjects 14 }

cLMobilityMCMONumberOfClients OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of clients reported
        by MO." 
    ::= { ciscoLwappMobilityMCGlobalObjects 15 }

cLMobilityMCNumberOfMCs OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of MCs." 
    ::= { ciscoLwappMobilityMCGlobalObjects 16 }

cLMobilityMCTotalNumberOfReportedAPs OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of APs reported
        by this MC, its peer MCs and its MAs." 
    ::= { ciscoLwappMobilityMCGlobalObjects 17 }

cLMobilityMCNumberOfReportedAPsInSubDomain OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total number of APs reported
        by this MC and its MAs." 
    ::= { ciscoLwappMobilityMCGlobalObjects 18 }

cLMobilityMCMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the mac address of its own mobility
        group." 
    ::= { ciscoLwappMobilityMCGlobalObjects 19 }

-- ********************************************************************
-- *  Global Dot11 Mobility Anchor Configuration
-- ********************************************************************

cLMobilityAnchorGroupKeepAliveNumber OBJECT-TYPE
    SYNTAX          Integer32 (3..20)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies how many successive
        ping attempts to the anchor should fail before the 
        anchor is declared DOWN."
    DEFVAL          { 3 } 
    ::= { cLMobilityAnchorGlobalDot11Config 1 }

cLMobilityAnchorGroupKeepAliveInterval OBJECT-TYPE
    SYNTAX          Integer32 (1..30)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the time interval
        (in seconds) between two consecutive ping attempts
        to an anchor."
    DEFVAL          { 10 } 
    ::= { cLMobilityAnchorGlobalDot11Config 2 }

cLMobilityAnchorSmtStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether it allows user to enable or
        disable symmetric mobility tunneling for the controller.

        The controller provides inter-subnet mobility 
        for clients roaming from one AP to another within
        a wireless LAN. This mobility is asymmetric in 
        nature where the client traffic to the wired 
        network is routed out directly via the 'foreign'
        controller. See the diagram above. This mechanism
        breaks when an upstream router has RPF enabled. 
        In this case the client traffic will be dropped 
        at the router because the RPF check ensures that
        the path back to the source address matches the 
        path the packet is coming from. 

        This attribute is aimed at addressing this issue. 

        It will allow enabling 'Symmetric Mobility
        Tunneling' or 'Bi-directional Tunneling'
        for mobile clients such that all the client
        traffic is sent to the 'anchor' controller and
        go successfully through RPF check. 

        When set to 'true', Symmetric Mobility Tunneling 
        will be enabled on the Controller on next reset. 

        When set to 'false', Symmetric Mobility Tunneling 
        will be disabled on the Controller on next reset.

        After setting this attribute to the desired value,
        user should reset the Controller for the change to
        take effect." 
    ::= { cLMobilityAnchorGlobalDot11Config 3 }

cLMobilityAnchorCurrentSmt OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents whether the Symmetric Mobility
        Tunneling is enabled or disabled on the controller.

        A value of 'true' indicates that Symmetric Mobility 
        Tunneling is currently enabled on the controller. 
        A value of 'false' indicates that Symmetric Mobility 
        Tunneling is currently disabled on the controller." 
    ::= { cLMobilityAnchorGlobalDot11Config 4 }

cLMobilityAnchorDscpValue OBJECT-TYPE
    SYNTAX          Integer32 (0..63)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the intercontroller DSCP value." 
    ::= { cLMobilityAnchorGlobalDot11Config 5 }

-- ********************************************************************
-- *  Global Mobility Group Configuration
-- ********************************************************************

cLMobilityMulticastMessagingEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the mobility multicast
        messaging feature is enabled or disabled on the 
        controller.

        A value of 'true' indicates that multicast messaging among 
        the mobility group members is enabled.
        A value of 'false' indicates that multicast messaging among
        the mobility group members is disabled." 
    ::= { cLMobilityMulticastGroupConfig 1 }

cLMobilityMulticastGroupTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityMulticastGroupEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table is used to configure multicast group
        IP address per mobility group. Entries are added to the 
        table when configuring multicast group IP address per
        mobility group."
    ::= { cLMobilityMulticastGroupConfig 2 }

cLMobilityMulticastGroupEntry OBJECT-TYPE
    SYNTAX          CLMobilityMulticastGroupEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table provides information about
        multicast group IP address per mobility group."
    INDEX           { cLMobilityGroupMacAddress } 
    ::= { cLMobilityMulticastGroupTable 1 }

CLMobilityMulticastGroupEntry ::= SEQUENCE {
        cLMobilityGroupMacAddress             MacAddress,
        cLMobilityMulticastGroupIPAddressType InetAddressType,
        cLMobilityMulticastGroupIPAddress     InetAddress
}

cLMobilityGroupMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the mobility group MAC address
        present on the controller." 
    ::= { cLMobilityMulticastGroupEntry 1 }

cLMobilityMulticastGroupIPAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the multicast group IP address
        type. The IP address is limited to IPv4 and IPv6." 
    ::= { cLMobilityMulticastGroupEntry 2 }

cLMobilityMulticastGroupIPAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the multicast group IP address per
        group. The IP address is limited to IPv4 and IPv6. 
        The IP address should be reset only after disabling 
        the mobility multicast mode
        (cLMobilityMulticastMessagingEnable)." 
    ::= { cLMobilityMulticastGroupEntry 3 }
 

-- **************************************************************
-- *         Mobility Group Members Operational Table
-- **************************************************************

cLMobilityGroupMembersOperTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityGroupMembersOperEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the MWAR List (statically configured
        members of the mobility group).Entries are created to the table
        when configuring mobility group members."
    ::= { ciscoLwappMobilityMIBObjects 9 }

cLMobilityGroupMembersOperEntry OBJECT-TYPE
    SYNTAX          CLMobilityGroupMembersOperEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents an Entry (conceptual row) in the
        cLMobilityGroupMembersOper table."
    INDEX           {
                        cLMobilityGroupMembersOperNodeAddressType,
                        cLMobilityGroupMembersOperNodeAddress
                    } 
    ::= { cLMobilityGroupMembersOperTable 1 }

CLMobilityGroupMembersOperEntry ::= SEQUENCE {
        cLMobilityGroupMembersOperNodeAddressType   InetAddressType,
        cLMobilityGroupMembersOperNodeAddress       InetAddress,
        cLMobilityGroupMembersOperTunnelStatus      Integer32,
        cLMobilityGroupMembersOperDataPathStatus    TruthValue,
        cLMobilityGroupMembersOperControlPathStatus TruthValue
}

cLMobilityGroupMembersOperNodeAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the IP Address type of the mobility
        member" 
    ::= { cLMobilityGroupMembersOperEntry 1 }

cLMobilityGroupMembersOperNodeAddress OBJECT-TYPE
    SYNTAX          InetAddress (SIZE  (4 | 16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the IP Address of the mobility member
        This object support for only IPv4 and IPv6 addresses and so 
        the size can be either 4 or 16 bytes." 
    ::= { cLMobilityGroupMembersOperEntry 2 }

cLMobilityGroupMembersOperTunnelStatus OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the tunnel status of the mobility
        member corresponding to cLMobilityGroupMembersOperNodeAddress." 
    ::= { cLMobilityGroupMembersOperEntry 3 }

cLMobilityGroupMembersOperDataPathStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the data path status of the mobility
        member corresponding to cLMobilityGroupMembersOperNodeAddress." 
    ::= { cLMobilityGroupMembersOperEntry 4 }

cLMobilityGroupMembersOperControlPathStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the control path status of the mobility
        member corresponding to cLMobilityGroupMembersOperNodeAddress." 
    ::= { cLMobilityGroupMembersOperEntry 5 }
 


cLMobilityGroupMembersTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityGroupMembersEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the MWAR List (statically configured
        members of the mobility group). Entries are added to the 
        table when configuring mobility group members."
    ::= { ciscoLwappMobilityMIBObjects 5 }

cLMobilityGroupMembersEntry OBJECT-TYPE
    SYNTAX          CLMobilityGroupMembersEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents an entry (conceptual row) in the
        cLMobilityGroupMembers table."
    INDEX           { cLMobilityGroupMacAddress } 
    ::= { cLMobilityGroupMembersTable 1 }

CLMobilityGroupMembersEntry ::= SEQUENCE {
        cLMobilityGroupMemberIPAddressType       InetAddressType,
        cLMobilityGroupMemberIPAddress           InetAddress,
        cLMobilityGroupMemberControlPathStatusUp TruthValue,
        cLMobilityGroupMemberDataPathStatusUp    TruthValue,
        cLMobilityGroupMemberHashKey             OCTET STRING,
        cLMobilityGroupMemberAddressType         InetAddressType,
        cLMobilityGroupMemberAddress             InetAddress,
        cLMobilityGroupMemberGroupName           SnmpAdminString,
        cLMobilityGroupMemberRowStatus           RowStatus,
        cLMobilityGroupMemberDataDtls            TruthValue
}

cLMobilityGroupMemberIPAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "This object represents the IP address type of the
        mobility member IP address represented by 
        cLMobilityGroupMemberIPAddress. The IP address is limited
        to IPv4 and IPv6. For clarity, this object is being
        deprecated in favor of the new read-write object 
        'cLMobilityGroupMemberAddressType." 
    ::= { cLMobilityGroupMembersEntry 1 }

cLMobilityGroupMemberIPAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "This object represents the IP address of the mobility
        member corresponding to cLMobilityGroupMacAddress. The
        IP address is limited to IPv4 and IPv6. For clarity, this 
        object is being deprecated in favor of the new read-write 
        object 'cLMobilityGroupMemberAddress." 
    ::= { cLMobilityGroupMembersEntry 2 }

cLMobilityGroupMemberControlPathStatusUp OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the control path status of the
        mobility member corresponding to 
        cLMobilityGroupMacAddress.
        A value of 'true' indicates that control path is up.
        A value of 'false' indicates that control path is down."
    DEFVAL          { false } 
    ::= { cLMobilityGroupMembersEntry 3 }

cLMobilityGroupMemberDataPathStatusUp OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the data path status of the
        mobility member corresponding to 
        cLMobilityGroupMacAddress.
        A value of 'true' indicates that data path is up.
        A value of 'false' indicates that data path is down."
    DEFVAL          { false } 
    ::= { cLMobilityGroupMembersEntry 4 }

cLMobilityGroupMemberHashKey OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (4..40))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the Hash key of the peer
        mobility member. 
        It is a 40 hex digit value or 'none' to
        clear the previously configured hash key" 
    ::= { cLMobilityGroupMembersEntry 5 }

cLMobilityGroupMemberAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the IP address type of the mobility
        member IP address represented by 
        cLMobilityGroupMemberIPAddress. The IP address is limited 
        to IPv4 and IPv6." 
    ::= { cLMobilityGroupMembersEntry 6 }

cLMobilityGroupMemberAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the IP address of the mobility
        member corresponding to cLMobilityGroupMacAddress. The IP 
        address is limited to IPv4 and IPv6." 
    ::= { cLMobilityGroupMembersEntry 7 }

cLMobilityGroupMemberGroupName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies member's group name. If left empty
        while adding a new group member, this assumes the default 
        mobility group name of the switch." 
    ::= { cLMobilityGroupMembersEntry 8 }

cLMobilityGroupMemberRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and is used to
        create and delete specific instances of rows in this 
        table." 
    ::= { cLMobilityGroupMembersEntry 9 }

cLMobilityGroupMemberDataDtls OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the data dtls status with a
        mobility member.Data DTLS modification can be performed
        once mobility member is created. 
        A value of 'true' indicates that data DTLS is enabled.
        A value of 'false' indicates that data DTLS is disabled."
    DEFVAL          { true } 
    ::= { cLMobilityGroupMembersEntry 10 }
 


cLMobilityForeignWlcMapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityForeignWlcMapEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table is used to create mappings of the foreign
        controller with the interface/interface group to be used,
        when clients are directly connected to the foreign 
        controller send the DHCP request to the anchor
        controller."
    ::= { ciscoLwappMobilityMIBObjects 6 }

cLMobilityForeignWlcMapEntry OBJECT-TYPE
    SYNTAX          CLMobilityForeignWlcMapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents a row in the
        cLMobilityForeignWlcIfMappingTable .Entries are added and 
        deleted by explicit user driven action."
    INDEX           {
                        cLMobilityAnchorWlanProfileName,
                        cLMobilityForeignWlcMapMacAddress
                    } 
    ::= { cLMobilityForeignWlcMapTable 1 }

CLMobilityForeignWlcMapEntry ::= SEQUENCE {
        cLMobilityForeignWlcMapMacAddress MacAddress,
        cLMobilityForeignWlcMapIf         SnmpAdminString,
        cLMobilityForeignWlcMapRowStatus  RowStatus
}

cLMobilityForeignWlcMapMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the MAC address of the foreign
        controller, to which the interface mapping is to be 
        configured." 
    ::= { cLMobilityForeignWlcMapEntry 1 }

cLMobilityForeignWlcMapIf OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..255))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies name of the interface/interface
        group which would be used for the communication with the
        clients connected to the foreign controller, represented by
        cLMobilityForeignWlcMapMacAddress." 
    ::= { cLMobilityForeignWlcMapEntry 2 }

cLMobilityForeignWlcMapRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and is used to
        create and delete specific instances of rows in this 
        table." 
    ::= { cLMobilityForeignWlcMapEntry 3 }
 


-- *******************************************************************
-- *    Mobility Statistics
-- *******************************************************************

cLMobilityIncomingCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the number of successfully incoming
        inter-WLC roaming count for this WLC. If a client roams in
        from other WLC with the same SSID and successfully
        re-associated, the count should be increased." 
    ::= { cLMobilityStats 1 }

cLMobilityOutgoingCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the number of successfully outgoing
        inter-WLC roaming count for this WLC. If a client roams 
        out to other WLC with the same SSID successfully, the
        count should be increased." 
    ::= { cLMobilityStats 2 }

-- *******************************************************************
-- *    DEFINITION OF OBJECTS ACCESSIBLE FOR NOTIFICATIONS ONLY
-- *******************************************************************

cLMobilityAnchorWlanId OBJECT-TYPE
    SYNTAX          Integer32 (1..16)
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object represents index of the WLAN in the
        controller." 
    ::= { cLMobilityTrapVariables 1 }

cLMobilityAnchorAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object represents the guest/anchor switch address
        type." 
    ::= { cLMobilityTrapVariables 2 }

cLMobilityAnchorAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object represents the guest/anchor switch address.
        The IP address is limited to IPv4 and IPv6." 
    ::= { cLMobilityTrapVariables 3 }

-- *******************************************************************
-- * END OF - DEFINITION OF OBJECTS ACCESSIBLE FOR NOTIFICATIONS ONLY
-- *******************************************************************
--   

-- *******************************************************************
-- *    NOTIFICATIONS
-- *******************************************************************

ciscoLwappMobilityAnchorControlPathDown NOTIFICATION-TYPE
    OBJECTS         {
                        cLMobilityAnchorAddressType,
                        cLMobilityAnchorAddress
                    }
    STATUS          current
    DESCRIPTION
        "This trap will be generated by the controller when,
        successive ICMP ping attempts to the anchor fails 
        and the anchor is conclusively down. 
        Variable cLMobilityAnchorAddress denotes the
        IP address of the anchor."
   ::= { ciscoLwappMobilityMIBNotifs 1 }

ciscoLwappMobilityAnchorControlPathUp NOTIFICATION-TYPE
    OBJECTS         {
                        cLMobilityAnchorAddressType,
                        cLMobilityAnchorAddress
                    }
    STATUS          current
    DESCRIPTION
        "This trap will be generated by the controller when,
        ICMP ping to the anchor is restored and anchor is 
        conclusively up. 
        Variable cLMobilityAnchorAddress denotes the
        IP address of the anchor."
   ::= { ciscoLwappMobilityMIBNotifs 2 }

ciscoLwappMobilityAnchorDataPathDown NOTIFICATION-TYPE
    OBJECTS         {
                        cLMobilityAnchorAddressType,
                        cLMobilityAnchorAddress
                    }
    STATUS          current
    DESCRIPTION
        "This trap will be generated by the controller when,
        successive EoIP ping attempts to the anchor fails
        and the anchor is conclusively down. 
        Variable cLMobilityAnchorAddress denotes the
        IP address of the anchor."
   ::= { ciscoLwappMobilityMIBNotifs 3 }

ciscoLwappMobilityAnchorDataPathUp NOTIFICATION-TYPE
    OBJECTS         {
                        cLMobilityAnchorAddressType,
                        cLMobilityAnchorAddress
                    }
    STATUS          current
    DESCRIPTION
        "This trap will be generated by the controller when,
        EoIP ping to the anchor is restored and anchor is 
        conclusively up. 
        Variable cLMobilityAnchorAddress denotes the
        IP address of the anchor."
   ::= { ciscoLwappMobilityMIBNotifs 4 }

ciscoLwappMobilityAllAnchorsOnWlanDown NOTIFICATION-TYPE
    OBJECTS         { cLMobilityAnchorWlanId }
    STATUS          current
    DESCRIPTION
        "This trap will be generated by the controller when,
        successive EoIP ping attempts to all the anchors on
        WLAN, denoted by cLMobilityAnchorWlanId, fails and 
        all the anchors are conclusively down."
   ::= { ciscoLwappMobilityMIBNotifs 5 }

ciscoLwappMobilityOneAnchorOnWlanUp NOTIFICATION-TYPE
    OBJECTS         { cLMobilityAnchorWlanId }
    STATUS          current
    DESCRIPTION
        "This trap will be generated by the controller when,
        successive EoIP and UDP ping to atleast one anchor 
        on the WLAN, denoted by cLMobilityAnchorWlanId, is 
        restored and anchor is conclusively up."
   ::= { ciscoLwappMobilityMIBNotifs 6 }
-- *******************************************************************
-- *   END OF -  NOTIFICATIONS
-- *******************************************************************
--   
-- *******************************************************************
-- *    Compliance statements
-- *******************************************************************

ciscoLwappMobilityMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityMIBConform 1 }

ciscoLwappMobilityMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityMIBConform 2 }


ciscoLwappMobilityMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappMobilityMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cLNplus1RedundancyRev01ConfigGroup,
                        cLNplus1RedundancyRev01StatusGroup,
                        cLNplus1RedundancyRev01NotifsGroup,
                        cLSymmetricTunnelingRev01ConfigGroup,
                        cLSymmetricTunnelingRev01StatusGroup
                    }
    ::= { ciscoLwappMobilityMIBCompliances 1 }

ciscoLwappMobilityMIBComplianceRev01 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappMobilityMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cLNplus1RedundancyRev01ConfigGroup,
                        cLNplus1RedundancyRev01StatusGroup,
                        cLNplus1RedundancyRev01NotifsGroup,
                        cLSymmetricTunnelingRev01ConfigGroup,
                        cLSymmetricTunnelingRev01StatusGroup,
                        cLMobilityGroupRev01ConfigGroup
                    }
    ::= { ciscoLwappMobilityMIBCompliances 2 }

ciscoLwappMobilityMIBComplianceRev02 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappMobilityMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cLNplus1RedundancyRev01ConfigGroup,
                        cLNplus1RedundancyRev01StatusGroup,
                        cLNplus1RedundancyRev01NotifsGroup,
                        cLSymmetricTunnelingRev01ConfigGroup,
                        cLSymmetricTunnelingRev01StatusGroup,
                        cLMobilityGroupMemberRev02ConfigGroup,
                        cLMobilityGroupMemberRev02StatusGroup
                    }
    ::= { ciscoLwappMobilityMIBCompliances 3 }

ciscoLwappMobilityMIBComplianceRev03 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappMobilityMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cLNplus1RedundancyRev01ConfigGroup,
                        cLNplus1RedundancyRev01StatusGroup,
                        cLNplus1RedundancyRev01NotifsGroup,
                        cLSymmetricTunnelingRev01ConfigGroup,
                        cLSymmetricTunnelingRev01StatusGroup,
                        cLMobilityGroupMemberRev02ConfigGroup,
                        cLMobilityGroupMemberRev02StatusGroup,
                        cLMobilityGroupMemberGlobalParametersGroup
                    }
    ::= { ciscoLwappMobilityMIBCompliances 4 }

-- *******************************************************************
-- *    Units of conformance
-- *******************************************************************

cLNplus1RedundancyRev01ConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLMobilityAnchorGroupKeepAliveNumber,
                        cLMobilityAnchorGroupKeepAliveInterval
                    }
    STATUS          current
    DESCRIPTION
        "This is a collection of objects which can
        configured to control functional parameters 
        of guest tunneling N+1 redundancy feature."
    ::= { ciscoLwappMobilityMIBGroups 1 }

cLNplus1RedundancyRev01StatusGroup OBJECT-GROUP
    OBJECTS         {
                        cLMobilityAnchorStatus,
                        cLMobilityAnchorRowStatus,
                        cLMobilityAnchorWlanId,
                        cLMobilityAnchorAddressType,
                        cLMobilityAnchorAddress
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents the information
        about the general status attributes of guest tunneling 
        N+1 redundancy feature."
    ::= { ciscoLwappMobilityMIBGroups 2 }

cLNplus1RedundancyRev01NotifsGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        ciscoLwappMobilityAnchorControlPathDown,
                        ciscoLwappMobilityAnchorControlPathUp,
                        ciscoLwappMobilityAnchorDataPathDown,
                        ciscoLwappMobilityAnchorDataPathUp,
                        ciscoLwappMobilityAllAnchorsOnWlanDown,
                        ciscoLwappMobilityOneAnchorOnWlanUp
                    }
    STATUS          current
    DESCRIPTION
        "This is a collection of notifications about the
        general functional behavior of guest tunneling 
        N+1 redundancy feature."
    ::= { ciscoLwappMobilityMIBGroups 3 }

cLSymmetricTunnelingRev01ConfigGroup OBJECT-GROUP
    OBJECTS         { cLMobilityAnchorSmtStatus }
    STATUS          current
    DESCRIPTION
        "This is a collection of objects which can be
        configured to control functional parameters 
        of symmetric mobility tunneling feature."
    ::= { ciscoLwappMobilityMIBGroups 4 }

cLSymmetricTunnelingRev01StatusGroup OBJECT-GROUP
    OBJECTS         {
                        cLMobilityAnchorCurrentSmt,
                        cLMobilityAnchorDscpValue
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents the information
        about the general status attributes of symmetric 
        tunneling feature."
    ::= { ciscoLwappMobilityMIBGroups 5 }

cLMobilityGroupRev01ConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLMobilityMulticastMessagingEnable,
                        cLMobilityMulticastGroupIPAddress,
                        cLMobilityMulticastGroupIPAddressType,
                        cLMobilityGroupMemberIPAddressType,
                        cLMobilityGroupMemberIPAddress,
                        cLMobilityGroupMemberControlPathStatusUp,
                        cLMobilityGroupMemberDataPathStatusUp,
                        cLMobilityForeignWlcMapIf,
                        cLMobilityForeignWlcMapRowStatus
                    }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects represents the
        information about the mobility groups and the
        interface mappings with foreign controllers."
    ::= { ciscoLwappMobilityMIBGroups 6 }

cLMobilityGroupMemberRev02StatusGroup OBJECT-GROUP
    OBJECTS         {
                        cLMobilityMulticastGroupIPAddress,
                        cLMobilityMulticastGroupIPAddressType,
                        cLMobilityGroupMemberControlPathStatusUp,
                        cLMobilityGroupMemberDataPathStatusUp,
                        cLMobilityIncomingCount,
                        cLMobilityOutgoingCount
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents the information
        about the Global Mobility Group Configuration of WLC."
    ::= { ciscoLwappMobilityMIBGroups 7 }

cLMobilityGroupMemberRev02ConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLMobilityMulticastMessagingEnable,
                        cLMobilityMulticastGroupIPAddress,
                        cLMobilityMulticastGroupIPAddressType,
                        cLMobilityGroupMemberControlPathStatusUp,
                        cLMobilityGroupMemberDataPathStatusUp,
                        cLMobilityGroupMemberHashKey,
                        cLMobilityGroupMemberAddressType,
                        cLMobilityGroupMemberAddress,
                        cLMobilityGroupMemberGroupName,
                        cLMobilityGroupMemberRowStatus,
                        cLMobilityForeignWlcMapIf,
                        cLMobilityForeignWlcMapRowStatus,
                        cLMobilityGroupMemberDataDtls
                    }
    STATUS          current
    DESCRIPTION
        "This is a collection of objects which can
        configured to Global Mobility Group Configuration of WLC."
    ::= { ciscoLwappMobilityMIBGroups 8 }

cLMobilityGroupMemberGlobalParametersGroup OBJECT-GROUP
    OBJECTS         {
                        cLMobilityMCMOEnableStatus,
                        cLMobilityMCMOAdminEnableStatus,
                        cLMobilityMCEnableStatus,
                        cLMobilityMCAdminEnableStatus,
                        cLMobilityMCMulticastMode,
                        cLMobilityMCKeepAliveCount,
                        cLMobilityMCKeepAliveInterval,
                        cLMobilityMCDscpValue,
                        cLMobilityMCMOPublicAddressType,
                        cLMobilityMCMOPublicAddress,
                        cLMobilityMCApCountLicensesInUse,
                        cLMobilityMCOwnGroupMulticastAddressType,
                        cLMobilityMCOwnGroupMulticastAddress,
                        cLMobilityMCMobilityGroupName,
                        cLMobilityMCMONumberOfClients,
                        cLMobilityMCNumberOfMCs,
                        cLMobilityMCTotalNumberOfReportedAPs,
                        cLMobilityMCNumberOfReportedAPsInSubDomain,
                        cLMobilityMCMacAddress,
                        cLMobilityGroupMembersOperControlPathStatus,
                        cLMobilityGroupMembersOperTunnelStatus,
                        cLMobilityGroupMembersOperDataPathStatus
                    }
    STATUS          current
    DESCRIPTION
        "This is a collection of objects which can
        configured to Global Mobility Group Configuration of WLC."
    ::= { ciscoLwappMobilityMIBGroups 9 }

END


-- %DNP%  MLC -Edit MLC

