-- *****************************************************************
-- CISCO-EVC-MIB.my : Cisco Ethernet Virtual Connection MIB
--   
-- January 2007, Viet Nguyen
-- April 2008, Pravin Gohite
--   
-- Copyright (c) 2007-2008, 2012 by Cisco Systems Inc.
--   
-- All rights reserved.
-- *****************************************************************

CISCO-EVC-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    NOTIFICATION-TYPE,
    OBJECT-TYPE,
    Unsigned32,
    Gauge32,
    Integer32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    TEXTUAL-CONVENTION,
    TruthValue,
    RowStatus,
    StorageType,
    MacAddress
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    VlanId,
    VlanIdOrNone
        FROM Q-BRIDGE-MIB
    ifIndex,
    InterfaceIndexOrZero
        FROM IF-MIB
    CiscoCosList
        FROM CISCO-TC
    ciscoMgmt
        FROM CISCO-SMI;


ciscoEvcMIB MODULE-IDENTITY
    LAST-UPDATED    "201205210000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-ethermibs@cisco.com"
    DESCRIPTION
        "Metro Ethernet services can support a wide range of
        applications and subscriber needs easily, efficiently
        and cost-effectively.  Using standard Ethernet interfaces, 
        subscribers can set up secure, private Ethernet Virtual 
        Connections, to connect their sites together and connect 
        to business partners, suppliers and the Internet.

        This MIB module defines the managed objects and notifications
        describing Ethernet Virtual Connections.

        Ethernet Virtual Connections (EVC), are defined by the Metro
        Ethernet Forum (MEF), as an association between two or more
        UNIs.  Frames within an EVC can only be exchanged among the
        associated UNIs.  Frames sent into the MEN via a particular
        UNI must not be delivered back to the UNI from which it 
        originated.  

        Along an EVC path, there are demarcation flow points on 
        associated ingress and egress interface, of every device, 
        through which the EVC passes.  A service instance represents
        these flow points where a service passes through an interface.  

        From an operational perspective, a service instance serves 
        three purposes: 
            1.  Defines the instance of a particular EVC service on
                a specific interface and identifies all frames that
                belongs to that particular service/flow.
            2.  To provide the capability of applying the configured 
                features to those frames belonging to the service.
            3.  To optionally define how to forward those frames in
                the data-path.  

        The association of a service instance to an EVC depicts
        an instance of an Ethernet flow on a particular interface
        for an end-to-end (UNI-to-UNI) Ethernet service for a 
        subscriber.

        The following diagram illustrates the association of
        EVC, UNIs and service instances.  UNI physical ports
        are depicted as 'U', and service instances as 'x'.

            CE             MEN            MEN            CE
          -------        -------        -------        -------
          |     |        |     |   ()   |     |        |     |
          |     |--------Ux   x|--(  )--|x   xU--------|     |
          |     |        |     |   ()   |     |        |     |
          -------        -------        -------        -------
                         ^                    ^
                         |                    |
                         -------- EVC ---------

        This MIB module addresses the functional areas of network
        management for EVC, including:

            The operational mode for interfaces that are providing
            Ethernet service(s).

            The service attributes regarding an interface behaving
            as UNI, such as CE-VLAN mapping and layer 2 control 
            protocol (eg. stp, vtp, cdp) processing.

            The provisioning of service instances to define flow 
            points for an Ethernet service.

            The operational status of EVCs for notifications
            of status changes, and EVC creation and deletion.

        Definition of terms and acronyms:

            B-Tag: Backbone Tag field in Ethernet 802.1ah frame

            CE: Customer Edge

            CE-VLAN: Customer Edge VLAN

            CoS: Class Of Service

            EVC: Ethernet Virtual Connection

            I-SID: Service Instance Identifier field in Ethernet 
            802.1ah frame

            MAC: Media Access Control

            MEN: Metro Ethernet Network 

            NNI: Network to Network Interface

            OAM: Operations Administration and Management

            PPPoE: Point-to-Point Protocol over Ethernet

            Service frame: An Ethernet frame transmitted across the 
            UNI toward the service provider or an Ethernet frame 
            transmitted across the UNI toward the Subscriber.

            Service Instance: A flow point of an Ethernet service

            Service provider: The organization providing Ethernet
            service(s).

            Subscriber: The organization purchasing and/or using 
            Ethernet service(s).

            UNI: User Network Interface
                 The physical demarcation point between the 
                 responsibility of the service provider and 
                 the responsibility of the Subscriber.

            UNI-C: User Network Interface, subscriber side

            UNI-N: User Network Interface, service provider side

            VLAN: Virtual Local Area Network"
    REVISION        "201205210000Z"
    DESCRIPTION
        "- Added following objects to cevcSITable:
        * cevcSICreationType
        * cevcSIType
        - Added following objects to cevcSIForwardBdTable:
         * cevcSIForwardBdNumberBase
         * cevcSIForwardBdNumber1kBitmap
         * cevcSIForwardBdNumber2kBitmap
         * cevcSIForwardBdNumber3kBitmap
         * cevcSIForwardBdNumber4kBitmap
        - Added MacSecurityViolation OID subtree and following objects:
        * cevcMacAddress
        * cevcMaxMacConfigLimit
        * cevcSIID
        - Deprecated cevcEvcNotificationGroup and added
                cevcEvcNotificationGroupRev1 and added 
                cevcMacSecurityViolationNotification
        - Deprecated cevcSIGroup and added cevcSIGroupRev1
         and added cevcSICreationType and cevcSIType
        - Deprecated cevcSIForwardGroup and added cevcSIForwardGroupRev1
         and added the new objects mentioned in cevcSIForwardBdTable
        - Added CevcMacSecurityViolationCause Textual convention
        - Added new ciscoEvcMIBComplianceRev2"
    REVISION        "200805010000Z"
    DESCRIPTION
        "- Added following enums to cevcSIOperStatus:
        * deleted(4)
        * errorDisabled(5)
        * unknown(6)

        - Added following named bits to cevcSIMatchEncapValid:
        * payloadTypes(3)
        * priorityCos(4)
        * dot1qNativeVlan(5)
        * dot1adNativeVlan(6)
        * encapExact(7)

        - The Object cevcSIMatchEncapPayloadType is replaced by
        new object cevcSIMatchEncapPayloadTypes to support multiple
        payload types for service instance match criteria.

        - Added new object cevcSIMatchEncapPriorityCos to 
        cevcSIMatchEncapTable.

        - Added new Compliance ciscoEvcMIBComplianceRev1.

        - Added new Object Group cevcSIMatchCriteriaGroupRev1.

        - Miscellaneous updates/corrections."
    REVISION        "200712200000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 613 }


ciscoEvcMIBNotifications  OBJECT IDENTIFIER
    ::= { ciscoEvcMIB 0 }

ciscoEvcMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoEvcMIB 1 }

ciscoEvcMIBConformance  OBJECT IDENTIFIER
    ::= { ciscoEvcMIB 2 }

cevcSystem  OBJECT IDENTIFIER
    ::= { ciscoEvcMIBObjects 1 }

cevcPort  OBJECT IDENTIFIER
    ::= { ciscoEvcMIBObjects 2 }

cevcEvc  OBJECT IDENTIFIER
    ::= { ciscoEvcMIBObjects 3 }

cevcServiceInstance  OBJECT IDENTIFIER
    ::= { ciscoEvcMIBObjects 4 }

cevcEvcNotificationConfig  OBJECT IDENTIFIER
    ::= { ciscoEvcMIBObjects 5 }

cevcMacSecurityViolation  OBJECT IDENTIFIER
    ::= { ciscoEvcMIBObjects 6 }


-- Textual Conventions

CevcMacSecurityViolationCauseType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "An integer value which identifies the cause for the MAC
        Security Violation.
        
        If the system MAC Address limit is exceeded, the
        cevcMacSecurityViolationCauseType will contain 
        'exceedSystemLimit' value.

        If the Bridge domain limit is exceeded, the
        cevcMacSecurityViolationCauseType will contain 
        'exceedBdLimit' value.

        If the Service Instance limit is exceeded, the
        cevcMacSecurityViolationCauseType will contain 
        'exceedSILimit' value.

        If the MAC address is present in the Black list
        then cevcMacSecurityViolationCauseType will contain 
        'blackListDeny' value."
        
        
    SYNTAX          INTEGER  {
                        exceedSystemLimit(1),
                        exceedBdLimit(2),
                        exceedSILimit(3),
                        blackListDeny(4)
                    }

CiscoEvcIndex ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "An integer-value which uniquely identifies the EVC."
    SYNTAX          Unsigned32 (1..4294967295)

CiscoEvcIndexOrZero ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This textual convention is an extension to textual
        convention 'CiscoEvcIndex'.  It includes the value of
        '0' in addition to the range of 1-429496725.  Value
        of '0' indicates that the EVC has been neither configured
        nor assigned."
    SYNTAX          Unsigned32 (0..4294967295)

CevcL2ControlProtocolType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Defines the different types of layer 2 control protocols:


        'other'
            None of the following.


        'cdp' 
            Cisco Discovery Protocol.


        'dtp'
            Dynamic Trunking Protocol.


        'pagp'
            Port Aggregration Protocol.


        'udld'
            UniDirectional Link Detection.


        'vtp' 
            Vlan Trunking Protocol.


        'lacp'
            Link Aggregation Control Protocol.


        'dot1x'
            IEEE 802.1x


        'stp'
            Spanning Tree Protocol."
    SYNTAX          INTEGER  {
                        other(1),
                        cdp(2),
                        dtp(3),
                        pagp(4),
                        udld(5),
                        vtp(6),
                        lacp(7),
                        dot1x(8),
                        stp(9)
                    }

ServiceInstanceTarget ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Denotes a generic service instance target.

        An ServiceInstanceTarget value is always interpreted within the
        context of an ServiceInstanceTargetType value.  Every usage of
        the ServiceInstanceTarget textual convention is required to
        specify the ServiceInstanceTargetType object which provides the
        context.  It is suggested that the ServiceInstanceTargetType
        object is logically registered before the object(s) which use
        the ServiceInstanceTarget textual convention if they appear in
        the same logical row.

        The value of an ServiceInstanceTarget object must always be
        consistent with the value of the associated
        ServiceInstanceTargetType object.  Attempts to set an
        ServiceInstanceTarget object to a value which is inconsistent
        with the associated ServiceInstanceTargetType must fail with an
        inconsistentValue error.

        When this textual convention is used as the syntax of an index
        object, there may be issues with the limit of 128
        sub-identifiers specified in SMIv2, STD 58.  In this
        case, the object definition MUST include a 'SIZE' clause
        to limit the number of potential instance sub-identifiers."
    SYNTAX          OCTET STRING (SIZE (0..40))

ServiceInstanceTargetType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "Defines the type of interface/media to which a service instance
        is attached.

            'other'
                None of the following.  This value MUST be used if the
                value of the corresponding ServiceInstanceTarget
                object is a zero-length string.

            'interface'
                Service instance is attached to the the interface
                defined by ServiceInstanceInterface textual
                convention.

        Each definition of a concrete ServiceInstanceTargetType value
        must be accompanied by a definition of a textual convention for
        use with that ServiceInstanceTargetType.

        To support future extensions, the ServiceInstanceTargetType
        textual convention SHOULD NOT be sub-typed in object type
        definitions.  It MAY be sub-typed in compliance statements in
        order to require only a subset of these target types for a
        compliant implementation.

        Implementations must ensure that ServiceInstanceTargetType
        objects and any dependent objects (e.g. ServiceInstanceTarget
        objects) are consistent.  An inconsistentValue error must be
        generated if an attempt to change an ServiceInstanceTargetType
        object would, for example, lead to an undefined
        ServiceInstanceTarget value.  In particular,
        ServiceInstanceTargetType/ServiceInstanceTarget pairs must be
        changed together if the service instance taget type changes."
    SYNTAX          INTEGER  {
                        other(1),
                        interface(2)
                    }
                    
ServiceInstanceInterface ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This textual convention indicates the ifIndex which identifies
        the interface that the service instance is attached, for which 
        the corresponding ifType has the value of (but not limited to)
        'ethernetCsmacd'.

            octets   contents     encoding
            1-4      ifIndex      network-byte order

        The corresponding ServiceInstanceTargetType value is
        interface(2)."
    SYNTAX          OCTET STRING (SIZE (4))
    
-- Mac Security Violation Attributes

cevcMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the MAC Address which has violated
         the Mac security rules." 
    ::= { cevcMacSecurityViolation 1 }

cevcMaxMacConfigLimit OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the maximum MAC configuration limit. This
        is also sent as a part of MAC security violation notification.
        Every platform has their own forwarding table limitation. User 
        can also set the maximum MAC configuration limit and if the 
        limit set by user is not supported by platform then the object
        returns error." 
    ::= { cevcMacSecurityViolation 2 }

cevcSIID OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the service instance ID for the MAC
        security violation notification." 
    ::= { cevcMacSecurityViolation 3 }

cevcViolationCause OBJECT-TYPE
    SYNTAX          CevcMacSecurityViolationCauseType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the MAC security violation cause.
        
        When the system MAC Address limit is exceeded, the
        cevcMacSecurityViolationCause will contain
        'exceedSystemLimit' value.

        When the Bridge domain limit is exceeded, the
        cevcMacSecurityViolationCause will contain
        'exceedBdLimit' value.

        When the Service Instance limit is exceeded, the
        cevcMacSecurityViolationCause will contain
        'exceedSILimit' value.

        If the MAC address is present in the Black list
        then cevcMacSecurityViolationCause will contain
        'blackListDeny' value." 
        
    ::= { cevcMacSecurityViolation 4 }

-- System Attributes

cevcMaxNumEvcs OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the maximum number of EVCs that the
        system supports." 
    ::= { cevcSystem 1 }

cevcNumCfgEvcs OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the actual number of EVCs currently
        configured on the system." 
    ::= { cevcSystem 2 }
-- Port  Table

cevcPortTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcPortEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides the operational mode and configuration
        limitations of the physical interfaces (ports) that provide
        Ethernet services for the MEN. 

        This table has a sparse depedent relationship on the ifTable, 
        containing a row for each ifEntry having an ifType of 
        'ethernetCsmacd' capable of supporting Ethernet services."
    ::= { cevcPort 1 }

cevcPortEntry OBJECT-TYPE
    SYNTAX          CevcPortEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents a port, a physical point, at which
        signals can enter or leave the network en route to or from
        another network to provide Ethernet services for the MEN.

        The system automatically creates an entry for each ifEntry in
        the ifTable having an ifType of 'ethernetCsmacd' capable of
        supporting Ethernet services and entries are automatically
        destroyed when the corresponding row in the ifTable is
        destroyed."
    INDEX           { ifIndex } 
    ::= { cevcPortTable 1 }

CevcPortEntry ::= SEQUENCE {
        cevcPortMode                   INTEGER,
        cevcPortMaxNumEVCs             Gauge32,
        cevcPortMaxNumServiceInstances Gauge32
}

cevcPortMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        uni(1),
                        nni(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Port denotes the physcial interface which can provide
        Ethernet services.  This object indicates the mode of the
        port and its operational behaviour in the MEN. 


           'uni'
               User Network Interface
               The port resides on the interface between the end user
               and the network.  Additional information related
               to the UNI is included in cevcUniTable.


            'nni'
                Network to Network Interface.  The port resides on the
                interface between two networks." 
    ::= { cevcPortEntry 1 }

cevcPortMaxNumEVCs OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the maximum number of EVCs that the
        interface can support." 
    ::= { cevcPortEntry 2 }

cevcPortMaxNumServiceInstances OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the maximum number of service instances
        that the interface can support." 
    ::= { cevcPortEntry 3 }
 

-- UNI Service Attributes

cevcUniTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcUniEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains a list of UNIs locally configured on the
        system.

        This table has a sparse dependent relationship on the 
        cevcPortTable, containing a row for each cevcPortEntry
        having a cevcPortMode column value 'uni'."
    ::= { cevcPort 2 }

cevcUniEntry OBJECT-TYPE
    SYNTAX          CevcUniEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents an UNI and its service attributes.

        The system automatically creates an entry when the system or
        the EMS/NMS creates a row in the cevcPortTable with a 
        cevcPortMode of 'uni'.  Likewise, the system automatically
        destroys an entry when the system or the EMS/NMS destroys the
        corresponding row in the cevcPortTable."
    INDEX           { ifIndex } 
    ::= { cevcUniTable 1 }

CevcUniEntry ::= SEQUENCE {
        cevcUniIdentifier        SnmpAdminString,
        cevcUniPortType          INTEGER,
        cevcUniServiceAttributes BITS
}

cevcUniIdentifier OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies a string-value assigned to a UNI for
        identification.  When the UNI identifier is configured by the
        system or the EMS/NMS, it should be unique among all UNIs for
        the MEN.

        If the UNI identifier value is not specified, the value of the
        cevcUniIdentifier column is a zero-length string."
    REFERENCE
        "MEF 16, 'Ethernet Local Management Interface (E-LMI)', 
        January 2006" 
    ::= { cevcUniEntry 1 }

cevcUniPortType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        dot1q(1),
                        dot1ad(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the UNI port type.


        'dot1q'
            The UNI port is an IEEE 802.1q port.   


        'dot1ad'
            The UNI port is an IEEE 802.1ad port."
    DEFVAL          { dot1q } 
    ::= { cevcUniEntry 2 }

cevcUniServiceAttributes OBJECT-TYPE
    SYNTAX          BITS {
                        serviceMultiplexing(0),
                        bundling(1),
                        allToOneBundling(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the UNI service attributes.


        'serviceMultiplexing'
            This bit specifies whether the UNI supports multiple
            EVCs.  Point-to-Point EVCs and Multipoint-to-Multipoint
            EVCs may be multiplexed in any combination at the UNI 
            if this bit is set to '1'.


        'bundling'
            This bit specifies whether the UNI has the bundling
            attribute configured.  If this bit is set to '1', more
            than one CE-VLAN ID can map to a particular EVC at the
            UNI. 


        'allToOneBundling'
            This bit specifies whether the UNI has the all to one
            bundling attribute.  If this bit is set to '1', all
            CE-VLAN IDs map to a single EVC at the UNI.

        To summarize the valid combinations of serviceMultiplexing(0),
        bundling(1) and allToOneBundling(2) bits for an UNI, consider 
        the following diagram:

                   VALID COMBINATIONS
        +---------------+-------+-------+-------+-------+-------+ 
        |UNI ATTRIBUTES |   1   |   2   |   3   |   4   |   5   |
        +---------------+-------+------+------------------------+
        |Service        |       |       |       |       |       |
        |Multiplexing   |       |   Y   |   Y   |       |       |
        |               |       |       |       |       |       |
        +---------------+-------+-------+-------+-------+-------+
        |               |       |       |       |       |       |
        |Bundling       |       |       |   Y   |   Y   |       |
        |               |       |       |       |       |       |
        +---------------+-------+-------+-------+-------+-------+
        |All to One     |       |       |       |       |       |
        |Bundling       |       |       |       |       |   Y   |
        |               |       |       |       |       |       |
        +---------------+-------+-------+------ +-------+-------+"
    DEFVAL          { { serviceMultiplexing , bundling } } 
    ::= { cevcUniEntry 3 }
 

-- Table for layer 2 control protocol processing

cevcPortL2ControlProtocolTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcPortL2ControlProtocolEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table lists the layer 2 control protocol processing
        attributes at UNI ports.  

        This table has an expansion dependent relationship on the 
        cevcUniTable, containing zero or more rows for each UNI."
    ::= { cevcPort 3 }

cevcPortL2ControlProtocolEntry OBJECT-TYPE
    SYNTAX          CevcPortL2ControlProtocolEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents the layer 2 control protocol processing
        at the UNI.

        The system automatically creates an entry for each layer 2
        control protocol type when an entry is created in the
        cevcUniTable, and entries are automatically destroyed when the
        system destroys the corresponding row in the cevcUniTable."
    INDEX           {
                        ifIndex,
                        cevcPortL2ControlProtocolType
                    } 
    ::= { cevcPortL2ControlProtocolTable 1 }

CevcPortL2ControlProtocolEntry ::= SEQUENCE {
        cevcPortL2ControlProtocolType   CevcL2ControlProtocolType,
        cevcPortL2ControlProtocolAction INTEGER
}

cevcPortL2ControlProtocolType OBJECT-TYPE
    SYNTAX          CevcL2ControlProtocolType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the type of layer 2 control
        protocol service frame as denoted by the value of 
        cevcPortL2ControlProtocolAction column." 
    ::= { cevcPortL2ControlProtocolEntry 1 }

cevcPortL2ControlProtocolAction OBJECT-TYPE
    SYNTAX          INTEGER  {
                        discard(1),
                        peer(2),
                        passToEvc(3),
                        peerAndPassToEvc(4)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the action to be taken for the given
        layer 2 control protocol service frames which matches the 
        cevcPortL2ControlProtocolType, including:


            'discard' 
                The port must discard all ingress service frames
                carrying the layer 2 control protocol service
                frames and the port must not generate any egress
                service frames carrying the layer 2 control protocol
                service frames.  When this action is set at the port,
                an EVC cannot process the layer 2 control protocol
                service frames.


            'peer' 
                The port must act as a peer, meaning it actively
                participates with the Customer Equipment, in the
                operation of the layer 2 control protocol service
                frames.  An example of this is port authentication
                service at the UNI with 802.1x or enhanced link OAM
                functionality by peering at the UNI with link OAM
                (IEEE 802.3ah).  When this action is set at the port,
                an EVC cannot process the layer 2 control protocol
                service frames.


            'passToEvc'
                The disposition of the service frames which are layer 2
                control protocol service frames must be determined by
                the layer 2 control protocol action attribute of the
                EVC, (see cevcSIL2ControlProtocolAction for further
                details).


            'peerAndPassToEvc' 
                The layer 2 control protocol service frames will be
                peered at the port and also passed to one or more EVCs
                for tunneling.  An example of this possibility is where
                an 802.1x authentication frame is peered at the UNI for
                UNI-based authentication, but also passed to a given
                EVC for customer end-to-end authentication."
    DEFVAL          { discard } 
    ::= { cevcPortL2ControlProtocolEntry 2 }
 

-- Table for UNI CE-VLAN ID/EVC Map

cevcUniCEVlanEvcTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcUniCEVlanEvcEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains for each UNI, a list of EVCs and the
        association of CE-VLANs to the EVC.  The CE-VLAN mapping is 
        locally significant to the UNI.

        This table has an expansion dependent relationship on the 
        cevcUniTable, containing zero or more rows for each UNI."
    ::= { cevcPort 4 }

cevcUniCEVlanEvcEntry OBJECT-TYPE
    SYNTAX          CevcUniCEVlanEvcEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents an EVC and the CE-VLANs that are mapped
        to it at an UNI.

        For example, if CE-VLANs 10, 20-30, 40 are mapped to an EVC
        indicated by  cevcUniEvcIndex = 1, at an UNI with ifIndex = 2,
        this table will contain following rows to represent above
        CE-VLAN map:

          cevcUniCEVlanEvcEndingVlan.2.1.10 = 0
          cevcUniCEVlanEvcEndingVlan.2.1.20 = 30
          cevcUniCEVlanEvcEndingVlan.2.1.40 = 0

        The system automatically creates an entry when the system
        creates an entry in the cevcUniTable and an entry is created in
        cevcSICEVlanTable for a service instance which is attached to
        an EVC on this UNI.  Likewise, the system automatically destroys
        an entry when the system or the EMS/NMS destroys the
        corresponding row in the cevcUniTable or in the
        cevcSICEVlanTable."
    INDEX           {
                        ifIndex,
                        cevcUniEvcIndex,
                        cevcUniCEVlanEvcBeginningVlan
                    } 
    ::= { cevcUniCEVlanEvcTable 1 }

CevcUniCEVlanEvcEntry ::= SEQUENCE {
        cevcUniEvcIndex               CiscoEvcIndex,
        cevcUniCEVlanEvcBeginningVlan VlanId,
        cevcUniCEVlanEvcEndingVlan    VlanIdOrNone
}

cevcUniEvcIndex OBJECT-TYPE
    SYNTAX          CiscoEvcIndex
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates an arbitrary integer-value that uniquely
        identifies the EVC attached at an UNI." 
    ::= { cevcUniCEVlanEvcEntry 1 }

cevcUniCEVlanEvcBeginningVlan OBJECT-TYPE
    SYNTAX          VlanId
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "If cevcUniCEVlanEvcEndingVlan is '0', then this object
        indicates a single VLAN in the list.

        If cevcUniCEVlanEvcEndingVlan is not '0', then this object
        indicates the first VLAN in a range of VLANs." 
    ::= { cevcUniCEVlanEvcEntry 2 }

cevcUniCEVlanEvcEndingVlan OBJECT-TYPE
    SYNTAX          VlanIdOrNone
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the last VLAN in a range of VLANs.  If
        the row does not describe a range, then the value of this
        column must be '0'." 
    ::= { cevcUniCEVlanEvcEntry 3 }
 

-- EVC Service Attributes

cevcEvcTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcEvcEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains a list of EVCs and their service
        attributes."
    ::= { cevcEvc 1 }

cevcEvcEntry OBJECT-TYPE
    SYNTAX          CevcEvcEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents the EVC configured on the system and
        its service atrributes.

        Entries in this table may be created and deleted via the
        cevcEvcRowStatus object or the management console on the
        system.

        Using SNMP, rows are created by a SET request setting the value
        of cevcEvcRowStatus column to 'createAndGo'or 'createAndWait'. 
        Rows are deleted by a SET request setting the value of
        cevcEvcRowStatus column to 'destroy'."
    INDEX           { cevcEvcIndex } 
    ::= { cevcEvcTable 1 }

CevcEvcEntry ::= SEQUENCE {
        cevcEvcIndex       CiscoEvcIndex,
        cevcEvcRowStatus   RowStatus,
        cevcEvcStorageType StorageType,
        cevcEvcIdentifier  SnmpAdminString,
        cevcEvcType        INTEGER,
        cevcEvcCfgUnis     Unsigned32
}

cevcEvcIndex OBJECT-TYPE
    SYNTAX          CiscoEvcIndex
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates an arbitrary integer-value that uniquely
        identifies the EVC." 
    ::= { cevcEvcEntry 1 }

cevcEvcRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object enables a SNMP peer to create, modify, and
        delete rows in the cevcEvcTable. 

        cevcEvcIdentifier column must have a valid value before a 
        row can be set to 'active'.

        Writable objects in this table can be modified while the
        value of cevcEvcRowStatus column is 'active'.

        An entry cannot be deleted if there exists a service instance
        which is referring to the cevcEvcEntry i.e. cevcSIEvcIndex
        in the cevcSITable has the same value as cevcEvcIndex being
        deleted." 
    ::= { cevcEvcEntry 2 }

cevcEvcStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies how the SNMP entity stores the data
        contained by the corresponding conceptual row.

        This object can be set to either 'volatile' or 'nonVolatile'.
        Other values are not applicable for this conceptual row and
        are not supported."
    DEFVAL          { volatile } 
    ::= { cevcEvcEntry 3 }

cevcEvcIdentifier OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..100))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies a string-value identifying the EVC.
        This value should be unique across the MEN."
    REFERENCE
        "MEF 16, 'Ethernet Local Management Interface (E-LMI)', 
        January 2006" 
    ::= { cevcEvcEntry 4 }

cevcEvcType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        pointToPoint(1),
                        multipointToMultipoint(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the type of EVC:


        'pointToPoint' 
            Exactly two UNIs are associated with one another.  An
            ingress service frame at one UNI must not result in an
            egress service frame at a UNI other than the other UNI
            in the EVC.


        'multipointToMultipoint'
            Two or more UNIs are associated with one another.  An
            ingress service frame at one UNI must not result in an
            egress service frame at a UNI that is not in the EVC."
    DEFVAL          { pointToPoint } 
    ::= { cevcEvcEntry 5 }

cevcEvcCfgUnis OBJECT-TYPE
    SYNTAX          Unsigned32 (2..4294967295)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the number of UNIs expected to be
        configured for the EVC in the MEN.  The underlying OAM
        protocol can use this value of UNIs to determine the EVC
        operational status, cevcEvcOperStatus.  For a 
        Multipoint-to-Multipoint EVC the minimum number of Uni's
        would be two."
    DEFVAL          { 2 } 
    ::= { cevcEvcEntry 6 }
 


cevcEvcStateTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcEvcStateEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table lists statical/status data of the EVC.

        This table has an one-to-one dependent relationship on the
        cevcEvcTable, containing a row for each EVC."
    ::= { cevcEvc 2 }

cevcEvcStateEntry OBJECT-TYPE
    SYNTAX          CevcEvcStateEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents status atrributes of an EVC.

        The system automatically creates an entry when the system or
        the EMS/NMS creates a row in the cevcEvcTable.  Likewise, the
        system automatically destroys an entry when the system or the
        EMS/NMS destroys the corresponding row in the cevcEvcTable."
    INDEX           { cevcEvcIndex } 
    ::= { cevcEvcStateTable 1 }

CevcEvcStateEntry ::= SEQUENCE {
        cevcEvcOperStatus INTEGER,
        cevcEvcActiveUnis Gauge32
}

cevcEvcOperStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        active(2),
                        partiallyActive(3),
                        inactive(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies the operational status of the EVC:


        'unknown'
            Not enough information available regarding the EVC to
            determine the operational status at this time or EVC 
            operational status is undefined.

        'active'
            Fully operational between the UNIs in the EVC.  


        'partiallyActive'
            Capable of transferring traffic among some but not all
            of the UNIs in the EVC.  This operational status is
            applicable only for Multipoint-to-Multipoint EVCs.


        'inactive'
            Not capable of transferring traffic among any of the
            UNIs in the EVC.  

        This value is derived from data gathered by underlying OAM
        protocol." 
    ::= { cevcEvcStateEntry 1 }

cevcEvcActiveUnis OBJECT-TYPE
    SYNTAX          Gauge32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of active UNIs for the EVC
        in the MEN.  This value is derived from data gathered by 
        underlying OAM Protocol." 
    ::= { cevcEvcStateEntry 2 }
 

-- Table for UNIs (local and remote) which are part of the EVC

cevcEvcUniTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcEvcUniEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains a list of UNI's for each EVC configured
        on the device.  The UNIs can be  local (i.e. physically 
        located on the system) or remote (i.e. not physically located
        on the device).  For local UNIs, the UNI Id is the same as 
        denoted by cevcUniIdentifier with the same ifIndex value as 
        cevcEvcLocalUniIfIndex.  For remote UNIs, the underlying OAM 
        protocol, if capable, provides the UNI Id via its protocol 
        messages.

        This table has an expansion dependent relationship on the
        cevcEvcTable, containing a row for each UNI that is in
        the EVC."
    ::= { cevcEvc 3 }

cevcEvcUniEntry OBJECT-TYPE
    SYNTAX          CevcEvcUniEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents a UNI, either local or remote, in the
        EVC.

        The system automatically creates an entry, when an UNI is
        attached to the EVC.  Entries are automatically destroyed
        when the system or the EMS/NMS destroys the corresponding 
        row in the cevcEvcTable or when an UNI is removed from the
        EVC."
    INDEX           {
                        cevcEvcIndex,
                        cevcEvcUniIndex
                    } 
    ::= { cevcEvcUniTable 1 }

CevcEvcUniEntry ::= SEQUENCE {
        cevcEvcUniIndex        Unsigned32,
        cevcEvcUniId           SnmpAdminString,
        cevcEvcUniOperStatus   INTEGER,
        cevcEvcLocalUniIfIndex InterfaceIndexOrZero
}

cevcEvcUniIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4294967295)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates an arbitrary integer-value that uniquely

        identifies the UNI in an EVC." 
    ::= { cevcEvcUniEntry 1 }

cevcEvcUniId OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the string-value identifying the UNI
        that is in the EVC.  For UNI that is local, this value is the
        same as cevcUniIdentifier for the same ifIndex value as 
        cevcEvcLocalUniIfIndex.  For UNI that is not on the system, 
        this value may be derived from the underlying OAM protocol.

        If the UNI identifier value is not specified for the UNI or it
        is unknown, the value of the cevcEvcUniId column is a
        zero-length string."
    REFERENCE
        "MEF 16, Ethernet Local Management Interface (E-LMI),
         January 2006" 
    ::= { cevcEvcUniEntry 2 }

cevcEvcUniOperStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        notReachable(2),
                        up(3),
                        down(4),
                        adminDown(5),
                        localExcessiveError(6),
                        remoteExcessiveError(7),
                        localInLoopback(8),
                        remoteInLoopback(9),
                        localOutLoopback(10),
                        remoteOutLoopback(11)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the operational status derived from data
        gathered by the OAM protocol for an UNI.


            'unknown' 
                Status is not known; possible reason could be caused
                by the OAM protocol has not provided information
                regarding the UNI.


            'notReachable'
                UNI is not reachable; possible reason could be caused
                by the OAM protocol messages having not been received
                for an excessive length of time.


            'up'
                UNI is active, up, and able to pass traffic.


            'down'
                UNI is down and not passing traffic.


            'adminDown'
                UNI has been administratively put in down state.


            'localExcessiveError'
                UNI has experienced excessive number of invalid frames
                on the local end of the physical link between UNI-C 
                and UNI-N.


            'remoteExcessiveError'
                UNI has experienced excessive number of invalid frames
                on the remote side of the physical connection between
                UNI-C and UNI-N.


            'localInLoopback'
                UNI is loopback on the local end of the physical link
                between UNI-C and UNI-N.


            'remoteInLoopback'
                UNI is looped back on the remote end of the link 
                between UNI-C and UNI-N.


            'localOutLoopback'
                UNI just transitioned out of loopback on the local end
                of the physcial link between UNI-C and UNI-N.

            'remoteOutLoopback'
                UNI just transitioned out of loopback on the remote 
                end of the physcial link between UNI-C and UNI-N." 
    ::= { cevcEvcUniEntry 3 }

cevcEvcLocalUniIfIndex OBJECT-TYPE
    SYNTAX          InterfaceIndexOrZero
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "When the UNI is local on the system, this object specifies
        the ifIndex of the UNI.  The value '0' of this column
        indicates remote UNI." 
    ::= { cevcEvcUniEntry 4 }
 

-- Service Instance Table

cevcSITable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcSIEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table lists each service instance and its service
        attributes."
    ::= { cevcServiceInstance 1 }

cevcSIEntry OBJECT-TYPE
    SYNTAX          CevcSIEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents a service instance configured on the
        system and its service attributes.

        Entries in this table may be created and deleted via the
        cevcSIRowStatus object or the management console on the
        system.

        Using SNMP, rows are created by a SET request setting the value
        of cevcSIRowStatus column to 'createAndGo'or 'createAndWait'. 
        Rows are deleted by a SET request setting the value of
        cevcSIRowStatus column to 'destroy'."
    INDEX           { cevcSIIndex } 
    ::= { cevcSITable 1 }

CevcSIEntry ::= SEQUENCE {
        cevcSIIndex          Unsigned32,
        cevcSIRowStatus      RowStatus,
        cevcSIStorageType    StorageType,
        cevcSITargetType     ServiceInstanceTargetType,
        cevcSITarget         ServiceInstanceTarget,
        cevcSIName           SnmpAdminString,
        cevcSIEvcIndex       CiscoEvcIndexOrZero,
        cevcSIAdminStatus    INTEGER,
        cevcSIForwardingType INTEGER,
        cevcSICreationType   INTEGER,
        cevcSIType           INTEGER
}

cevcSIIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4294967295)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates an arbitrary integer-value that uniquely
        identifies a service instance.  An implementation MAY assign
        an ifIndex-value assigned to the service instance to
        cevcSIIndex." 
    ::= { cevcSIEntry 1 }

cevcSIRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object enables a SNMP peer to create, modify, and delete
        rows in the cevcSITable.

        This object cannot be set to 'active' until following
        corresponding objects are assigned to valid values:

           - cevcSITargetType
           - cevcSITarget
           - cevcSIName
           - cevcSIType

        Following writable objects in this table cannot be modified
        while the value of cevcSIRowStatus is 'active':

           - cevcSITargetType
           - cevcSITarget
           - cevcSIName
           - cevcSIType

        Objects in this table and all other tables that have the same
        cevcSIIndex value as an index disappear when cevcSIRowStatus is
        set to 'destroy'." 
    ::= { cevcSIEntry 2 }

cevcSIStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies how the SNMP entity stores the data
        contained by the corresponding conceptual row.

        This object can be set to either 'volatile' or 'nonVolatile'.
        Other values are not applicable for this conceptual row and
        are not supported."
    DEFVAL          { volatile } 
    ::= { cevcSIEntry 3 }

cevcSITargetType OBJECT-TYPE
    SYNTAX          ServiceInstanceTargetType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates the type of interface/media to which a
        service instance has an attachment." 
    ::= { cevcSIEntry 4 }

cevcSITarget OBJECT-TYPE
    SYNTAX          ServiceInstanceTarget
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates the target to which a service instance
        has an attachment.

        If the target is unknown, the value of the cevcSITarget column
        is a zero-length string." 
    ::= { cevcSIEntry 5 }

cevcSIName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The textual name of the service instance.  The value of this
        column should be the name of the component as assigned by the
        local interface/media type and should be be suitable for use
        in commands entered at the device's 'console'.  This might be
        text name, such as 'si1' or a simple service instance number, 
        such as '1', depending on the interface naming syntax of the
        device.

        If there is no local name or this object is otherwise not
        applicable, then this object contains a zero-length string." 
    ::= { cevcSIEntry 6 }

cevcSIEvcIndex OBJECT-TYPE
    SYNTAX          CiscoEvcIndexOrZero
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the EVC Index that the service instance
        is associated.  The value of '0' this column indicates that
        the service instance is not associated to an EVC.

        If the value of cevcSIEvcIndex column is not '0', there must
        exist an active row in the cevcEvcTable with the same index
        value for cevcEvcIndex."
    DEFVAL          { 0 } 
    ::= { cevcSIEntry 7 }

cevcSIAdminStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        up(1),
                        down(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the desired state of the Service
        Instance.  


            'up'
                Ready to transfer traffic.  When a system initializes,
                all service instances start with this state.  


            'down'
                The service instance is administratively down and is
                not capable of transferring traffic."
    DEFVAL          { up } 
    ::= { cevcSIEntry 8 }

cevcSIForwardingType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(0),
                        bridgeDomain(1)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates technique used by a service instance to
        forward service frames.

            'other'
                If the forwarding behavior of a service instance is
                not defined or unknown, this object is set to other(0).


            'bridgeDomain'
                Bridge domain is used to forward service frames by a
                service instance.  If cevcSIForwardingType is 
                'bridgeDomain(1)', there must exist an active
                row in the cevcSIForwardBdTable with the same
                index value of cevcSIIndex.  The object
                cevcSIForwardBdNumber indicates the identifier of
                the bridge domain component being used." 
    ::= { cevcSIEntry 9 }

cevcSICreationType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        static(1),
                        dynamic(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object specifies whether the service instance created
        is statically configured by the user or is dynamically created.

              'static'
                  If the service instance is configured manually this  
                  object is set to static(1).

              'dynamic'
                  If the service instance is created dynamically
                   by the first sign of life of an Ethernet frame,
                    then this object is set to dynamic(2) for 
                    the service instance." 
    ::= { cevcSIEntry 10 }

cevcSIType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        regular(1),
                        trunk(2),
                        l2context(3)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the type of the service instance. It
        mentions if the service instance is either a regular or trunk
        or l2context service instance.

                'regular'
                      If a service instance is configured without  
                      any type specified, then it is a regular service 
                      instance.
                      

                'trunk'
                      If the service instance is configured
                      with trunk type, then it is a trunk service
                      instance. For a trunk service instance,
                      its Bridge domain IDs are derived from 
                      encapsulation VLAN plus an optional offset
                       (refer cevcSIForwardBdNumberBase object).
                     

                  'l2context'
                      If the service instance is configured 
                      with dynamic type, then it is a L2 context 
                      service instance. The Ethernet L2 Context
                      is a statically configured service instance
                      which contains the Ethernet Initiator
                      for attracting the first sign of life. In other
                      words, Ethernet L2 Context service instance is
                      used for catching the first sign of life of 
                      Ethernet frames to create dynamic Ethernet 
                      sessions service instances."
    ::= { cevcSIEntry 11 }
 

-- Service Instance Attributes

cevcSIStateTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcSIStateEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table lists statical status data of the service instance.

        This table has an one-to-one dependent relationship on the
        cevcSITable, containing a row for each service instance."
    ::= { cevcServiceInstance 2 }

cevcSIStateEntry OBJECT-TYPE
    SYNTAX          CevcSIStateEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents operational status of a service instance.

        The system automatically creates an entry when the system or
        the EMS NMS creates a row in the cevcSITable.  Likewise, the
        system automatically destroys an entry when the system or the
        EMS NMS destroys the corresponding row in the cevcSITable."
    INDEX           { cevcSIIndex } 
    ::= { cevcSIStateTable 1 }

CevcSIStateEntry ::= SEQUENCE {
        cevcSIOperStatus INTEGER
}

cevcSIOperStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        up(1),
                        down(2),
                        adminDown(3),
                        deleted(4),
                        errorDisabled(5),
                        unknown(6)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the operational status of the Service
        Instance.


            'up' 
                Service instance is fully operational and able to
                transfer traffic.


            'down'
                Service instance is down and not capable of
                transferring traffic, and is not administratively
                configured to be down by management system. 


            'adminDown'
                Service instance has been explicitly configured to
                administratively down by a management system and is not
                capable of transferring traffic.


            'deleted'
                Service instance has been deleted.


            'errorDisabled'
                Service instance has been shut down due to MAC 
                security violations. 


            'unknown'
                Operational status of service instance is unknown or
                undefined." 
    ::= { cevcSIStateEntry 1 }
 

-- VLAN Rewrite Table

cevcSIVlanRewriteTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcSIVlanRewriteEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table lists the rewrite adjustments of the service
        frame's VLAN tags for service instances.

        This table has an expansion dependent relationship on the
        cevcSITable, containing a row for a VLAN adjustment
        for ingress and egress frames at each service instance."
    ::= { cevcServiceInstance 3 }

cevcSIVlanRewriteEntry OBJECT-TYPE
    SYNTAX          CevcSIVlanRewriteEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents the VLAN adjustment for a Service
        Instance."
    INDEX           {
                        cevcSIIndex,
                        cevcSIVlanRewriteDirection
                    } 
    ::= { cevcSIVlanRewriteTable 1 }

CevcSIVlanRewriteEntry ::= SEQUENCE {
        cevcSIVlanRewriteDirection     INTEGER,
        cevcSIVlanRewriteRowStatus     RowStatus,
        cevcSIVlanRewriteStorageType   StorageType,
        cevcSIVlanRewriteAction        INTEGER,
        cevcSIVlanRewriteEncapsulation INTEGER,
        cevcSIVlanRewriteVlan1         VlanId,
        cevcSIVlanRewriteVlan2         VlanId,
        cevcSIVlanRewriteSymmetric     TruthValue
}

cevcSIVlanRewriteDirection OBJECT-TYPE
    SYNTAX          INTEGER  {
                        ingress(1),
                        egress(2)
                    }
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the VLAN adjustment for 'ingress'
        frames or 'egress' frames on the service instance." 
    ::= { cevcSIVlanRewriteEntry 1 }

cevcSIVlanRewriteRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object enables a SNMP peer to create, modify, and delete
        rows in the cevcSIVlanRewriteTable.

        cevcSIVlanRewriteAction and cevcSIVlanRewriteEncapsulation must
        have valid values before this object can be set to 'active'.

        Writable objects in this table can be modified while the
        value of cevcSIVlanRewriteRowStatus column is 'active'." 
    ::= { cevcSIVlanRewriteEntry 2 }

cevcSIVlanRewriteStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies how the SNMP entity stores the data
        contained by the corresponding conceptual row.

        This object can be set to either 'volatile' or 'nonVolatile'.
        Other values are not applicable for this conceptual row and
        are not supported."
    DEFVAL          { volatile } 
    ::= { cevcSIVlanRewriteEntry 3 }

cevcSIVlanRewriteAction OBJECT-TYPE
    SYNTAX          INTEGER  {
                        push1(1),
                        push2(2),
                        pop1(3),
                        pop2(4),
                        translate1To1(5),
                        translate1To2(6),
                        translate2To1(7),
                        translate2To2(8)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the rewrite action the device performs
        for the service instance, including:

            'push1'
                Add cevcSIVlanRewriteVlan1 as the VLAN tag to the
                service frame.


            'push2'
                Add cevcSIVlanRewriteVlan1 as the outer VLAN tag 
                and cevcSIVlanRewriteVlan2 as the inner VLAN tag of
                the service frame.


            'pop1'
                Remove the outermost VLAN tag from the service frame.


            'pop2'
                Remove the two outermost VLAN tags from the service
                frame.


            'translate1To1'
                Replace the outermost VLAN tag with the 
                cevcSIVlanRewriteVlan1 tag.


           'translate1To2'
               Replace the outermost VLAN tag with
               cevcSIVlanRewriteVlan1 and add cevcSIVlanRewriteVlan2
               to the second VLAN tag of the service frame.


            'translate2To1'
                Remove the outermost VLAN tag and replace the second
                VLAN tag with cevcSIVlanVlanRewriteVlan1.


           'translate2To2'
               Replace the outermost VLAN tag with
               cevcSIVlanRewriteVlan1 and the second VLAN tag with
               cevcSIVlanRewriteVlan2." 
    ::= { cevcSIVlanRewriteEntry 4 }

cevcSIVlanRewriteEncapsulation OBJECT-TYPE
    SYNTAX          INTEGER  {
                        dot1q(1),
                        dot1ad(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the encapsulation type to
        process for the service instance.


            'dot1q'
                The IEEE 802.1q encapsulation.


            'dot1ad'
                The IEEE 802.1ad encapsulation." 
    ::= { cevcSIVlanRewriteEntry 5 }

cevcSIVlanRewriteVlan1 OBJECT-TYPE
    SYNTAX          VlanId
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the outermost VLAN ID tag of the
        frame for the service instance.  This object is valid 
        only when cevcSIVlanRewriteAction is 'push1', 'push2',
        'translate1To1', 'translate1To2', 'translate2To1', or 
        'translate2To2'." 
    ::= { cevcSIVlanRewriteEntry 6 }

cevcSIVlanRewriteVlan2 OBJECT-TYPE
    SYNTAX          VlanId
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the second VLAN ID tag of the
        frame for the service instance.  This object is valid 
        only when cevcSIVlanRewriteAction is 'push2',
        'translate1To2', or 'translate2To2'." 
    ::= { cevcSIVlanRewriteEntry 7 }

cevcSIVlanRewriteSymmetric OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is valid only when cevcSIVlanRewriteDirection is
        'ingress'.  The value 'true' of this column specifies that
        egress packets are tagged with a VLAN specified by an active
        row in cevcSIPrimaryVlanTable.

        There could only be one VLAN value assigned in the 
        cevcSIPrimaryVlanTable, i.e. only one 'active' entry
        that has the same index value of cevcSIIndex column and
        corresponding instance of cevcSIPrimaryVlanEndingVlan
        column has value '0'."
    DEFVAL          { false } 
    ::= { cevcSIVlanRewriteEntry 8 }
 

-- Table for EVC layer 2 control protocol processing

cevcSIL2ControlProtocolTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcSIL2ControlProtocolEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table lists the layer 2 control protocol processing
        attributes at service instances.  

        This table has an expansion dependent relationship on the 
        cevcSITable, containing a row for each layer 2 
        control protocol disposition at each service instance."
    ::= { cevcServiceInstance 4 }

cevcSIL2ControlProtocolEntry OBJECT-TYPE
    SYNTAX          CevcSIL2ControlProtocolEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents the layer 2 control protocol processing
        at a service instance.

        The system automatically creates an entry for each layer 2
        control protocol type when an entry is created in the
        cevcSITable, and entries are automatically destroyed when the
        system destroys the corresponding row in the cevcSITable."
    INDEX           {
                        cevcSIIndex,
                        cevcSIL2ControlProtocolType
                    } 
    ::= { cevcSIL2ControlProtocolTable 1 }

CevcSIL2ControlProtocolEntry ::= SEQUENCE {
        cevcSIL2ControlProtocolType   CevcL2ControlProtocolType,
        cevcSIL2ControlProtocolAction INTEGER
}

cevcSIL2ControlProtocolType OBJECT-TYPE
    SYNTAX          CevcL2ControlProtocolType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The layer 2 control protocol service frame that the
        service instance is to process as defined by object
        cevcSIL2ControlProtocolAction." 
    ::= { cevcSIL2ControlProtocolEntry 1 }

cevcSIL2ControlProtocolAction OBJECT-TYPE
    SYNTAX          INTEGER  {
                        discard(1),
                        tunnel(2),
                        forward(3)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The actions to be taken for a given layer 2 control protocol
        service frames that matches cevcSIL2ControlProtocolType, 
        including:


            'discard'
                The MEN must discard all ingress service frames 
                carrying the layer 2 control protocol service frames
                on the EVC and the MEN must not generate any egress
                service frames carrying the layer 2 control protocol
                frames on the EVC.


            'tunnel'
                Forward the layer 2 control protocol service frames 
                with the MAC address changed as defined by the
                individual layer 2 control protocol.  The EVC does not
                process the layer 2 protocol service frames.  If a 
                layer 2 control protocol service frame is to be
                tunneled, all the UNIs in the EVC must be configured to
                pass the layer 2 control protocol service frames to the
                EVC, cevcPortL2ControlProtocolAction column has the
                value of 'passToEvc' or 'peerAndPassToEvc'.


            'forward'
                Forward the layer 2 conrol protocol service frames as
                data; similar to tunnel but layer 2 control protocol
                service frames are forwarded without changing the MAC
                address."
    DEFVAL          { discard } 
    ::= { cevcSIL2ControlProtocolEntry 2 }
 

-- Service Instance CE-VLAN List Table

cevcSICEVlanTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcSICEVlanEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the CE-VLAN map list for each Service
        Instance.

        This table has an expansion dependent relationship on the
        cevcSITable, containing a row for each CE-VLAN or a range of
        CE-VLANs that are mapped to a service instance."
    ::= { cevcServiceInstance 5 }

cevcSICEVlanEntry OBJECT-TYPE
    SYNTAX          CevcSICEVlanEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry contains the CE-VLANs that are mapped at a Service
        Instance.

        Entries in this table may be created and deleted via the
        cevcSICEVlanRowStatus object or the management console on the
        system.

        Using SNMP, rows are created by a SET request setting the value
        of cevcSICEVlanRowStatus column to 'createAndGo' or
        'createAndWait'.  Rows are deleted by a SET request setting the
        value of cevcSICEVlanRowStatus column to 'destroy'."
    INDEX           {
                        cevcSIIndex,
                        cevcSICEVlanBeginningVlan
                    } 
    ::= { cevcSICEVlanTable 1 }

CevcSICEVlanEntry ::= SEQUENCE {
        cevcSICEVlanBeginningVlan VlanId,
        cevcSICEVlanRowStatus     RowStatus,
        cevcSICEVlanStorageType   StorageType,
        cevcSICEVlanEndingVlan    VlanIdOrNone
}

cevcSICEVlanBeginningVlan OBJECT-TYPE
    SYNTAX          VlanId
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "If cevcSICEVlanEndingVlan is '0', then this object
        indicates a single VLAN in the list.

        If cevcSICEVlanEndingVlan is not '0', then this object
        indicates the first VLAN in a range of VLANs." 
    ::= { cevcSICEVlanEntry 1 }

cevcSICEVlanRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object enables a SNMP peer to create, modify, and delete
        rows in the cevcSICEVlanTable.

        This object cannot be set to 'active' until all objects have 
        been assigned valid values.

        Writable objects in this table can be modified while the
        value of the cevcSICEVlanRowStatus column is 'active'." 
    ::= { cevcSICEVlanEntry 2 }

cevcSICEVlanStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies how the SNMP entity stores the data
        contained by the corresponding conceptual row.

        This object can be set to either 'volatile' or 'nonVolatile'.
        Other values are not applicable for this conceptual row and
        are not supported."
    DEFVAL          { volatile } 
    ::= { cevcSICEVlanEntry 3 }

cevcSICEVlanEndingVlan OBJECT-TYPE
    SYNTAX          VlanIdOrNone
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates the last VLAN in a range of VLANs.  If
        the row does not describe a range, then the value of this
        column must be '0'." 
    ::= { cevcSICEVlanEntry 4 }
 

-- Service Instance Match Criteria Table

cevcSIMatchCriteriaTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcSIMatchCriteriaEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the match criteria for each Service
        Instance.

        This table has an expansion dependent relationship on the
        cevcSITable, containing a row for each group of  match
        criteria of each service instance."
    ::= { cevcServiceInstance 6 }

cevcSIMatchCriteriaEntry OBJECT-TYPE
    SYNTAX          CevcSIMatchCriteriaEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents a group of match criteria for a service
        instance.  Each entry in the table with the same cevcSIIndex and
        different cevcSIMatchCriteriaIndex represents an OR operation of
        the match criteria for the service instance.

        Entries in this table may be created and deleted via the
        cevcSIMatchRowStatus object or the management console on the
        system.

        Using SNMP, rows are created by a SET request setting the value
        of cevcSIMatchRowStatus column to 'createAndGo' or
        'createAndWait'.  Rows are deleted by a SET request setting the
        value of cevcSIMatchRowStatus column to 'destroy'."
    INDEX           {
                        cevcSIIndex,
                        cevcSIMatchCriteriaIndex
                    } 
    ::= { cevcSIMatchCriteriaTable 1 }

CevcSIMatchCriteriaEntry ::= SEQUENCE {
        cevcSIMatchCriteriaIndex Unsigned32,
        cevcSIMatchRowStatus     RowStatus,
        cevcSIMatchStorageType   StorageType,
        cevcSIMatchCriteriaType  INTEGER
}

cevcSIMatchCriteriaIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4294967295)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates an arbitrary integer-value that uniquely
        identifies a match criteria for a service instance." 
    ::= { cevcSIMatchCriteriaEntry 1 }

cevcSIMatchRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object enables a SNMP peer to create, modify, and delete
        rows in the cevcSIMatchCriteriaTable.

        If the value of cevcSIMatchCriteriaType column is 'dot1q(1)'
        or 'dot1ad(2)' or 'untaggedAndDot1q' or 'untaggedAndDot1ad,
        then cevcSIMatchCriteriaRowStatus can not be set to 'active'
        until there exist an active row in the cevcSIMatchEncapTable
        with the same index value for cevcSIIndex and
        cevcSIMatchCriteriaIndex.

        Writable objects in this table can be modified while the
        value of the cevcSIMatchRowStatus column is 'active'." 
    ::= { cevcSIMatchCriteriaEntry 2 }

cevcSIMatchStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies how the SNMP entity stores the data
        contained by the corresponding conceptual row.

        This object can be set to either 'volatile' or 'nonVolatile'.
        Other values are not applicable for this conceptual row and
        are not supported."
    DEFVAL          { volatile } 
    ::= { cevcSIMatchCriteriaEntry 3 }

cevcSIMatchCriteriaType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(1),
                        dot1q(2),
                        dot1ad(3),
                        untagged(4),
                        untaggedAndDot1q(5),
                        untaggedAndDot1ad(6),
                        priorityTagged(7),
                        defaultTagged(8)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the criteria used to match a service
        instance.

            'unknown'
                Match criteria for the service instance is not
                defined or unknown.


            'dot1q'
                The IEEE 802.1q encapsulation is used as a match
                criteria for the service instance.  The ether type
                value of the IEEE 802.1q tag is specified by the
                object cevcSIEncapEncapsulation with the same 
                index value of cevcSIIndex and
                cevcSIMatchCreriaIndex.


            'dot1ad'
                The IEEE 802.1ad encapsulation is used as a match
                criteria for the service instance.  The ether type
                value of the IEEE 802.1ad tag is specified by the
                cevcSIEncapEncapsulation column with the same index
                value of cevcSIIndex and cevcSIMatchCreriaIndex.

            'untagged'
                Service instance processes untagged service frames.
                Only one service instance on the interface/media
                type can use untagged frames as a match criteria.


            'untaggedAndDot1q'
                Both untagged frames and the IEEE 802.1q encapsulation
                are used as a match criteria for the service instance.
                Only one service instance on the interface/media
                type can use untagged frames as a match criteria.
                The ether type value of the IEEE 802.1q tag is
                specified by the cevcSIEncapEncapsulation column
                with the same index value of cevcSIIndex and
                cevcSIMatchCreriaIndex.

            'untaggedAndDot1ad'
                Both untagged frames and the IEEE 802.1ad encapsulation
                are used as a match criteria for the service instance.
                Only one service instance on the interface/media
                type can use untagged frames as a match criteria.
                The ether type value of the IEEE 802.1ad tag is
                specified by the cevcSIEncapEncapsulation column
                with the same index value of cevcSIIndex and
                cevcSIMatchCreriaIndex.


            'priorityTagged'
                Service instance processes priority tagged frames.
                Only one service instance on the interface/media
                type can use priority tagged frames as a match 
                criteria.


            'defaultTagged'
                Service instance is a default service instance.  The
                default service instance processes frames with VLANs
                that do not match to any other service instances
                configured on the interface/media type.  Only one
                service instance on the interface/media type can be
                the default service instance." 
    ::= { cevcSIMatchCriteriaEntry 4 }
 

-- Service Instance Encapsulation Match Criteria Table

cevcSIMatchEncapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcSIMatchEncapEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the encapsulation based match criteria for
        each service instance.  

        This table has a sparse dependent relationship on the 
        cevcSIMatchCriteriaTable, containing a row for each match 
        criteria having one of the following values for 
        cevcSIMatchCriteriaType:

            - 'dot1q'
            - 'dot1ad'
            - 'untaggedAndDot1q'
            - 'untaggedAndDot1ad'
            - 'priorityTagged'"
    ::= { cevcServiceInstance 7 }

cevcSIMatchEncapEntry OBJECT-TYPE
    SYNTAX          CevcSIMatchEncapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents a group of encapulation match criteria
        for a service instance.

        Entries in this table may be created and deleted via the
        cevcSIMatchEncapRowStatus object or the management console
        on the system.

        Using SNMP, rows are created by a SET request setting the value
        of cevcSIMatchEncapRowStatus column to 'createAndGo' or
        'createAndWait'.  Rows are deleted by a SET request setting the
        value of cevcSIMatchEncapRowStatus column to 'destroy'."
    INDEX           {
                        cevcSIIndex,
                        cevcSIMatchCriteriaIndex
                    } 
    ::= { cevcSIMatchEncapTable 1 }

CevcSIMatchEncapEntry ::= SEQUENCE {
        cevcSIMatchEncapRowStatus     RowStatus,
        cevcSIMatchEncapStorageType   StorageType,
        cevcSIMatchEncapValid         BITS,
        cevcSIMatchEncapEncapsulation INTEGER,
        cevcSIMatchEncapPrimaryCos    CiscoCosList,
        cevcSIMatchEncapSecondaryCos  CiscoCosList,
        cevcSIMatchEncapPayloadType   INTEGER,
        cevcSIMatchEncapPayloadTypes  BITS,
        cevcSIMatchEncapPriorityCos   CiscoCosList
}

cevcSIMatchEncapRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object enables a SNMP peer to create, modify, and delete
        rows in the cevcSIMatchEncapTable.

        This object cannot be set to 'active' until
        cevcSIEncapEncapsulation and objects referred by 
        cevcSIMatchEncapValid have been assigned their respective
        valid values.

        Writable objects in this table can be modified while the value
        of the cevcSIEncapMatchRowStatus column is 'active'." 
    ::= { cevcSIMatchEncapEntry 1 }

cevcSIMatchEncapStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies how the SNMP entity stores the data
        contained by the corresponding conceptual row.

        This object can be set to either 'volatile' or 'nonVolatile'.
        Other values are not applicable for this conceptual row and
        are not supported."
    DEFVAL          { volatile } 
    ::= { cevcSIMatchEncapEntry 2 }

cevcSIMatchEncapValid OBJECT-TYPE
    SYNTAX          BITS {
                        primaryCos(0),
                        secondaryCos(1),
                        payloadType(2),
                        payloadTypes(3),
                        priorityCos(4),
                        dot1qNativeVlan(5),
                        dot1adNativeVlan(6),
                        encapExact(7)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the encapsulation criteria used to match
        a service instance.


            'primaryCos'
                The 'primaryCos' bit set to '1' specifies the
                Class of Service is used as service match criteria for
                the service instance.  When this bit is set to '1'
                there must exist aleast one active rows in the
                cevcSIPrimaryVlanTable which has the same index values
                of cevcSIIndex and cevcSIMatchCriteriaIndex.  When
                'primaryCos' bit is '1', the cevcSIPrimaryCos column
                indicates the CoS value(s).

            'secondaryCos'
                The 'secondaryCos' bit set to '1' specifies the
                Class of Service is used as service match criteria for
                the service instance.  When this bit is set to '1'
                there must exist aleast one active rows in the
                cevcSISecondaryVlanTable which has the same index
                values of cevcSIIndex and cevcSIMatchCriteriaIndex.
                When 'secondaryCos' bit is '1', the
                cevcSISecondaryCos column indicates the CoS 
                value(s).


            'payloadType'
                This bit set to '1' specifies that the value of
                corresponding instance of cevcSIMatchEncapPayloadType
                is used as service match criteria for the service
                instance.


            'payloadTypes'
                This bit set to '1' specifies that the value of
                corresponding instance of cevcSIMatchEncapPayloadTypes
                is used as service match criteria for the service
                instance.


            'priorityCos'
                This bit set to '1' specifies that the value of
                corresponding instance of cevcSIMatchEncapPriorityCos
                is used as service match criteria for the service
                instance.


            'dot1qNativeVlan'
                This bit set to '1' specifies that the IEEE 802.1q
                tag with native vlan is used as service match 
                criteria for the service instance.


            'dot1adNativeVlan'
                This bit set to '1' specifies that the IEEE 802.1ad
                tag with native vlan is used as service match 
                criteria for the service instance.


            'encapExact'
                This bit set to '1' specifies that a service frame is
                mapped to the service instance only if it matches
                exactly to the encapsulation specified by the service
                instance." 
    ::= { cevcSIMatchEncapEntry 3 }

cevcSIMatchEncapEncapsulation OBJECT-TYPE
    SYNTAX          INTEGER  {
                        dot1qEthertype0x8100(1),
                        dot1qEthertype0x9100(2),
                        dot1qEthertype0x9200(3),
                        dot1qEthertype0x88A8(4),
                        dot1adEthertype0x88A8(5),
                        dot1ahEthertype0x88A8(6)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the encapsulation type used as service
        match criteria.  The object also specifies the Ethertype for
        egress packets on the service instance.


            'dot1qEthertype0x8100'
                The IEEE 801.1q encapsulation with ether type value
                0x8100.


            'dot1qEthertype0x9100'
                The IEEE 801.1q encapsulation with ether type value
                0x9100.


            'dot1qEthertype0x9200'
                The IEEE 801.1q encapsulation with ether type value
                0x9200.


            'dot1qEthertype0x88A8'
                 The IEEE 801.1q encapsulation with ether type value
                 0x88A8.


            'dot1adEthertype0x88A8'
                The IEEE 801.1ad encapsulation with ether type value
                0x88A8.


            'dot1ahEthertype0x88A8'
                The IEEE 801.1ah encapsulation with ether type value
                0x88A8." 
    ::= { cevcSIMatchEncapEntry 4 }

cevcSIMatchEncapPrimaryCos OBJECT-TYPE
    SYNTAX          CiscoCosList
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the CoS values which the Service
        Instance uses as service match criteria.  This object is valid
        only when 'primaryVlans' and 'primaryCos' bits are set to '1'
        in corresponding instance of the object
        cevcSIMatchEncapValid." 
    ::= { cevcSIMatchEncapEntry 5 }

cevcSIMatchEncapSecondaryCos OBJECT-TYPE
    SYNTAX          CiscoCosList
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the CoS values which the Service
        Instance uses as service match criteria.  This object is valid
        only when 'secondaryVlans' and 'secondaryCos' bits are set to
        '1' in corresponding instance of the object
        cevcSIMatchEncapValid." 
    ::= { cevcSIMatchEncapEntry 6 }

cevcSIMatchEncapPayloadType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        other(1),
                        payloadType0x0800ip(2)
                    }
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "This object specifies the PayloadType(etype/protocol type)
        values that the service instance uses as a service match
        criteria.  This object is required when the forwarding of
        layer-2 ethernet packet is done through the payloadType i.e IP
        etc.


            'other'
                None of the following.


            'payloadType0x0800ip'
                Payload type value for IP is 0x0800.


        This object is valid only when 'payloadType' bit is set to '1'
        in corresponding instance of the object 
        cevcSIMatchEncapValid.

        This object is deprecated by cevcSIMatchEncapPayloadTypes." 
    ::= { cevcSIMatchEncapEntry 7 }

cevcSIMatchEncapPayloadTypes OBJECT-TYPE
    SYNTAX          BITS {
                        payloadTypeIPv4(0),
                        payloadTypeIPv6(1),
                        payloadTypePPPoEDiscovery(2),
                        payloadTypePPPoESession(3),
                        payloadTypePPPoEAll(4)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the etype/protocol type values that
        service instance uses as a service match criteria.  This
        object is required when the forwarding of layer-2 ethernet
        packet is done through the payload ether type i.e IP etc.


            'payloadTypeIPv4'
                Ethernet payload type value for IPv4 protocol.


            'payloadTypeIPv6'
                Ethernet payload type value for IPv6 protocol.


            'payloadTypePPPoEDiscovery'
                Ethernet payload type value for PPPoE discovery
                stage.


            'payloadTypePPPoESession'
                Ethernet payload type value for PPPoE session
                stage.


            'payloadTypePPPoEAll'
                All ethernet payload type values for PPPoE protocol.

        This object is valid only when 'payloadTypes' bit is set to
        '1' in corresponding instance of the object
        cevcSIMatchEncapValid.

        This object deprecates cevcSIMatchEncapPayloadType." 
    ::= { cevcSIMatchEncapEntry 8 }

cevcSIMatchEncapPriorityCos OBJECT-TYPE
    SYNTAX          CiscoCosList
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the priority CoS values which the
        service instance uses as service match criteria.  This 
        object is valid only when 'priorityCos' bit is set to '1'
        in corresponding instance of the object cevcSIMatchEncapValid." 
    ::= { cevcSIMatchEncapEntry 9 }
 

-- Service Instance Primary Vlan List Table

cevcSIPrimaryVlanTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcSIPrimaryVlanEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the primary VLAN ID list for each Service
        Instance.

        This table has an expansion dependent relationship on the 
        cevcSIMatchEncapTable, containing zero or more rows for each 
        encapsulation match criteria."
    ::= { cevcServiceInstance 8 }

cevcSIPrimaryVlanEntry OBJECT-TYPE
    SYNTAX          CevcSIPrimaryVlanEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry specifies a single VLAN or a range of VLANs
        contained in the primary VLAN list that's part of the 
        encapsulation match criteria.

        Entries in this table may be created and deleted via the
        cevcSIPrimaryVlanRowStatus object or the management console
        on the system.

        Using SNMP, rows are created by a SET request setting the value
        of the cevcSIPrimaryVlanRowStatus column to 'createAndGo' or
        'createAndWait'.  Rows are deleted by a SET request setting the
        value of the cevcSIPrimaryVlanRowStatus column to 'destroy'."
    INDEX           {
                        cevcSIIndex,
                        cevcSIMatchCriteriaIndex,
                        cevcSIPrimaryVlanBeginningVlan
                    } 
    ::= { cevcSIPrimaryVlanTable 1 }

CevcSIPrimaryVlanEntry ::= SEQUENCE {
        cevcSIPrimaryVlanBeginningVlan VlanId,
        cevcSIPrimaryVlanRowStatus     RowStatus,
        cevcSIPrimaryVlanStorageType   StorageType,
        cevcSIPrimaryVlanEndingVlan    VlanIdOrNone
}

cevcSIPrimaryVlanBeginningVlan OBJECT-TYPE
    SYNTAX          VlanId
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "If cevcSIPrimaryVlanEndingVlan is '0', then this object
        indicates a single VLAN in the list.

        If cevcSIPrimaryVlanEndingVlan is not '0', then this object
        indicates the first VLAN in a range of VLANs." 
    ::= { cevcSIPrimaryVlanEntry 1 }

cevcSIPrimaryVlanRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object enables a SNMP peer to create, modify, and delete
        rows in the cevcSIPrimaryVlanTable.

        This column cannot be set to 'active' until all objects have 
        been assigned valid values.

        Writable objects in this table can be modified while the
        value of the cevcSIPrimaryVlanRowStatus column is 'active'." 
    ::= { cevcSIPrimaryVlanEntry 2 }

cevcSIPrimaryVlanStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies how the SNMP entity stores the data
        contained by the corresponding conceptual row.

        This object can be set to either 'volatile' or 'nonVolatile'.
        Other values are not applicable for this conceptual row and
        are not supported."
    DEFVAL          { volatile } 
    ::= { cevcSIPrimaryVlanEntry 3 }

cevcSIPrimaryVlanEndingVlan OBJECT-TYPE
    SYNTAX          VlanIdOrNone
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates the last VLAN in a range of VLANs.  If
        the row does not describe a range, then the value of this
        column must be '0'." 
    ::= { cevcSIPrimaryVlanEntry 4 }
 

-- Service Instance Secondary Vlan List Table

cevcSISecondaryVlanTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcSISecondaryVlanEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the seconadary VLAN ID list for each
        service instance.

        This table has an expansion dependent relationship on the 
        cevcSIMatchEncapTable, containing zero or more rows for each 
        encapsulation match criteria."
    ::= { cevcServiceInstance 9 }

cevcSISecondaryVlanEntry OBJECT-TYPE
    SYNTAX          CevcSISecondaryVlanEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry specifies a single VLAN or a range of VLANs
        contained in the secondary VLAN list that's part of the 
        encapsulation match criteria.

        Entries in this table may be created and deleted via the
        cevcSISecondaryVlanRowStatus object or the management console
        on the system.

        Using SNMP, rows are created by a SET request setting the value
        of the cevcSISecondaryVlanRowStatus column to 'createAndGo' or
        'createAndWait'.  Rows are deleted by a SET request setting the
        value of the cevcSISecondaryVlanRowStatus column to 'destroy'."
    INDEX           {
                        cevcSIIndex,
                        cevcSIMatchCriteriaIndex,
                        cevcSISecondaryVlanBeginningVlan
                    } 
    ::= { cevcSISecondaryVlanTable 1 }

CevcSISecondaryVlanEntry ::= SEQUENCE {
        cevcSISecondaryVlanBeginningVlan VlanId,
        cevcSISecondaryVlanRowStatus     RowStatus,
        cevcSISecondaryVlanStorageType   StorageType,
        cevcSISecondaryVlanEndingVlan    VlanIdOrNone
}

cevcSISecondaryVlanBeginningVlan OBJECT-TYPE
    SYNTAX          VlanId
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "If cevcSISecondaryVlanEndingVlan is '0', then this object
        indicates a single VLAN in the list.

        If cevcSISecondaryVlanEndingVlan is not '0', then this
        object indicates the first VLAN in a range of VLANs." 
    ::= { cevcSISecondaryVlanEntry 1 }

cevcSISecondaryVlanRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object enables a SNMP peer to create, modify, and delete
        rows in the cevcSISecondaryVlanTable.

        This column can not be set to 'active' until all objects have 
        been assigned valid values.

        Writable objects in this table can be modified while the
        value of cevcSISecondaryVlanRowStatus column is 'active'." 
    ::= { cevcSISecondaryVlanEntry 2 }

cevcSISecondaryVlanStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies how the SNMP entity stores the data
        contained by the corresponding conceptual row.

        This object can be set to either 'volatile' or 'nonVolatile'.
        Other values are not applicable for this conceptual row and
        are not supported."
    DEFVAL          { volatile } 
    ::= { cevcSISecondaryVlanEntry 3 }

cevcSISecondaryVlanEndingVlan OBJECT-TYPE
    SYNTAX          VlanIdOrNone
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates the last VLAN in a range of VLANs.  If
        the row does not describe a range, then the value of this
        column must be '0'." 
    ::= { cevcSISecondaryVlanEntry 4 }
 

-- Service Instance Forwarding Bridge Domain Table

cevcSIForwardBdTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CevcSIForwardBdEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the forwarding bridge domain information
        for each service instance.

        This table has a sparse dependent relationship on the 
        cevcSITable, containing a row for each service instance having 
        a cevcSIForwardingType of 'bridgeDomain'."
    ::= { cevcServiceInstance 10 }

cevcSIForwardBdEntry OBJECT-TYPE
    SYNTAX          CevcSIForwardBdEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This entry represents an bridged domain used to forward service
        frames by the service instance.

        Entries in this table may be created and deleted via the
        cevcSIForwardBdRowStatus object or the management console
        on the system.

        Using SNMP, rows are created by a SET request setting the value
        of the cevcSIForwardBdRowStatus column to 'createAndGo' or
        'createAndWait'.  Rows are deleted by a SET request setting the
        value of the cevcSIForwardBdRowStatus column to 'destroy'."
    INDEX           { cevcSIIndex } 
    ::= { cevcSIForwardBdTable 1 }

CevcSIForwardBdEntry ::= SEQUENCE {
        cevcSIForwardBdRowStatus      RowStatus,
        cevcSIForwardBdStorageType    StorageType,
        cevcSIForwardBdNumber         Unsigned32,
        cevcSIForwardBdNumberBase     INTEGER,
        cevcSIForwardBdNumber1kBitmap OCTET STRING,
        cevcSIForwardBdNumber2kBitmap OCTET STRING,
        cevcSIForwardBdNumber3kBitmap OCTET STRING,
        cevcSIForwardBdNumber4kBitmap OCTET STRING
}

cevcSIForwardBdRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object enables a SNMP peer to create, modify, and delete
        rows in the cevcSIForwardBdTable.

        This column can not be set to 'active' until all objects have 
        been assigned valid values.

        Writable objects in this table can be modified while the
        value of the cevcSIForwardBdRowStatus column is 'active'." 
    ::= { cevcSIForwardBdEntry 1 }

cevcSIForwardBdStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies how the SNMP entity stores the data
        contained by the corresponding conceptual row.

        This object can be set to either 'volatile' or 'nonVolatile'.
        Other values are not applicable for this conceptual row and
        are not supported."
    DEFVAL          { volatile } 
    ::= { cevcSIForwardBdEntry 2 }

cevcSIForwardBdNumber OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "The bridge domain identifier that is associated with the
        service instance.

        A bridge domain refers to a layer 2 broadcast domain spanning
        a set of physical or virtual ports.  Frames are switched 
        Multicast and unknown destination unicast frames are flooded
        within the confines of the bridge domain."
        
    ::= { cevcSIForwardBdEntry 3 }

cevcSIForwardBdNumberBase OBJECT-TYPE
    SYNTAX    INTEGER  {
                        bdNumBase0(0),
                        bdNumBase4096(4096),
                        bdNumBase8192(8192),
                        bdNumBase12288(12288),
                        bdNumBase16384(16384)
                    }

    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
      "This object specifies the base of bridge domain. The bridge
	   domain range is 1~16k, cevcSIForwardBdNumberBase is to track what
	   is the base of each 4k bitmap. In this way we can specify all the 
	   16k bridge domains using four 1k bitmaps and having the base which
	   describes that is the base of each 4k bitmap. The four 1k bitmaps,
       cevcSIForwardBdNumber1kBitmap represents 0~1023,
	   cevcSIForwardBdNumber2kBitmap represents 1024~2047,
	   cevcSIForwardBdNumber3kBitmap represents 2048~3071,
	   cevcSIForwardBdNumber4kBitmap represents 3072~4095
	   And cevcSIForwardBdNumberBase is one of 0, 4096, 8192, 12288, 
	   16384.
       SNMP Administrator can use cevcSIForwardBdNumberBase + (position 
       of the set bit in four 1k bitmaps) to get BD number of a 
       service instance."   
    ::= { cevcSIForwardBdEntry 4 }

cevcSIForwardBdNumber1kBitmap OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE(0..128))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies a string of octets containing one bit 
        per Bridge domain per service instance(generally we have one
        bridge domain per nontrunk service instance but can have more
        than one bridge configured with a trunk service instance).
        The first octet corresponds to Bridge domains with 
        Bridge domain ID values of 0 through 7; the second octet to
        Bridge domains 8 through 15; etc. Thus, this 128-octet bitmap
        represents bridge domain ID value 0~1023.
        
        For each Bridge domain configured, the bit corresponding to
        that bridge domain is set to '1'. SNMP Administrator uses
        cevcSIForwardBdNumberBase + (position of the set bit in 
        bitmap)to calculate BD number of a service instance.
        
        Note that if the length of this string is less than 128 octets, 
        any 'missing' octets are assumed to contain the value zero. An 
        NMS may omit any zero-valued octets from the end of this string 
        in order to reduce SetPDU size, and the agent may also omit 
        zero-valued trailing octets, to reduce the size of GetResponse 
        PDUs."   
    DEFVAL { "" }    
    ::= { cevcSIForwardBdEntry 5 }

cevcSIForwardBdNumber2kBitmap OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE(0..128))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
         "This object specifies a string of octets containing one bit 
        per Bridge domain per service instance(generally we have one
        bridge domain per nontrunk service instance but can have more
        than one bridge configured with a trunk service instance).
        The first octet corresponds to Bridge domains with 
        Bridge domain ID values of 1024 through 1031; the second 
        octet to Bridge domains 1032 through 1039; etc. Thus, this 
        128-octet bitmap represents bridge domain ID value 1024~2047.

        For each Bridge domain configured, the bit corresponding to
        that bridge domain is set to 1. SNMP Administrator uses
        cevcSIForwardBdNumberBase + (position of the set bit in 
        bitmap)to calculate BD number of a service instance.  
        
        Note that if the length of this string is less than 128 octets, 
        any 'missing' octets are assumed to contain the value zero. An 
        NMS may omit any zero-valued octets from the end of this string 
        in order to reduce SetPDU size, and the agent may also omit 
        zero-valued trailing octets, to reduce the size of GetResponse 
        PDUs."      
    DEFVAL { "" }     
    ::= { cevcSIForwardBdEntry 6 }

cevcSIForwardBdNumber3kBitmap OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE(0..128))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies a string of octets containing one bit
        per Bridge domain per service instance(generally we have one
        bridge domain per non-trunk service instance but can have more
        than one bridge configured with a trunk service instance).
        The first octet corresponds to Bridge domains with Bridgedomain
        ID values of 2048 through 2055; the second octet to Bridge 
        domains 2056 through 2063; etc. Thus, this 128-octet bitmap
        represents bridge domain ID value 2048~3071.
        
        For each Bridge domain configured, the bit corresponding to
        that bridge domain is set to 1. SNMP Administrator uses
        cevcSIForwardBdNumberBase + (position of the set bit in
         bitmap)to calculate BD number of a service instance.  
        
        Note that if the length of this string is less than 128 octets, 
        any 'missing' octets are assumed to contain the value zero. An 
        NMS may omit any zero-valued octets from the end of this string 
        in order to reduce SetPDU size, and the agent may also omit 
        zero-valued trailing octets, to reduce the size of GetResponse 
        PDUs."
    DEFVAL { "" }    
    ::= { cevcSIForwardBdEntry 7 }

cevcSIForwardBdNumber4kBitmap OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE(0..128))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies a string of octets containing one bit 
        per Bridge domain per service instance(generally we have one
        bridge domain per non-trunk service instance but can have more
        than one bridge configured with a trunk service instance).
        The first octet corresponds to Bridge domains with 
        Bridgedomain ID values of 3078 through 3085; the second octet 
        to Bridge domains 3086 through 3093; etc. Thus, this 128-octet
         bitmap represents bridge domain ID value 3072~4095.

        For each Bridge domain configured, the bit corresponding to
        that bridge domain is set to 1. SNMP Administrator uses
        cevcSIForwardBdNumberBase + (position of the set bit in
         bitmap)to calculate BD number of a service instance.  
        
        Note that if the length of this string is less than 128 octets, 
        any 'missing' octets are assumed to contain the value zero. An 
        NMS may omit any zero-valued octets from the end of this string 
        in order to reduce SetPDU size, and the agent may also omit 
        zero-valued trailing octets, to reduce the size of GetResponse 
        PDUs." 
    DEFVAL { "" }    
    ::= { cevcSIForwardBdEntry 8 }
 


-- Notification Configuration

cevcEvcNotifyEnabled OBJECT-TYPE
    SYNTAX          BITS {
                        status(0),
                        creation(1),
                        deletion(2),
                        macSecurityViolation(3)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the system generation of notification,
        including:

            'status'
                This bit set to '1' specifies the system 
                generation of cevcEvcStatusChangedNotification.


            'creation'
                This bit set to '1' specifies the system
               generation of cevcEvcCreationNotification.


            'deletion'
                This bit set to '1' specifices the system
                generation of cevcEvcDeletionNotification.
                
            'macSecurityViolation'
              This bit set to '1' specifies the system 
              generation of cevcMacSecurityViolation." 
                          
    ::= { cevcEvcNotificationConfig 1 }


-- Notifications

ciscoEvcNotificationPrefix  OBJECT IDENTIFIER
    ::= { ciscoEvcMIBNotifications 0 }


cevcEvcStatusChangedNotification NOTIFICATION-TYPE
    OBJECTS         {
                        cevcEvcOperStatus,
                        cevcEvcCfgUnis,
                        cevcEvcActiveUnis
                    }
    STATUS          current
    DESCRIPTION
        "A device generates this notification when an EVC's
        operational status changes, or the number of active UNIs 
        associated with the EVC (cevcNumActiveUnis) changes."
   ::= { ciscoEvcNotificationPrefix 1 }

cevcEvcCreationNotification NOTIFICATION-TYPE
    OBJECTS         { cevcEvcOperStatus }
    STATUS          current
    DESCRIPTION
        "A device generates this notification upon the creation of an
        EVC."
   ::= { ciscoEvcNotificationPrefix 2 }

cevcEvcDeletionNotification NOTIFICATION-TYPE
    OBJECTS         { cevcEvcOperStatus }
    STATUS          current
    DESCRIPTION
        "A device generates this notification upon the deletion of
        an EVC."
   ::= { ciscoEvcNotificationPrefix 3 }

cevcMacSecurityViolationNotification NOTIFICATION-TYPE
    OBJECTS         {
                        ifIndex,
                        cevcSIForwardBdNumberBase,
                        cevcSIForwardBdNumber1kBitmap,
                        cevcSIForwardBdNumber2kBitmap,
                        cevcSIForwardBdNumber3kBitmap,
                        cevcSIForwardBdNumber4kBitmap,
                        cevcSIID,
                        cevcMacAddress,
                        cevcMaxMacConfigLimit,
                        cevcViolationCause
                    }
    STATUS          current
    DESCRIPTION
        "A SNMP entity generates this notification
         in the following cases: 

        When the system MAC Address limit is exceeded, the
        cevcMacSecurityViolationCauseType will contain 
        'exceedSystemLimit' value.

        When the Bridge domain limit is exceeded, the
        cevcMacSecurityViolationCauseType will contain 
        'exceedBdLimit' value.

        When the Service Instance limit is exceeded, the
        cevcMacSecurityViolationCauseType will contain 
        'exceedSILimit' value.

        If the MAC address is present in the Black list
        then cevcMacSecurityViolationCauseType will contain 
        'blackListDeny' value.
        
        Description of all the varbinds for this Notification is
        as follows:
        
        ifIndex indicates the interface index which identifies
        the interface that the service instance is attached.
        
        cevcSIForwardBdNumberBase indicates the base of bridge domain.
        The bridge domain range is 1~16k, this object is to track the
         base of each 4k bitmap.
         
        cevcSIForwardBdNumber1kBitmap indicates a string of octets 
        containing one bit per Bridge domain per service instance. This
        128-octet bitmap represents bridge domain ID values 0~1023.
        
        cevcSIForwardBdNumber2kBitmap indicates a string of octets 
        containing one bit per Bridge domain per service instance. This
        128-octet bitmap represents bridge domain ID values 1024~2047.
        
        cevcSIForwardBdNumber3kBitmap indicates a string of octets 
        containing one bit per Bridge domain per service instance. This
        128-octet bitmap represents bridge domain ID values 2048~3071.
        
        cevcSIForwardBdNumber4kBitmap indicates a string of octets 
        containing one bit per Bridge domain per service instance. This
        128-octet bitmap represents bridge domain ID values 3072~4095.
          
        cevcSIID indicates the service instance ID for the Mac
        security violation notification.
        
        cevcMacAddress indicates the Mac address which has violated
        the Mac security rules.
         
        cevcMaxMacConfigLimit indicates the maximum Mac configuration 
        limit. This is also sent as a part of Mac security violation 
        notification.
        
        cevcViolationCause indicates the Mac security violation cause."
   ::= { ciscoEvcNotificationPrefix 4 }
-- Conformance Information

ciscoEvcMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoEvcMIBConformance 1 }

ciscoEvcMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoEvcMIBConformance 2 }


ciscoEvcMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The new compliance statement for entities which implement
        the CISCO-EVC-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cevcSystemGroup,
                        cevcPortGroup,
                        cevcEvcGroup,
                        cevcSIGroup,
                        cevcEvcNotificationConfigGroup,
                        cevcEvcNotificationGroup
                    }

    GROUP           cevcSICosMatchCriteriaGroup
    DESCRIPTION
        "This group is optional for Cos MatchCriteria."

    GROUP           cevcSIVlanRewriteGroup
    DESCRIPTION
        "This group is optional for the Vlan Rewrite for Service
        Instance."

    GROUP           cevcSIMatchCriteriaGroup
    DESCRIPTION
        "This group is optional for the Match Criteria information of
        of a service instance."

    GROUP           cevcSIForwardGroup
    DESCRIPTION
        "This group is optional for the Forwarding information of
        service instance."

    OBJECT          cevcPortL2ControlProtocolAction
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcUniIdentifier
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcUniPortType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcUniServiceAttributes
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcEvcIdentifier
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcEvcType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcEvcCfgUnis
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcEvcStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcEvcRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSITargetType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSITarget
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapEncapsulation
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapPrimaryCos
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapSecondaryCos
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapPayloadType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIName
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIEvcIndex
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIAdminStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIL2ControlProtocolAction
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteAction
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteEncapsulation
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteVlan1
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteVlan2
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteSymmetric
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcEvcNotifyEnabled
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIForwardingType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSICEVlanRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchCriteriaType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSICEVlanStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIPrimaryVlanRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIPrimaryVlanStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapValid
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSICEVlanEndingVlan
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIPrimaryVlanEndingVlan
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSISecondaryVlanRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSISecondaryVlanStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSISecondaryVlanEndingVlan
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIForwardBdRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIForwardBdStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIForwardBdNumber
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { ciscoEvcMIBCompliances 1 }

ciscoEvcMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities which implement
        the CISCO-EVC-MIB.

        This compliance module deprecates
        ciscoEvcMIBCompliance."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cevcSystemGroup,
                        cevcPortGroup,
                        cevcEvcGroup,
                        cevcSIGroup,
                        cevcEvcNotificationConfigGroup,
                        cevcEvcNotificationGroup
                    }

    GROUP           cevcSICosMatchCriteriaGroup
    DESCRIPTION
        "This group is optional for Cos MatchCriteria."

    GROUP           cevcSIVlanRewriteGroup
    DESCRIPTION
        "This group is optional for the Vlan Rewrite for Service
        Instance."

    GROUP           cevcSIMatchCriteriaGroupRev1
    DESCRIPTION
        "This group is optional for the Match Criteria information of
        of a service instance."

    GROUP           cevcSIForwardGroup
    DESCRIPTION
        "This group is optional for the Forwarding information of
        service instance."

    OBJECT          cevcPortMode
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcUniIdentifier
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcUniPortType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcUniServiceAttributes
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcPortL2ControlProtocolAction
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcEvcRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcEvcStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcEvcIdentifier
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcEvcType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcEvcCfgUnis
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSITargetType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSITarget
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIName
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIEvcIndex
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIAdminStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIForwardingType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteAction
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteEncapsulation
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteVlan1
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteVlan2
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIVlanRewriteSymmetric
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIL2ControlProtocolAction
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSICEVlanRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSICEVlanStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSICEVlanEndingVlan
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchCriteriaType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapValid
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapEncapsulation
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapPrimaryCos
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapSecondaryCos
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapPayloadTypes
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIMatchEncapPriorityCos
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIPrimaryVlanRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIPrimaryVlanStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIPrimaryVlanEndingVlan
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSISecondaryVlanRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSISecondaryVlanStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSISecondaryVlanEndingVlan
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIForwardBdRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIForwardBdStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcSIForwardBdNumber
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT          cevcEvcNotifyEnabled
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { ciscoEvcMIBCompliances 2 }

ciscoEvcMIBComplianceRev2 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for entities which implement
        the CISCO-EVC-MIB.

        This compliance module deprecates
        ciscoEvcMIBComplianceRev1."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cevcSystemGroup,
                        cevcPortGroup,
                        cevcEvcGroup,
                        cevcSIGroupRev1,
                        cevcEvcNotificationConfigGroup,
                        cevcEvcNotificationGroupRev1
                    }

    GROUP           cevcSICosMatchCriteriaGroup
    DESCRIPTION
        "This group is optional for Cos MatchCriteria."

    GROUP           cevcSIVlanRewriteGroup
    DESCRIPTION
        "This group is optional for the Vlan Rewrite for Service
        Instance."

    GROUP           cevcSIMatchCriteriaGroupRev1
    DESCRIPTION
        "This group is optional for the Match Criteria information of
        of a service instance."

    GROUP           cevcSIForwardGroupRev1
    DESCRIPTION
        "This group is optional for the Forwarding information of
        service instance."

    GROUP           cevcMacSecurityViolationGroup
    DESCRIPTION
        "This group is optional for Mac Security Violation for any 
         of the following cases:
			- System Mac address limit exceeded
			- Bridge domain limit exceeded
			- Service Instance limit exceeded
			- If the Mac address is present in Black list"

    OBJECT          cevcPortMode
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write Access not required"

    OBJECT          cevcUniIdentifier
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcUniPortType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcUniServiceAttributes
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcPortL2ControlProtocolAction
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcEvcRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcEvcIdentifier
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcEvcType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcEvcCfgUnis
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIVlanRewriteRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSITargetType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSITarget
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIName
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIEvcIndex
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIAdminStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIForwardingType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIVlanRewriteStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIVlanRewriteAction
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIVlanRewriteEncapsulation
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIVlanRewriteVlan1
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIVlanRewriteVlan2
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIVlanRewriteSymmetric
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSICEVlanRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSICEVlanStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSICEVlanEndingVlan
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIMatchRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIMatchStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIMatchCriteriaType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIMatchEncapRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIMatchEncapStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIMatchEncapValid
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIMatchEncapEncapsulation
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIMatchEncapPrimaryCos
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIMatchEncapSecondaryCos
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIMatchEncapPayloadTypes
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIMatchEncapPriorityCos
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIPrimaryVlanRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIPrimaryVlanStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIPrimaryVlanEndingVlan
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSISecondaryVlanRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSISecondaryVlanStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSISecondaryVlanEndingVlan
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIForwardBdRowStatus
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIForwardBdStorageType
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIForwardBdNumberBase
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIForwardBdNumber1kBitmap
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIForwardBdNumber2kBitmap
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIForwardBdNumber3kBitmap
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcSIForwardBdNumber4kBitmap
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"

    OBJECT          cevcEvcNotifyEnabled
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access not required"
    ::= { ciscoEvcMIBCompliances 3 }

-- Units of Conformance

cevcSystemGroup OBJECT-GROUP
    OBJECTS         {
                        cevcMaxNumEvcs,
                        cevcNumCfgEvcs
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing system configuration
        of EVCs."
    ::= { ciscoEvcMIBGroups 1 }

cevcPortGroup OBJECT-GROUP
    OBJECTS         {
                        cevcPortMode,
                        cevcPortMaxNumEVCs,
                        cevcPortMaxNumServiceInstances,
                        cevcPortL2ControlProtocolAction,
                        cevcUniIdentifier,
                        cevcUniPortType,
                        cevcUniServiceAttributes,
                        cevcUniCEVlanEvcEndingVlan
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing configuration
        for ports in an EVC."
    ::= { ciscoEvcMIBGroups 2 }

cevcEvcGroup OBJECT-GROUP
    OBJECTS         {
                        cevcEvcIdentifier,
                        cevcEvcType,
                        cevcEvcOperStatus,
                        cevcEvcCfgUnis,
                        cevcEvcActiveUnis,
                        cevcEvcStorageType,
                        cevcEvcRowStatus,
                        cevcEvcUniId,
                        cevcEvcUniOperStatus,
                        cevcEvcLocalUniIfIndex
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing configuration and
        status information for EVCs."
    ::= { ciscoEvcMIBGroups 3 }

cevcSIGroup OBJECT-GROUP
    OBJECTS         {
                        cevcSIName,
                        cevcSITargetType,
                        cevcSITarget,
                        cevcSIEvcIndex,
                        cevcSIRowStatus,
                        cevcSIStorageType,
                        cevcSIAdminStatus,
                        cevcSIOperStatus,
                        cevcSIL2ControlProtocolAction,
                        cevcSIVlanRewriteAction,
                        cevcSIVlanRewriteEncapsulation,
                        cevcSIVlanRewriteVlan1,
                        cevcSIVlanRewriteVlan2,
                        cevcSIVlanRewriteSymmetric,
                        cevcSIVlanRewriteStorageType,
                        cevcSIVlanRewriteRowStatus,
                        cevcSIForwardingType,
                        cevcSICEVlanRowStatus,
                        cevcSICEVlanStorageType,
                        cevcSICEVlanEndingVlan,
                        cevcSIMatchStorageType,
                        cevcSIMatchRowStatus,
                        cevcSIMatchCriteriaType,
                        cevcSIMatchEncapRowStatus,
                        cevcSIMatchEncapStorageType,
                        cevcSIMatchEncapValid,
                        cevcSIMatchEncapEncapsulation,
                        cevcSIPrimaryVlanRowStatus,
                        cevcSIPrimaryVlanStorageType,
                        cevcSIPrimaryVlanEndingVlan
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects providing configuration and
        match criteria for service instances.
        cevcSIGroup object is superseded by cevcSIGroupRev1."
    ::= { ciscoEvcMIBGroups 4 }

cevcSIVlanRewriteGroup OBJECT-GROUP
    OBJECTS         {
                        cevcSIVlanRewriteAction,
                        cevcSIVlanRewriteEncapsulation,
                        cevcSIVlanRewriteVlan1,
                        cevcSIVlanRewriteVlan2,
                        cevcSIVlanRewriteSymmetric,
                        cevcSIVlanRewriteStorageType,
                        cevcSIVlanRewriteRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects which provides VLAN rewrite
        information for a service instance."
    ::= { ciscoEvcMIBGroups 5 }

cevcSICosMatchCriteriaGroup OBJECT-GROUP
    OBJECTS         {
                        cevcSIMatchEncapPrimaryCos,
                        cevcSIMatchEncapSecondaryCos
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects which provides CoS match criteria
        for a service instance."
    ::= { ciscoEvcMIBGroups 6 }

cevcSIMatchCriteriaGroup OBJECT-GROUP
    OBJECTS         {
                        cevcSIMatchRowStatus,
                        cevcSIMatchStorageType,
                        cevcSIMatchCriteriaType,
                        cevcSIMatchEncapRowStatus,
                        cevcSIMatchEncapStorageType,
                        cevcSIMatchEncapValid,
                        cevcSIMatchEncapEncapsulation,
                        cevcSIMatchEncapPrimaryCos,
                        cevcSIMatchEncapSecondaryCos,
                        cevcSIMatchEncapPayloadType,
                        cevcSIPrimaryVlanRowStatus,
                        cevcSIPrimaryVlanStorageType,
                        cevcSIPrimaryVlanEndingVlan,
                        cevcSISecondaryVlanRowStatus,
                        cevcSISecondaryVlanStorageType,
                        cevcSISecondaryVlanEndingVlan
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects providing match criteria information
        for service instances.
        cevcSIMatchCriteriaGroup object is superseded by 
        cevcSIMatchCriteriaGroupRev1."
    ::= { ciscoEvcMIBGroups 7 }

cevcSIForwardGroup OBJECT-GROUP
    OBJECTS         {
                        cevcSIForwardingType,
                        cevcSIForwardBdRowStatus,
                        cevcSIForwardBdStorageType,
                        cevcSIForwardBdNumber
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of objects providing service frame forwarding
        information for service instances.
        cevcSIForwardGroup object is superseded by 
        cevcSIForwardGroupRev1."
    ::= { ciscoEvcMIBGroups 8 }

cevcEvcNotificationConfigGroup OBJECT-GROUP
    OBJECTS         { cevcEvcNotifyEnabled }
    STATUS          current
    DESCRIPTION
        "A collection of objects for configuring notification
        of this MIB." 
    ::= { ciscoEvcMIBGroups 9 }

cevcEvcNotificationGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        cevcEvcStatusChangedNotification,
                        cevcEvcCreationNotification,
                        cevcEvcDeletionNotification
                    }
    STATUS          deprecated
    DESCRIPTION
        "A collection of notifications that this MIB module is
        required to implement.
        cevcEvcNotificationGroup object is superseded by 
        cevcEvcNotificationGroupRev1."
    ::= { ciscoEvcMIBGroups 10 }

cevcSIMatchCriteriaGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cevcSIMatchRowStatus,
                        cevcSIMatchStorageType,
                        cevcSIMatchCriteriaType,
                        cevcSIMatchEncapRowStatus,
                        cevcSIMatchEncapStorageType,
                        cevcSIMatchEncapValid,
                        cevcSIMatchEncapEncapsulation,
                        cevcSIMatchEncapPrimaryCos,
                        cevcSIMatchEncapSecondaryCos,
                        cevcSIMatchEncapPayloadTypes,
                        cevcSIMatchEncapPriorityCos,
                        cevcSIPrimaryVlanRowStatus,
                        cevcSIPrimaryVlanStorageType,
                        cevcSIPrimaryVlanEndingVlan,
                        cevcSISecondaryVlanRowStatus,
                        cevcSISecondaryVlanStorageType,
                        cevcSISecondaryVlanEndingVlan
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing match criteria information
        for service instances.

        This group deprecates the old group cevcSIMatchCriteriaGroup."
    ::= { ciscoEvcMIBGroups 11 }


cevcEvcNotificationGroupRev1 NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        cevcEvcStatusChangedNotification,
                        cevcEvcCreationNotification,
                        cevcEvcDeletionNotification,
                        cevcMacSecurityViolationNotification
                    }
    STATUS          current
    DESCRIPTION
        "A collection of notifications that this MIB module is
        required to implement.

        This module deprecates the cevcNotificationGroup"
    ::= { ciscoEvcMIBGroups 12 }

cevcSIGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cevcSIName,
                        cevcSITargetType,
                        cevcSITarget,
                        cevcSIEvcIndex,
                        cevcSIRowStatus,
                        cevcSIStorageType,
                        cevcSIAdminStatus,
                        cevcSIOperStatus,
                        cevcPortL2ControlProtocolAction,
                        cevcSIVlanRewriteAction,
                        cevcSIVlanRewriteEncapsulation,
                        cevcSIVlanRewriteVlan1,
                        cevcSIVlanRewriteVlan2,
                        cevcSIVlanRewriteSymmetric,
                        cevcSIVlanRewriteRowStatus,
                        cevcSIVlanRewriteStorageType,
                        cevcSIForwardingType,
                        cevcSICEVlanRowStatus,
                        cevcSICEVlanStorageType,
                        cevcSICEVlanEndingVlan,
                        cevcSIMatchStorageType,
                        cevcSIMatchCriteriaType,
                        cevcSIMatchEncapRowStatus,
                        cevcSIMatchEncapStorageType,
                        cevcSIMatchEncapValid,
                        cevcSIMatchEncapEncapsulation,
                        cevcSIPrimaryVlanRowStatus,
                        cevcSIPrimaryVlanStorageType,
                        cevcSIPrimaryVlanEndingVlan,
                        cevcSIMatchRowStatus,
                        cevcSICreationType,
                        cevcSIType
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing configuration and
        match criteria for service instances.
        This module deprecates the cevcSIGroup"
    ::= { ciscoEvcMIBGroups 13 }

cevcSIForwardGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cevcSIForwardingType,
                        cevcSIForwardBdRowStatus,
                        cevcSIForwardBdStorageType,
                        cevcSIForwardBdNumberBase,
                        cevcSIForwardBdNumber1kBitmap,
                        cevcSIForwardBdNumber2kBitmap,
                        cevcSIForwardBdNumber3kBitmap,
                        cevcSIForwardBdNumber4kBitmap
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing service frame forwarding
        information for service instances.

        This module deprecates cevcSIForwardGroup"
    ::= { ciscoEvcMIBGroups 14 }

cevcMacSecurityViolationGroup OBJECT-GROUP
    OBJECTS         {
                        cevcMacAddress,
                        cevcMaxMacConfigLimit,
                        cevcSIID,
                        cevcViolationCause
                    }
    STATUS          current
    DESCRIPTION
        "A collection of objects providing the maximum configured MAC
        limit, the MAC address, service instance ID and Violation 
        cause for  Mac Security Violation Information."
    ::= { ciscoEvcMIBGroups 15 }

END
















