-- *******************************************************************
-- CISCO-LWAPP-MOBILITY-EXT-MIB.my
-- January 2011, Srinath Candadai
--   
-- Copyright (c) 2011-2019 by Cisco Systems Inc.
-- All rights reserved.
-- *******************************************************************

CISCO-LWAPP-MOBILITY-EXT-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
    Unsigned32,
    Counter32,
    Counter64
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    TEXTUAL-CONVENTION,
    MacAddress,
    DateAndTime,
    TruthValue,
    RowStatus,
    StorageType
        FROM SNMPv2-TC
    InetAddressType,
    InetAddress
        FROM INET-ADDRESS-MIB
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    VlanIndex
        FROM Q-BRIDGE-MIB
    cLWlanIndex
        FROM CISCO-LWAPP-WLAN-MIB
    Dscp
        FROM CISCO-QOS-PIB-MIB
    cLWlanWlanPolicyName
        FROM CISCO-LWAPP-WLAN-POLICY-MIB
    ciscoMgmt
        FROM CISCO-SMI;


-- ********************************************************************
-- *  MODULE IDENTITY
-- ********************************************************************

ciscoLwappMobilityExtMIB MODULE-IDENTITY
    LAST-UPDATED    "201906200000Z"
    ORGANIZATION    "Cisco Systems Inc."
    CONTACT-INFO
            "Cisco Systems,
            Customer Service

            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            Email: cs-snmp@cisco.com"
    DESCRIPTION
        "This MIB is intended to be implemented on all those
        devices operating as Central Controllers (CC) that
        terminate the Light Weight Access Point Protocol
        tunnel from Light-weight LWAPP Access Points.

        This MIB provides configuration and status information
        about the 802.11 WLAN mobility.                 

        The relationship between CC and the LWAPP APs
        can be depicted as follows:


           +......+     +......+     +......+           +......+
           +      +     +      +     +      +           +      +
           +  CC  +     +  CC  +     +  CC  +           +  CC  +
           +      +     +      +     +      +           +      +
           +......+     +......+     +......+           +......+
           ..            .             .                 .
           ..            .             .                 .
           .  .            .             .                 .
           .    .            .             .                 .
           .      .            .             .                 .
           .        .            .             .                 .
           +......+ +......+     +......+      +......+         
           +......+
           +      + +      +     +      +      +      +          +     
           +
           +  AP  + +  AP  +     +  AP  +      +  AP  +          +  AP 
           +
           +      + +      +     +      +      +      +          +     
           +
           +......+ +......+     +......+      +......+         
           +......+
           .              .             .                 .
           .  .              .             .                 .
           .    .              .             .                 .
           .      .              .             .                 .
           .        .              .             .                 .
           +......+ +......+     +......+      +......+         
           +......+
           +      + +      +     +      +      +      +          +     
           +
           +  MN  + +  MN  +     +  MN  +      +  MN  +          +  MN 
           +
           +      + +      +     +      +      +      +          +     
           +
           +......+ +......+     +......+      +......+         
           +......+



           The LWAPP tunnel exists between the controller and
           the APs.  The MNs communicate with the APs through
           the protocol defined by the 802.11 standard.


           LWAPP APs, upon bootup, discover and join one of the
           controllers and the controller pushes the configuration,
           that includes the WLAN parameters, to the LWAPP APs.

           The APs then encapsulate all the 802.11 frames from
           wireless clients inside LWAPP frames and forward
           the LWAPP frames to the controller.


                              GLOSSARY

           Access Point ( AP )

           An entity that contains an 802.11 medium access
           control ( MAC ) and physical layer ( PHY ) interface
           and provides access to the distribution services via
           the wireless medium for associated clients.  

           LWAPP APs encapsulate all the 802.11 frames in
           LWAPP frames and sends it to the controller to which
           it is logically connected.


           Basic Service Set Identifier (BSSID)

           The identifier for the service set comprising of
           all the 802.11 stations under the control of
           one coordinating Access Point.  This identifier
           happens to be the MAC address of the dot11 radio
           interface of the Access Point.  The wireless
           clients that associate with the Access Point
           get the wired uplink through this particular 
           dot11 interface. 


           Central Controller ( CC )

           The central entity that terminates the LWAPP protocol
           tunnel from the LWAPP APs.  Throughout this MIB,
           this entity also referred to as 'controller'. 


           Light Weight Access Point Protocol ( LWAPP ) 

           This is a generic protocol that defines the 
           communication between the Access Points and the
           Central Controller. 


           Mobility Oracle (MO)

           When a Central Controller in the Mobility Group is 
           designated as Mobility Oracle, then all the Mobility 
           Controller's (MC) traffic is tunnelled to it by other
           Mobility Controllers. Currently, MO resides along with MC
           but MC can reside in a box without MO.


           Mobility Controller (MC)

           When a Central Controller in the Mobility Group is 
           designated as Mobility Controller, then all the Mobile 
           Anchor's traffic is tunnelled to it by other Anchors.
           Each MC has its own/self mobility agent (MA), but MA can
           reside in a box without MC.


           Mobility Agent (MA)

           The Mobility Agent is an entity residing on the access 
           switch that manages mobility events on the switch, and 
           communicates with the Mobility Controller. Access Points
           can associate directly with MA.


           Wireless LAN Controller (WLC)

           Wireless LAN Controller are legacy mobility device which 
           can participate in the new mobility architecture.


           Mobility Manager

           The Mobility Manager is the management entity in a mobility
           controller or mobility agent.


           Mobile Node ( MN )

           A roaming 802.11 wireless device in a wireless
           network associated with an access point. 


           Anchor MC, Anchor MA

           Anchor MC or Anchor MA is the mobility entity where a mobile
           client was first anchored or associated. This is equivalent 
           to home agent (HA).


           Associated MC, Associated MA

           Associated MC or Associated MA is the mobility entity where 
           a mobile client roamed and get associated. This is equivalent
           to foreign agent (FA). It can be local or remote.


           Mobility 

           Concept by which a Mobile Node can roam from one 
           Access Point to another Access Point, across multiple
           Central Controllers, without need for repeated 
           authentication. 


           Mobility Group

           A set of Central Controllers which exchange Mobile 
           Node's authentication information, so that the Mobile
           Node upon roaming need not re-authenticate.  


           Switch Peer Group (SPG)

           A set of mobility agents (MAs) form a Switch Peer Group.
           One or more SPGs are associated with one mobility 
           controller (MC). Traffic between mobility agents within
           a SPG group goes directly between them - not through their
           associated MC


           Mobility Anchor

           When a Central Controller in the Mobility Group is 
           designated as Mobility Anchor, then all the Mobile 
           Node's traffic is tunnelled to it by other
           Controllers in the Mobility Group.


           Guest Tunneling (GT)

           The concept of designating a Central Controller in 
           the Mobility Group as Mobility Anchor, so that all
           the Mobile Node's traffic is tunnelled to it by other
           Controllers in the Mobility Group.              


           Station Management (SMT)

           This term refers to the internal management of the
           802.11 protocol operations by the AP to work
           cooperatively with the other APs and 802.11
           devices in the network.


           Ethernet over Internet Protocol (EoIP)

           Ethernet over IP (EoIP) is a protocol that creates 
           an Ethernet tunnel between two routers on top of an
           IP connection. The EoIP interface appears as an 
           Ethernet interface.


           Reverse path filtering (RPF) 

           Reverse path filtering (RPF) is a feature provided
           by most modern Internet Protocol routers, which may
           be used to reduce the risk of customers attacking
           other internet hosts. One of the problems network
           service providers face today is hackers generating
           packets with fake source IP addresses, a technique
           known as spoofing. This is often done in order to
           initiate a denial-of-service attack against another
           internet host or network.
           Since the source IP addresses of the incoming packets
           change, often randomly, and for every packet, the
           target of such an attack can't easily filter out the
           attacking packets. However, the source of the attack,
           i.e. the network service provider of the attacking 
           host, has a simple way to stop such packets from ever
           leaving its network. A router always knows which 
           networks are reachable via any of its interfaces. 

           By checking the source IP address of all packets 
           coming in via an interface against the networks known
           to be behind that interface, the router can simply 
           drop packets that aren't supposed to come from there.

           Hence, reverse path filtering filters packets 
           according to the 'reverse path' to their source 
           IP address. If the path back to the source IP address 
           does not match the path the packet is coming from,
           it is dropped.

           REFERENCE

           [1] Part 11 Wireless LAN Medium Access Control ( MAC )
           and Physical Layer ( PHY ) Specifications.


           [2] Draft-obara-capwap-lwapp-00.txt, IETF Light 
           Weight Access Point Protocol."
    REVISION        "201906200000Z"
    DESCRIPTION
        "Added C9800-specific attributes."
    REVISION        "201705020000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 846 }


ciscoLwappMobilityExtMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtMIB 0 }

ciscoLwappMobilityExtMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtMIB 1 }

ciscoLwappMobilityExtMIBConform  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtMIB 2 }

ciscoLwappMobilityExtGlobalObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtMIBObjects 1 }

ciscoLwappMobilityExtTableObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtMIBObjects 2 }

ciscoLwappMobilityExtNotifObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtMIBObjects 3 }

ciscoLwappMobilityExtMCGlobalObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtGlobalObjects 1 }

ciscoLwappMobilityExtMCMAGlobalObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtGlobalObjects 2 }

ciscoLwappMobilityExtMAGlobalObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtGlobalObjects 3 }

ciscoLwappMobilityExtMCStats  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtGlobalObjects 4 }

ciscoLwappMobilityExtMAStats  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtGlobalObjects 5 }

ciscoLwappMobilityExtGlobalStats  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtGlobalObjects 6 }


CiscoAbsZeroBasedCounter64 ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "This TC describes an object which counts events with the
        following semantics: objects of this type will be set to
        zero(0) on creation and will thereafter count appropriate
        events, it locks at the maximum value of 18,446,744,073,709,551
        ,615 if the counter overflows.
        This TC may be used only in situations where wrapping is
        not possible or extremely unlikely situation."
    SYNTAX          Counter64

-- *******************************************************************
-- Mobility Controller (MC) global parameters
-- *******************************************************************

cLMobilityExtMCMOEnableStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the current status of the
        Mobility Oracle (MO).
        A value of 'true' indicates Mobility Oracle is enabled. 
        A value of 'false' indicates Mobility Oracle (MO) 
        is disabled."
    DEFVAL          { false } 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 1 }

cLMobilityExtMCMOAdminEnableStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the user to enable or disable
        MO mode.  
        A value of 'true' indicates both Mobility 
        Oracle (MO) is enabled. 
        A value of 'false' indicates Mobility Oracle (MO)
        is disabled.
        Please note that cLMobilityExtMOEnableStatus (operational 
        value)can be false even if cLMobilityExtMOAdminEnableStatus is 
        true."
    DEFVAL          { false } 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 2 }

cLMobilityExtMCEnableStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the current status of
        Mobility Controller (MC).  The controller can 
        operate either in MC/MA or MA only mode. 
        A value of 'true' indicates Mobility 
        Controller (MC) is enabled. 
        A value of 'false' indicates Mobility Controller (MC)
        is disabled."
    DEFVAL          { false } 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 3 }

cLMobilityExtMCAdminEnableStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the user to enable or disable
        MC mode.  The controller can operate 
        either in MC/MA or MA only mode. 
        A value of 'true' indicates both Mobility 
        Controller (MC) is enabled. 
        A value of 'false' indicates Mobility Controller (MC)
        is disabled.
        Please note that cLMobilityExtMCEnableStatus (operational 
        value)can be false even if cLMobilityExtMCAdminEnableStatus is 
        true."
    DEFVAL          { false } 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 4 }

cLMobilityExtMCMulticastMode OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the user to enable or disable
        multicast  mode.
        A value of 'true' indicates multicast mode 
        is enabled.
        A value of 'false' indicates multicast mode 
        is disabled."
    DEFVAL          { false } 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 5 }

cLMobilityExtMCKeepAliveCount OBJECT-TYPE
    SYNTAX          Unsigned32 (3..20)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the keep alive count.
        If keep alive response is not received consecutively
        for N (keep alive count) times, the mobility link is
        declared as down."
    DEFVAL          { 3 } 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 6 }

cLMobilityExtMCKeepAliveInterval OBJECT-TYPE
    SYNTAX          Unsigned32 (1..30)
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the keep alive interval. This object is
        valid for MC, not MA." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 7 }

cLMobilityExtMCDscpValue OBJECT-TYPE
    SYNTAX          Dscp
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the Differentiated Services Code Point
        (DSCP) value. Here it is used for classifying and managing 
        mobility control packets and providing quality of service (QoS)
        on IP networks. Valid value ranges from 0 to 63."
    DEFVAL          { 0 } 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 8 }

cLMobilityExtMCMOPublicAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the MO's public IP address type." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 9 }

cLMobilityExtMCMOPublicAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the MO's public IP address.The
        type of this address is determined by the value of
        cLMobilityExtMCMOPublicAddressType object." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 10 }

cLMobilityExtMCApCountLicensesInUse OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the total APs directly associated
        with this MC and its MAs. Each Access point that joins 
        the Controller acquires a licence from the controller." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 11 }

cLMobilityExtMCOwnGroupMulticastAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the multicast IP address type of its own
        mobility group." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 12 }

cLMobilityExtMCOwnGroupMulticastAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the multicast IP address of its own
        mobility group. The type of this address is determined by the 
        value of cLMobilityExtMCOwnGroupMulticastAddressType object." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 13 }

cLMobilityExtMCMobilityGroupName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the name for this mobility group." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 14 }

cLMobilityExtMCMONumberOfClients OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of clients reported
        by MO." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 15 }

cLMobilityExtMCNumberOfMCs OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of MCs within a mobility
        domain." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 16 }

cLMobilityExtMCTotalNumberOfReportedAPs OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of APs reported
        by this MC, its peer MCs and its MAs." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 17 }

cLMobilityExtMCNumberOfReportedAPsInSubDomain OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of APs reported
        by this MC and its MAs." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 18 }

cLMobilityExtMCOwnGroupMulticastAddressv6Type OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the multicast IP address type of its own
        mobility group." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 19 }

cLMobilityExtMCOwnGroupMulticastAddressv6 OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the multicast IPv6 address of its own
        mobility group." 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 20 }

cLMobilityExtMCMulticastModev6 OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object allows the user to enable or disable
        IPv6 multicast  mode.
        A value of 'true' indicates IPv6 multicast mode
        is enabled.
        A value of 'false' indicates IPv6 multicast mode
        is disabled."
    DEFVAL          { false } 
    ::= { ciscoLwappMobilityExtMCGlobalObjects 21 }

-- *******************************************************************
-- Mobility Manager global parameters (applicable to both MC and MA)
-- *******************************************************************

cLMobilityExtMgrAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the mobility manager's IP address type.
        The mobility manager is the management entity of MC or MA." 
    ::= { ciscoLwappMobilityExtMCMAGlobalObjects 1 }

cLMobilityExtMgrAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the mobility manager's IP address. The
        type of this address is determined by the value of
        cLMobilityExtMgrAddressType." 
    ::= { ciscoLwappMobilityExtMCMAGlobalObjects 2 }

cLMobilityExtMgrNetmaskType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the mobility manager's netmask type." 
    ::= { ciscoLwappMobilityExtMCMAGlobalObjects 3 }

cLMobilityExtMgrNetmask OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the mobility manager's netmask. The
        type of this address is determined by the value of 
        cLMobilityExtMgrNetmaskType." 
    ::= { ciscoLwappMobilityExtMCMAGlobalObjects 4 }

cLMobilityExtMgrMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the mac address for this mobility
        manager." 
    ::= { ciscoLwappMobilityExtMCMAGlobalObjects 5 }

cLMobilityExtMgrVlanId OBJECT-TYPE
    SYNTAX          VlanIndex
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the VLAN ID for this mobility manager." 
    ::= { ciscoLwappMobilityExtMCMAGlobalObjects 6 }

cLMobilityExtMgrName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the name for this mobility manager." 
    ::= { ciscoLwappMobilityExtMCMAGlobalObjects 7 }

cLMobilityExtMgrInterfaceType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        management(1),
                        ap(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the mobility manager interface type.
        It can be of two types:
        management(1) - For in-band management of the controller.
        ap(2) -  For L3 communications between the controller 
                 and LWAPP APs." 
    ::= { ciscoLwappMobilityExtMCMAGlobalObjects 8 }

cLMobilityExtNewArchitectureEnableStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the current status of the
        new mobility feature.
        A value of 'true' indicates new mobility is enabled.
        A value of 'false' indicates new mobility is disabled." 
    ::= { ciscoLwappMobilityExtMCMAGlobalObjects 9 }

cLMobilityExtNewArchitectureAdminEnableStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies users to enable or disable
        new mobility feature.
        A value of 'true' indicates new mobility is enabled.
        A value of 'false' indicates new mobility is disabled." 
    ::= { ciscoLwappMobilityExtMCMAGlobalObjects 10 }

cLMobilityExtSecureCipher OBJECT-TYPE
    SYNTAX          INTEGER  {
                        disable(1),
                        aes256sha1(2),
                        aes256sha2(3)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies to configure secure ciphers, AES256+SHA
        or AES256+SHA2 for mobility tunnel.
        disable(1) - Implies that controllers will continue 
                     to use default ciphers for mobility  tunnel.
        aes256sha1(2) - Implies that controllers will use
                        AES256_SHA cipher for mobility tunnel.
        aes256sha2(3) - Implies that controllers will use 
                        AES256_SHA256 cipher for mobility tunnel." 
    ::= { ciscoLwappMobilityExtMCMAGlobalObjects 11 }

cLMobilityExtEncryptionStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the current status of the
        encryption in the mobility tunnel.
        A value of 'true' indicates encryption is enabled.
        A value of 'false' indicates encryption is disabled." 
    ::= { ciscoLwappMobilityExtMCMAGlobalObjects 12 }
-- *******************************************************************
-- Switch Peer Group Table (applicable to MC only)
-- *******************************************************************

cLMobilityExtSpgTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtSpgEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the
        802.11 LWAPP mobility Switch Peer Group (SPG)."
    ::= { ciscoLwappMobilityExtTableObjects 1 }

cLMobilityExtSpgEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtSpgEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information about
        one 802.11 LWAPP mobility SPG configured on this controller."
    INDEX           { cLMobilityExtSpgGroupName } 
    ::= { cLMobilityExtSpgTable 1 }

CLMobilityExtSpgEntry ::= SEQUENCE {
        cLMobilityExtSpgGroupName            SnmpAdminString,
        cLMobilityExtSpgGroupId              Unsigned32,
        cLMobilityExtSpgBridgeDomainId       Unsigned32,
        cLMobilityExtSpgMemberCount          Unsigned32,
        cLMobilityExtSpgMulticastAddressType InetAddressType,
        cLMobilityExtSpgMulticastAddress     InetAddress,
        cLMobilityExtSpgMulticastMode        TruthValue,
        cLMobilityExtSpgStorageType          StorageType,
        cLMobilityExtSpgRowStatus            RowStatus
}

cLMobilityExtSpgGroupName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the group name for this SPG." 
    ::= { cLMobilityExtSpgEntry 1 }

cLMobilityExtSpgGroupId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the group ID for this SPG.
        This object is used in the control data packet for SPG." 
    ::= { cLMobilityExtSpgEntry 2 }

cLMobilityExtSpgBridgeDomainId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the bridge domain ID for this SPG." 
    ::= { cLMobilityExtSpgEntry 3 }

cLMobilityExtSpgMemberCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of members on this SPG." 
    ::= { cLMobilityExtSpgEntry 4 }

cLMobilityExtSpgMulticastAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the member's multicast IP address
        type." 
    ::= { cLMobilityExtSpgEntry 5 }

cLMobilityExtSpgMulticastAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the member's multicast IP address.
        The type of this address is determined by the value of
        cLMobilityExtSpgMulticastAddressType." 
    ::= { cLMobilityExtSpgEntry 6 }

cLMobilityExtSpgMulticastMode OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the user to enable or disable
        multicast  mode.
        A value of 'true' indicates multicast mode 
        is enabled.
        A value of 'false' indicates multicast mode 
        is disabled." 
    ::= { cLMobilityExtSpgEntry 7 }

cLMobilityExtSpgStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the storage type for this
        conceptual row." 
    ::= { cLMobilityExtSpgEntry 8 }

cLMobilityExtSpgRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and used
        to create and delete specific instances of rows             
        in this table." 
    ::= { cLMobilityExtSpgEntry 9 }
 

-- *******************************************************************
-- Switch Peer Group Member table (applicable to MC only)
-- *******************************************************************

cLMobilityExtSpgMemberTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtSpgMemberEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the
        802.11 LWAPP mobility Switch Peer Group (SPG) members."
    ::= { ciscoLwappMobilityExtTableObjects 2 }

cLMobilityExtSpgMemberEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtSpgMemberEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information about
        one 802.11 LWAPP mobility SPG member configured 
        on this controller."
    INDEX           {
                        cLMobilityExtSpgGroupName,
                        cLMobilityExtSpgMemberPrivateAddressType,
                        cLMobilityExtSpgMemberPrivateAddress
                    } 
    ::= { cLMobilityExtSpgMemberTable 1 }

CLMobilityExtSpgMemberEntry ::= SEQUENCE {
        cLMobilityExtSpgMemberPrivateAddressType InetAddressType,
        cLMobilityExtSpgMemberPrivateAddress     InetAddress,
        cLMobilityExtSpgMemberStatus             INTEGER,
        cLMobilityExtSpgMemberPublicAddressType  InetAddressType,
        cLMobilityExtSpgMemberPublicAddress      InetAddress,
        cLMobilityExtSpgMemberRowStatus          RowStatus
}

cLMobilityExtSpgMemberPrivateAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the member's private IP address type." 
    ::= { cLMobilityExtSpgMemberEntry 1 }

cLMobilityExtSpgMemberPrivateAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the member's private IP address.
        The type of this address is determined by the value of
        cLMobilityExtSpgMemberPrivateAddressType." 
    ::= { cLMobilityExtSpgMemberEntry 2 }

cLMobilityExtSpgMemberStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        notconfigured(0),
                        datapathdown(1),
                        controlpathdown(2),
                        bothdown(3),
                        up(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the operational and connectivity
        status of the member.

        notconfigured(0) - This means group member is not configured
                           for ICMP or EoIP pings.

        datapathdown(1) - This means group member is not responding
                          to EoIP pings.

        controlpathdown(2) - This means successive ICMP pings
                             to the group member have failed.

        bothdown(3) - This means group member is not responding
                      to ICMP or EOIP pings.

        up(4) - This means group member is responding to
                both EOIP and ICMP pings." 
    ::= { cLMobilityExtSpgMemberEntry 3 }

cLMobilityExtSpgMemberPublicAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the member's public IP address type." 
    ::= { cLMobilityExtSpgMemberEntry 4 }

cLMobilityExtSpgMemberPublicAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the member's public IP address. The
        type of this address is determined by the value of
        cLMobilityExtSpgMemberPublicAddressType." 
    ::= { cLMobilityExtSpgMemberEntry 5 }

cLMobilityExtSpgMemberRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and used
        to create and delete specific instances of rows             
        in this table." 
    ::= { cLMobilityExtSpgMemberEntry 6 }
 

-- *******************************************************************
-- Mobility Group Member table (applicable to MC only)
-- *******************************************************************

cLMobilityExtGroupMemberTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtGroupMemberEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the
        802.11 LWAPP mobility group members."
    ::= { ciscoLwappMobilityExtTableObjects 3 }

cLMobilityExtGroupMemberEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtGroupMemberEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information about
        one 802.11 LWAPP mobility member configured 
        on this controller."
    INDEX           {
                        cLMobilityExtGroupMemberPrivateAddressType,
                        cLMobilityExtGroupMemberPrivateAddress
                    } 
    ::= { cLMobilityExtGroupMemberTable 1 }

CLMobilityExtGroupMemberEntry ::= SEQUENCE {
        cLMobilityExtGroupMemberPrivateAddressType   InetAddressType,
        cLMobilityExtGroupMemberPrivateAddress       InetAddress,
        cLMobilityExtGroupMemberGroupName            SnmpAdminString,
        cLMobilityExtGroupMemberPublicAddressType    InetAddressType,
        cLMobilityExtGroupMemberPublicAddress        InetAddress,
        cLMobilityExtGroupMemberStatus               INTEGER,
        cLMobilityExtGroupMemberMacAddress           MacAddress,
        cLMobilityExtGroupMemberMulticastAddressType InetAddressType,
        cLMobilityExtGroupMemberMulticastAddress     InetAddress,
        cLMobilityExtGroupMemberHashKey              OCTET STRING,
        cLMobilityExtGroupMemberRowStatus            RowStatus
}

cLMobilityExtGroupMemberPrivateAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the member's private IP address type." 
    ::= { cLMobilityExtGroupMemberEntry 1 }

cLMobilityExtGroupMemberPrivateAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the member's private IP address. The
        type of this address is determined by the value of
        cLMobilityExtGroupMemberPrivateAddressType." 
    ::= { cLMobilityExtGroupMemberEntry 2 }

cLMobilityExtGroupMemberGroupName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the member's mobility group name." 
    ::= { cLMobilityExtGroupMemberEntry 3 }

cLMobilityExtGroupMemberPublicAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the member's public IP address type." 
    ::= { cLMobilityExtGroupMemberEntry 4 }

cLMobilityExtGroupMemberPublicAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the member's public IP address. The
        type of this address is determined by the value of
        cLMobilityExtGroupMemberPublicAddressType." 
    ::= { cLMobilityExtGroupMemberEntry 5 }

cLMobilityExtGroupMemberStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        notconfigured(0),
                        datapathdown(1),
                        controlpathdown(2),
                        bothdown(3),
                        up(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the operational and connectivity
        status of the member.
        notconfigured(0) - This means group member is not configured
                           for ICMP or EoIP pings.

        datapathdown(1) - This means group member is not responding
                          to EoIP pings.

        controlpathdown(2) - This means successive ICMP pings
                             to the group member have failed.

        bothdown(3) - This means group member is not responding
                      to ICMP or EOIP pings.

        up(4) - This means group member is responding to
                both EOIP and ICMP pings." 
    ::= { cLMobilityExtGroupMemberEntry 6 }

cLMobilityExtGroupMemberMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the member's MAC address." 
    ::= { cLMobilityExtGroupMemberEntry 7 }

cLMobilityExtGroupMemberMulticastAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This used indicates the member's multicast IP address type." 
    ::= { cLMobilityExtGroupMemberEntry 8 }

cLMobilityExtGroupMemberMulticastAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the member's multicast IP address.
        The type of this address is determined by the value of
        cLMobilityExtGroupMemberMulticastAddressType." 
    ::= { cLMobilityExtGroupMemberEntry 9 }

cLMobilityExtGroupMemberHashKey OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (4..40))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the hash key of the peer mobility
        member. It is a 40 digit hex value or 'none'. Value 'none' is 
        used to clear the previously configured hash key." 
    ::= { cLMobilityExtGroupMemberEntry 10 }

cLMobilityExtGroupMemberRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and used
        to create and delete specific instances of rows             
        in this table." 
    ::= { cLMobilityExtGroupMemberEntry 11 }
 

-- *******************************************************************
-- Per WLAN, anchors table (applicable to MC and MA only)
-- *******************************************************************

cLMobilityExtAnchorTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtAnchorEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the
        802.11 LWAPP Mobility Anchors on individual WLANs.

               +...............+
               +               +
               +    ROUTER     +
               +   10.16.1.1   +
               +...............+
                      ..
                    .    .
                  .        .
                .            .
              .                .
            .                    .
        10.16.109.112        10.16.105.39
        +......+   <<-------->>   +......+
        +      +  [3]CC2 tunnels  +      +
        +  CC1 +   MN1's traffic  +  CC2 +
        +      +   to Anchor CC1  +      +
        +......+   using EoIP     +......+
           .                        .
           . Anchor        Foreign  .
           .                        .
        +......+                  +......+
        +      +                  +      +
        +  AP1 +                  +  AP2 +
        +      +                  +      +
        +......+                  +......+
        WLAN '1'   .                        ^   WLAN '1'
        .                          |
        .           [2] associates  |
        .              with AP2/CC2  |
        .                             |
        +......+   [1]              +......+
        +      +  moves to region   +      +
        +  MN1 +  ---------->>>     +  MN1 +
        +      +  serviced by AP2   +      +
        +......+                    +......+
        10.16.109.199               10.16.109.199

        In the above diagram, Central Controllers CC1 and CC2 have
        been configured in a Mobility Group.

        Currently the Mobile Node 'MN1' obtains its IP from the
        Central Controller 'CC1' with which it first associates
        via WLAN '1' through Access Point 'AP1'. 'CC1'
        obtains DHCP address, say 10.16.109.199 for client 'MN1'.
        Now the client 'MN1' is identified by 10.16.109.199 for
        further communication with the network and the
        communication happens via 'CC1'.

        Since, 'CC1' and 'CC2' are in same mobility group, 'CC1'
        sends the authentication block of 'MN1' to 'CC2'.


        Central Controller 'CC2' has an associated Access Point
        'AP2' which beams WLAN '1' and uses 10.16.105.0 /
        255.255.255.0 subnet instead.

        Next, the Mobile Node 'MN1' moves out of range of 'AP1'
        and gets in to proximity with 'AP2' and continues to use
        WLAN '1'. 'CC2' locally authenticates 'MN1' against
        authentication block shared from 'CC1'. 'CC2' forwards all
        traffic from 'MN1' to router. This is called WLAN mobility.

        But hold on, 'CC2' uses 10.16.105.0 / 255.255.255.0 subnet
        for WLAN '1'. So we have two problems here :

        a> Traffic of 10.16.109.0 / 255.255.255.0 subnet has to be
        accessible from 10.16.105.0 / 255.255.255.0 subnet.

        b> Unneccessary overloading of 10.16.105.0 / 255.255.255.0
        subnet by traffic from 10.16.109.0 / 255.255.255.0 subnet.

        How do we address these issues ??

        If an EoIP tunnel can be established between 'CC1' and 'CC2'
        and 'CC1' sends all traffic bound to 'MN1', 10.16.109.199,
        on this tunnel to 'CC2', which in turn forwards it to 'MN1',
        then, above two subnet-problems are resolved. This is called
        Mobility Anchoring. 'CC1' is the Mobility Anchor and 'CC2' is
        the 'Foreign' for WLAN '1'.

        As per the configuration, user creates a Mobility Anchor entry
        in 'CC2' for WLAN '1' with IP address as 'CC1', i.e.
        10.16.109.112. So, when 'MN1' connects to WLAN '1' via
        'AP2', then 'CC2' establishes EoIP tunnel with 10.16.109.112
        and forwards the packets to 'MN1'.

        Given the above example, the cLMobilityAnchorEntry on 'CC2'
        looks like :

        ------------------------------------------------------------------
        |      MIB - ATTRIBUTES           |       ROW#1        |  ROW#2  |
        ------------------------------------------------------------------
        | cLWlanIndex                     |     1              |         |
        ------------------------------------------------------------------
        | cLMobilityExtAnchorAssociatedMCAddressType |   ipv4    |       |
        ------------------------------------------------------------------
        | cLMobilityExtAnchorAssociatedMCAddress | 10.16.109.112 |       |
        ------------------------------------------------------------------
        | cLMobilityExtAnchorStatus          |        up(4)    |         |
        ------------------------------------------------------------------
        | cLMobilityExtAnchorRowStatus       |    active(1)    |         |
        ------------------------------------------------------------------

        This feature has advantages for both security and load
        balancing.  It can be used to restrict a WLAN to a single
        subnet, regardless of the MN's entry point into the network.
        A 'public' or guest WLAN can thus be accessed throughout an
        enterprise, but still is restricted to a specific subnet.
        It can also be used to provide some geographic load balancing,
        since the WLANs can represent a particular section of a
        building (ie., engineering, marketing).  Those groups can be
        'anchored' on a particular subnet/switch rather than on the
        CC of first occurrence (ie., the switch controlling the APs
        by the front door)."
    ::= { ciscoLwappMobilityExtTableObjects 4 }

cLMobilityExtAnchorEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtAnchorEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information about
        one 802.11 LWAPP Mobility Anchor(MA) configured on a WLAN
        on this controller."
    INDEX           {
                        cLWlanIndex,
                        cLMobilityExtAnchorAssociatedMCAddressType,
                        cLMobilityExtAnchorAssociatedMCAddress
                    } 
    ::= { cLMobilityExtAnchorTable 1 }

CLMobilityExtAnchorEntry ::= SEQUENCE {
        cLMobilityExtAnchorAssociatedMCAddressType InetAddressType,
        cLMobilityExtAnchorAssociatedMCAddress     InetAddress,
        cLMobilityExtAnchorStatus                  INTEGER,
        cLMobilityExtAnchorRowStatus               RowStatus,
        cLMobilityExtAnchorPriority                INTEGER
}

cLMobilityExtAnchorAssociatedMCAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the anchor's IP address type." 
    ::= { cLMobilityExtAnchorEntry 1 }

cLMobilityExtAnchorAssociatedMCAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the anchor's IP address. The type
        of this address is determined by the value of
        cLMobilityExtAnchorAssociatedMCAddressType." 
    ::= { cLMobilityExtAnchorEntry 2 }

cLMobilityExtAnchorStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        notconfigured(0),
                        datapathdown(1),
                        controlpathdown(2),
                        bothdown(3),
                        up(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the operational and connectivity
        status of the Mobility Anchor(MA).
        notconfigured(0) - This means anchor is not configured
                           for ICMP or EoIP pings.

        datapathdown(1) - This means anchor is not responding
                          to EoIP pings.

        controlpathdown(2) - This means successive ICMP pings
                             to the anchor have failed.

        bothdown(3) - This means anchor is not responding
                      to ICMP or EOIP pings.

        up(4) - This means anchor is responding to
                both EOIP and ICMP pings." 
    ::= { cLMobilityExtAnchorEntry 3 }

cLMobilityExtAnchorRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and used
        to create and delete specific instances of rows
        in this table." 
    ::= { cLMobilityExtAnchorEntry 4 }

cLMobilityExtAnchorPriority OBJECT-TYPE
    SYNTAX          INTEGER  {
                        local(1),
                        primary(2),
                        secondary(3),
                        tertiary(4)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the priority configured for
        an anchor WLC mapped on a WLAN.
        local(1) - Local priority can't be configured. This indicates 
                   that anchor WLC is configured with its own IP.

        primary(2) - This indicates that anchor WLC configured with 
                     this priority will have highest priority.

        secondary(3) - This indicates that anchor WLC configured with 
                       this priority will have medium priority.

        tertiary(4) - This indicates that anchor WLC configured with 
                      this priority will have lowest priority." 
    ::= { cLMobilityExtAnchorEntry 5 }
 

-- *******************************************************************
-- Mobility Controllers table reported by Mobility Oracle (MO)
-- *******************************************************************

cLMobilityExtMOMCTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtMOMCEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the
        802.11 LWAPP Mobility Controllers on this MO."
    ::= { ciscoLwappMobilityExtTableObjects 5 }

cLMobilityExtMOMCEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtMOMCEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information about
        one 802.11 LWAPP Mobility Controller on this MO."
    INDEX           {
                        cLMobilityExtMOMCAddressType,
                        cLMobilityExtMOMCAddress
                    } 
    ::= { cLMobilityExtMOMCTable 1 }

CLMobilityExtMOMCEntry ::= SEQUENCE {
        cLMobilityExtMOMCAddressType InetAddressType,
        cLMobilityExtMOMCAddress     InetAddress,
        cLMobilityExtMOMCMacAddress  MacAddress,
        cLMobilityExtMOMCLinkStatus  INTEGER,
        cLMobilityExtMOMCClientCount Unsigned32
}

cLMobilityExtMOMCAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the MC's IP address type." 
    ::= { cLMobilityExtMOMCEntry 1 }

cLMobilityExtMOMCAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the MC's IP address. The
        type of this address is determined by the value of
        cLMobilityExtMOMCAddressType." 
    ::= { cLMobilityExtMOMCEntry 2 }

cLMobilityExtMOMCMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the MC's MAC address." 
    ::= { cLMobilityExtMOMCEntry 3 }

cLMobilityExtMOMCLinkStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        notconfigured(0),
                        datapathdown(1),
                        controlpathdown(2),
                        bothdown(3),
                        up(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the operational and connectivity
        status of the MC.

        notconfigured(0) - This means MC is not configured
                           for ICMP or EoIP pings.

        datapathdown(1) - This means MC is not responding
                          to EoIP pings.

        controlpathdown(2) - This means successive ICMP pings
                             to the MC have failed.

        bothdown(3) - This means MC is not responding
                      to ICMP or EOIP pings.

        up(4) - This means MC is responding to
                both EOIP and ICMP pings." 
    ::= { cLMobilityExtMOMCEntry 4 }

cLMobilityExtMOMCClientCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of clients associated to the
        MC." 
    ::= { cLMobilityExtMOMCEntry 5 }
 

-- *******************************************************************
-- Mobility Clients table reported by Mobility Controller (MC)
-- *******************************************************************

cLMobilityExtMCClientTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtMCClientEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the
        802.11 LWAPP Mobility Clients on this MC."
    ::= { ciscoLwappMobilityExtTableObjects 6 }

cLMobilityExtMCClientEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtMCClientEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information about
        one 802.11 LWAPP Mobility Clients on this MC."
    INDEX           { cLMobilityExtMCClientMacAddress } 
    ::= { cLMobilityExtMCClientTable 1 }

CLMobilityExtMCClientEntry ::= SEQUENCE {
        cLMobilityExtMCClientMacAddress                 MacAddress,
        cLMobilityExtMCClientAnchorMCPrivateAddressType InetAddressType,
        cLMobilityExtMCClientAnchorMCPrivateAddress     InetAddress,
        cLMobilityExtMCClientAssociatedMCAddressType    InetAddressType,
        cLMobilityExtMCClientAssociatedMCAddress        InetAddress,
        cLMobilityExtMCClientAddressType                InetAddressType,
        cLMobilityExtMCClientAddress                    InetAddress,
        cLMobilityExtMCClientState                      INTEGER,
        cLMobilityExtMCClientAssociationTime            DateAndTime,
        cLMobilityExtMCClientLocalClient                TruthValue,
        cLMobilityExtMCClientAnchorMCGroupId            Unsigned32,
        cLMobilityExtMCClientAssociatedMCGroupId        Unsigned32,
        cLMobilityExtMCClientAssociatedMAAddressType    InetAddressType,
        cLMobilityExtMCClientAssociatedMAAddress        InetAddress,
        cLMobilityExtMCClientAnchorMAAddressType        InetAddressType,
        cLMobilityExtMCClientAnchorMAAddress            InetAddress,
        cLMobilityExtMCClientUpTime                     CiscoAbsZeroBasedCounter64
}

cLMobilityExtMCClientMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the client's MAC address." 
    ::= { cLMobilityExtMCClientEntry 1 }

cLMobilityExtMCClientAnchorMCPrivateAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's anchor MC private
        IP address type." 
    ::= { cLMobilityExtMCClientEntry 2 }

cLMobilityExtMCClientAnchorMCPrivateAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's anchor MC private
        IP address. The type of this address is determined by
        the value of cLMobilityExtMCClientAnchorMCPrivateAddressType." 
    ::= { cLMobilityExtMCClientEntry 3 }

cLMobilityExtMCClientAssociatedMCAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's associated MC
        (local or foreign) IP address type." 
    ::= { cLMobilityExtMCClientEntry 4 }

cLMobilityExtMCClientAssociatedMCAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's associated MC
        (local or foreign) IP address. The type of this 
        address is determined by the value of 
        cLMobilityExtMCClientAssociatedMCAddressType." 
    ::= { cLMobilityExtMCClientEntry 5 }

cLMobilityExtMCClientAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client IP address type." 
    ::= { cLMobilityExtMCClientEntry 6 }

cLMobilityExtMCClientAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client IP address. The type
        of this address is determined by the value of
        cLMobilityExtMCClientAddressType." 
    ::= { cLMobilityExtMCClientEntry 7 }

cLMobilityExtMCClientState OBJECT-TYPE
    SYNTAX          INTEGER  {
                        init(0),
                        local(1),
                        foreign(2),
                        anchor(3)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client state.
        init(0) - Client is not associated. 
        local(1) - Client is local to Mobility Controller.
        foreign(2) - Client is foreign to Mobility Controller.
        anchor(3) - Client is anchor to Mobility Controller." 
    ::= { cLMobilityExtMCClientEntry 8 }

cLMobilityExtMCClientAssociationTime OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "This object indicates the client's association time.
        The object cLMobilityExtMCClientUpTime represents the MC 
        client up time since its association.
        cLMobilityExtMCClientAssociationTime object is superseded by 
        cLMobilityExtMCClientUpTime." 
    ::= { cLMobilityExtMCClientEntry 9 }

cLMobilityExtMCClientLocalClient OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates whether the client is local.
        A value of 'true' indicates the client is local. 
        A value of 'false' indicates the client is not local to this 
        MC." 
    ::= { cLMobilityExtMCClientEntry 10 }

cLMobilityExtMCClientAnchorMCGroupId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's anchor MC mobility
        group ID." 
    ::= { cLMobilityExtMCClientEntry 11 }

cLMobilityExtMCClientAssociatedMCGroupId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's associated MC
        (local or foreign) mobility group ID." 
    ::= { cLMobilityExtMCClientEntry 12 }

cLMobilityExtMCClientAssociatedMAAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the MA local or foreign IP
        address type." 
    ::= { cLMobilityExtMCClientEntry 13 }

cLMobilityExtMCClientAssociatedMAAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the MA local or foreign IP address.
        The type of this address is determined by the value of
        cLMobilityExtMCClientAssociatedMAAddressType." 
    ::= { cLMobilityExtMCClientEntry 14 }

cLMobilityExtMCClientAnchorMAAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the MA anchor's IP address type." 
    ::= { cLMobilityExtMCClientEntry 15 }

cLMobilityExtMCClientAnchorMAAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the MA anchor's IP address. The
        type of this address is determined by the value of
        cLMobilityExtMCClientAnchorMAAddressType." 
    ::= { cLMobilityExtMCClientEntry 16 }

cLMobilityExtMCClientUpTime OBJECT-TYPE
    SYNTAX          CiscoAbsZeroBasedCounter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The object indicates the MC client up time since its
        association." 
    ::= { cLMobilityExtMCClientEntry 17 }
 

-- *******************************************************************
-- Mobility Clients table reported by Mobility Oracle (MO)
-- *******************************************************************

cLMobilityExtMOClientTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtMOClientEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the
        802.11 LWAPP Mobility Clients on this MO."
    ::= { ciscoLwappMobilityExtTableObjects 7 }

cLMobilityExtMOClientEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtMOClientEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information about
        one 802.11 LWAPP mobility Clients on this MO."
    INDEX           { cLMobilityExtMOClientMacAddress } 
    ::= { cLMobilityExtMOClientTable 1 }

CLMobilityExtMOClientEntry ::= SEQUENCE {
        cLMobilityExtMOClientMacAddress                     MacAddress,
        cLMobilityExtMOClientAnchorMCPublicAddressType      InetAddressType,
        cLMobilityExtMOClientAnchorMCPublicAddress          InetAddress,
        cLMobilityExtMOClientAnchorMCPrivateAddressType     InetAddressType,
        cLMobilityExtMOClientAnchorMCPrivateAddress         InetAddress,
        cLMobilityExtMOClientAssociatedMCPublicAddressType  InetAddressType,
        cLMobilityExtMOClientAssociatedMCPublicAddress      InetAddress,
        cLMobilityExtMOClientAssociatedMCPrivateAddressType InetAddressType,
        cLMobilityExtMOClientAssociatedMCPrivateAddress     InetAddress,
        cLMobilityExtMOClientAddressType                    InetAddressType,
        cLMobilityExtMOClientAddress                        InetAddress,
        cLMobilityExtMOClientLocalTime                      DateAndTime,
        cLMobilityExtMOClientAssociationTime                Counter64,
        cLMobilityExtMOClientUpTime                         CiscoAbsZeroBasedCounter64
}

cLMobilityExtMOClientMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the client MAC address." 
    ::= { cLMobilityExtMOClientEntry 1 }

cLMobilityExtMOClientAnchorMCPublicAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's anchor MC public
        IP address type." 
    ::= { cLMobilityExtMOClientEntry 2 }

cLMobilityExtMOClientAnchorMCPublicAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's anchor MC public
        IP address. The type of this address is determined by the 
        value of cLMobilityExtMOClientAnchorMCPublicAddressType." 
    ::= { cLMobilityExtMOClientEntry 3 }

cLMobilityExtMOClientAnchorMCPrivateAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's anchor MC private
        IP address type." 
    ::= { cLMobilityExtMOClientEntry 4 }

cLMobilityExtMOClientAnchorMCPrivateAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's anchor MC private
        IP address. The type of this address is determined by 
        the value of cLMobilityExtMOClientAnchorMCPrivateAddressType." 
    ::= { cLMobilityExtMOClientEntry 5 }

cLMobilityExtMOClientAssociatedMCPublicAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's associated MC
        (local or foreign) public IP address type." 
    ::= { cLMobilityExtMOClientEntry 6 }

cLMobilityExtMOClientAssociatedMCPublicAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's associated MC
        (local or foreign) public IP address. The type of 
        this address is determined by the value of
        cLMobilityExtMOClientAssociatedMCPublicAddressType." 
    ::= { cLMobilityExtMOClientEntry 7 }

cLMobilityExtMOClientAssociatedMCPrivateAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's associated MC
        (local or foreign) private IP address type." 
    ::= { cLMobilityExtMOClientEntry 8 }

cLMobilityExtMOClientAssociatedMCPrivateAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's associated MC
        (local or foreign) private IP address. The
        type of this address is determined by the value of
        cLMobilityExtMOClientAssociatedMCPrivateAddressType." 
    ::= { cLMobilityExtMOClientEntry 9 }

cLMobilityExtMOClientAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client IP address type." 
    ::= { cLMobilityExtMOClientEntry 10 }

cLMobilityExtMOClientAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client IP address. The
        type of this address is determined by the value of
        cLMobilityExtMOClientAddressType." 
    ::= { cLMobilityExtMOClientEntry 11 }

cLMobilityExtMOClientLocalTime OBJECT-TYPE
    SYNTAX          DateAndTime
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's local time." 
    ::= { cLMobilityExtMOClientEntry 12 }

cLMobilityExtMOClientAssociationTime OBJECT-TYPE
    SYNTAX          Counter64
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          deprecated
    DESCRIPTION
        "This object represents the client's association time.
        The object cLMobilityExtMOClientUpTime represents the 
        up time of the MO client since its association
        cLMobilityExtMOClientAssociationTime object is superseded
        by cLMobilityExtMOClientUpTime." 
    ::= { cLMobilityExtMOClientEntry 13 }

cLMobilityExtMOClientUpTime OBJECT-TYPE
    SYNTAX          CiscoAbsZeroBasedCounter64
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the client's up time since its
        association." 
    ::= { cLMobilityExtMOClientEntry 14 }
 

-- *******************************************************************
-- Mobility AP Manager table (applicable to Mobility Controller
-- with AP-manager interface )
-- *******************************************************************

cLMobilityExtApMgrTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtApMgrEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the
        802.11 LWAPP mobility AP Manager."
    ::= { ciscoLwappMobilityExtTableObjects 8 }

cLMobilityExtApMgrEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtApMgrEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information about
        one 802.11 LWAPP mobility AP Manager configured 
        on this controller."
    INDEX           { cLMobilityExtApMgrName } 
    ::= { cLMobilityExtApMgrTable 1 }

CLMobilityExtApMgrEntry ::= SEQUENCE {
        cLMobilityExtApMgrName          SnmpAdminString,
        cLMobilityExtApMgrAddressType   InetAddressType,
        cLMobilityExtApMgrAddress       InetAddress,
        cLMobilityExtApMgrNetmaskType   InetAddressType,
        cLMobilityExtApMgrNetmask       InetAddress,
        cLMobilityExtApMgrMacAddress    MacAddress,
        cLMobilityExtApMgrVlanId        Unsigned32,
        cLMobilityExtApMgrInterfaceType INTEGER,
        cLMobilityExtApMgrRowStatus     RowStatus
}

cLMobilityExtApMgrName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the name for this AP manager." 
    ::= { cLMobilityExtApMgrEntry 1 }

cLMobilityExtApMgrAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the AP manager's IP address type." 
    ::= { cLMobilityExtApMgrEntry 2 }

cLMobilityExtApMgrAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the AP manager's IP address. The
        type of this address is determined by the value of
        cLMobilityExtApMgrAddressType." 
    ::= { cLMobilityExtApMgrEntry 3 }

cLMobilityExtApMgrNetmaskType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the AP manager's netmask type." 
    ::= { cLMobilityExtApMgrEntry 4 }

cLMobilityExtApMgrNetmask OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the AP manager's netmask. The
        type of this address is determined by the value of
        cLMobilityExtApMgrNetmaskType." 
    ::= { cLMobilityExtApMgrEntry 5 }

cLMobilityExtApMgrMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the mac address for this AP manager." 
    ::= { cLMobilityExtApMgrEntry 6 }

cLMobilityExtApMgrVlanId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the VLAN Id for this AP manager." 
    ::= { cLMobilityExtApMgrEntry 7 }

cLMobilityExtApMgrInterfaceType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        management(1),
                        ap(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the AP manager interface type.
        It can be of two types:
        management(1) - For in-band management of the controller.
        ap(2) - For L3 communications between the controller and LWAPP 
                APs." 
    ::= { cLMobilityExtApMgrEntry 8 }

cLMobilityExtApMgrRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and used
        to create and delete specific instances of rows             
        in this table." 
    ::= { cLMobilityExtApMgrEntry 9 }
 

-- *******************************************************************
-- Mobility Foreign WLC Map table (applicable to WLC)
-- *******************************************************************

cLMobilityExtForeignWlcMapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtForeignWlcMapEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains mappings of the foreign controller
        with the interface/interface group to be used, when clients
        directly connected to the foreign controller send the DHCP
        request to the anchor controller."
    ::= { ciscoLwappMobilityExtTableObjects 9 }

cLMobilityExtForeignWlcMapEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtForeignWlcMapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a row in the
        cLMobilityExtForeignWlcIfMappingTable. The entries are added 
        and deleted by explicit user driven action."
    INDEX           {
                        cLWlanIndex,
                        cLMobilityExtForeignWlcAddressType,
                        cLMobilityExtForeignWlcAddress
                    } 
    ::= { cLMobilityExtForeignWlcMapTable 1 }

CLMobilityExtForeignWlcMapEntry ::= SEQUENCE {
        cLMobilityExtForeignWlcAddressType  InetAddressType,
        cLMobilityExtForeignWlcAddress      InetAddress,
        cLMobilityExtForeignWlcMapIf        SnmpAdminString,
        cLMobilityExtForeignWlcMapRowStatus RowStatus
}

cLMobilityExtForeignWlcAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the IP address type of
        the foreign controller,to which the interface 
        mapping is to be configured." 
    ::= { cLMobilityExtForeignWlcMapEntry 1 }

cLMobilityExtForeignWlcAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the IP address of
        the foreign controller,to which the interface 
        mapping is to be configured. The type of this address
        is determined by the value of
        cLMobilityExtForeignWlcAddressType." 
    ::= { cLMobilityExtForeignWlcMapEntry 2 }

cLMobilityExtForeignWlcMapIf OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies name of the
        interface/interface group which would be 
        used for the communication with the clients 
        connected to the foreign controller ." 
    ::= { cLMobilityExtForeignWlcMapEntry 3 }

cLMobilityExtForeignWlcMapRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and used
        to create and delete specific instances of rows             
        in this table." 
    ::= { cLMobilityExtForeignWlcMapEntry 4 }
 

-- *******************************************************************
-- Mobility group info table (applicable to Mobility Controller)
-- *******************************************************************

cLMobilityExtGroupTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtGroupEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the
        mobility groups where clients from this MC can roam."
    ::= { ciscoLwappMobilityExtTableObjects 10 }

cLMobilityExtGroupEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtGroupEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information about
        one mobility group."
    INDEX           { cLMobilityExtGroupName } 
    ::= { cLMobilityExtGroupTable 1 }

CLMobilityExtGroupEntry ::= SEQUENCE {
        cLMobilityExtGroupName                   SnmpAdminString,
        cLMobilityExtGroupMulticastAddressType   InetAddressType,
        cLMobilityExtGroupMulticastAddress       InetAddress,
        cLMobilityExtGroupRowStatus              RowStatus,
        cLMobilityExtGroupMulticastMode          TruthValue,
        cLMobilityExtGroupMulticastModev6        TruthValue,
        cLMobilityExtGroupMulticastAddressv6Type InetAddressType,
        cLMobilityExtGroupMulticastAddressv6     InetAddress
}

cLMobilityExtGroupName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the name for the mobility group." 
    ::= { cLMobilityExtGroupEntry 1 }

cLMobilityExtGroupMulticastAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the multicast IP address type
        for the mobility group." 
    ::= { cLMobilityExtGroupEntry 2 }

cLMobilityExtGroupMulticastAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the multicast IP address for the
        mobility group. The type of this address is determined
        by the value of cLMobilityExtGroupMulticastAddressType." 
    ::= { cLMobilityExtGroupEntry 3 }

cLMobilityExtGroupRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and used
        to create and delete specific instances of rows             
        in this table." 
    ::= { cLMobilityExtGroupEntry 4 }

cLMobilityExtGroupMulticastMode OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the IPv4 multicast mode for the
        mobility group." 
    ::= { cLMobilityExtGroupEntry 5 }

cLMobilityExtGroupMulticastModev6 OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the IPv6 multicast mode for the
        mobility group." 
    ::= { cLMobilityExtGroupEntry 6 }

cLMobilityExtGroupMulticastAddressv6Type OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the multicast IPv6 address type
        for the mobility group." 
    ::= { cLMobilityExtGroupEntry 7 }

cLMobilityExtGroupMulticastAddressv6 OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the multicast IPv6 address for the
        mobility group." 
    ::= { cLMobilityExtGroupEntry 8 }
 

-- *******************************************************************
-- Mobility Agent (MA) peer member table
-- *******************************************************************

cLMobilityExtMAPeerTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtMAPeerEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the
        802.11 LWAPP SPG peer members of this MA."
    ::= { ciscoLwappMobilityExtTableObjects 11 }

cLMobilityExtMAPeerEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtMAPeerEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information about
        one 802.11 LWAPP mobility SPG peer member of this MA."
    INDEX           {
                        cLMobilityExtMAPeerPrivateAddressType,
                        cLMobilityExtMAPeerPrivateAddress
                    } 
    ::= { cLMobilityExtMAPeerTable 1 }

CLMobilityExtMAPeerEntry ::= SEQUENCE {
        cLMobilityExtMAPeerPrivateAddressType InetAddressType,
        cLMobilityExtMAPeerPrivateAddress     InetAddress,
        cLMobilityExtMAPeerPublicAddressType  InetAddressType,
        cLMobilityExtMAPeerPublicAddress      InetAddress,
        cLMobilityExtMAPeerLinkStatus         INTEGER
}

cLMobilityExtMAPeerPrivateAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents this MA peer's private IP address type." 
    ::= { cLMobilityExtMAPeerEntry 1 }

cLMobilityExtMAPeerPrivateAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents this MA peer's private IP address. The
        type of this address is determined by the value of
        cLMobilityExtMAPeerPrivateAddressType." 
    ::= { cLMobilityExtMAPeerEntry 2 }

cLMobilityExtMAPeerPublicAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates this MA peer's public IP address type." 
    ::= { cLMobilityExtMAPeerEntry 3 }

cLMobilityExtMAPeerPublicAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates this MA peer's public address. The
        type of this address is determined by the value of
        cLMobilityExtMAPeerPublicAddressType." 
    ::= { cLMobilityExtMAPeerEntry 4 }

cLMobilityExtMAPeerLinkStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        notconfigured(0),
                        datapathdown(1),
                        controlpathdown(2),
                        bothdown(3),
                        up(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the control path and data path status
        of the link between this MA and its peer MA in the same SPG.

        notconfigured(0) - This means group member is not configured
                           for ICMP or EoIP pings.

        datapathdown(1) - This means group member is not responding
                          to EoIP pings.

        controlpathdown(2) - This means successive ICMP pings
                             to the group member have failed.

        bothdown(3) - This means group member is not responding
                      to ICMP or EOIP pings.

        up(4) - This means group member is responding to
                both EOIP and ICMP pings." 
    ::= { cLMobilityExtMAPeerEntry 5 }
 

-- *******************************************************************
-- Mobility Agent (MA) statistics reported by Mobility Controller
-- *******************************************************************

cLMobilityExtMCMAStatisticsTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtMCMAStatisticsEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the
        MA statistics as reported by this MC."
    ::= { ciscoLwappMobilityExtTableObjects 12 }

cLMobilityExtMCMAStatisticsEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtMCMAStatisticsEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information about
        statistics of one MA that is associated with this MC."
    INDEX           {
                        cLMobilityExtMCMAPrivateAddressType,
                        cLMobilityExtMCMAPrivateAddress
                    } 
    ::= { cLMobilityExtMCMAStatisticsTable 1 }

CLMobilityExtMCMAStatisticsEntry ::= SEQUENCE {
        cLMobilityExtMCMAPrivateAddressType InetAddressType,
        cLMobilityExtMCMAPrivateAddress     InetAddress,
        cLMobilityExtMCMAClientCount        Unsigned32
}

cLMobilityExtMCMAPrivateAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the MA's private IP address type." 
    ::= { cLMobilityExtMCMAStatisticsEntry 1 }

cLMobilityExtMCMAPrivateAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the MA's private IP address. The
        type of this address is determined by the value of
        cLMobilityExtMCMAPrivateAddressType." 
    ::= { cLMobilityExtMCMAStatisticsEntry 2 }

cLMobilityExtMCMAClientCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the MA's client count." 
    ::= { cLMobilityExtMCMAStatisticsEntry 3 }
 

-- *******************************************************************
-- Associated APs reported to Mobility Controller
-- *******************************************************************

cLMobilityExtMCAPTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtMCAPEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the
        APs that are reported by this MC, its peer MCs and its MAs."
    ::= { ciscoLwappMobilityExtTableObjects 13 }

cLMobilityExtMCAPEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtMCAPEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information about AP that
        is reported by this MC or its peer MC or its MA."
    INDEX           { cLMobilityExtMCAPMacAddress } 
    ::= { cLMobilityExtMCAPTable 1 }

CLMobilityExtMCAPEntry ::= SEQUENCE {
        cLMobilityExtMCAPMacAddress                 MacAddress,
        cLMobilityExtMCAPName                       SnmpAdminString,
        cLMobilityExtMCAPReportingDeviceAddressType InetAddressType,
        cLMobilityExtMCAPReportingDeviceAddress     InetAddress,
        cLMobilityExtMCAPReportingDeviceType        INTEGER
}

cLMobilityExtMCAPMacAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the reported AP's mac address." 
    ::= { cLMobilityExtMCAPEntry 1 }

cLMobilityExtMCAPName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the reported AP's name." 
    ::= { cLMobilityExtMCAPEntry 2 }

cLMobilityExtMCAPReportingDeviceAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object insdicates the reporting device's IP address type." 
    ::= { cLMobilityExtMCAPEntry 3 }

cLMobilityExtMCAPReportingDeviceAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the reporting device's IP address. The
        type of this address is determined by the value of 
        cLMobilityExtMCAPReportingDeviceAddressType." 
    ::= { cLMobilityExtMCAPEntry 4 }

cLMobilityExtMCAPReportingDeviceType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        peerMC(0),
                        associatedMA(1),
                        localMC(2)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the reporting device's type:
        this MC, or its peer MC or its MA.
        peerMC(0) - The reporting device is peer Mobility Controller. 
        associatedMA(1) - The reporting device is Mobility Agent.
        localMC(2) - The reporting device is local Mobility Controller." 
    ::= { cLMobilityExtMCAPEntry 5 }
 

-- *******************************************************************
-- Associated APs count reported to Mobility Controller
-- *******************************************************************

cLMobilityExtMCAPCountTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityExtMCAPCountEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table contains the information about the total number
        of APs that are reported by this MC, its peer MCs and its MAs."
    ::= { ciscoLwappMobilityExtTableObjects 14 }

cLMobilityExtMCAPCountEntry OBJECT-TYPE
    SYNTAX          CLMobilityExtMCAPCountEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents information on total number
        of APs that is reported by this MC or its peer MC or its MA."
    INDEX           {
                        cLMobilityExtMCAPCountReportingDeviceAddressType,
                        cLMobilityExtMCAPCountReportingDeviceAddress
                    } 
    ::= { cLMobilityExtMCAPCountTable 1 }

CLMobilityExtMCAPCountEntry ::= SEQUENCE {
        cLMobilityExtMCAPCountReportingDeviceAddressType InetAddressType,
        cLMobilityExtMCAPCountReportingDeviceAddress     InetAddress,
        cLMobilityExtMCAPCount                           Unsigned32
}

cLMobilityExtMCAPCountReportingDeviceAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the reporting device's IP address type." 
    ::= { cLMobilityExtMCAPCountEntry 1 }

cLMobilityExtMCAPCountReportingDeviceAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the reporting device's IP address. The
        type of this address is determined by the value of
        cLMobilityExtMCAPCountReportingDeviceAddressType." 
    ::= { cLMobilityExtMCAPCountEntry 2 }

cLMobilityExtMCAPCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of APs reported by
        this device: this MC, or its peer MC or its MA." 
    ::= { cLMobilityExtMCAPCountEntry 3 }
 


cLMobilityAnchorPolicyEntryTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLMobilityAnchorPolicyEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides information about
        one 802.11 LWAPP Mobility Anchor configured with a policy name
        on this controller"
    ::= { ciscoLwappMobilityExtTableObjects 15 }

cLMobilityAnchorWlanPolicyEntry OBJECT-TYPE
    SYNTAX          CLMobilityAnchorPolicyEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table provides information about
        one 802.11 LWAPP Mobility Anchor configured with a policy name
        on this controller.
        Each row represent an Ip anchor associated with a policy.
        A row is added when a new anchor is added"
    INDEX           {
                        cLWlanWlanPolicyName,
                        cLMobilityAnchorPolicyMCAddressType,
                        cLMobilityAnchorPolicyMCAddress
                    } 
    ::= { cLMobilityAnchorPolicyEntryTable 1 }

CLMobilityAnchorPolicyEntry ::= SEQUENCE {
        cLMobilityAnchorPolicyMCAddressType InetAddressType,
        cLMobilityAnchorPolicyMCAddress     InetAddress,
        cLMobilityAnchorPolicyRowStatus     RowStatus,
        cLMobilityAnchorPolicyMCPriority    INTEGER
}

cLMobilityAnchorPolicyMCAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the anchor's IP address type." 
    ::= { cLMobilityAnchorWlanPolicyEntry 1 }

cLMobilityAnchorPolicyMCAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the anchor's IP address" 
    ::= { cLMobilityAnchorWlanPolicyEntry 2 }

cLMobilityAnchorPolicyRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and used
        to create and delete specific instances of rows
        in this table." 
    ::= { cLMobilityAnchorWlanPolicyEntry 3 }

cLMobilityAnchorPolicyMCPriority OBJECT-TYPE
    SYNTAX          INTEGER  {
                        local(1),
                        primary(2),
                        secondary(3),
                        tertiary(4)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies priority of the mobility anchor (for the foreign
        controller)
        A value of '1' indicates local anchor priority (this is not permitted
        to be configured)
        A value of '2' indicates primary anchor priority.
        A value of '3' indicated secondary anchor priority.
        A value of '4' indicated tertiary anchor priority." 
    ::= { cLMobilityAnchorWlanPolicyEntry 4 }
 


-- *******************************************************************
-- Mobility Agent (MA) global parameters
-- *******************************************************************

cLMobilityExtMAMCPublicAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the MC's public IP address type
        for this MA." 
    ::= { ciscoLwappMobilityExtMAGlobalObjects 1 }

cLMobilityExtMAMCPublicAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the MC's public IP address
        for this MA. The type of this address is determined by 
        the value of cLMobilityExtMAMCPublicAddressType." 
    ::= { ciscoLwappMobilityExtMAGlobalObjects 2 }

cLMobilityExtMAMCPrivateAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the MC's private IP address type
        for this MA." 
    ::= { ciscoLwappMobilityExtMAGlobalObjects 3 }

cLMobilityExtMAMCPrivateAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the MC's private IP address for
        this MA. The type of this address is determined by the 
        value of cLMobilityExtMAMCPrivateAddressType." 
    ::= { ciscoLwappMobilityExtMAGlobalObjects 4 }

cLMobilityExtMAToMCLinkStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        notconfigured(0),
                        datapathdown(1),
                        controlpathdown(2),
                        bothdown(3),
                        up(4)
                    }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the control path and data path status
        of the link between this Mobility Agent(MA) and its  mobility 
        controller.
        notconfigured(0) - This indicates that link between MA and MC 
                           is not configured for ICMP or EoIP pings.

        datapathdown(1) - This indicates that link between MA and MC is 
                          not responding to EoIP pings.

        controlpathdown(2) - This indicates that link between MA and MC 
                             successive ICMP pings to the group have 
                             failed.

        bothdown(3) - This indicates that link between MA and MC is not 
                      responding to ICMP or EOIP pings.

        up(4) - This indicates that link between MA and MC is 
                responding to both EOIP and ICMP pings." 
    ::= { ciscoLwappMobilityExtMAGlobalObjects 5 }

cLMobilityExtMASpgPeerCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the number of peer members of this
        mobility agent (MA)." 
    ::= { ciscoLwappMobilityExtMAGlobalObjects 6 }

cLMobilityExtMASpgName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..32))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the Switch Peer Group (SPG) name where
        this MA belongs." 
    ::= { ciscoLwappMobilityExtMAGlobalObjects 7 }

cLMobilityExtMAOwnMulticastAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the multicast address type for
        the own SPG group. SPG represents the switch peer group which
        indicates the proximity group inside which the WiFi
        client has most likelihood of roaming. Each device belongs
        to a SPG which is identified by a SPG name and optionally
        it could have a multicast ip address as well." 
    ::= { ciscoLwappMobilityExtMAGlobalObjects 8 }

cLMobilityExtMAOwnMulticastAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the multicast address for the own
        SPG group. The type of this address is determined by the
        value of cLMobilityExtMAOwnMulticastAddressType." 
    ::= { ciscoLwappMobilityExtMAGlobalObjects 9 }

cLMobilityExtMAKeepAliveCount OBJECT-TYPE
    SYNTAX          Unsigned32 (3..20)
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the keep alive count.
        If keep alive response is not received consecutively
        for N (keep alive count) times, the mobility link is
        declared as down."
    DEFVAL          { 3 } 
    ::= { ciscoLwappMobilityExtMAGlobalObjects 10 }

cLMobilityExtMAKeepAliveInterval OBJECT-TYPE
    SYNTAX          Unsigned32 (1..30)
    UNITS           "seconds"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the keep alive interval.
        Each MA sends periodically keep alive packet to other
        mobility devices (MA or MC)."
    DEFVAL          { 10 } 
    ::= { ciscoLwappMobilityExtMAGlobalObjects 11 }

cLMobilityExtMADscpValue OBJECT-TYPE
    SYNTAX          Dscp
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the Differentiated Services Code Point
        (DSCP) value. Here it is used for classifying and managing 
        mobility control packets and providing quality of service (QoS)
        on IP networks."
    DEFVAL          { 0 } 
    ::= { ciscoLwappMobilityExtMAGlobalObjects 12 }

-- *******************************************************************
-- Mobility Controller (MC) statistics
-- *******************************************************************

cLMobilityExtMCReceivedTotal OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number
        of mobility control messages received by 
        the Mobility Controller." 
    ::= { ciscoLwappMobilityExtMCStats 1 }

cLMobilityExtMCReceivedDrops OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number
        of mobility control messages dropped by 
        Mobility Controller." 
    ::= { ciscoLwappMobilityExtMCStats 2 }

cLMobilityExtMCProtocolReceiveErrors OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of mobility control
        error messages received by the Mobility Controller.The 
        counter represents the received packet errors as seen by the
        controller deviating from the proprietary mobility protocol
        which is instrumental in achieving the seamless WiFi client
        roaming." 
    ::= { ciscoLwappMobilityExtMCStats 3 }

cLMobilityExtMCProtocolTransmitErrors OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of
        mobility control error messages on transmit 
        side of Mobility Controller.The counter represents the
        transmit packet errors as seen by the controller deviating 
        from the proprietary mobility protocol,which is instrumental
        in achieving the seamless WiFi client roaming." 
    ::= { ciscoLwappMobilityExtMCStats 4 }

cLMobilityExtMCStateErrors OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the state transition
        errors on Mobility Controller." 
    ::= { ciscoLwappMobilityExtMCStats 5 }

cLMobilityExtMCProtocolRetransmitted OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of control
        messages retransmitted by Mobility Controller." 
    ::= { ciscoLwappMobilityExtMCStats 6 }

cLMobilityExtMCHandoffRequestsReceived OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the handoff requests
        received by Mobility Controller." 
    ::= { ciscoLwappMobilityExtMCStats 7 }

cLMobilityExtMCHandoffCompleteReceived OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the handoff completion
        received  by Mobility Controller." 
    ::= { ciscoLwappMobilityExtMCStats 8 }

cLMobilityExtMCHandoffClientDeleteReceived OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number of client
        deletes received by Mobility Controller." 
    ::= { ciscoLwappMobilityExtMCStats 9 }

cLMobilityExtMCHandoffRequestsTransmitted OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the handoff requests
        transmitted by Mobility Controller." 
    ::= { ciscoLwappMobilityExtMCStats 10 }

cLMobilityExtMCHandoffCompleteTransmitted OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the handoff completion
        transmitted by Mobility Controller." 
    ::= { ciscoLwappMobilityExtMCStats 11 }

cLMobilityExtMCHandoffClientDeleteTransmitted OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the nubmer of client deletes
        transmitted by Mobility Controller." 
    ::= { ciscoLwappMobilityExtMCStats 12 }

cLMobilityExtMCTotalClientCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total client count
        on Mobility Controller." 
    ::= { ciscoLwappMobilityExtMCStats 13 }

cLMobilityExtMCWgbCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the WGB(Work Group Bridge)
        count on Mobility Controller." 
    ::= { ciscoLwappMobilityExtMCStats 14 }

-- *************************************************************
-- extra trap variables definining here
-- *************************************************************

cLMobilityExtNotifyObjectSourceIPAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object represents the source address type." 
    ::= { ciscoLwappMobilityExtNotifObjects 1 }

cLMobilityExtNotifyObjectSourceIPAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object represents the sourc address. The type
        of this address is determined by the value of
        cLMobilityExtNotifyObjectSourceIPAddressType." 
    ::= { ciscoLwappMobilityExtNotifObjects 2 }

cLMobilityExtNotifyObjectSourceType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(0),
                        mobilityAgent(1),
                        mobilityController(2),
                        mobilityOracle(3)
                    }
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object represents mobility source type.
        unknown(0) - The source of the messages is unknown. 
        mobilityAgent(1) - The source of the messages is Mobility 
                           Agent.
        mobilityController(2) - The source of the messages is Mobility
                                Controller.
        mobilityOracle(3) - The source of the messages is Mobility 
                            Oracle." 
    ::= { ciscoLwappMobilityExtNotifObjects 3 }

cLMobilityExtNotifyObjectDestinationType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unknown(0),
                        mobilityAgent(1),
                        mobilityController(2),
                        mobilityOracle(3)
                    }
    MAX-ACCESS      accessible-for-notify
    STATUS          current
    DESCRIPTION
        "This object represents the mobility destination type.
        unknown(0) - The destination of the messages is unknown. 
        mobilityAgent(1) - The destination of the messages is Mobility 
                           Agent.
        mobilityController(2) - The destination of the messages is 
                                Mobility Controller.
        mobilityOracle(3) - The destination of the messages is Mobility 
                            Oracle." 
    ::= { ciscoLwappMobilityExtNotifObjects 4 }

-- *******************************************************************
-- Mobility Agent (MA) statistics
-- *******************************************************************

cLMobilityExtMAReceivedTotal OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number
        of mobility control messages received by 
        the Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 1 }

cLMobilityExtMAReceivedDrops OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number
        of mobility control messages dropped by 
        Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 2 }

cLMobilityExtMAProtocolReceiveErrors OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number
        of mobility control error messages received 
        by the Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 3 }

cLMobilityExtMAProtocolTransmitErrors OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number
        of mobility control error messages on 
        transmit side of Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 4 }

cLMobilityExtMAStateErrors OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the state transition
        errors on Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 5 }

cLMobilityExtMAProtocolRetransmitted OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total number
        of control messages retransmitted by 
        Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 6 }

cLMobilityExtMATotalClients OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total clients
        connected to Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 7 }

cLMobilityExtMALocalClients OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates local clients connected
        to  Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 8 }

cLMobilityExtMAAnchoredClients OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the anchored clients
        connected to Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 9 }

cLMobilityExtMAForeignedClients OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the foreign clients
        connected to Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 10 }

cLMobilityExtMATotalInterGroupHandoffReceived OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total inter group
        handoff received by Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 11 }

cLMobilityExtMATotalIntraGroupHandoffReceived OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total intra group
        handoffs received by Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 12 }

cLMobilityExtMATotalHandoffEndRequestReceived OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total handoff end
        requests received by Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 13 }

cLMobilityExtMATotalInterGroupHandoffSent OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total inter group
        handoffs sent by Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 14 }

cLMobilityExtMATotalIntraGroupHandoffSent OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total intra group
        handoffs sent by Mobility Agent." 
    ::= { ciscoLwappMobilityExtMAStats 15 }

cLMobilityExtReceivedTotal OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total received ." 
    ::= { ciscoLwappMobilityExtGlobalStats 1 }

cLMobilityExtTransmitTotal OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total transmitted." 
    ::= { ciscoLwappMobilityExtGlobalStats 2 }

cLMobilityExtTotalResourceAllocation OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total resources allocated ." 
    ::= { ciscoLwappMobilityExtGlobalStats 3 }

cLMobilityExtTotalResourceFree OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the total resources free ." 
    ::= { ciscoLwappMobilityExtGlobalStats 4 }

-- *******************************************************************
-- *   NOTIFICATIONS
-- *******************************************************************

ciscoLwappMobilityControlPathDown NOTIFICATION-TYPE
    OBJECTS         {
                        cLMobilityExtNotifyObjectSourceIPAddressType,
                        cLMobilityExtNotifyObjectSourceIPAddress,
                        cLMobilityExtNotifyObjectSourceType,
                        cLMobilityExtNotifyObjectDestinationType
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent by the agent when
        a mobility control path goes down."
   ::= { ciscoLwappMobilityExtMIBNotifs 1 }

ciscoLwappMobilityControlPathUp NOTIFICATION-TYPE
    OBJECTS         {
                        cLMobilityExtNotifyObjectSourceIPAddressType,
                        cLMobilityExtNotifyObjectSourceIPAddress,
                        cLMobilityExtNotifyObjectSourceType,
                        cLMobilityExtNotifyObjectDestinationType
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent by the agent when
        a mobility control path goes up."
   ::= { ciscoLwappMobilityExtMIBNotifs 2 }

ciscoLwappMobilityDataPathDown NOTIFICATION-TYPE
    OBJECTS         {
                        cLMobilityExtNotifyObjectSourceIPAddressType,
                        cLMobilityExtNotifyObjectSourceIPAddress,
                        cLMobilityExtNotifyObjectSourceType,
                        cLMobilityExtNotifyObjectDestinationType
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent by the agent when
        a mobility data path goes down."
   ::= { ciscoLwappMobilityExtMIBNotifs 3 }

ciscoLwappMobilityDataPathUp NOTIFICATION-TYPE
    OBJECTS         {
                        cLMobilityExtNotifyObjectSourceIPAddressType,
                        cLMobilityExtNotifyObjectSourceIPAddress,
                        cLMobilityExtNotifyObjectSourceType,
                        cLMobilityExtNotifyObjectDestinationType
                    }
    STATUS          current
    DESCRIPTION
        "This notification is sent by the agent when
        a mobility data path goes up."
   ::= { ciscoLwappMobilityExtMIBNotifs 4 }
-- *******************************************************************
-- *    Compliance statements
-- *******************************************************************

ciscoLwappMobilityExtMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtMIBConform 1 }

ciscoLwappMobilityExtMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoLwappMobilityExtMIBConform 2 }


ciscoLwappMobilityExtMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappMobilityExtMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cLMobilityExtConfigGroup,
                        ciscoLwappMobilityExtNotifyObjectsGroup,
                        ciscoLwappMobilityExtNotifsGroup
                    }
    ::= { ciscoLwappMobilityExtMIBCompliances 1 }

ciscoLwappMobilityExtMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappMobilityExtMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cLMobilityExtConfigGroupRev1,
                        ciscoLwappMobilityExtNotifyObjectsGroup,
                        ciscoLwappMobilityExtNotifsGroup
                    }
    ::= { ciscoLwappMobilityExtMIBCompliances 2 }

ciscoLwappMobilityExtMIBComplianceRev2 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappMobilityExtMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cLMobilityExtConfigGroupRev1,
                        cLMobilityExtMAStatsConfigGroup,
                        ciscoLwappMobilityExtNotifyObjectsGroup,
                        ciscoLwappMobilityExtNotifsGroup
                    }
    ::= { ciscoLwappMobilityExtMIBCompliances 3 }

ciscoLwappMobilityExtMIBComplianceRev3 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappMobilityExtMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        cLMobilityExtConfigGroupRev1,
                        cLMobilityExtMAStatsConfigGroup,
                        ciscoLwappMobilityExtNotifyObjectsGroup,
                        ciscoLwappMobilityExtNotifsGroup,
                        ciscoLwappMobilityExtMCMAStatsGroup,
                        cLMobilityExtAnchorConfigGroup
                    }
    ::= { ciscoLwappMobilityExtMIBCompliances 4 }

-- *******************************************************************
-- *    Units of conformance
-- *******************************************************************

cLMobilityExtConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLMobilityExtMCMOEnableStatus,
                        cLMobilityExtMCMOAdminEnableStatus,
                        cLMobilityExtMCEnableStatus,
                        cLMobilityExtMCAdminEnableStatus,
                        cLMobilityExtMCMulticastMode,
                        cLMobilityExtMCMulticastModev6,
                        cLMobilityExtMCKeepAliveCount,
                        cLMobilityExtMCKeepAliveInterval,
                        cLMobilityExtMCDscpValue,
                        cLMobilityExtMCMOPublicAddressType,
                        cLMobilityExtMCMOPublicAddress,
                        cLMobilityExtMCApCountLicensesInUse,
                        cLMobilityExtMCOwnGroupMulticastAddressType,
                        cLMobilityExtMCOwnGroupMulticastAddress,
                        cLMobilityExtMCOwnGroupMulticastAddressv6Type,
                        cLMobilityExtMCOwnGroupMulticastAddressv6,
                        cLMobilityExtMCMobilityGroupName,
                        cLMobilityExtMCMONumberOfClients,
                        cLMobilityExtMCNumberOfMCs,
                        cLMobilityExtMCTotalNumberOfReportedAPs,
                        cLMobilityExtMCNumberOfReportedAPsInSubDomain,
                        cLMobilityExtMgrAddressType,
                        cLMobilityExtMgrAddress,
                        cLMobilityExtMgrNetmaskType,
                        cLMobilityExtMgrNetmask,
                        cLMobilityExtMgrMacAddress,
                        cLMobilityExtMgrVlanId,
                        cLMobilityExtMgrName,
                        cLMobilityExtMgrInterfaceType,
                        cLMobilityExtNewArchitectureEnableStatus,
                        cLMobilityExtNewArchitectureAdminEnableStatus,
                        cLMobilityExtMCClientAnchorMCPrivateAddressType,
                        cLMobilityExtMCClientAnchorMCPrivateAddress,
                        cLMobilityExtMCClientAnchorMCGroupId,
                        cLMobilityExtMCClientAssociatedMCGroupId,
                        cLMobilityExtMCClientAssociatedMAAddressType,
                        cLMobilityExtMCClientAssociatedMAAddress,
                        cLMobilityExtMCClientAnchorMAAddressType,
                        cLMobilityExtMCClientAnchorMAAddress,
                        cLMobilityExtSpgGroupId,
                        cLMobilityExtSpgBridgeDomainId,
                        cLMobilityExtSpgMemberCount,
                        cLMobilityExtSpgMulticastAddressType,
                        cLMobilityExtSpgMulticastAddress,
                        cLMobilityExtSpgMulticastMode,
                        cLMobilityExtSpgRowStatus,
                        cLMobilityExtSpgMemberStatus,
                        cLMobilityExtSpgMemberPublicAddressType,
                        cLMobilityExtSpgMemberPublicAddress,
                        cLMobilityExtSpgMemberRowStatus,
                        cLMobilityExtGroupMemberGroupName,
                        cLMobilityExtGroupMemberPublicAddressType,
                        cLMobilityExtGroupMemberPublicAddress,
                        cLMobilityExtGroupMemberStatus,
                        cLMobilityExtGroupMemberMacAddress,
                        cLMobilityExtGroupMemberMulticastAddressType,
                        cLMobilityExtGroupMemberMulticastAddress,
                        cLMobilityExtGroupMemberHashKey,
                        cLMobilityExtGroupMemberRowStatus,
                        cLMobilityExtAnchorStatus,
                        cLMobilityExtAnchorRowStatus,
                        cLMobilityExtMOMCMacAddress,
                        cLMobilityExtMOMCLinkStatus,
                        cLMobilityExtMOMCClientCount,
                        cLMobilityExtMCClientAssociatedMCAddressType,
                        cLMobilityExtMCClientAssociatedMCAddress,
                        cLMobilityExtMCClientAddressType,
                        cLMobilityExtMCClientAddress,
                        cLMobilityExtMCClientState,
                        cLMobilityExtMCClientAssociationTime,
                        cLMobilityExtMCClientLocalClient,
                        cLMobilityExtMOClientAnchorMCPublicAddressType,
                        cLMobilityExtMOClientAnchorMCPublicAddress,
                        cLMobilityExtMOClientAnchorMCPrivateAddressType,
                        cLMobilityExtMOClientAnchorMCPrivateAddress,
                        cLMobilityExtMOClientAssociatedMCPublicAddressType,
                        cLMobilityExtMOClientAssociatedMCPublicAddress,
                        cLMobilityExtMOClientAssociatedMCPrivateAddressType,
                        cLMobilityExtMOClientAssociatedMCPrivateAddress,
                        cLMobilityExtMOClientAddressType,
                        cLMobilityExtMOClientAddress,
                        cLMobilityExtMOClientLocalTime,
                        cLMobilityExtMOClientAssociationTime,
                        cLMobilityExtApMgrAddressType,
                        cLMobilityExtApMgrAddress,
                        cLMobilityExtApMgrNetmaskType,
                        cLMobilityExtApMgrNetmask,
                        cLMobilityExtApMgrMacAddress,
                        cLMobilityExtApMgrVlanId,
                        cLMobilityExtApMgrInterfaceType,
                        cLMobilityExtApMgrRowStatus,
                        cLMobilityExtForeignWlcMapIf,
                        cLMobilityExtForeignWlcMapRowStatus,
                        cLMobilityExtGroupMulticastAddressType,
                        cLMobilityExtGroupMulticastAddress,
                        cLMobilityExtGroupMulticastMode,
                        cLMobilityExtGroupMulticastModev6,
                        cLMobilityExtGroupMulticastAddressv6Type,
                        cLMobilityExtGroupMulticastAddressv6,
                        cLMobilityExtGroupRowStatus,
                        cLMobilityExtMAPeerPublicAddressType,
                        cLMobilityExtMAPeerPublicAddress,
                        cLMobilityExtMAPeerLinkStatus,
                        cLMobilityExtMCMAClientCount,
                        cLMobilityExtMCAPName,
                        cLMobilityExtMCAPReportingDeviceAddressType,
                        cLMobilityExtMCAPReportingDeviceAddress,
                        cLMobilityExtMCAPReportingDeviceType,
                        cLMobilityExtMCAPCount,
                        cLMobilityExtMAMCPublicAddressType,
                        cLMobilityExtMAMCPublicAddress,
                        cLMobilityExtMAMCPrivateAddressType,
                        cLMobilityExtMAMCPrivateAddress,
                        cLMobilityExtMAToMCLinkStatus,
                        cLMobilityExtMASpgPeerCount,
                        cLMobilityExtMASpgName,
                        cLMobilityExtMAOwnMulticastAddressType,
                        cLMobilityExtMAOwnMulticastAddress,
                        cLMobilityExtMAKeepAliveCount,
                        cLMobilityExtMAKeepAliveInterval,
                        cLMobilityExtMADscpValue,
                        cLMobilityExtMCReceivedTotal,
                        cLMobilityExtMCReceivedDrops,
                        cLMobilityExtMCProtocolReceiveErrors,
                        cLMobilityExtMCProtocolTransmitErrors,
                        cLMobilityExtMCStateErrors,
                        cLMobilityExtMCProtocolRetransmitted,
                        cLMobilityExtMCHandoffRequestsReceived,
                        cLMobilityExtMCHandoffCompleteReceived,
                        cLMobilityExtMCHandoffClientDeleteReceived,
                        cLMobilityExtMCHandoffRequestsTransmitted,
                        cLMobilityExtMCHandoffCompleteTransmitted,
                        cLMobilityExtMCHandoffClientDeleteTransmitted,
                        cLMobilityExtMCTotalClientCount,
                        cLMobilityExtMCWgbCount
                    }
    STATUS          deprecated
    DESCRIPTION
        "This is a collection of objects which can
        be configured to control Mobility parameters.
        cLMobilityExtConfigGroup object is superseded by 
        cLMobilityExtConfigGroupRev1."
    ::= { ciscoLwappMobilityExtMIBGroups 1 }

ciscoLwappMobilityExtNotifyObjectsGroup OBJECT-GROUP
    OBJECTS         {
                        cLMobilityExtNotifyObjectSourceIPAddressType,
                        cLMobilityExtNotifyObjectSourceIPAddress,
                        cLMobilityExtNotifyObjectSourceType,
                        cLMobilityExtNotifyObjectDestinationType
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects provide the information
        about mobility trap configuration and trap definition.
        These objects are defined under
        cwciscoLwappMobilityExtNotifObjects."
    ::= { ciscoLwappMobilityExtMIBGroups 2 }

ciscoLwappMobilityExtNotifsGroup NOTIFICATION-GROUP
   NOTIFICATIONS    {
                        ciscoLwappMobilityControlPathDown,
                        ciscoLwappMobilityControlPathUp,
                        ciscoLwappMobilityDataPathDown,
                        ciscoLwappMobilityDataPathUp
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects provides the information
        about the notifications sent by the agent related
        to mobility."
    ::= { ciscoLwappMobilityExtMIBGroups 3 }

cLMobilityExtConfigGroupRev1 OBJECT-GROUP
    OBJECTS         {
                        cLMobilityExtMCMOEnableStatus,
                        cLMobilityExtMCMOAdminEnableStatus,
                        cLMobilityExtMCEnableStatus,
                        cLMobilityExtMCAdminEnableStatus,
                        cLMobilityExtMCMulticastMode,
                        cLMobilityExtMCMulticastModev6,
                        cLMobilityExtMCKeepAliveCount,
                        cLMobilityExtMCKeepAliveInterval,
                        cLMobilityExtMCDscpValue,
                        cLMobilityExtMCMOPublicAddressType,
                        cLMobilityExtMCMOPublicAddress,
                        cLMobilityExtMCApCountLicensesInUse,
                        cLMobilityExtMCOwnGroupMulticastAddressType,
                        cLMobilityExtMCOwnGroupMulticastAddress,
                        cLMobilityExtMCOwnGroupMulticastAddressv6Type,
                        cLMobilityExtMCOwnGroupMulticastAddressv6,
                        cLMobilityExtMCMobilityGroupName,
                        cLMobilityExtMCMONumberOfClients,
                        cLMobilityExtMCNumberOfMCs,
                        cLMobilityExtMCTotalNumberOfReportedAPs,
                        cLMobilityExtMCNumberOfReportedAPsInSubDomain,
                        cLMobilityExtMgrAddressType,
                        cLMobilityExtMgrAddress,
                        cLMobilityExtMgrNetmaskType,
                        cLMobilityExtMgrNetmask,
                        cLMobilityExtMgrMacAddress,
                        cLMobilityExtMgrVlanId,
                        cLMobilityExtMgrName,
                        cLMobilityExtMgrInterfaceType,
                        cLMobilityExtNewArchitectureEnableStatus,
                        cLMobilityExtNewArchitectureAdminEnableStatus,
                        cLMobilityExtMCClientAnchorMCPrivateAddressType,
                        cLMobilityExtMCClientAnchorMCPrivateAddress,
                        cLMobilityExtMCClientAnchorMCGroupId,
                        cLMobilityExtMCClientAssociatedMCGroupId,
                        cLMobilityExtMCClientAssociatedMAAddressType,
                        cLMobilityExtMCClientAssociatedMAAddress,
                        cLMobilityExtMCClientAnchorMAAddressType,
                        cLMobilityExtMCClientAnchorMAAddress,
                        cLMobilityExtSpgGroupId,
                        cLMobilityExtSpgBridgeDomainId,
                        cLMobilityExtSpgMemberCount,
                        cLMobilityExtSpgMulticastAddressType,
                        cLMobilityExtSpgMulticastAddress,
                        cLMobilityExtSpgMulticastMode,
                        cLMobilityExtSpgRowStatus,
                        cLMobilityExtSpgMemberStatus,
                        cLMobilityExtSpgMemberPublicAddressType,
                        cLMobilityExtSpgMemberPublicAddress,
                        cLMobilityExtSpgMemberRowStatus,
                        cLMobilityExtGroupMemberGroupName,
                        cLMobilityExtGroupMemberPublicAddressType,
                        cLMobilityExtGroupMemberPublicAddress,
                        cLMobilityExtGroupMemberStatus,
                        cLMobilityExtGroupMemberMacAddress,
                        cLMobilityExtGroupMemberMulticastAddressType,
                        cLMobilityExtGroupMemberMulticastAddress,
                        cLMobilityExtGroupMemberHashKey,
                        cLMobilityExtGroupMemberRowStatus,
                        cLMobilityExtAnchorStatus,
                        cLMobilityExtAnchorRowStatus,
                        cLMobilityExtMOMCMacAddress,
                        cLMobilityExtMOMCLinkStatus,
                        cLMobilityExtMOMCClientCount,
                        cLMobilityExtMCClientAssociatedMCAddressType,
                        cLMobilityExtMCClientAssociatedMCAddress,
                        cLMobilityExtMCClientAddressType,
                        cLMobilityExtMCClientAddress,
                        cLMobilityExtMCClientState,
                        cLMobilityExtMCClientLocalClient,
                        cLMobilityExtMOClientAnchorMCPublicAddressType,
                        cLMobilityExtMOClientAnchorMCPublicAddress,
                        cLMobilityExtMOClientAnchorMCPrivateAddressType,
                        cLMobilityExtMOClientAnchorMCPrivateAddress,
                        cLMobilityExtMOClientAssociatedMCPublicAddressType,
                        cLMobilityExtMOClientAssociatedMCPublicAddress,
                        cLMobilityExtMOClientAssociatedMCPrivateAddressType,
                        cLMobilityExtMOClientAssociatedMCPrivateAddress,
                        cLMobilityExtMOClientAddressType,
                        cLMobilityExtMOClientAddress,
                        cLMobilityExtMOClientLocalTime,
                        cLMobilityExtApMgrAddressType,
                        cLMobilityExtApMgrAddress,
                        cLMobilityExtApMgrNetmaskType,
                        cLMobilityExtApMgrNetmask,
                        cLMobilityExtApMgrMacAddress,
                        cLMobilityExtApMgrVlanId,
                        cLMobilityExtApMgrInterfaceType,
                        cLMobilityExtApMgrRowStatus,
                        cLMobilityExtForeignWlcMapIf,
                        cLMobilityExtForeignWlcMapRowStatus,
                        cLMobilityExtGroupMulticastAddressType,
                        cLMobilityExtGroupMulticastAddress,
                        cLMobilityExtGroupMulticastMode,
                        cLMobilityExtGroupMulticastModev6,
                        cLMobilityExtGroupMulticastAddressv6Type,
                        cLMobilityExtGroupMulticastAddressv6,
                        cLMobilityExtGroupRowStatus,
                        cLMobilityExtMAPeerPublicAddressType,
                        cLMobilityExtMAPeerPublicAddress,
                        cLMobilityExtMAPeerLinkStatus,
                        cLMobilityExtMCMAClientCount,
                        cLMobilityExtMCAPName,
                        cLMobilityExtMCAPReportingDeviceAddressType,
                        cLMobilityExtMCAPReportingDeviceAddress,
                        cLMobilityExtMCAPReportingDeviceType,
                        cLMobilityExtMCAPCount,
                        cLMobilityExtMAMCPublicAddressType,
                        cLMobilityExtMAMCPublicAddress,
                        cLMobilityExtMAMCPrivateAddressType,
                        cLMobilityExtMAMCPrivateAddress,
                        cLMobilityExtMAToMCLinkStatus,
                        cLMobilityExtMASpgPeerCount,
                        cLMobilityExtMASpgName,
                        cLMobilityExtMAOwnMulticastAddressType,
                        cLMobilityExtMAOwnMulticastAddress,
                        cLMobilityExtMAKeepAliveCount,
                        cLMobilityExtMAKeepAliveInterval,
                        cLMobilityExtMADscpValue,
                        cLMobilityExtMCReceivedTotal,
                        cLMobilityExtMCReceivedDrops,
                        cLMobilityExtMCProtocolReceiveErrors,
                        cLMobilityExtMCProtocolTransmitErrors,
                        cLMobilityExtMCStateErrors,
                        cLMobilityExtMCProtocolRetransmitted,
                        cLMobilityExtMCHandoffRequestsReceived,
                        cLMobilityExtMCHandoffCompleteReceived,
                        cLMobilityExtMCHandoffClientDeleteReceived,
                        cLMobilityExtMCHandoffRequestsTransmitted,
                        cLMobilityExtMCHandoffCompleteTransmitted,
                        cLMobilityExtMCHandoffClientDeleteTransmitted,
                        cLMobilityExtMCTotalClientCount,
                        cLMobilityExtMCWgbCount,
                        cLMobilityExtMOClientUpTime,
                        cLMobilityExtMCClientUpTime
                    }
    STATUS          current
    DESCRIPTION
        "This is a collection of objects which can
        be configured to control mobility parameters."
    ::= { ciscoLwappMobilityExtMIBGroups 4 }

cLMobilityExtMAStatsConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLMobilityExtMAReceivedTotal,
                        cLMobilityExtMAReceivedDrops,
                        cLMobilityExtMAProtocolReceiveErrors,
                        cLMobilityExtMAProtocolTransmitErrors,
                        cLMobilityExtMAStateErrors,
                        cLMobilityExtMAProtocolRetransmitted,
                        cLMobilityExtMATotalClients,
                        cLMobilityExtMALocalClients,
                        cLMobilityExtMAAnchoredClients,
                        cLMobilityExtMAForeignedClients,
                        cLMobilityExtMATotalInterGroupHandoffReceived,
                        cLMobilityExtMATotalIntraGroupHandoffReceived,
                        cLMobilityExtMATotalHandoffEndRequestReceived,
                        cLMobilityExtMATotalInterGroupHandoffSent,
                        cLMobilityExtMATotalIntraGroupHandoffSent,
                        cLMobilityExtReceivedTotal,
                        cLMobilityExtTransmitTotal,
                        cLMobilityExtTotalResourceAllocation,
                        cLMobilityExtTotalResourceFree
                    }
    STATUS          current
    DESCRIPTION
        "This is collection of MA stat objects which
        can be configure to control mobility parameters."
    ::= { ciscoLwappMobilityExtMIBGroups 5 }

ciscoLwappMobilityExtMCMAStatsGroup OBJECT-GROUP
    OBJECTS         { cLMobilityExtEncryptionStatus }
    STATUS          current
    DESCRIPTION
        "This object represents the current status of the
        encryption in the mobilty tunnel."
    ::= { ciscoLwappMobilityExtMIBGroups 6 }

cLMobilityExtAnchorConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLMobilityExtAnchorPriority,
                        cLMobilityExtAnchorStatus,
                        cLMobilityExtAnchorRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "This object specifies the priority configured for
        an Anchor WLC mapped on a WLAN."
    ::= { ciscoLwappMobilityExtMIBGroups 7 }

END


-- %DNP%  MLC -Edit MLC

