-- *******************************************************************
-- CISCO-LWAPP-WLAN-MIB.my
-- This MIB helps to manage the WLANs on the controller
-- January 2006, Devesh Pujari, Prasanna Viswakumar
--   
-- Copyright (c) 2006-2007, 2009-2010, 2016-2019 by Cisco Systems, Inc.
-- All rights reserved.
-- *******************************************************************

CISCO-LWAPP-WLAN-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY,
    OBJECT-TYPE,
    Unsigned32,
    Gauge32,
    TimeTicks,
    Integer32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    TimeStamp,
    TruthValue,
    RowStatus,
    StorageType,
    DisplayString,
    MacAddress
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    InetAddressType,
    InetAddress
        FROM INET-ADDRESS-MIB
    CiscoURLStringOrEmpty
        FROM CISCO-TC
    ciscoMgmt
        FROM CISCO-SMI;


ciscoLwappWlanMIB MODULE-IDENTITY
    LAST-UPDATED    "201904100000Z"
    ORGANIZATION    "Cisco Systems Inc."
    CONTACT-INFO
            "Cisco Systems,
            Customer Service
            Postal: 170 West Tasman Drive
            San Jose, CA  95134
            USA
            Tel: +1 800 553-NETS

            Email: cs-wnbu-snmp@cisco.com"
    DESCRIPTION
        "This MIB is intended to be implemented on all those
        devices operating as Central Controllers (CC)  that
        terminate the Light Weight Access Point Protocol
        tunnel from Cisco Light-weight LWAPP Access Points.

        This MIB helps to manage the WLANs on the controller.

        The relationship between CC and the LWAPP APs
        can be depicted as follows:

        +......+     +......+     +......+           +......+
        +      +     +      +     +      +           +      +
        +  CC  +     +  CC  +     +  CC  +           +  CC  +
        +      +     +      +     +      +           +      +
        +......+     +......+     +......+           +......+
        ..            .             .                 .
        ..            .             .                 .
        .  .            .             .                 .
        .    .            .             .                 .
        .      .            .             .                 .
        .        .            .             .                 .
        +......+ +......+     +......+      +......+          +......+
        +      + +      +     +      +      +      +          +      +
        +  AP  + +  AP  +     +  AP  +      +  AP  +          +  AP  +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+
        .              .             .                 .
        .  .              .             .                 .
        .    .              .             .                 .
        .      .              .             .                 .
        .        .              .             .                 .
        +......+ +......+     +......+      +......+          +......+
        +      + +      +     +      +      +      +          +      +
        +  MN  + +  MN  +     +  MN  +      +  MN  +          +  MN  +
        +      + +      +     +      +      +      +          +      +
        +......+ +......+     +......+      +......+          +......+

        The LWAPP tunnel exists between the controller and
        the APs.  The MNs communicate with the APs through
        the protocol defined by the 802.11 standard.

        LWAPP APs, upon bootup, discover and join one of the
        controllers and the controller pushes the configuration,
        that includes the WLAN parameters, to the LWAPP APs.
        The APs then encapsulate all the 802.11 frames from
        wireless clients inside LWAPP frames and forward
        the LWAPP frames to the controller.

                           GLOSSARY

        Access Point ( AP )

        An entity that contains an 802.11 medium access
        control ( MAC ) and physical layer ( PHY ) interface
        and provides access to the distribution services via
        the wireless medium for associated clients.  

        LWAPP APs encapsulate all the 802.11 frames in
        LWAPP frames and sends it to the controller to which
        it is logically connected to.

        Central Controller ( CC )

        The central entity that terminates the LWAPP protocol
        tunnel from the LWAPP APs.  Throughout this MIB,
        this entity also referred to as 'controller'.

        Light Weight Access Point Protocol ( LWAPP ) 

        This is a generic protocol that defines the
        communication between the Access Points and the
        controllers.

        Mobile Node ( MN )

        A roaming 802.11 wireless device in a wireless
        network associated with an access point. 

        Access Control List ( ACL )

        A list of rules used to restrict the traffic reaching 
        an interface or the CPU or WLAN.  Each ACL is an ordered
        set of rules and actions.  If a rule matches then the 
        action for that rule is applied to the packet.

        802.1x

        The IEEE ratified standard for enforcing port based
        access control.  This was originally intended for
        use on wired LANs and later extended for use in
        802.11 WLAN environments.  This defines an
        architecture with three main parts - a supplicant
        (Ex. an 802.11 wireless client), an authenticator
        (the AP) and an authentication server(a Radius
        server).  The authenticator passes messages back
        and forth between the supplicant and the
        authentication server to enable the supplicant
        get authenticated to the network.

        Temporal Key Integrity Protocol ( TKIP )

        A security protocol defined to enhance the limitations
        of WEP.  Message Integrity Check and per-packet keying
        on all WEP-encrypted frames are two significant
        enhancements provided by TKIP to WEP.

        Cisco Key Integrity Protocol ( CKIP )

        A proprietary implementation similar to TKIP.  CKIP
        implements key permutation for protecting the CKIP
        key against attacks.  Other features of CKIP include
        expansion of encryption key to 16 bytes of length for
        key protection and MIC to ensure data integrity.

        Wired Equivalent Privacy ( WEP )

        A security method defined by 802.11. WEP uses a
        symmetric key stream cipher called RC4 to encrypt the
        data packets.

        Wi-Fi Protected Access ( WPA )

        Wi-Fi Protected Access (WPA and WPA2) are security
        systems created in response to several serious
        weaknesses found in Wired Equivalent Privacy (WEP).
        WPA implements the majority of the IEEE 802.11i
        standard, and was intended as an intermediate
        measure to take the place of WEP while 802.11i was
        prepared. WPA is designed to work with all wireless
        network interface cards, but not necessarily with
        first generation wireless access points.

        WLAN Layer 2 Security

        WLAN layer 2 (MAC) security defines the encryption and 
        authentication approaches such as 802.1x, WPA, 
        WPA2, CKIP and WEP.                

        Delivery Traffic Indication Map ( DTIM )

        DTIM is measured in beacon intervals and is the time 
        period during which multicast/broadcast packets are
        sent to clients. This helps client to go in Power Saving
        mode and helps to save battery power.

        Network Admission Control (NAC)

        Cisco NAC uses the network infrastructure to enforce security
        policy compliance on all devices that seek to access network
        computing resources. With the Cisco NAC appliance, network
        administrators can authenticate, authorize, evaluate, and
        remediate wired, wireless, and remote users and their machines
        prior to network access. The Cisco NAC appliance identifies
        whether networked devices such as laptops, IP phones, or game
        consoles are compliant with network security policies, and
        repairs any vulnerabilities before it permits access to the
        network.

        Out of Band (OOB)

        Out-of-band deployments require user traffic to traverse through
        the NAC appliance only within authentication, posture
        assessment, and remediation. When a user is authenticated and
        passes all policy checks, the traffic is switched normally
        through the network and bypasses the NAC server.

        Band Select

        The 2.4 GHz band is congested and clients have to contend with
        numerous performance challenges. These consist of interference
        from Bluetooth, microwave ovens, cordless phones, etc.;
        protection mechanisms from 802.11b legacy clients; and
        co-channel interference from other access points due to
        802.11bg?s limit of three non-overlapping channels. Allowing
        client Wi-Fi radios capable of dual band (2.4 and 5 GHz)
        operation move to the less congested 5 GHz radios would improve
        the overall performance of the network.
        The Band Select algorithm is based on probe response suppression
        on clients 2.4G radio. The feature is OFF by default and has to
        be manually switched ON globally for a WLC. It can be optionally
        over-ridden per-SSID to disallow it.

        Network Access Identifier ( NAI )

        In order to provide roaming services, it is necessary 
        to have a standardized method for  identifying users. 
        NAI is actually the user identity submitted by the client 
        during network authentication.

        KTS (Key Telephone System)

        Key Telephone System is an alternative to a 
        private branch exchange (PBX)phone system. 
        A KTS is equipped with several buttons that allow 
        a caller to directly select outgoing lines or 
        incoming calls, and use intercom and
        conference facilities.

        HALO (Hyperlocation)

        Hyperlocation is a technique of calculating location using 
        Angle of Arrival(AoA) tracks 802.11 OFDM clients 
        (meaning 802.11a/g/n/ac clients) that are associated(connected) 
        on the network and is able to do so with much higher accuracy 
        than conventional Real Time Location Systems(RTLS) that rely 
        on only RSSI (RF Signal Strength).

        PakRSSI (Packet Received Signal Strength Indicator)

        PakRSSI is a measurement of the power present in a received radio signal.

        POE (Power Over Ethernet)

        Power over Ethernet or PoE describes any of several standardized 
        or ad-hoc systems which pass electrical power along with data on 
        Ethernet cabling. This allows a single cable to provide both data 
        connection and electrical power to devices such as wireless
        access points or IP cameras.

        Multicast Domain Name System (mDNS)

        This is the underlying protocol that is used for Service 
        advertisement and discovery in technologies like Bonjour, 
        Zero Touch Configuration 

        REFERENCE

        [1] Wireless LAN Medium Access Control ( MAC ) and
        Physical Layer ( PHY ) Specifications.

        [2] Draft-obara-capwap-lwapp-00.txt, IETF Light 
        Weight Access Point Protocol 

        [3] IEEE 802.11 - The original 1 Mbit/s and 2 Mbit/s, 
        2.4 GHz RF and IR standard."
    REVISION        "201904090000Z"
    DESCRIPTION
        "Added following new table
        - cLWlan11axConfigTable
        Added new compliance objects
        - ciscoLwappWlanMIBComplianceRev10
        Added new compliance object group
        - ciscoLwappWlan11axConfigGroup.
        Added following entries to cLWlanConfigTable
        - cLWlanMdnsMode."
    REVISION        "201809030000Z"
    DESCRIPTION
        "Added following entries to cLWlanConfigTable
        - cLWlan11kAssistedRoamingEnable 
        - cLWlan11kNeighborListEnable
        - cLWlan11kDualbandNeigListEnable
        - cLWlanEapProfileName
        - cLWlanSetEapProfileName
        - cLWlanMaxClientsAllowedPerAP
        - cLWlan11vDMSEnable
        Added following entries to cLWlanConfigTable
        - cLWlanIosAuthorizationMethodListName 
        - cLWlanIosWebAuthAuthorizationMethodListName
        - cLWlanIosMacOverrideMethodListName
        Added the following conformance group
        - ciscoLwappWlan11kConfigGroup
        Deprecated the following Compliance group
        - ciscoLwappWlanMIBComplianceRev10
        Added the following Compliance group
        - ciscoLwappWlanMIBComplianceRev11."
    REVISION        "201807050000Z"
    DESCRIPTION
        "Added new table
        -cLPolicyWlanSchedulingTable.
        Added allowPvtGrp(4) in the object cLWlanP2PBlocking.
        Added following objects in cLAPGroupConfigTable
        -cLApGroupGlobalWebAuthConfig
        -cLApGroupExternalWebAuthUrl."
    REVISION        "201803070000Z"
    DESCRIPTION
        "Added the following objects to the table cLWlanConfigQosTable
        -cLWlanWlanDSAverageDataRate
        -cLWlanWlanUSAverageDataRate
        -cLWlanWlanDSBurstDataRate
        -cLWlanWlanUSBurstDataRate
        -cLWlanWlanDSAvgRealTimeDataRate
        -cLWlanWlanUSAvgRealTimeDataRate
        -cLWlanWlanDSBurstRealTimeDataRate
        -cLWlanWlanUSBurstRealTimeDataRate"
    REVISION        "201707220000Z"
    DESCRIPTION
        "Removed the changes done on revision
        201612080000Z"
    REVISION        "201612080000Z"
    DESCRIPTION
        "Added the following objects
        -cLWlanSelfAnchorEnabled
        -cLWlan11acMuMimoEnabled
        -cLWlanFlexibleNetflowEntry
        -cLWlanFlexibleNetflowPolicyTypeIndex
        -cLWlanFlexibleNetflowMonitorName
        -cLWlanFlexibleNetflowRowStatus

        Added new table
        -cLWlanFlexibleNetflowTable

        Added new compliance objects
        -ciscoLwappWlanMIBComplianceRev9

        Added new compliance object groups
        -ciscoLwappWlanQosConfigGroup 
        -ciscoLwappWlanConfigGroupSup4 
        -ciscoLwappWlan11uConfigGroupsup2 
        -ciscoLwappAPGroupsVlanConfigGroupSup1 
        -cLAPGroupsVenueConfigGroup 
        -cLAPGroupsMultipleVenueGroup 
        -ciscoLwappWlanConfigClientGroupSup2 
        -ciscoLwappWlanConfigFlexibleNetflowGroup 
        -ciscoLwappWlanConfigGroupSup5 
        -ciscoLwappAPGroupsVlanConfigGroupSup2 
        -ciscoLwappWlanConfigGroupSup6 
        -ciscoLwappWlanConfigGroupSup7 
        -ciscoLwappWlanConfigGroupSup8 
        -ciscoLwappWlan11vConfigGroup"
    REVISION        "201612080000Z"
    DESCRIPTION
        "Added the following objects
        - cLWlan11vBssTransEnable         
        - cLWlan11vDisassocImmiEnable     
        - cLWlan11vDisassocTimer          
        - cLWlan11vOpRoamDisassocTimer    
        Added new group    
        - ciscoLwappWlan11vConfigGroup
        Added new compliance 
        ciscoLwappWlanMIBComplianceRev9 which
        deprecates ciscoLwappWlanMIBComplianceRev8."
    REVISION        "201604070000Z"
    DESCRIPTION
        "Added new tables ciscoLwappAPGroupsHyperlocationConfig to
        support Hyperlocation feature and ciscoLwappAPGroupsPortConfig
        to support AP Group LAN port configurations.
        Added new groups ciscoLwappWlanConfigGroupSup8,
        ciscoLwappWlanConfigGroupSup9. Added new compliance 
        ciscoLwappWlanMIBComplianceRev8 which
        deprecates ciscoLwappWlanMIBComplianceRev7."
    REVISION        "201504230000Z"
    DESCRIPTION
        "Added Default value to the cLWlanMulticastInterface object."
    REVISION        "201504170000Z"
    DESCRIPTION
        "Added cLWlan11acMuMimoEnabled object to cLWlanConfigEntry.
        ciscoLwappWlanMIBComplianceRev6 is superceded by 
        ciscoLwappWlanMIBComplianceRev7
        Added new group ciscoLwappWlanConfigGroupSup6."
    REVISION        "201411050000Z"
    DESCRIPTION
        "Added the cLWlanSelfAnchorEnabled to support
        the mobility self anchor.
        cLAPGroupsVlanMappingInterfaceName is superceded by
        cLAPGroupsVlanMappingInterfaceNameRev1.
        ciscoLwappAPGroupsVlanConfigGroup  is superceded by
        ciscoLwappAPGroupsVlanConfigGroupSup2.
        ciscoLwappWlanMIBComplianceRev5 is superceded by 
        ciscoLwappWlanMIBComplianceRev6
        Added cLWlanUniversalAdmin  object to cLWlanConfigEntry.
        Added new group ciscoLwappWlanConfigGroupSup5."
    REVISION        "201303300000Z"
    DESCRIPTION
        "Added cLWlanFlexibleNetflowTable to support AVC feature.
        Added new object group 
        CiscoLwappWlanConfigFlexibleNetflowGroup.
            Added new compliance ciscoLwappWlanMIBComplianceRev5 which
        deprecates ciscoLwappWlanMIBComplianceRev4."
    REVISION        "201206210000Z"
    DESCRIPTION
        "Added the following objects
        WLAN QoS Config table,
        AP group Venue Table,
        ciscoLwappWlanQosConfigGroup 
                ciscoLwappWlanConfigGroupSup4 
                ciscoLwappWlan11uConfigGroupsup2     
                ciscoLwappWlanHotSpot2ConfigGroupSup1 
                ciscoLwappAPGroupsVlanConfigGroupSup1
                cLAPGroupsVenueConfigGroup 
                cLAPGroupsMultipleVenueGroup
                ciscoLwappWlanConfigClientGroupSup2
                WLAN IOS objects.
                -
                Added the following objects to cLWlan11uTable.
        cLWlan11uHessid,
        cLWlan11uNetworkAuthType,
        cLWlan11uOui,
        cLWlan11uOuiIsBeacon,
        cWlan11uOuiRowStatus,
        cLWlan11uOuiStorageType,
        cLWlan11uRealmName,
        cLWlan11uRealmRowStatus,
        cLWlan11uRealmEapMethod,
        cLWlan11uRealmEapRowStatus,
        cLWlan11uRealmEapAuthMethod,
        cLWlan11uRealmEapAuthParam,
        cLWlan11uRealmEapAuthRowStatus,
        cLWlan11uDomainName,
        cLWlan11uDomainRowStatus,
        cLWlan11u3gppCountryCode,
        cLWlan11u3gppNetworkCode,
        cLWlan11u3gppRowStatus,
        cLWlan11uIpAddressAvailIpv4,
        cLWlan11uIpAddressAvailIpv6
        -
        Added the following OBJECT-GROUPs:
        ciscoLwappWlan11uConfigGroupsup1
        ciscoLwappWlanServiceAdvertisementConfigGroup,
        ciscoLwappWlanHotSpot2ConfigGroup
        -
        Added new compliance ciscoLwappWlanMIBComplianceRev4 which
        deprecates ciscoLwappWlanMIBComplianceRev3."
    REVISION        "201103100000Z"
    DESCRIPTION
        "Added the following objects to cLWlanConfigTable.
        cLWlanReAnchorRoamedVoiceClientsEnable, 
        cLWlanMulticastInterfaceEnable, 
        cLWlanMulticastInterface, 
        cLWlanMulticastDirectEnable, 
        cLWlanNACPostureSupport, 
        cLWlanMaxClientsAccepted, 
        cLWlanScanDeferPriority, 
        cLWlanScanDeferTime, 
        cLWlanLanSubType, 
        cLWlanWebAuthOnMacFilterFailureEnabled, 
        cLWlanStaticIpTunnelingEnabled. 
        - 
        Added new group ciscoLwappWlanConfigGroupSup3. 
        - 
        Added new compliance ciscoLwappWlanMIBComplianceRev3 which
        deprecates ciscoLwappWlanMIBComplianceRev2."
    REVISION        "201003030000Z"
    DESCRIPTION
        "Added the following OBJECT-GROUPs:
        ciscoLwappWlan11uConfigGroup
        ciscoLwappAPGroupsVlanConfigGroup
        ciscoLwappWlanConfigGroupSup2
        ciscoLwappWlanConfigClientGroupSup1"
    REVISION        "200704020000Z"
    DESCRIPTION
        "Added following object in cLWlanConfigClientTable
        cLWlanP2PBlocking"
    REVISION        "200702030000Z"
    DESCRIPTION
        "Added following objects in cLWlanConfigTable:
        cLWlanProfileName
        cLWlanSsid 
        cLWlanDiagChan
        cLWlanStorageType
        Added following table:
        cLWlanConfigClientTable  
        Added the following OBJECT-GROUPs:
        ciscoLwappWlanConfigGroupSup1 
        ciscoLwappWlanConfigClientGroup 
        Added ciscoLwappWlanMIBComplianceRev1 MODULE-COMPLIANCE."
    REVISION        "200603210000Z"
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { ciscoMgmt 512 }


ciscoLwappWlanMIBNotifs  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIB 0 }

ciscoLwappWlanMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIB 1 }

ciscoLwappWlanMIBConform  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIB 2 }

ciscoLwappWlanConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIBObjects 1 }

ciscoLwappAPGroupsVlanConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIBObjects 2 }

ciscoLwappWlan11uConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIBObjects 3 }

ciscoLwappWlanServiceAdvertisementConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIBObjects 4 }

ciscoLwappWlanHotSpot2Config  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIBObjects 5 }

ciscoLwappAPGroupNasIdConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIBObjects 6 }

ciscoLwappPolicyConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIBObjects 7 }

ciscoLwappAPGroupsHyperlocationConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIBObjects 8 }

ciscoLwappAPGroupsPortConfig  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIBObjects 9 }

-- ********************************************************************
-- WLAN configuration
-- ********************************************************************

cLWlanConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlanConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the WLAN configuration sent by
        the controller to the LWAPP APs for their operation.

        LWAPP APs exchange configuration messages with the
        controller and get the required configuration for
        their 802.11 related operations.  As part of these
        messages, the WLAN configuration is pushed by the
        controller to the LWAPP APs.  

        This table doesn't have any dependencies on other
        existing tables.  By defining cLWlanIndex, the
        unique identifier for a WLAN, this table provides
        a common index structure for use in several other
        new tables that populate information on security
        related attributes like authentication, encryption,
        802.11 parameters, Quality-of-Service attributes
        etc., that would relate to a particular WLAN.

        Rows are added or deleted by explicit 
        management actions initiated by the user from a
        network management station through the 
        cLWlanRowStatus object."
    ::= { ciscoLwappWlanConfig 1 }

cLWlanConfigEntry OBJECT-TYPE
    SYNTAX          CLWlanConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the WLAN
        configuration sent by the controller to LWAPP APs
        for use during their operations. entries can be 
        added/deleted by explicit management actions by 
        NMS or by user console"
    INDEX           { cLWlanIndex } 
    ::= { cLWlanConfigTable 1 }

CLWlanConfigEntry ::= SEQUENCE {
        cLWlanIndex                            Unsigned32,
        cLWlanRowStatus                        RowStatus,
        cLWlanProfileName                      SnmpAdminString,
        cLWlanSsid                             OCTET STRING,
        cLWlanDiagChan                         TruthValue,
        cLWlanStorageType                      StorageType,
        cLWlanIsWired                          TruthValue,
        cLWlanIngressInterface                 OCTET STRING,
        cLWlanNACSupport                       TruthValue,
        cLWlanWepKeyChange                     TimeStamp,
        cLWlanChdEnable                        TruthValue,
        cLWlan802dot11anDTIM                   Unsigned32,
        cLWlan802dot11bgnDTIM                  Unsigned32,
        cLWlanLoadBalancingEnable              TruthValue,
        cLWlanBandSelectEnable                 TruthValue,
        cLWlanPassiveClientEnable              TruthValue,
        cLWlanReAnchorRoamedVoiceClientsEnable TruthValue,
        cLWlanMulticastInterfaceEnable         TruthValue,
        cLWlanMulticastInterface               SnmpAdminString,
        cLWlanMulticastDirectEnable            TruthValue,
        cLWlanNACPostureSupport                TruthValue,
        cLWlanMaxClientsAccepted               Unsigned32,
        cLWlanScanDeferPriority                BITS,
        cLWlanScanDeferTime                    Unsigned32,
        cLWlanLanSubType                       INTEGER,
        cLWlanWebAuthOnMacFilterFailureEnabled TruthValue,
        cLWlanStaticIpTunnelingEnabled         TruthValue,
        cLWlanKtsCacSupportEnabled             TruthValue,
        cLWlanWifiDirectPolicyStatus           INTEGER,
        cLWlanWebAuthIPv6AclName               SnmpAdminString,
        cLWlanHotSpot2Enabled                  TruthValue,
        cLWlanMaxClientsAllowedPerRadio        Unsigned32,
        cLWlanDhcpDeviceProfiling              TruthValue,
        cLWlanMacAuthOverDot1xEnabled          TruthValue,
        cLWlanUserTimeout                      Unsigned32,
        cLWlanUserIdleThreshold                Unsigned32,
        cLWlanHttpDeviceProfiling              TruthValue,
        cLWlanHotSpotClearConfig               INTEGER,
        cLWlanRadiusAuthFourthServer           DisplayString,
        cLWlanRadiusAuthFifthServer            DisplayString,
        cLWlanRadiusAuthSixthServer            DisplayString,
        cLWlanRadiusAcctFourthServer           DisplayString,
        cLWlanRadiusAcctFifthServer            DisplayString,
        cLWlanRadiusAcctSixthServer            DisplayString,
        cLWlanSelfAnchorEnabled                TruthValue,
        cLWlanUniversalAdmin                   TruthValue,
        cLWlan11acMuMimoEnabled                TruthValue,
        cLWlan11vDisassocImmiEnable            TruthValue,
        cLWlan11vDisassocTimer                 Unsigned32,
        cLWlan11vOpRoamDisassocTimer           Unsigned32,
        cLWlan11kAssistedRoamingEnable         TruthValue,
        cLWlan11kNeighborListEnable            TruthValue,
        cLWlan11kDualbandNeigListEnable        TruthValue,
        cLWlan11vDMSEnable                     TruthValue,
        cLWlan11vBssTransEnable                TruthValue,
        cLWlanEapProfileName                   SnmpAdminString,
        cLWlanSetEapProfileName                TruthValue,
        cLWlanMaxClientsAllowedPerAP           Unsigned32,
        cLWlanMdnsMode                         INTEGER
}

cLWlanIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..517)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies one instance of
        a WLAN on the controller. The value 513-517 indicates
        wired clients." 
    ::= { cLWlanConfigEntry 1 }

cLWlanRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and used
        to create, modify and delete specific instances of rows
        in this table.
        This table supports modification of writable objects when the
        RowStatus is 'active'.
        The following objects are mandatory for successful
        creation of an entry:
            cLWlanProfileName 
            cLWlanSsid." 
    ::= { cLWlanConfigEntry 2 }

cLWlanProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..64))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the profile name assigned
        to this WLAN. The name assigned to a WLAN has to be 
        unique across all the WLANs on the controller.
        An administrator can assign a meaningful
        name that could later be used to refer a particular 
        WLAN on the controller.  This object cannot be 
        modified when cLWlanRowStatus is 'active'." 
    ::= { cLWlanConfigEntry 3 }

cLWlanSsid OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (1..32))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the SSID assigned to
        this WLAN. The access points will broadcast this SSID 
        on this WLAN. Different WLAN could use the same SSID as
        long as the layer 2 security is different. This object 
        cannot be modified when cLWlanRowStatus is 'active'." 
    ::= { cLWlanConfigEntry 4 }

cLWlanDiagChan OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to configure this WLAN as a diagnostic
        WLAN. A value of 'true' indicates that the WLAN can be used for
        diagnostic purposes. A value of 'false' indicates that the WLAN
        can not be used for diagnostic purposes."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 5 }

cLWlanStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represnts the storage type for this
        conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cLWlanConfigEntry 6 }

cLWlanIsWired OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to configure this WLAN as a
        wired or wireless WLAN. A value of 'true'  indicates 
        that this is a wired WLAN.  A value of 'false' 
        indicates that this is a wireless WLAN." 
    ::= { cLWlanConfigEntry 7 }

cLWlanIngressInterface OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (0..32))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the ingress interface attached to the
        wireless lan." 
    ::= { cLWlanConfigEntry 8 }

cLWlanNACSupport OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to configure the NAC- Out Of
        Band(OOB) support for the WLAN.
        A value of 'true'  indicates that
        the WLAN supports the NAC- Out Of Band(OOB) feature.  
        A value of 'false' indicates that
        the WLAN does not support the NAC- Out Of Band(OOB)
        feature."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 9 }

cLWlanWepKeyChange OBJECT-TYPE
    SYNTAX          TimeStamp
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the time when the
        static WEP key was changed by the user." 
    ::= { cLWlanConfigEntry 10 }

cLWlanChdEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates whether Coverage Hole Detection
        (CHD) is enabled on the controller. A value of 'true'
        indicates CHD is on and a value of 'false' indicates 
        CHD is turned off for this WLAN."
    DEFVAL          { true } 
    ::= { cLWlanConfigEntry 11 }

cLWlan802dot11anDTIM OBJECT-TYPE
    SYNTAX          Unsigned32 (1..255)
    UNITS           "Beacon Intervals"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents DTIM configuration per WLAN for each
        802.11 network.  
        The DTIM value is measured in Beacon Intervals."
    DEFVAL          { 1 } 
    ::= { cLWlanConfigEntry 12 }

cLWlan802dot11bgnDTIM OBJECT-TYPE
    SYNTAX          Unsigned32 (1..255)
    UNITS           "Beacon Intervals"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents DTIM configuration per WLAN for each
        802.11 network.  
        The DTIM value is measured in Beacon Intervals."
    DEFVAL          { 1 } 
    ::= { cLWlanConfigEntry 13 }

cLWlanLoadBalancingEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates whether Load Balancing is
        enabled on the controller for this WLAN . A value of 'true'
        indicates Load Balance is on and a value of 'false' indicates 
        Load Balance is turned off for this WLAN."
    DEFVAL          { true } 
    ::= { cLWlanConfigEntry 14 }

cLWlanBandSelectEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates whether Band Select is enabled
        on the controller for this WLAN. A value of 'true'
        indicates Band Select is on and a value of 'false' indicates 
        Band Select is turned off for this WLAN."
    DEFVAL          { true } 
    ::= { cLWlanConfigEntry 15 }

cLWlanPassiveClientEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether passive client is enabled
        on the controller for this WLAN. A value of 'true'
        indicates passive client is on and a value of 'false' indicates
        passive client is turned off for this WLAN."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 16 }

cLWlanReAnchorRoamedVoiceClientsEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether the Roamed Voice Client
        Re-Anchoring feature is enabled on the controller for this
        WLAN.
        A value of 'true' indicates the roamed voice clients will get
        re-anchored.
        A value of 'false' indicates the roamed voice clients 
        re-anchoring is turned off for this WLAN."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 17 }

cLWlanMulticastInterfaceEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether multicast interface
        is enabled on the controller. A value of 'true'
        indicates that multicast interface feature is enabled
        and the interface represented by 'cLWlanMulticastInterface'
        would be used for the multicast traffic on this WLAN.
        A value of 'false' indicates that multicast interface
        feature is turned off for this WLAN."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 18 }

cLWlanMulticastInterface OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the interface, which would be used
        for the multicast traffic for all the clients that are 
        associated to this WLAN."
    DEFVAL          { "default" } 
    ::= { cLWlanConfigEntry 19 }

cLWlanMulticastDirectEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether multicast direct is enabled
        on the controller for this WLAN. 
        A value of 'true' indicates multicast direct is ON. 
        A value of 'false' indicates multicast direct is turned 
        off for this WLAN."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 20 }

cLWlanNACPostureSupport OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to configure the NAC-Posture
        support for the WLAN.
        A value of 'true'  indicates that the WLAN supports the 
        NAC-Posture feature.
        A value of 'false' indicates that the WLAN does not support the
        NAC-Posture feature."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 21 }

cLWlanMaxClientsAccepted OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the maximum number of client connection
        allowed for this WLAN. 
        A value of 0 indicates that there is no limit on maximum 
        allowed clients for this WLAN."
    DEFVAL          { 0 } 
    ::= { cLWlanConfigEntry 22 }

cLWlanScanDeferPriority OBJECT-TYPE
    SYNTAX          BITS {
                        bit0(0),
                        bit1(1),
                        bit2(2),
                        bit3(3),
                        bit4(4),
                        bit5(5),
                        bit6(6),
                        bit7(7)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the priority of packets
        that defer the off-channel scan. This is used in 
        off-channel scanning to improve performance
        for medical devices using Radio Resource Management.
        Each bit represents a packet type for which off-channel
        scanning needs to be deferred.
        bit0 - Best effort.
        bit1 - Background
        bit2 - Spare
        bit3 - Excellent effort
        bit4 - Controlled load
        bit5 - Video, less than 100-ms latency and jitter
        bit6 - Voice, less than 10-ms latency and jitter
        bit7 - Network control"
    DEFVAL          { { bit5 , bit6 } } 
    ::= { cLWlanConfigEntry 23 }

cLWlanScanDeferTime OBJECT-TYPE
    SYNTAX          Unsigned32 (0..60000)
    UNITS           "milliseconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the minimum number of milliseconds
        that must elapse without the appearance of a specified packet
        before the access point radios begin an off-channel scan."
    DEFVAL          { 100 } 
    ::= { cLWlanConfigEntry 24 }

cLWlanLanSubType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        wirelessLan(1),
                        guestLan(2),
                        remoteLan(3),
                        other(4)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the sub-type of the LAN created.
        This has to be congruent with cLWlanIswired. 
        If cLWlanIswired is set to 'true', allowed values are
        guestLan(2)
        and remoteLan(3). 
        If cLWlanIswired is set to 'false', allowed value is
        wirelessLan(1).
        A value of other(4) will be returned if it doesnt match any
        values defined here. This value is not configurable." 
    ::= { cLWlanConfigEntry 25 }

cLWlanWebAuthOnMacFilterFailureEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to configure the Web based
        authentication on Mac Filter failure support for the WLAN.
        A value of 'true' enables Web authentication on MAC 
        filter failure for the WLAN. 
        A value of 'false' disables Web authentication on MAC
        filter failure for the WLAN."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 26 }

cLWlanStaticIpTunnelingEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to configure the Static IP Tunneling
        of clients feature support for the WLAN.
        A value of 'true' enables static IP Tunneling of client
        for the WLAN. 
        A value of 'false' disables static IP Tunneling of client
        for the WLAN."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 27 }

cLWlanKtsCacSupportEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to configure the KTS CAC
        support for the WLAN.
        A value of 'true' enables the KTS based CAC support
        for this wlan.
        A value of 'false' disables the KTS based CAC support
        for this wlan."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 28 }

cLWlanWifiDirectPolicyStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        disable(1),
                        allow(2),
                        notAllow(3)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to allow/disallow wi-fi
        direct clients to/from joining the infrastructure            
        network.
        disable(1) - WFD is completely disabled.
        allow(2)  -  allow WFD clients
        disallow(3) - controller rejects association request from WFD
        clients only if it has P2P IE with concurrency enabled." 
    ::= { cLWlanConfigEntry 29 }

cLWlanWebAuthIPv6AclName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the name of the Web Auth
        IPv6 ACL applied to this WLAN.
        If it is required to remove the ACL
        name for a WLAN, it should be set to 'none'.
        ACL's are applied in the following priority order -
        interfaces ACLs, WLAN ACLs, client ACLs." 
    ::= { cLWlanConfigEntry 30 }

cLWlanHotSpot2Enabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the hotSpot2 feature for this WLAN.
        A value of 'true' enables the HotSpot2
        for this wlan.
        A value of 'false' disables the HotSpot2
        for this wlan."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 31 }

cLWlanMaxClientsAllowedPerRadio OBJECT-TYPE
    SYNTAX          Unsigned32 (1..200)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the maximum allowed clients
        per AP radio for a WLAN."
    DEFVAL          { 200 } 
    ::= { cLWlanConfigEntry 32 }

cLWlanDhcpDeviceProfiling OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the status of
        DHCP Device Profiling feature for this WLAN.
        A value of 'true' enables DHCP Device Profiling on this wlan.
        A value of 'false' disables DHCP  the Device Profiling 
        on this wlan."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 33 }

cLWlanMacAuthOverDot1xEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the configuration state of
        authentication failover to  Dot1x for the WLAN.
        A value of 'true' enables mac auth or dot1x
        for the WLAN.
        A value of 'false' disables mac auth or dot1x
         for the WLAN."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 34 }

cLWlanUserTimeout OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the timeout value of user for a WLAN."
    DEFVAL          { 300 } 
    ::= { cLWlanConfigEntry 35 }

cLWlanUserIdleThreshold OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "bytes"
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the user idle threshold value in bytes
        for a WLAN."
    DEFVAL          { 0 } 
    ::= { cLWlanConfigEntry 36 }

cLWlanHttpDeviceProfiling OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the status of
        HTTP Device Profiling feature for this WLAN.
        A value of 'true' enables HTTP Device Profiling on this wlan.
        A value of 'false' disables the HTTP Device Profiling 
        on this wlan."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 37 }

cLWlanHotSpotClearConfig OBJECT-TYPE
    SYNTAX          INTEGER  {
                        enable(1),
                        disable(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to clear all the configuration
        related to HotSpot feature at WLAN level.
        A value of 'enable' would clear the configuration.
        When queries for the current value, always 'disable'
        would be returned."
    DEFVAL          { disable } 
    ::= { cLWlanConfigEntry 38 }

cLWlanRadiusAuthFourthServer OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..21))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Fourth
        Radius Authentication Server for this wlan." 
    ::= { cLWlanConfigEntry 39 }

cLWlanRadiusAuthFifthServer OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..21))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Fifth
        Radius Authentication Server for this wlan." 
    ::= { cLWlanConfigEntry 40 }

cLWlanRadiusAuthSixthServer OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..21))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Sixth
        Radius Authentication Server for this wlan." 
    ::= { cLWlanConfigEntry 41 }

cLWlanRadiusAcctFourthServer OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..21))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Fourth
        Radius Accounting Server for this wlan." 
    ::= { cLWlanConfigEntry 42 }

cLWlanRadiusAcctFifthServer OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..21))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Fifth
        Radius Accounting Server for this wlan." 
    ::= { cLWlanConfigEntry 43 }

cLWlanRadiusAcctSixthServer OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..21))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Sixth
        Radius Accounting Server for this wlan." 
    ::= { cLWlanConfigEntry 44 }

cLWlanSelfAnchorEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether self anchoring
        is enabled for the wlan."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 64 }

cLWlanUniversalAdmin OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object allows universal admin mode.
        to be enabled on a 802.1X/WPA/WPA2 secured WLAN."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 65 }

cLWlan11acMuMimoEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to configure 11ac Mu Mimo mode for
        the WLAN.
        A value of 'true' enables Mu Mimo mode for the WLAN. 
        A value of 'false' disables Mu Mimo mode for the WLAN."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 66 }

cLWlan11vDisassocImmiEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates whether 11v BSS Transition Disassociation
        Imminent is enabled on the controller for this WLAN.
        A value of 'true' indicates Disassociation Imminent is enabled
        for the WLAN.
        A value of 'false' indicates Disassociation Imminent is disabled
        for the WLAN."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 67 }

cLWlan11vDisassocTimer OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "Target Beacons Transmission Times"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates 11v BSS Transition Disassociation
        Imminent timer for this WLAN."
    DEFVAL          { 200 } 
    ::= { cLWlanConfigEntry 73 }

cLWlan11vOpRoamDisassocTimer OBJECT-TYPE
    SYNTAX          Unsigned32 (0..40)
    UNITS           "Target Beacon Transmission Times"
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates 11v BSS Transition Optimized Roaming
        Disassociation Imminent timer for this WLAN." 
    ::= { cLWlanConfigEntry 74 }

cLWlan11kAssistedRoamingEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether 11k Assisted Roaming Prediction
        Optimization is enabled on the controller for this WLAN.
        A value of 'true' enables 11k Assisted Roaming Prediction
        A value of 'false' disables 11k Assisted Roaming Prediction"
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 84 }

cLWlan11kNeighborListEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether 11k Neighbor List
        is enabled on the controller for this WLAN.
        A value of 'true' enables 11k Neighbor list
        A value of 'false' disables 11k Neighbor list"
    DEFVAL          { true } 
    ::= { cLWlanConfigEntry 85 }

cLWlan11kDualbandNeigListEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether 11k Neighbor List Dual Band
        is enabled on the controller for this WLAN.
        A value of 'true' enables 11k Neighbor list dual band
        A value of 'false' disables 11k Neighbor list dual band"
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 86 }

cLWlan11vDMSEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies whether 11v Directed Multicast Service
        is enabled on the controller for this WLAN.
        A value of 'true' indicates that 11v Directed Multicast Service
        is enabled.
        A value of 'false' indicates that 11v Directed Multicast
        Service is disabled."
    DEFVAL          { true } 
    ::= { cLWlanConfigEntry 87 }

cLWlan11vBssTransEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object indicates whether 11v BSS Transition is enabled on
        the controller for this WLAN.
        A value of 'true' indicates BSS Transition is enabled for the
        WLAN.
        A value of 'false' indicates BSS Transition is disabled for the
        WLAN."
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 93 }

cLWlanEapProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Eap profile name configured for
        this WLAN." 
    ::= { cLWlanConfigEntry 96 }

cLWlanSetEapProfileName OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether eap profile name is set or not
        on the controller for this WLAN.
        A value of 'true' specifies eap profile name is set
        A value of 'false' specifies eap profile name is not set"
    DEFVAL          { false } 
    ::= { cLWlanConfigEntry 97 }

cLWlanMaxClientsAllowedPerAP OBJECT-TYPE
    SYNTAX          Unsigned32 (0..400)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the maximum allowed clients
        per AP radio for a WLAN."
    DEFVAL          { 0 } 
    ::= { cLWlanConfigEntry 98 }

cLWlanMdnsMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        bridge(0),
                        drop(1),
                        gateway(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the mdns mode of the WLAN
        0 indicates  WLAN is in Bridge mode for mDNS packets 
        1 indicates  WLAN is is Drop mode for mdns packets
        2 indicates  WLAN is in Gateway mode for mDNS packets"
    DEFVAL          { bridge } 
    ::= { cLWlanConfigEntry 99 }
 

-- ********************************************************************
-- *        WLAN 11u  Table
-- ********************************************************************

cLWlan11uTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlan11uEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the generic 802.11u
        configuration for a particular WLAN in a
        controller.

        This table has a one-to-one relationship with
        cLWlanConfigTable. There exist a row in this 
        table corresponding to each   row representing 
        a WLAN in cLWlanConfigTable."
    ::= { ciscoLwappWlan11uConfig 1 }

cLWlan11uEntry OBJECT-TYPE
    SYNTAX          CLWlan11uEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the generic 802.11u
        configuration for a WLAN."
    INDEX           { cLWlanIndex } 
    ::= { cLWlan11uTable 1 }

CLWlan11uEntry ::= SEQUENCE {
        cLWlan11uStatus             TruthValue,
        cLWlan11uInternetAccess     TruthValue,
        cLWlan11uNetworkType        INTEGER,
        cLWlan11uVenueGroup         INTEGER,
        cLWlan11uVenueType          INTEGER,
        cLWlan11uVenueName          SnmpAdminString,
        cLWlan11uHessid             MacAddress,
        cLWlan11uNetworkAuthType    INTEGER,
        cLWlan11uIpAddressAvailIpv4 INTEGER,
        cLWlan11uIpAddressAvailIpv6 INTEGER
}

cLWlan11uStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is used to configure the 802.11u support
        for this WLAN. A value of 'true' indicates that 802.11u
        support is enabled for this WLAN and a  value of 'false'
        indicates that the support  is disabled for this WLAN."
    DEFVAL          { false } 
    ::= { cLWlan11uEntry 1 }

cLWlan11uInternetAccess OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is used to configure the internet access
        with respect to 802.11u feature for this WLAN.
        A value of 'true' indicates that internet access is
        enabled for this WLAN and a  value of 'false' indicates
        that the internet access  is disabled for this WLAN."
    DEFVAL          { true } 
    ::= { cLWlan11uEntry 2 }

cLWlan11uNetworkType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        invalid(1),
                        private(2),
                        privateWithGuestAccess(3),
                        chargeablePublicNetwork(4),
                        freePublicNetwork(5),
                        testOrEquipment(6),
                        wildcard(7),
                        personnalDeviceNetwork(8),
                        emgerencyServiceOnlyNetwork(9),
                        notConfigured(255)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the network type with respect
        to  802.11u feature , for this WLAN.
           invalid (1)                : Invalid network type.
           private(2)                 : Non-authorized users are not 
                                        permitted on this network.
           privateWithGuestAccess(3)  : Private network but guest 
                                        accounts area available. 
           chargeablePublicNetwork(4) : The network is accessible to
                                        anyone, however, access to the 
                                        network requires payment.
           freePublicNetwork(5)       : The network is accessible to 
                                        anyone and no charges apply 
                                        for the network use. 
           testOrEquipment(6)         : The network is used for test or 
                                        experimental purposes only.
           wildcard(6)                : Wildcard network type.
           personnalDeviceNetwork(8)  : The network is accessible only 
                                        by Personnal Device.
           emgerencyServiceOnlyNetwork(9) : Emergency Service 
                                            network Type." 
    ::= { cLWlan11uEntry 3 }

cLWlan11uVenueGroup OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unspecified(1),
                        assembly(2),
                        business(3),
                        educational(4),
                        factoryAndIndustrial(5),
                        institutional(6),
                        mercantile(7),
                        residential(8),
                        storage(9),
                        utilityAndMisc(10),
                        vehicular(11),
                        outdoor(12)
                    }
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object indicates the venue group with respect
        to 802.11u feature , for this WLAN."
    DEFVAL          { unspecified } 
    ::= { cLWlan11uEntry 4 }

cLWlan11uVenueType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unspecified(1),
                        assembly(2),
                        business(3),
                        educational(4),
                        factoryAndIndustrial(5),
                        institutional(6),
                        mercantile(7),
                        residential(8),
                        storage(9),
                        utilityAndMisc(10),
                        vehicular(11),
                        outdoor(12)
                    }
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This object indicates the venue type within
        a particular venue group, with respect
        to  802.11u feature , for this WLAN.
        The Venue group-Venue Type relationship is per
        the following table:
        Venue Group Venue Type Code Venue Description
        =========== =============== =================
             0            0         Unspecified
             0            1-255     Reserved
             1            0         Unspecified Assembly
             1            1         Arena
             1            2         Stadium
             1            3         Passenger Terminal (e.g.,
                                    airport, port, bus station, ferry
                                    terminal, train station)
             1            4         Amphitheater
             1            5         Amusement Park
             1            6         Place of Worship
             1            7         Convention Center
             1            8         Library
             1            9         Museum
             1            10        Restaurant
             1            11        Theater
             1            12        Bar
             1            13        Coffee Shop
             1            14        Zoo or Aquarium
             1            15        Emergency Coordination Center
             1            16-255    Reserved
             2            0         Unspecified Business
             2            1         Doctor or Dentist office
             2            2         Bank
             2            3         Fire Station
             2            4         Police Station
             2            6         Post Office
             2            7         Professional Office
             2            8         Research and Development Facility
             2            9         Attorney Office
             2            10-255    Reserved
             3            0         Unspecified Educational
             3            1         School, Primary
             3            2         School, Secondary
             3            3         University or College
             3            4-255     Reserved
             4            0         Unspecified Factory and Industrial
             4            1         Factory
             4            2-255     Reserved
             5            0         Unspecified Institutional
             5            1         Hospital
             5            2         Long-Term Care Facility (e.g.,
                                    Nursing home, Hospice, etc.)
             5            3         Alcohol and Drug Re-habilitation
                                    Center
             5            4         Group Home
             5            5         Prison or Jail
             5            6-255     Reserved
             6            0         Unspecified Mercantile
             6            1         Retail Store
             6            2         Grocery Market
             6            3         Automotive Service Station
             6            4-255     Reserved
             7            0         Unspecified Residential
             7            1         Hotel or Motel
             7            2         Dormitory
             7            3         Boarding House
             7            4-255     Reserved
             8            0-255     Reserved
             9            0-255     Reserved
             10           0         Unspecified Vehicular
             10           1         Automobile or Truck 
             10           2         Airplane
             10           3         Bus
             10           4         Ferry
             10           5         Ship or Boat
             10           6         Train
             10           7-255     Reserved
             11           0         Unspecified Outdoor
             11           1         Muni-mesh Network
             11           2         City Park
             11           3-255     Reserved"
    DEFVAL          { unspecified } 
    ::= { cLWlan11uEntry 5 }

cLWlan11uVenueName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..255))
    MAX-ACCESS      read-write
    STATUS          deprecated
    DESCRIPTION
        "This is the venue name defined for this WLAN
        with respect to  802.11u feature." 
    ::= { cLWlan11uEntry 6 }

cLWlan11uHessid OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is used to configure the Hessid for this WLAN." 
    ::= { cLWlan11uEntry 8 }

cLWlan11uNetworkAuthType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        acceptance(1),
                        enrollment(2),
                        redirection(3),
                        dnsRedirection(4),
                        notConfigured(5)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object is used to configure the NetworkAuthType
        for a WLAN"
    DEFVAL          { notConfigured } 
    ::= { cLWlan11uEntry 9 }

cLWlan11uIpAddressAvailIpv4 OBJECT-TYPE
    SYNTAX          INTEGER  {
                        notAvailable(1),
                        public(2),
                        portRestricted(3),
                        singleNATPrivate(4),
                        doubleNATPrivate(5),
                        portRestrictedAndSingleNATPrivate(6),
                        portRestrictedAndDoubleNATPrivate(7),
                        unKnown(8)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the IPv4 Address Availability."
    DEFVAL          { notAvailable } 
    ::= { cLWlan11uEntry 10 }

cLWlan11uIpAddressAvailIpv6 OBJECT-TYPE
    SYNTAX          INTEGER  {
                        notAvailable(1),
                        available(2),
                        unKnown(3)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the IPv6 Address Availability."
    DEFVAL          { notAvailable } 
    ::= { cLWlan11uEntry 11 }
 

-- ********************************************************************
-- *        WLAN 11u OUI Table
-- ********************************************************************

cLWlan11uOuiTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlan11uOuiEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the OUI
        (organizational unique identifier) 
        configuration for a particular WLAN.
        OUIs are assigned by IEEE.
        A WLAN can have up to 32 OUIs defined.
        OUI configuration per WLAN is required 
        for the 802.11u feature to work.

        Rows are added or deleted by explicit 
        management actions initiated by the user from a
        network management station through the 
        cLWlan11uOuiRowStatus object."
    ::= { ciscoLwappWlan11uConfig 2 }

cLWlan11uOuiEntry OBJECT-TYPE
    SYNTAX          CLWlan11uOuiEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the OUI
        (organizational unique identifier) 
        configuration for a particular WLAN.
        OUIs are assigned by IEEE.
        A WLAN can have up to 32 OUIs defined.
        OUI configuration per WLAN is required 
        for the 802.11u feature to work."
    INDEX           {
                        cLWlanIndex,
                        cLWlan11uOuiIndex
                    } 
    ::= { cLWlan11uOuiTable 1 }

CLWlan11uOuiEntry ::= SEQUENCE {
        cLWlan11uOuiIndex       Unsigned32,
        cLWlan11uOui            OCTET STRING,
        cLWlan11uOuiIsBeacon    TruthValue,
        cLWlan11uOuiRowStatus   RowStatus,
        cLWlan11uOuiStorageType StorageType
}

cLWlan11uOuiIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies one instance of a OUI
        on a WLAN.Each WLAN can have up to 32 OUIs defined.
        Each OUI should be unique." 
    ::= { cLWlan11uOuiEntry 1 }

cLWlan11uOui OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (6 | 10))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "The OUI field is a public OUI assigned by the IEEE.
        Each OUI identifies a roaming consortium 
        (group of SSPs with inter-SSP roaming agreement) 
        or a single SSP.WLAN can have up to 32 OUIs defined.
        Each OUI defined for a WLAN should be unique.
        For example the value for Cisco is 004096." 
    ::= { cLWlan11uOuiEntry 2 }

cLWlan11uOuiIsBeacon OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to configure this particular
        OUI as one of the beacon OUIs.
        Beacon can carry at most 3 OUIs.
        User should be able to select 0-3 OUIs 
        (from the already configured OUIs for this WLAN). 
        A value of 'true'  indicates that this OUI would 
        be carried in beacon.  A value of 'false' 
        indicates that this OUI is not a beacon OUI."
    DEFVAL          { false } 
    ::= { cLWlan11uOuiEntry 3 }

cLWlan11uOuiRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Row Status for creation/deletion of a particular
        OUI entry in the table." 
    ::= { cLWlan11uOuiEntry 4 }

cLWlan11uOuiStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represnts the storage type for this
        conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cLWlan11uOuiEntry 5 }
 

-- ********************************************************************
-- *        WLAN 11u Realm Table
-- ********************************************************************

cLWlan11uRealmTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlan11uRealmEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the realm (NAI) details per WLAN.
        In order to provide roaming services, 
        it is necessary to have a standardized method for 
        identifying users. NAI is the user identity 
        submitted by the client during network authentication. 
        Each realm entry should be unique."
    ::= { ciscoLwappWlan11uConfig 3 }

cLWlan11uRealmEntry OBJECT-TYPE
    SYNTAX          CLWlan11uRealmEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the realm (NAI)
        configuration for a particular WLAN.A WLAN can have 
        up to 32 realm defined"
    INDEX           {
                        cLWlanIndex,
                        cLWlan11uRealmIndex
                    } 
    ::= { cLWlan11uRealmTable 1 }

CLWlan11uRealmEntry ::= SEQUENCE {
        cLWlan11uRealmIndex     Unsigned32,
        cLWlan11uRealmName      SnmpAdminString,
        cLWlan11uRealmRowStatus RowStatus
}

cLWlan11uRealmIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..128)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies,  one instance of
        a realm EAP entry (NAI) on a WLAN. 
        Each realm entry should be unique." 
    ::= { cLWlan11uRealmEntry 1 }

cLWlan11uRealmName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..128))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the NAI name.
        In order to provide roaming services, 
        it is necessary to have a standardized method for 
        identifying users. NAI is  the user identity 
        submitted by the client during network authentication.
        In roaming, the purpose of the NAI is to identify the 
        user as well as to assist in the routing of the authentication
        request.  
        Please note that the NAI may not necessarily be 
        the same as the user's e-mail address or the user identity
        submitted in an application layer authentication." 
    ::= { cLWlan11uRealmEntry 2 }

cLWlan11uRealmRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Row Status for creation/deletion of a particular realm
        entry (NAI)from the table" 
    ::= { cLWlan11uRealmEntry 3 }
 

-- ********************************************************************
-- *        WLAN 11u Realm Eap Table
-- ********************************************************************

cLWlan11uRealmEapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlan11uRealmEapEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the EAP method configured per realm
        for a particular WLAN. A realm can have up to 4 EAP 
        method defined. The EAP method supported are
        LEAP,PEAP,EAP-FAST and EAP-TLS."
    ::= { ciscoLwappWlan11uConfig 4 }

cLWlan11uRealmEapEntry OBJECT-TYPE
    SYNTAX          CLWlan11uRealmEapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the EAP method
        configured per realm for a particular WLAN. 
        A realm can have up to 4 EAP method defined. 
        The EAP method supported are LEAP,PEAP,EAP-FAST and EAP-TLS."
    INDEX           {
                        cLWlanIndex,
                        cLWlan11uRealmIndex,
                        cLWlan11uRealmEapIndex
                    } 
    ::= { cLWlan11uRealmEapTable 1 }

CLWlan11uRealmEapEntry ::= SEQUENCE {
        cLWlan11uRealmEapIndex     Unsigned32,
        cLWlan11uRealmEapMethod    INTEGER,
        cLWlan11uRealmEapRowStatus RowStatus
}

cLWlan11uRealmEapIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..4)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies one instance of
        a EAP entry configured per a realm for a particular WLAN." 
    ::= { cLWlan11uRealmEapEntry 1 }

cLWlan11uRealmEapMethod OBJECT-TYPE
    SYNTAX          INTEGER  {
                        none(1),
                        leap(2),
                        peap(3),
                        eapTls(4),
                        eapFast(5),
                        eapSim(6),
                        eapTtls(7),
                        eapAka(8)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the EAP method defined." 
    ::= { cLWlan11uRealmEapEntry 2 }

cLWlan11uRealmEapRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Row Status for creation/deletion of a particular EAP
        entry from the table" 
    ::= { cLWlan11uRealmEapEntry 3 }
 

-- ********************************************************************
-- *        WLAN 11u Realm Eap Auth Table
-- ********************************************************************

cLWlan11uRealmEapAuthTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlan11uRealmEapAuthEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the authentication method details
        configured per EAP method for particular realm. 
        There can be up to 10 authentication configuration 
        entries per EAP method."
    ::= { ciscoLwappWlan11uConfig 5 }

cLWlan11uRealmEapAuthEntry OBJECT-TYPE
    SYNTAX          CLWlan11uRealmEapAuthEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the authentication
        method details configured per EAP method for particular realm. 
        There can be up to 10 authentication configuration 
        entries per EAP method."
    INDEX           {
                        cLWlanIndex,
                        cLWlan11uRealmIndex,
                        cLWlan11uRealmEapIndex,
                        cLWlan11uRealmEapAuthIndex
                    } 
    ::= { cLWlan11uRealmEapAuthTable 1 }

CLWlan11uRealmEapAuthEntry ::= SEQUENCE {
        cLWlan11uRealmEapAuthIndex          Unsigned32,
        cLWlan11uRealmEapAuthMethod         INTEGER,
        cLWlan11uRealmEapAuthParam          INTEGER,
        cLWlan11uRealmEapAuthCredentialType INTEGER,
        cLWlan11uRealmEapAuthRowStatus      RowStatus
}

cLWlan11uRealmEapAuthIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..10)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies one instance of
        a auth entry configured per a EAP for a particular WLAN." 
    ::= { cLWlan11uRealmEapAuthEntry 1 }

cLWlan11uRealmEapAuthMethod OBJECT-TYPE
    SYNTAX          INTEGER  {
                        nonEapInnerAuthType(1),
                        innerAuthEapType(2),
                        credentialType(3),
                        tunneledEapCredentialType(4)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the authentication method defined."
    DEFVAL          { nonEapInnerAuthType } 
    ::= { cLWlan11uRealmEapAuthEntry 2 }

cLWlan11uRealmEapAuthParam OBJECT-TYPE
    SYNTAX          INTEGER  {
                        none(1),
                        pap(2),
                        chap(3),
                        mschap(4),
                        mschapV2(5),
                        leap(6),
                        peap(7),
                        eapTls(8),
                        eapFast(9),
                        eapSim(10),
                        eapTtls(11),
                        eapAka(12),
                        sim(13),
                        usim(14),
                        nfcSecure(15),
                        hardwareToken(16),
                        softToken(17),
                        certificate(18),
                        usernamePassword(19),
                        reserved(20),
                        anonynous(21),
                        vendorSpecific(22)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the  authentication parameter
        defined for a particular authentication method.
        The Autentication Parameter and the Authentication Method
        relationship as follows

         Method      Parameter      Description
        =========== =============== =================
          1          1              Reserved
          1          2              PAP
          1          3              CHAP
          1          4              MSCHAP
          1          5              MSCHAPV2
          2          6              LEAP
          2          7              PEAP
          2          8              EAP-TLS     
          2          9              EAP-FAST
          2          10             EAP-SIM
          2          11             EAP-TTLS
          2          12             EAP-AKA
          3          13             SIM
          3          14             USIM
          3          15             NFCSECURE
          3          16             HARDWARE TOKEN
          3          17             SOFT TOKEN
          3          18             CERTIFICATE
          3          19             USERNAME PASSWORD
          3          20             RESERVED
          3          21             Anonynous
          3          22             Vendor Specific"
    DEFVAL          { none } 
    ::= { cLWlan11uRealmEapAuthEntry 3 }

cLWlan11uRealmEapAuthCredentialType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        sim(1),
                        usim(2),
                        nfcSecure(3),
                        hardwareToken(4),
                        softToken(5),
                        certificate(6),
                        usernamePassword(7),
                        reserved(8),
                        anonynous(9),
                        vendorSpecific(10)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the credential type defined for a particular
        authentication method."
    DEFVAL          { sim } 
    ::= { cLWlan11uRealmEapAuthEntry 4 }

cLWlan11uRealmEapAuthRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Row Status for creation/deletion of a particular auth
        entry from the table" 
    ::= { cLWlan11uRealmEapAuthEntry 5 }
 

-- ********************************************************************
-- *        WLAN 11u Domain Table
-- ********************************************************************

cLWlan11uDomainTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlan11uDomainEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the Domain Entry
        configuration for a particular WLAN in a
        controller.
        Rows are added or deleted by explicit 
        management actions initiated by the user from a
        network management station through the 
        cLWlan11uDomainRowStatus object"
    ::= { ciscoLwappWlan11uConfig 6 }

cLWlan11uDomainEntry OBJECT-TYPE
    SYNTAX          CLWlan11uDomainEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the Domain
        configuration for a particular WLAN.
        A WLAN can have up to 10 domains defined."
    INDEX           {
                        cLWlanIndex,
                        cLWlan11uDomainIndex
                    } 
    ::= { cLWlan11uDomainTable 1 }

CLWlan11uDomainEntry ::= SEQUENCE {
        cLWlan11uDomainIndex     Unsigned32,
        cLWlan11uDomainName      SnmpAdminString,
        cLWlan11uDomainRowStatus RowStatus
}

cLWlan11uDomainIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..32)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies one instance of a Domain
        on a WLAN.Each WLAN can have up to 10 Domains defined.
        Each Domain should be unique." 
    ::= { cLWlan11uDomainEntry 1 }

cLWlan11uDomainName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..255))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the domain name for this particular
        Index." 
    ::= { cLWlan11uDomainEntry 2 }

cLWlan11uDomainRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Row Status for creation/deletion of a particular
        Domain entry in the table." 
    ::= { cLWlan11uDomainEntry 3 }
 

-- ********************************************************************
-- *        WLAN 11u 3gpp Table
-- ********************************************************************

cLWlan11u3gppTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlan11u3gppEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the 3gpp info
        configuration for a particular WLAN in a
        controller.
        Rows are added or deleted by explicit 
        management actions initiated by the user from a
        network management station through the 
        cLWlan11u3gppRowStatus object"
    ::= { ciscoLwappWlan11uConfig 7 }

cLWlan11u3gppEntry OBJECT-TYPE
    SYNTAX          CLWlan11u3gppEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the Domain
        configuration for a particular WLAN.
        A WLAN can have up to 32 operator defined."
    INDEX           {
                        cLWlanIndex,
                        cLWlan11u3gppIndex
                    } 
    ::= { cLWlan11u3gppTable 1 }

CLWlan11u3gppEntry ::= SEQUENCE {
        cLWlan11u3gppIndex       Unsigned32,
        cLWlan11u3gppCountryCode OCTET STRING,
        cLWlan11u3gppNetworkCode OCTET STRING,
        cLWlan11u3gppRowStatus   RowStatus
}

cLWlan11u3gppIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..32)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies one instance of a 3gpp
        on a WLAN.Each WLAN can have up to 32 3gpps defined.
        Each 3gpp should be unique." 
    ::= { cLWlan11u3gppEntry 1 }

cLWlan11u3gppCountryCode OBJECT-TYPE
    SYNTAX          OCTET STRING
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the Language defined for this 3gpp Index." 
    ::= { cLWlan11u3gppEntry 2 }

cLWlan11u3gppNetworkCode OBJECT-TYPE
    SYNTAX          OCTET STRING
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the Language defined for this 3gpp Index." 
    ::= { cLWlan11u3gppEntry 3 }

cLWlan11u3gppRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Row Status for creation/deletion of a particular
        3gpp entry in the table." 
    ::= { cLWlan11u3gppEntry 4 }
 

-- ********************************************************************
-- *        WLAN Service Advertisement Table
-- ********************************************************************

cLWlanServiceAdvertisementTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlanServiceAdvertisementEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the generic service advertisement
        configuration for a particular WLAN in a
        controller.

        This table has a one-to-one relationship with
        cLWlanConfigTable. There exist a row in this
        table corresponding to each   row representing
        a WLAN in cLWlanConfigTable."
    ::= { ciscoLwappWlanServiceAdvertisementConfig 1 }

cLWlanServiceAdvertisementEntry OBJECT-TYPE
    SYNTAX          CLWlanServiceAdvertisementEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the generic 802.11u
        configuration for a WLAN."
    INDEX           { cLWlanIndex } 
    ::= { cLWlanServiceAdvertisementTable 1 }

CLWlanServiceAdvertisementEntry ::= SEQUENCE {
        cLWlanServiceAdvertisementStatus          TruthValue,
        cLWlanServiceAdvertisementMsapServerIndex Unsigned32
}

cLWlanServiceAdvertisementStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the MSAP status for this WLAN.
        A value of true enables MSAP for this WLAN.
        A value of false disbales MSAP for this WLAN."
    DEFVAL          { false } 
    ::= { cLWlanServiceAdvertisementEntry 1 }

cLWlanServiceAdvertisementMsapServerIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..10)
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the Index for the MSAP Server." 
    ::= { cLWlanServiceAdvertisementEntry 5 }
 


cLWlanHotSpot2OperatorTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlanHotSpot2OperatorEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the Operator
        configuration for a particular WLAN in a
        controller.
        Rows are added or deleted by explicit 
        management actions initiated by the user from a
        network management station through the 
        cLWlanHotSpot2OperatorRowStatus object"
    ::= { ciscoLwappWlanHotSpot2Config 1 }

cLWlanHotSpot2OperatorEntry OBJECT-TYPE
    SYNTAX          CLWlanHotSpot2OperatorEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the Domain
        configuration for a particular WLAN.
        A WLAN can have up to 32 operator defined."
    INDEX           {
                        cLWlanIndex,
                        cLWlanHotSpot2OperatorIndex
                    } 
    ::= { cLWlanHotSpot2OperatorTable 1 }

CLWlanHotSpot2OperatorEntry ::= SEQUENCE {
        cLWlanHotSpot2OperatorIndex     Unsigned32,
        cLWlanHotSpot2OperatorName      SnmpAdminString,
        cLWlanHotSpot2OperatorLanguage  SnmpAdminString,
        cLWlanHotSpot2OperatorRowStatus RowStatus
}

cLWlanHotSpot2OperatorIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..32)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies one instance of a Operator
        on a WLAN.Each WLAN can have up to 32 Operators defined.
        Each Operator should be unique." 
    ::= { cLWlanHotSpot2OperatorEntry 1 }

cLWlanHotSpot2OperatorName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..255))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the Operator name for this particular
        Index." 
    ::= { cLWlanHotSpot2OperatorEntry 2 }

cLWlanHotSpot2OperatorLanguage OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..3))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the Language defined for this Operator Index." 
    ::= { cLWlanHotSpot2OperatorEntry 3 }

cLWlanHotSpot2OperatorRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Row Status for creation/deletion of a particular
        Operator entry in the table." 
    ::= { cLWlanHotSpot2OperatorEntry 4 }
 


cLWlanHotSpot2PortConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlanHotSpot2PortConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies one instance of
        Port-Protocol Configuration on a WLAN.Each WLAN can 
        have up to 10 port configuration defined.Each configuration 
        should be unique."
    ::= { ciscoLwappWlanHotSpot2Config 2 }

cLWlanHotSpot2PortConfigEntry OBJECT-TYPE
    SYNTAX          CLWlanHotSpot2PortConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the Port-Protocol
        configuration for a particular WLAN.
        A WLAN can have up to 10 port configurations defined."
    INDEX           {
                        cLWlanIndex,
                        cLWlanHotSpot2PortConfigIndex
                    } 
    ::= { cLWlanHotSpot2PortConfigTable 1 }

CLWlanHotSpot2PortConfigEntry ::= SEQUENCE {
        cLWlanHotSpot2PortConfigIndex      Unsigned32,
        cLWlanHotSpot2PortConfigIpProtocol INTEGER,
        cLWlanHotSpot2PortConfigPortNumber INTEGER,
        cLWlanHotSpot2PortConfigStatus     INTEGER,
        cLWlanHotSpot2PortConfigRowStatus  RowStatus
}

cLWlanHotSpot2PortConfigIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies one instance of a Port
        Configuration on a WLAN.Each WLAN can have up to 32 Port
        Configurations defined.Each Port Configuration should be 
        unique." 
    ::= { cLWlanHotSpot2PortConfigEntry 1 }

cLWlanHotSpot2PortConfigIpProtocol OBJECT-TYPE
    SYNTAX          INTEGER  {
                        icmp(1),
                        ftp(6),
                        ikev2(17),
                        esp(50)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the Port Ip protocol
        for this index for a WLAN" 
    ::= { cLWlanHotSpot2PortConfigEntry 2 }

cLWlanHotSpot2PortConfigPortNumber OBJECT-TYPE
    SYNTAX          INTEGER  {
                        icmp-esp(0),
                        ftp(20),
                        ssh(22),
                        ttls-vpn(443),
                        ikev2(500),
                        pptp-vpn(1723),
                        ipsec-nat(4500),
                        voip(5060)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the Port Number for this index
        for a WLAN. This object indicates the Port Number 
        with respect to an IP Protocol.
        The Protocol Port Number relationship is per
        the following table:
        IP Protocol Port Number     Description
        =========== =============== =================
          1            0         ICMP
          6            20        FTP
          6            22        SSH
          6            443       TLS
          6            1723      PPTP-VPN
          6            5060      VoIP
          17           5060      VoIP
          17           4500      IKEv
          17           500       IKEv2
          50           0         ESP" 
    ::= { cLWlanHotSpot2PortConfigEntry 3 }

cLWlanHotSpot2PortConfigStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        closed(1),
                        open(2),
                        unknown(3)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the Port Status
        for this instance for a WLAN" 
    ::= { cLWlanHotSpot2PortConfigEntry 4 }

cLWlanHotSpot2PortConfigRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Row Status for creation/deletion of a particular
        PortConfig entry in the table." 
    ::= { cLWlanHotSpot2PortConfigEntry 5 }
 


cLWlanHotSpot2ConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlanHotSpot2ConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the generic HotSpot2
        configuration for a particular WLAN in a
        controller.

        This table has a one-to-one relationship with
        cLWlanConfigTable. There exist a row in this
        table corresponding to each   row representing
        a WLAN in cLWlanConfigTable."
    ::= { ciscoLwappWlanHotSpot2Config 3 }

cLWlanHotSpot2ConfigEntry OBJECT-TYPE
    SYNTAX          CLWlanHotSpot2ConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the generic HotSpot2
        configuration for a WLAN."
    INDEX           { cLWlanIndex } 
    ::= { cLWlanHotSpot2ConfigTable 1 }

CLWlanHotSpot2ConfigEntry ::= SEQUENCE {
        cLWlanHotSpot2WanLinkStatus    INTEGER,
        cLWlanHotSpot2WanSymLinkStatus INTEGER,
        cLWlanHotSpot2WanDownLinkSpeed Unsigned32,
        cLWlanHotSpot2WanUpLinkSpeed   Unsigned32
}

cLWlanHotSpot2WanLinkStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        linkUp(1),
                        linkDown(2),
                        linkInTestState(3),
                        notConfigured(4)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the status of the link with respect to
        WAN metrics configuration." 
    ::= { cLWlanHotSpot2ConfigEntry 1 }

cLWlanHotSpot2WanSymLinkStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        different(1),
                        same(2)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the symmetry of the link with respect to
        WAN metrics configuration. A value of 'different(1)' 
        indicates that link speed is different in uplink and 
        downlink(ex:ADSL). A value of 'same(2)' indicates that
        link speed is same in uplink and downlink(ex:DSL)." 
    ::= { cLWlanHotSpot2ConfigEntry 2 }

cLWlanHotSpot2WanDownLinkSpeed OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the down link speed of WAN Backhaul
        in kbps." 
    ::= { cLWlanHotSpot2ConfigEntry 3 }

cLWlanHotSpot2WanUpLinkSpeed OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the up link speed of WAN Backhaul
        in kbps." 
    ::= { cLWlanHotSpot2ConfigEntry 4 }
 


cLAPGroupsHyperlocationConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLAPGroupsHyperlocationConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table for configuring Hyperlocation
        settings allowed for each AP Group.
        Each site can have a set of HALO and PakRSSI
        parameters associated with it."
    ::= { ciscoLwappAPGroupsHyperlocationConfig 1 }

cLAPGroupsHyperlocationConfigEntry OBJECT-TYPE
    SYNTAX          CLAPGroupsHyperlocationConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLAPGroupsHyperlocationConfigEntry.
        cLAPGroupName is mandatory for creating an entry in
        CLAPGroupsHyperlocationConfigEntry ."
    INDEX           { cLAPGroupName } 
    ::= { cLAPGroupsHyperlocationConfigTable 1 }

CLAPGroupsHyperlocationConfigEntry ::= SEQUENCE {
        cLAPGroupsHyperlocationEnable     TruthValue,
        cLAPGroupsPakRssiThreshold        Integer32,
        cLAPGroupsPakRssiThresholdTrigger Gauge32,
        cLAPGroupsPakRssiNtpIpAddressType InetAddressType,
        cLAPGroupsPakRssiNtpAddress       InetAddress
}

cLAPGroupsHyperlocationEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the state of Hyperlocation.
        A value of 'true' indicates that Hyperlocation is enabled. 
        A value of 'false' indicates that Hyperlocation is disabled."
    DEFVAL          { false } 
    ::= { cLAPGroupsHyperlocationConfigEntry 1 }

cLAPGroupsPakRssiThreshold OBJECT-TYPE
    SYNTAX          Integer32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the threshold value for
        Packet RSSI location feature. Valid range is
        -100 dbm to -50 dbm."
    DEFVAL          { -100 } 
    ::= { cLAPGroupsHyperlocationConfigEntry 2 }

cLAPGroupsPakRssiThresholdTrigger OBJECT-TYPE
    SYNTAX          Gauge32 (1..100)
    UNITS           "dbm"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the trigger threshold
        value for Packet RSSI location feature. Valid
        range is 1 dbm to 100 dbm."
    DEFVAL          { 10 } 
    ::= { cLAPGroupsHyperlocationConfigEntry 3 }

cLAPGroupsPakRssiNtpIpAddressType OBJECT-TYPE
    SYNTAX          InetAddressType
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the NTP server
        IP address type for Packet RSSI location feature." 
    ::= { cLAPGroupsHyperlocationConfigEntry 4 }

cLAPGroupsPakRssiNtpAddress OBJECT-TYPE
    SYNTAX          InetAddress
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the NTP server
        IP address for Packet RSSI location feature." 
    ::= { cLAPGroupsHyperlocationConfigEntry 5 }
 


cLAPGroupConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLAPGroupConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table for configuring general parameters for an AP group"
    ::= { ciscoLwappAPGroupsVlanConfig 6 }

cLAPGroupConfigEntry OBJECT-TYPE
    SYNTAX          CLAPGroupConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLAPGroupConfigTable for
        configuring general parameters for an AP group"
    INDEX           { cLAPGroupName } 
    ::= { cLAPGroupConfigTable 1 }

CLAPGroupConfigEntry ::= SEQUENCE {
        cLApGroupPreferMode          INTEGER,
        cLApGroupGlobalWebAuthConfig TruthValue,
        cLApGroupExternalWebAuthUrl  CiscoURLStringOrEmpty
}

cLApGroupPreferMode OBJECT-TYPE
    SYNTAX          INTEGER  {
                        ipv4(1),
                        ipv6(2),
                        disable(3)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies prefer-mode of AP-Group." 
    ::= { cLAPGroupConfigEntry 1 }

cLApGroupGlobalWebAuthConfig OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether the web authentication is set
        per Ap Group or not.
        A value of 'true' indicates that webauth is enabled on Ap Group.
        A value of 'false' indicates that webauth is disabled on Ap Group."
    DEFVAL          { false } 
    ::= { cLAPGroupConfigEntry 2 }

cLApGroupExternalWebAuthUrl OBJECT-TYPE
    SYNTAX          CiscoURLStringOrEmpty
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the URL to which the client webpage
        will be directed for authentication when a client joins the
        WLAN part of an AP group."
    DEFVAL          { "" } 
    ::= { cLAPGroupConfigEntry 3 }
 


cLAPGroupsPortConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLAPGroupsPortConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table for configuring port
        settings allowed for each AP Group."
    ::= { ciscoLwappAPGroupsPortConfig 1 }

cLAPGroupsPortConfigEntry OBJECT-TYPE
    SYNTAX          CLAPGroupsPortConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLAPGroupsPortConfigEntry.
        cLAPGroupName is mandatory for creating a entry in
        CLAPGroupsPortConfigEntry ."
    INDEX           {
                        cLAPGroupName,
                        cLAPGroupsLANPortNumber
                    } 
    ::= { cLAPGroupsPortConfigTable 1 }

CLAPGroupsPortConfigEntry ::= SEQUENCE {
        cLAPGroupsLANPortNumber    Unsigned32,
        cLAPGroupsLANPortStatus    INTEGER,
        cLAPGroupsLANPortPoeStatus INTEGER,
        cLAPGroupsLANPortRlanName  SnmpAdminString,
        cLAPGroupsLANPortRowStatus RowStatus
}

cLAPGroupsLANPortNumber OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies the LAN port number
        of an AP Group. Each AP Group can have up to 3 LAN ports." 
    ::= { cLAPGroupsPortConfigEntry 1 }

cLAPGroupsLANPortStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        disabled(0),
                        enabled(1)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the LAN port state.
        A value of 'true' indicates that selected LAN Port is enabled. A value
        of 'false' indicates that LAN Port is disabled."
    DEFVAL          { disabled } 
    ::= { cLAPGroupsPortConfigEntry 2 }

cLAPGroupsLANPortPoeStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        notsupported(0),
                        disabled(1),
                        enabled(2)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the LAN port POE state.
        A value of 'true' indicates that POE is enabled. A value
        of 'false' indicates that POE is disabled."
    DEFVAL          { disabled } 
    ::= { cLAPGroupsPortConfigEntry 3 }

cLAPGroupsLANPortRlanName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..64))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the remote LAN name of the corresponding port." 
    ::= { cLAPGroupsPortConfigEntry 4 }

cLAPGroupsLANPortRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and used
        to create and delete specific instances of rows 
        in this table. cLAPGroupName and cLAPGroupsLANPortNumber
        are mandatory for creating and deleting an entry." 
    ::= { cLAPGroupsPortConfigEntry 5 }
 


cLAPGroupsExtModuleConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLAPGroupsExtModuleConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table for configuring external module settings allowed for each AP Group.
        An entry in this table is created for each AP group."
    ::= { ciscoLwappAPGroupsPortConfig 2 }

cLAPGroupsExtModuleConfigEntry OBJECT-TYPE
    SYNTAX          CLAPGroupsExtModuleConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLAPGroupsExtModuleConfigEntry.
        cLAPGroupName is mandatory for creating an entry in
        CLAPGroupsExtModuleConfigEntry ."
    INDEX           { cLAPGroupName } 
    ::= { cLAPGroupsExtModuleConfigTable 1 }

CLAPGroupsExtModuleConfigEntry ::= SEQUENCE {
        cLAPGroupsExtModuleStatus   INTEGER,
        cLAPGroupsExtModuleRlanName SnmpAdminString
}

cLAPGroupsExtModuleStatus OBJECT-TYPE
    SYNTAX          INTEGER  {
                        disabled(0),
                        enabled(1)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the external module state.
        A value of 'true' indicates that external module is enabled. A value
        of 'false' indicates that external module is disabled."
    DEFVAL          { disabled } 
    ::= { cLAPGroupsExtModuleConfigEntry 1 }

cLAPGroupsExtModuleRlanName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the remote lan name of the external module." 
    ::= { cLAPGroupsExtModuleConfigEntry 2 }
 

-- ********************************************************************
-- *       AP Groups Vlan Config
-- ********************************************************************

cLAPGroupsVlanConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLAPGroupsVlanConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table for the WLAN-interface-mappings and WLAN-NAC
        settings allowed for each configured site.
        Each site can have a set of WLANs associated
        with it.

        Rows are added or deleted by explicit 
        management actions initiated by the user from a
        network management station through the 
        cLAPGroupsVlanConfigRowStatus object."
    ::= { ciscoLwappAPGroupsVlanConfig 1 }

cLAPGroupsVlanConfigEntry OBJECT-TYPE
    SYNTAX          CLAPGroupsVlanConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLAPGroupsVlanMappingTable.
        cLWlanProfileName is mandatory for creating a entry in
        cLWlanConfigEntry."
    INDEX           {
                        cLAPGroupName,
                        cLWlanProfileName
                    } 
    ::= { cLAPGroupsVlanConfigTable 1 }

CLAPGroupsVlanConfigEntry ::= SEQUENCE {
        cLAPGroupName                          OCTET STRING,
        cLAPGroupsVlanMappingInterfaceName     OCTET STRING,
        cLAPGroupNACSupport                    TruthValue,
        cLAPGroupsVlanConfigRowStatus          RowStatus,
        cLAPGroupsVlanConfigStorageType        StorageType,
        cLAPGroupsWlanOrderIndex               Unsigned32,
        cLAPGroupsVlanMappingInterfaceNameRev1 OCTET STRING
}

cLAPGroupName OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (1..64))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object uniquely identifies a AP group.
        The string is an unique name assigned to a site." 
    ::= { cLAPGroupsVlanConfigEntry 1 }

cLAPGroupsVlanMappingInterfaceName OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (1..32))
    MAX-ACCESS      read-create
    STATUS          deprecated
    DESCRIPTION
        "This object represents the interface to be used
        when a client connects to the 'cLWlanProfileName' 
        WLAN on the AP.
        When an AP is associated with a site, and the site
        has an associated set of WLANs, then only those 
        WLANs are beamed by the AP.
        cLAPGroupsVlanMappingInterfaceName object is superseded 
        by cLAPGroupsVlanMappingInterfaceNameRev1." 
    ::= { cLAPGroupsVlanConfigEntry 2 }

cLAPGroupNACSupport OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object is used to configure the NAC- Out Of
        Band(OOB) support for this AP groups VLAN.
        A value of 'true'  indicates that the AP group
        supports the NAC- Out Of Band(OOB) feature. 
        A value of 'false' indicates that the AP group
        does not support the NAC- Out Of Band(OOB) feature."
    DEFVAL          { false } 
    ::= { cLAPGroupsVlanConfigEntry 3 }

cLAPGroupsVlanConfigRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and used
        to create and delete specific instances of rows 
        in this table." 
    ::= { cLAPGroupsVlanConfigEntry 4 }

cLAPGroupsVlanConfigStorageType OBJECT-TYPE
    SYNTAX          StorageType
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represnts the storage type for this
        conceptual row."
    DEFVAL          { nonVolatile } 
    ::= { cLAPGroupsVlanConfigEntry 5 }

cLAPGroupsWlanOrderIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represnts the position of a wlan in each
        AP group. When a WLAN is added to an AP group, it will be
        placed in the lowest available slot in an array of size 16.
        This index will determine the order in which the WLAN is
        applied on an AP in that group." 
    ::= { cLAPGroupsVlanConfigEntry 6 }

cLAPGroupsVlanMappingInterfaceNameRev1 OBJECT-TYPE
    SYNTAX          OCTET STRING (SIZE  (1..128))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the interface to be used
        when a client connects to the 'cLWlanProfileName' 
        WLAN on the AP.
        When an AP is associated with a site, and the site
        has an associated set of WLANs, then only those 
        WLANs are beamed by the AP." 
    ::= { cLAPGroupsVlanConfigEntry 7 }
 


cLAPGroupsVenueConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLAPGroupsVenueConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table for the configuring Venue details
        for a  configured site."
    ::= { ciscoLwappAPGroupsVlanConfig 2 }

cLAPGroupsVenueConfigEntry OBJECT-TYPE
    SYNTAX          CLAPGroupsVenueConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLAPGroupsVlanMappingTable.
        cLWlanProfileName is mandatory for creating a entry in
        cLWlanConfigEntry."
    INDEX           { cLAPGroupName } 
    ::= { cLAPGroupsVenueConfigTable 1 }

CLAPGroupsVenueConfigEntry ::= SEQUENCE {
        cLAPGroupsVenueConfigVenueGroup INTEGER,
        cLAPGroupsVenueConfigVenueType  INTEGER,
        cLAPGroupsVenueConfigVenueName  SnmpAdminString,
        cLAPGroupsVenueConfigLanguage   SnmpAdminString,
        cLAPGroupsOperatingClass        BITS
}

cLAPGroupsVenueConfigVenueGroup OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unspecified(1),
                        assembly(2),
                        business(3),
                        educational(4),
                        factoryAndIndustrial(5),
                        institutional(6),
                        mercantile(7),
                        residential(8),
                        storage(9),
                        utilityAndMisc(10),
                        vehicular(11),
                        outdoor(12)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the venue group
        for this AP Group."
    DEFVAL          { unspecified } 
    ::= { cLAPGroupsVenueConfigEntry 1 }

cLAPGroupsVenueConfigVenueType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        unspecified(1),
                        unspecifiedAssembly(2),
                        arena(3),
                        stadium(4),
                        passengerTerminal(5),
                        amphitheater(6),
                        amusementPark(7),
                        placeOfWorship(8),
                        conventionCenter(9),
                        library(10),
                        museum(11),
                        restaurant(12),
                        theater(13),
                        bar(14),
                        coffeeShop(15),
                        zooOrAquarium(16),
                        emergencyCoordinationCenter(17),
                        unspecifiedBusiness(18),
                        doctorOrDentistOffice(19),
                        bank(20),
                        fireStation(21),
                        policeStation(22),
                        postOffice(23),
                        professionalOffice(24),
                        researchAndDevelopmentFacility(25),
                        attorneyOffice(26),
                        unspecifiedEducational(27),
                        schoolPrimary(28),
                        schoolSecondary(29),
                        universityOrCollege(30),
                        unspecifiedFactoryAndIndustrial(31),
                        factory(32),
                        unspecifiedInstitutional(33),
                        hospital(34),
                        longTermCareFacility(35),
                        alcoholAndDrugRehabilitationCenter(36),
                        groupHome(37),
                        prisonOrJail(38),
                        unspecifiedMercantile(39),
                        retailStore(40),
                        groceryMarket(41),
                        atomotiveServiceStation(42),
                        shoppingMall(43),
                        gasStation(44),
                        unspecifiedResidential(45),
                        privateResidence(46),
                        hotelOrMotel(47),
                        dormitory(48),
                        boardingHouse(49),
                        unspecifiedStorage(50),
                        unspecifiedUtility(51),
                        unspecifiedVehicular(52),
                        automobileOrTruck(53),
                        airplane(54),
                        bus(55),
                        ferry(56),
                        shipOrBoat(57),
                        train(58),
                        motorBike(59),
                        unspecifiedOutdoor(60),
                        muniMeshNetwork(61),
                        cityPark(62),
                        restArea(63),
                        trafficControl(64),
                        busStop(65),
                        kiosk(66)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object indicates the venue type within
        a particular venue group,for this AP Group.
         The Venue group-Venue Type relationship is per
         the following table:
            Venue Group Venue Type Code Venue Description
            =========== =============== =================
                 0            0         Unspecified
                 0            1-255     Reserved
                 1            0         Unspecified Assembly
                 1            1         Arena
                 1            2         Stadium
                 1            3         Passenger Terminal (e.g.,
                                        airport, port, bus station, 
                                        ferry terminal, train station)
                 1            4         Amphitheater
                 1            5         Amusement Park
                 1            6         Place of Worship
                 1            7         Convention Center
                 1            8         Library
                 1            9         Museum
                 1            10        Restaurant
                 1            11        Theater
                 1            12        Bar
                 1            13        Coffee Shop
                 1            14        Zoo or Aquarium
                 1            15        Emergency Coordination Center
                 1            16-255    Reserved
                 2            0         Unspecified Business
                 2            1         Doctor or Dentist office
                 2            2         Bank
                 2            3         Fire Station
                 2            4         Police Station
                 2            6         Post Office
                 2            7         Professional Office
                 2            8         Research and Development 
                                        Facility
                 2            9         Attorney Office
                 2            10-255    Reserved
                 3            0         Unspecified Educational
                 3            1         School, Primary
                 3            2         School, Secondary
                 3            3         University or College
                 3            4-255     Reserved
                 4            0         Unspecified Factory and 
                                        Industrial Factory
                 4            2-255     Reserved
                 5            0         Unspecified Institutional
                 5            1         Hospital
                 5            2         Long-Term Care Facility (e.g.,
                                        Nursing home, Hospice, etc.)
                 5            3         Alcohol and Drug Re-habilitation
                                        Center
                 5            4         Group Home
                 5            5         Prison or Jail 
                 5            6-255     Reserved
                 6            0         Unspecified Mercantile
                 6            1         Retail Store
                 6            2         Grocery Market
                 6            3         Automotive Service Station
                 6            4-255     Reserved
                 7            0         Unspecified Residential
                 7            1         Hotel or Motel  
                 7            2         Dormitory
                 7            3         Boarding House
                 7            4-255     Reserved
                 8            0-255     Reserved
                 9            0-255     Reserved
                10           0         Unspecified Vehicular
                10           1         Automobile or Truck
                10           2         Airplane
                10           3         Bus
                10           4         Ferry
                10           5         Ship or Boat
                10           6         Train
                10           7-255     Reserved
                11           0         Unspecified Outdoor
                11           1         Muni-mesh Network
                11           2         City Park
                11           3-255     Reserved"
    DEFVAL          { unspecified } 
    ::= { cLAPGroupsVenueConfigEntry 2 }

cLAPGroupsVenueConfigVenueName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..252))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This is the venue name defined for this AP Group." 
    ::= { cLAPGroupsVenueConfigEntry 3 }

cLAPGroupsVenueConfigLanguage OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..3))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This is the Language defined for this AP Group." 
    ::= { cLAPGroupsVenueConfigEntry 4 }

cLAPGroupsOperatingClass OBJECT-TYPE
    SYNTAX          BITS {
                        class81(0),
                        class83(1),
                        class84(2),
                        class112(3),
                        class113(4),
                        class115(5),
                        class116(6),
                        class117(7),
                        class118(8),
                        class119(9),
                        class120(10),
                        class121(11),
                        class122(12),
                        class123(13),
                        class124(14),
                        class125(15),
                        class126(16),
                        class127(17)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the the group of channels on the
        frequency band(s) the access network operates." 
    ::= { cLAPGroupsVenueConfigEntry 5 }
 


cLAPGroupsMultipleVenueTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLAPGroupsMultipleVenueEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Table for configuring multiple venues
        for a  configured site."
    ::= { ciscoLwappAPGroupsVlanConfig 3 }

cLAPGroupsMultipleVenueEntry OBJECT-TYPE
    SYNTAX          CLAPGroupsMultipleVenueEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLAPGroupsMultipleVenueTable.
        cLAPGroupsMultipleVenueLanguage is mandatory
        for creating a row in this table."
    INDEX           {
                        cLAPGroupName,
                        cLAPGroupsMultipleVenueLanguage
                    } 
    ::= { cLAPGroupsMultipleVenueTable 1 }

CLAPGroupsMultipleVenueEntry ::= SEQUENCE {
        cLAPGroupsMultipleVenueLanguage  SnmpAdminString,
        cLAPGroupsMultipleVenueName      SnmpAdminString,
        cLAPGroupsMultipleVenueRowStatus RowStatus
}

cLAPGroupsMultipleVenueLanguage OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..3))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This is the Language defined for the particular venue name
        entry." 
    ::= { cLAPGroupsMultipleVenueEntry 1 }

cLAPGroupsMultipleVenueName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..252))
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the one of the venue names defined for this AP Group." 
    ::= { cLAPGroupsMultipleVenueEntry 2 }

cLAPGroupsMultipleVenueRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Row Status for creation/deletion of a particular
        venue entry in the table." 
    ::= { cLAPGroupsMultipleVenueEntry 3 }
 


cLAPGroupNasIdConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLAPGroupNasIdConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table for the configuring NAS-ID for an AP group."
    ::= { ciscoLwappAPGroupNasIdConfig 1 }

cLAPGroupNasIdConfigEntry OBJECT-TYPE
    SYNTAX          CLAPGroupNasIdConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLAPGroupNasIdConfigTable for the configuring NAS-ID for an AP group."
    INDEX           { cLAPGroupName } 
    ::= { cLAPGroupNasIdConfigTable 1 }

CLAPGroupNasIdConfigEntry ::= SEQUENCE {
        cLAPGroupNasId SnmpAdminString
}

cLAPGroupNasId OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the NAS-ID to this AP group
        NAS-ID string is sent to radius server by WLC (as radius client)
        via authentication request, which can be used to classify users
        to different groups then radius server can reply a customized
        authentication response" 
    ::= { cLAPGroupNasIdConfigEntry 1 }
 


cLAPGroupsPolicyTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLAPGroupsPolicyEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table for the policies to be mapped
        to each AP group on the controller.
        Rows are added or deleted by explicit 
        management actions initiated by the user from a
        network management station through the 
        cLAPGroupsPolicyRowStatus object."
    ::= { ciscoLwappAPGroupsVlanConfig 4 }

cLAPGroupsPolicyEntry OBJECT-TYPE
    SYNTAX          CLAPGroupsPolicyEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLAPGroupsPolicyTable"
    INDEX           {
                        cLAPGroupName,
                        cLAPGroupsPolicyWlanId,
                        cLAPGroupsPolicyPriIndex
                    } 
    ::= { cLAPGroupsPolicyTable 1 }

CLAPGroupsPolicyEntry ::= SEQUENCE {
        cLAPGroupsPolicyWlanId      Unsigned32,
        cLAPGroupsPolicyPriIndex    Unsigned32,
        cLAPGroupsPolicyIndex       Unsigned32,
        cLAPGroupsPolicyWlanProfile SnmpAdminString,
        cLAPGroupsPolicyRowStatus   RowStatus
}

cLAPGroupsPolicyWlanId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the Index of the WLAN
        on which the Policy will get applied. The WLAN
        should be present on the AP group." 
    ::= { cLAPGroupsPolicyEntry 1 }

cLAPGroupsPolicyPriIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object represents the Priority Index of the policy
        configured on the AP Group. The Policies will 
            get applied in the order of the priority index." 
    ::= { cLAPGroupsPolicyEntry 2 }

cLAPGroupsPolicyIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object uniquely specifies a Policy
        Added to an AP group." 
    ::= { cLAPGroupsPolicyEntry 3 }

cLAPGroupsPolicyWlanProfile OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (1..64))
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object represents the profile name assigned
        to this WLAN. This value is assigned during wlan 
        creation using cLWlanProfileName." 
    ::= { cLAPGroupsPolicyEntry 4 }

cLAPGroupsPolicyRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Row Status for
        creation/deletion of a particular
        venue entry in the table." 
    ::= { cLAPGroupsPolicyEntry 5 }
 


cLAPGroupQinqConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLAPGroupQinqConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table for the configuring QinQ for an AP group,
        QinQ is used to append an external VLAN tag for client based on AP Group"
    ::= { ciscoLwappAPGroupsVlanConfig 5 }

cLAPGroupQinqConfigEntry OBJECT-TYPE
    SYNTAX          CLAPGroupQinqConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLAPGroupQinqConfigTable for the configuring QinQ for an AP group,
        QinQ is used to append an external VLAN tag for client which
        connected to the AP that belong to this AP Group"
    INDEX           { cLAPGroupName } 
    ::= { cLAPGroupQinqConfigTable 1 }

CLAPGroupQinqConfigEntry ::= SEQUENCE {
        cLAPGroupTrafficQinqEnabled TruthValue,
        cLAPGroupDhcpQinqEnabled    TruthValue,
        cLAPGroupQinqServiceVlanId  Integer32
}

cLAPGroupTrafficQinqEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the QinQ state for this AP group
        QinQ is used to append an external VLAN tag for client which
        connected to the AP that belong to this AP Group
        - A value of 'true' indicates QinQ is enabled.
        - A value of 'false' indicates the QinQ is disabled." 
    ::= { cLAPGroupQinqConfigEntry 1 }

cLAPGroupDhcpQinqEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the QinQ state for this AP group
        QinQ is used to append an external VLAN tag for client which
        connected to the AP that belong to this AP Group
        - A value of 'true' indicates that dhcp QinQ is enabled.
        - A value of 'false indicates that dhcp QinQ is disabled." 
    ::= { cLAPGroupQinqConfigEntry 2 }

cLAPGroupQinqServiceVlanId OBJECT-TYPE
    SYNTAX          Integer32 (1..4095)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the QinQ service vlan ID for this AP group" 
    ::= { cLAPGroupQinqConfigEntry 3 }
 

-- ********************************************************************
-- WLAN Client Configuration
-- ********************************************************************

cLWlanConfigClientTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlanConfigClientEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the WLAN configuration for
        the 802.11 wireless clients that are associated 
        with the APs that have joined this controller.

        The creation of a new row in cLWlanConfigTable,
        through an explicit network management action,
        results in creation of an entry in this table.
        Similarly, deletion of a row in
        cLWlanConfigTable through user action causes the
        deletion of corresponding row in this table.

        This table has an one-to-one relationship with
        cLWlanConfigTable. There exists an entry in this 
        table for each corresponding entry in the 
        cLWlanConfigTable."
    ::= { ciscoLwappWlanConfig 2 }

cLWlanConfigClientEntry OBJECT-TYPE
    SYNTAX          CLWlanConfigClientEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in this
        table and provides the information about the
        clients associated on the WLAN, uniquely identified by
        the cLWlanIndex."
    INDEX           { cLWlanIndex } 
    ::= { cLWlanConfigClientTable 1 }

CLWlanConfigClientEntry ::= SEQUENCE {
        cLWlanClientAclName     DisplayString,
        cLWlanP2PBlocking       INTEGER,
        cLWlanClientIPv6AclName DisplayString
}

cLWlanClientAclName OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the name of the ACL applied
        to this WLAN.  If it is required to remove the ACL
        name for a WLAN, it should be set to 'none'.
        ACL's are applied in the following priority order - 
        interfaces ACLs, WLAN ACLs, client ACLs." 
    ::= { cLWlanConfigClientEntry 1 }

cLWlanP2PBlocking OBJECT-TYPE
    SYNTAX          INTEGER  {
                        disable(1),
                        drop(2),
                        forwardUp(3),
                        allowPvtGrp(4)
                    }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents per WLAN peer-to-peer
        blocking behavior on controller. Peer-to-peer          
        blocking means traffic between two clients on          
        same VLAN will not be bridged.          

            disable   : Peer-to-peer blocking is disabled          
                        and traffic is bridged locally          
                        within the controller.          
            drop      : The packet will be discarded.          
            forwardUp : The packet will be forwarded on the          
                        upstream VLAN. The device 'north' of          
                        the controller can then make the          
                        decision about what to do with the          
                        packet.
            allowPvtGrp : The packet will be bridged if both
                        source and destination have same 'ipsk-tag',
                        if mac-filtering is disabled the packet
                        will be discarded." 
    ::= { cLWlanConfigClientEntry 2 }

cLWlanClientIPv6AclName OBJECT-TYPE
    SYNTAX          DisplayString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the name of the IPv6 ACL applied
        to this WLAN.  If it is required to remove the ACL
        name for a WLAN, it should be set to 'none'.
        ACL's are applied in the following priority order - 
        interfaces ACLs, WLAN ACLs, client ACLs." 
    ::= { cLWlanConfigClientEntry 3 }
 

-- ********************************************************************
-- WLAN QoS Configuration
-- ********************************************************************

cLWlanConfigQosTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlanConfigQosEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the QoS configuration for
        the WLAN.

        The creation of a new row in cLWlanConfigTable,
        through an explicit network management action,
        results in creation of an entry in this table.
        Similarly, deletion of a row in
        cLWlanConfigTable through user action causes the
        deletion of corresponding row in this table.

        This table has an one-to-one relationship with
        cLWlanConfigTable. There exists an entry in this 
        table for each corresponding entry in the 
        cLWlanConfigTable."
    ::= { ciscoLwappWlanConfig 3 }

cLWlanConfigQosEntry OBJECT-TYPE
    SYNTAX          CLWlanConfigQosEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in this
        table and provides the information about the
        QoS parameters on the WLAN, uniquely identified by
        the cLWlanIndex."
    INDEX           { cLWlanIndex } 
    ::= { cLWlanConfigQosTable 1 }

CLWlanConfigQosEntry ::= SEQUENCE {
        cLWlanClientDSAverageDataRate       Unsigned32,
        cLWlanClientUSAverageDataRate       Unsigned32,
        cLWlanClientDSBurstDataRate         Unsigned32,
        cLWlanClientUSBurstDataRate         Unsigned32,
        cLWlanClientDSAvgRealTimeDataRate   Unsigned32,
        cLWlanClientUSAvgRealTimeDataRate   Unsigned32,
        cLWlanClientDSBurstRealTimeDataRate Unsigned32,
        cLWlanClientUSBurstRealTimeDataRate Unsigned32,
        cLWlanSsidDSAverageDataRate         Unsigned32,
        cLWlanSsidUSAverageDataRate         Unsigned32,
        cLWlanSsidDSBurstDataRate           Unsigned32,
        cLWlanSsidUSBurstDataRate           Unsigned32,
        cLWlanSsidDSAvgRealTimeDataRate     Unsigned32,
        cLWlanSsidUSAvgRealTimeDataRate     Unsigned32,
        cLWlanSsidDSBurstRealTimeDataRate   Unsigned32,
        cLWlanSsidUSBurstRealTimeDataRate   Unsigned32,
        cLWlanWlanDSAverageDataRate         Unsigned32,
        cLWlanWlanUSAverageDataRate         Unsigned32,
        cLWlanWlanDSBurstDataRate           Unsigned32,
        cLWlanWlanUSBurstDataRate           Unsigned32,
        cLWlanWlanDSAvgRealTimeDataRate     Unsigned32,
        cLWlanWlanUSAvgRealTimeDataRate     Unsigned32,
        cLWlanWlanDSBurstRealTimeDataRate   Unsigned32,
        cLWlanWlanUSBurstRealTimeDataRate   Unsigned32
}

cLWlanClientDSAverageDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies Average Data Rate per user on downstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 1 }

cLWlanClientUSAverageDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies Average Data Rate per user on upstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 2 }

cLWlanClientDSBurstDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies Burst Data Rate per user on downstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 3 }

cLWlanClientUSBurstDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies Burst Data Rate per user on upstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 4 }

cLWlanClientDSAvgRealTimeDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies average real time
        Data Rate per user on downstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 5 }

cLWlanClientUSAvgRealTimeDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies average real time
        Data Rate per user on upstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 6 }

cLWlanClientDSBurstRealTimeDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies burst real time
        Data Rate per user on downstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 7 }

cLWlanClientUSBurstRealTimeDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies burst real time
        Data Rate per user on upstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 8 }

cLWlanSsidDSAverageDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies Average
        Data Rate per user on downstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 9 }

cLWlanSsidUSAverageDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies Average
        Data Rate per user on upstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 10 }

cLWlanSsidDSBurstDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies Burst
        Data Rate per user on downstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 11 }

cLWlanSsidUSBurstDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies Burst
        Data Rate per user on upstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 12 }

cLWlanSsidDSAvgRealTimeDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies average real time
        Data Rate per user on downstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 13 }

cLWlanSsidUSAvgRealTimeDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies average real time
        Data Rate per user on upstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 14 }

cLWlanSsidDSBurstRealTimeDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies burst real time
        Data Rate per user on downstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 15 }

cLWlanSsidUSBurstRealTimeDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies burst real time
        Data Rate per user on upstream.
        Value of 0 indicates the feature is disabled." 
    ::= { cLWlanConfigQosEntry 16 }

cLWlanWlanDSAverageDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "kbytes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies average data rate per
        wlan on downstream. Value of 0 indicates that 
        feature is disabled." 
    ::= { cLWlanConfigQosEntry 17 }

cLWlanWlanUSAverageDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "kbytes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies average data rate per
        wlan on upstream. Value of 0 indicates that 
        feature is disabled." 
    ::= { cLWlanConfigQosEntry 18 }

cLWlanWlanDSBurstDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "kbytes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies burst data rate per
        wlan on downstream. Value of 0 indicates 
        that feature is disabled." 
    ::= { cLWlanConfigQosEntry 19 }

cLWlanWlanUSBurstDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "kbytes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies burst data rate per
        wlan on upstream. Value of 0 indicates that 
        feature is disabled." 
    ::= { cLWlanConfigQosEntry 20 }

cLWlanWlanDSAvgRealTimeDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "kbytes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies average real time data rate
        per wlan on downstream. Value of 0 indicates that 
        feature is disabled." 
    ::= { cLWlanConfigQosEntry 21 }

cLWlanWlanUSAvgRealTimeDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "kbytes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies average real time data rate
        per wlan on upstream. Value of 0 indicates that 
        feature is disabled." 
    ::= { cLWlanConfigQosEntry 22 }

cLWlanWlanDSBurstRealTimeDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "kbytes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies burst real time data rate
        per wlan on downstream. Value of 0 indicates that 
        feature is disabled." 
    ::= { cLWlanConfigQosEntry 23 }

cLWlanWlanUSBurstRealTimeDataRate OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "kbytes"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies burst real time data rate
        per wlan on upstream. Value of 0 indicates that 
        feature is disabled." 
    ::= { cLWlanConfigQosEntry 24 }
 

-- ********************************************************************
-- WLAN IOS Configuration
-- ********************************************************************

cLWlanConfigIosTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlanConfigIosEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the WLAN configuration for
        IOS profiles configured on the switch.

        The creation of a new row in cLWlanConfigTable,
        through an explicit network management action,
        results in creation of an entry in this table.
        Similarly, deletion of a row in
        cLWlanConfigTable through user action causes the
        deletion of corresponding row in this table.

        This table has an one-to-one relationship with
        cLWlanConfigTable. There exists an entry in this 
        table for each corresponding entry in the 
        cLWlanConfigTable."
    ::= { ciscoLwappWlanConfig 4 }

cLWlanConfigIosEntry OBJECT-TYPE
    SYNTAX          CLWlanConfigIosEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in this
        table and provides the information about the
        clients associated on the WLAN, uniquely identified by
        the cLWlanIndex."
    INDEX           { cLWlanIndex } 
    ::= { cLWlanConfigIosTable 1 }

CLWlanConfigIosEntry ::= SEQUENCE {
        cLWlanIosAccountingMethodListName           SnmpAdminString,
        cLWlanIosAuthenticationMethodListName       SnmpAdminString,
        cLWlanIosMacFilteringMethodListName         SnmpAdminString,
        cLWlanIosWebAuthMethodListName              SnmpAdminString,
        cLWlanIosQosUpStreamProfileName             SnmpAdminString,
        cLWlanIosQosDownStreamProfileName           SnmpAdminString,
        cLWlanIngressDHCPOption82Format             Unsigned32,
        cLWlanIngressDHCPOption82Ascii              TruthValue,
        cLWlanIngressDHCPOption82Rid                TruthValue,
        cLWlanIngressDHCPOption82Enable             TruthValue,
        cLWlanIosScanDeferPriority                  Unsigned32,
        cLWlanIosWebAuthParameterMapName            SnmpAdminString,
        cLWlanIosQosClientUpStreamProfileName       SnmpAdminString,
        cLWlanIosQosClientDownStreamProfileName     SnmpAdminString,
        cLWlanIosAuthorizationMethodListName        SnmpAdminString,
        cLWlanIosWebAuthAuthorizationMethodListName SnmpAdminString,
        cLWlanIosMacOverrideMethodListName          SnmpAdminString
}

cLWlanIosAccountingMethodListName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the method list name used for
        accounting on this WLAN." 
    ::= { cLWlanConfigIosEntry 1 }

cLWlanIosAuthenticationMethodListName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the method list name used for
        802.1x authentication on this WLAN. This could be 
        LDAP, RADIUS, LOCAL AUTH." 
    ::= { cLWlanConfigIosEntry 2 }

cLWlanIosMacFilteringMethodListName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the method list name used for
        mac filtering on this WLAN." 
    ::= { cLWlanConfigIosEntry 3 }

cLWlanIosWebAuthMethodListName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the method list name used for
        WEB AUTH on this WLAN." 
    ::= { cLWlanConfigIosEntry 4 }

cLWlanIosQosUpStreamProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the profile name used for
        upstream QOS configuration on this WLAN." 
    ::= { cLWlanConfigIosEntry 5 }

cLWlanIosQosDownStreamProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the profile name used for
        downstream QOS configuration on this WLAN." 
    ::= { cLWlanConfigIosEntry 6 }

cLWlanIngressDHCPOption82Format OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the DHCP
        Option82 format for this WLAN." 
    ::= { cLWlanConfigIosEntry 7 }

cLWlanIngressDHCPOption82Ascii OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the DHCP Option82 Ascii option
        for this WLAN." 
    ::= { cLWlanConfigIosEntry 8 }

cLWlanIngressDHCPOption82Rid OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the DHCP Option82 Rid option
        for this WLAN." 
    ::= { cLWlanConfigIosEntry 9 }

cLWlanIngressDHCPOption82Enable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the DHCP Option82 state
        for this WLAN." 
    ::= { cLWlanConfigIosEntry 10 }

cLWlanIosScanDeferPriority OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies the priority of packets
        that defer the off-channel scan. This is used in 
        off-channel scanning to improve performance
        for medical devices using Radio Resource Management.
        Each bit represents a packet type for which off-channel
        scanning needs to be deferred." 
    ::= { cLWlanConfigIosEntry 11 }

cLWlanIosWebAuthParameterMapName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the web auth parameter name
        on this WLAN." 
    ::= { cLWlanConfigIosEntry 12 }

cLWlanIosQosClientUpStreamProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the profile name used for
        upstream QOS client configuration on this WLAN." 
    ::= { cLWlanConfigIosEntry 13 }

cLWlanIosQosClientDownStreamProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the profile name used for
        downstream QOS client configuration on this WLAN." 
    ::= { cLWlanConfigIosEntry 14 }

cLWlanIosAuthorizationMethodListName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the method list name used for
        802.1x authorization on this WLAN. This could be 
        LDAP, RADIUS, LOCAL AUTH." 
    ::= { cLWlanConfigIosEntry 15 }

cLWlanIosWebAuthAuthorizationMethodListName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the method list name used for
        webauth authorization on this WLAN. This could be 
        LDAP, RADIUS, LOCAL AUTH." 
    ::= { cLWlanConfigIosEntry 16 }

cLWlanIosMacOverrideMethodListName OBJECT-TYPE
    SYNTAX          SnmpAdminString (SIZE  (0..64))
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object represents the method list name used for
        mab authorization on this WLAN. This could be 
        LDAP, RADIUS, LOCAL AUTH." 
    ::= { cLWlanConfigIosEntry 17 }
 

-- ********************************************************************
-- *        WLAN Flexible Netflow Table
-- ********************************************************************

cLWlanFlexibleNetflowTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlanFlexibleNetflowEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the flexible netflow policy details
        per WLAN for AVC.
        The creation of a new row in cLWlanFlexibleConfigTable,
        through an explicit network management action,
        results in creation of an entry in this table.
        Similarly, deletion of a row in
        cLWlanConfigTable through user action causes the
        deletion of corresponding rows in this table.
        For each wlan, there will be zero to many instances of 
        flexible netflow policies."
    ::= { ciscoLwappWlanConfig 5 }

cLWlanFlexibleNetflowEntry OBJECT-TYPE
    SYNTAX          CLWlanFlexibleNetflowEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in this
        table and provides the information about the flexible
        netflow policy types associated on the WLAN, uniquely 
        identified by the cLWlanIndex and 
        cLWlanFlexibleNetflowPolicyTypeIndex."
    INDEX           {
                        cLWlanIndex,
                        cLWlanFlexibleNetflowPolicyTypeIndex
                    } 
    ::= { cLWlanFlexibleNetflowTable 1 }

CLWlanFlexibleNetflowEntry ::= SEQUENCE {
        cLWlanFlexibleNetflowPolicyTypeIndex INTEGER,
        cLWlanFlexibleNetflowMonitorName     SnmpAdminString,
        cLWlanFlexibleNetflowRowStatus       RowStatus
}

cLWlanFlexibleNetflowPolicyTypeIndex OBJECT-TYPE
    SYNTAX          INTEGER  {
                        none(0),
                        ipv4InputPolicy(1),
                        ipv4OutputPolicy(2),
                        ipv6InputPolicy(3),
                        ipv6OutputPolicy(4),
                        datalinkInputPolicy(5),
                        datalinkOutputPolicy(6)
                    }
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object is used to set the netflow traffic direction
        for AVC.
        none(0)  capture no traffic
        IPV4 Input Policy(1) - IPV4 input policy
        IPV4OutputPolicy(2) - IPV4 output policy
        IPV6InputPolicy(3) - IPV6 input policy
        IPV6OutputPolicy(4) - IPV6 output policy
        DatalinkInputPolicy(5) - Datalink input policy
        DatalinkOutputPolicy(6) - Datalink output policy." 
    ::= { cLWlanFlexibleNetflowEntry 1 }

cLWlanFlexibleNetflowMonitorName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object represents the flexible netflow
        monitor name assigned to this WLAN." 
    ::= { cLWlanFlexibleNetflowEntry 2 }

cLWlanFlexibleNetflowRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Row Status for creation/deletion of a particular
        flexible netflow policy
        entry from the table" 
    ::= { cLWlanFlexibleNetflowEntry 3 }
 


cLPolicyConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLPolicyConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table for the native Profiling Policies
        on the Wireless LAN controller.
        Rows are added or deleted by explicit 
        management actions initiated by the user from a
        network management station through the 
        cLPolicyRowStatus object."
    ::= { ciscoLwappPolicyConfig 1 }

cLPolicyConfigEntry OBJECT-TYPE
    SYNTAX          CLPolicyConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLPolicyConfigTable."
    INDEX           { cLPolicyIndex } 
    ::= { cLPolicyConfigTable 1 }

CLPolicyConfigEntry ::= SEQUENCE {
        cLPolicyIndex              Unsigned32,
        cLPolicyName               SnmpAdminString,
        cLPolicyRoleName           SnmpAdminString,
        cLPolicyEapType            INTEGER,
        cLPolicyAclName            SnmpAdminString,
        cLPolicyVlanId             Unsigned32,
        cLPolicyQosProfile         INTEGER,
        cLPolicySessionTimeout     Unsigned32,
        cLPolicySleepTimeout       Unsigned32,
        cLPolicyRowStatus          RowStatus,
        cLPolicyFlexAclName        SnmpAdminString,
        cLPolicyAvcProfileName     SnmpAdminString,
        cLPolicyMdnsProfileName    SnmpAdminString,
        cLPolicyFlexVlanId         Unsigned32,
        cLPolicyUrlAclName         SnmpAdminString,
        cLPolicyOpendnsProfileName SnmpAdminString
}

cLPolicyIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the Index of the
        native profiling classification policy
        configured on the Wireless LAN Controller." 
    ::= { cLPolicyConfigEntry 1 }

cLPolicyName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies a
        native profiling classification policy
        configured on the Wireless LAN Controller." 
    ::= { cLPolicyConfigEntry 2 }

cLPolicyRoleName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the category of users
        to which a Policy is to be applied." 
    ::= { cLPolicyConfigEntry 3 }

cLPolicyEapType OBJECT-TYPE
    SYNTAX          INTEGER  {
                        none(1),
                        leap(2),
                        eapFast(3),
                        eapTls(4),
                        peap(5)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies  the EAP type to be
        applied on client." 
    ::= { cLPolicyConfigEntry 4 }

cLPolicyAclName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the ACL  to be
        applied on client." 
    ::= { cLPolicyConfigEntry 5 }

cLPolicyVlanId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the VLAN  to be
        applied on client." 
    ::= { cLPolicyConfigEntry 6 }

cLPolicyQosProfile OBJECT-TYPE
    SYNTAX          INTEGER  {
                        none(1),
                        silver(2),
                        gold(3),
                        platinum(4),
                        bronze(5)
                    }
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the QoS  to be
        applied on client." 
    ::= { cLPolicyConfigEntry 7 }

cLPolicySessionTimeout OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the session timeout
        to be applied on client." 
    ::= { cLPolicyConfigEntry 8 }

cLPolicySleepTimeout OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the sleep timeout
        to be applied on client." 
    ::= { cLPolicyConfigEntry 9 }

cLPolicyRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Row Status for
        creation/deletion of a particular
        policy entry in the table." 
    ::= { cLPolicyConfigEntry 10 }

cLPolicyFlexAclName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the FlexConnect ACL
        to be applied on client using a Policy.
        This will be effective only on locally 
        switched WLANs." 
    ::= { cLPolicyConfigEntry 11 }

cLPolicyAvcProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the avc profilename  to be
        applied on client." 
    ::= { cLPolicyConfigEntry 12 }

cLPolicyMdnsProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the MDNS profile name  to be
        applied on client." 
    ::= { cLPolicyConfigEntry 13 }

cLPolicyFlexVlanId OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the flex VLAN  to be
        applied on client ." 
    ::= { cLPolicyConfigEntry 14 }

cLPolicyUrlAclName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the URL ACL  to be
        applied on client ." 
    ::= { cLPolicyConfigEntry 15 }

cLPolicyOpendnsProfileName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the opendns profile name  to be
        applied on client ." 
    ::= { cLPolicyConfigEntry 16 }
 


cLPolicyDeviceTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLPolicyDeviceEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table for the device types to be
        added in each native Profiling Policy
        on the controller.
        Rows are added or deleted by explicit 
        management actions initiated by the user from a
        network management station through the 
        cLPolicyDeviceRowStatus object."
    ::= { ciscoLwappPolicyConfig 2 }

cLPolicyDeviceEntry OBJECT-TYPE
    SYNTAX          CLPolicyDeviceEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLPolicyConfigTable."
    INDEX           {
                        cLPolicyIndex,
                        cLPolicyDeviceIndex
                    } 
    ::= { cLPolicyDeviceTable 1 }

CLPolicyDeviceEntry ::= SEQUENCE {
        cLPolicyDeviceIndex     Unsigned32,
        cLPolicyDeviceName      SnmpAdminString,
        cLPolicyDeviceRowStatus RowStatus
}

cLPolicyDeviceIndex OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object indicates the index of the device
        type configured on the policy." 
    ::= { cLPolicyDeviceEntry 1 }

cLPolicyDeviceName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies name of the device
        configured on the policy." 
    ::= { cLPolicyDeviceEntry 2 }

cLPolicyDeviceRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Row Status for
        creation/deletion of a particular
        device entry in the table." 
    ::= { cLPolicyDeviceEntry 3 }
 


cLPolicyActiveHoursTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLPolicyActiveHoursEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "A table for the active hours to be
        added in each native Profiling Policy
        on the controller.
        Rows are added or deleted by explicit 
        management actions initiated by the user from a
        network management station through the 
        cLPolicyActiveHoursRowStatus object."
    ::= { ciscoLwappPolicyConfig 3 }

cLPolicyActiveHoursEntry OBJECT-TYPE
    SYNTAX          CLPolicyActiveHoursEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in cLPolicyActiveHoursTable."
    INDEX           {
                        cLPolicyIndex,
                        cLPolicyActiveDay
                    } 
    ::= { cLPolicyActiveHoursTable 1 }

CLPolicyActiveHoursEntry ::= SEQUENCE {
        cLPolicyActiveDay            INTEGER,
        cLPolicyActiveStartTime      TimeTicks,
        cLPolicyActiveEndTime        TimeTicks,
        cLPolicyActiveHoursRowStatus RowStatus
}

cLPolicyActiveDay OBJECT-TYPE
    SYNTAX          INTEGER  {
                        mon(1),
                        tue(2),
                        wed(3),
                        thu(4),
                        fri(5),
                        sat(6),
                        sun(7)
                    }
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the Index of the day
        for which active hours is configured on the policy." 
    ::= { cLPolicyActiveHoursEntry 1 }

cLPolicyActiveStartTime OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies a start of active hours
        for a day added to a Policy." 
    ::= { cLPolicyActiveHoursEntry 2 }

cLPolicyActiveEndTime OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies a end of active hours
        for a day added to a Policy." 
    ::= { cLPolicyActiveHoursEntry 3 }

cLPolicyActiveHoursRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies the Row Status for
        creation/deletion of a particular
         entry in the table." 
    ::= { cLPolicyActiveHoursEntry 4 }
 

-- ********************************************************************
-- *   WLAN 11ax Config Table
-- ********************************************************************

cLWlan11axConfigTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLWlan11axConfigEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the WLAN configuration for
        the 802.11ax APs that have joined this controller.

        The creation of a new row in cLWlanConfigTable,
        through an explicit network management action,
        results in creation of an entry in this table.
        Similarly, deletion of a row in
        cLWlanConfigTable through user action causes the
        deletion of corresponding row in this table.

        This table has an one-to-one relationship with
        cLWlanConfigTable. There exists an entry in this
        table for each corresponding entry in the
        cLWlanConfigTable."
    ::= { ciscoLwappWlanConfig 9 }

cLWlan11axConfigEntry OBJECT-TYPE
    SYNTAX          CLWlan11axConfigEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry represents a conceptual row in this
        table and provides the information about the
        clients associated on the WLAN, uniquely identified by
        the cLWlanIndex."
    INDEX           { cLWlanIndex } 
    ::= { cLWlan11axConfigTable 1 }

CLWlan11axConfigEntry ::= SEQUENCE {
        cLWlan11axMuMimoUplinkEnable    TruthValue,
        cLWlan11axMuMimoDownlinkEnable  TruthValue,
        cLWlan11axOfdmaUplinkEnable     TruthValue,
        cLWlan11axOfdmaDownlinkEnable   TruthValue,
        cLWlan11axTargetWaketimeEnable  TruthValue,
        cLWlan11axBssColorModeEnable    TruthValue,
        cLWlan11axBssColorCode          Unsigned32,
        cLWlan11axBssPartialColorEnable TruthValue
}

cLWlan11axMuMimoUplinkEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether 11ax Multi User Multiple Input
        Multiple output Uplink is enabled or disabled for the WLAN.
        MIMO is an antenna technology for wireless communications in 
        which multiple antennas are used at both the source 
        (transmitter) and the destination (receiver).The 802.11ax 
        Multi-user MIMO allow more users to claim MIMO simultaneously.

        A value of 'true' indicates that 11ax MU MIMO uplink is enabled
        on WLAN.
        A value of 'false' indicates that 11ax MU MIMO uplink is 
        disabled on the WLAN."
    DEFVAL          { false } 
    ::= { cLWlan11axConfigEntry 1 }

cLWlan11axMuMimoDownlinkEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether 11ax Multi User Multiple Input
        Multiple Output Downlink is enabled or disabled for the WLAN.
        MIMO is an antenna technology for wireless communications in 
        which multiple antennas are used at both the source
        (transmitter) and the destination (receiver).The 802.11ax
        Multi-user MIMO allow more users to claim MIMO simultaneously.

        A value of 'true' indicates that 11ax MU MIMO Downlink is 
        enabled on the WLAN.
        A value of 'false' indicates that 11ax MU MIMO Downlink is 
        disabled on the WLAN"
    DEFVAL          { false } 
    ::= { cLWlan11axConfigEntry 2 }

cLWlan11axOfdmaUplinkEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether 11ax Orthogonal Frequency
        Division Multiple Access uplink is enabled or disabled for the
        WLAN.OFDMA allows multiple users to transmit simultaneously
        and share the available bandwidth of a channel where each user
        is allotted a portion of the available spectrum.This allows the
        access point to satisfy the data rate requirements of each 
        individual user.
        A value of 'true' indicates that 11ax OFDMA Uplink is enabled
        on the WLAN.
        A value of 'false' indicates that 11ax OFDMA Uplink is 
        disabled on the WLAN."
    DEFVAL          { false } 
    ::= { cLWlan11axConfigEntry 3 }

cLWlan11axOfdmaDownlinkEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether 11ax Orthogonal Frequency
        Division Multiple Access downlink is enabled or disabled for 
        the WLAN. OFDMA allows multiple users to transmit 
        simultaneously and share the available bandwidth of a channel
        where each user is allotted a portion of the available 
        spectrum.This allows the access point to satisfy the data rate
        requirements of each individual user.

        A value of 'true' indicates that 11ax OFDMA Downlink is 
        enabled on the WLAN.
        A value of 'false' indicates that 11ax OFDMA Downlink is 
        disabled on the WLAN."
    DEFVAL          { false } 
    ::= { cLWlan11axConfigEntry 4 }

cLWlan11axTargetWaketimeEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether 11ax TargetWaketime is enabled
        or disabled for the WLAN.
        Target Wake Time (TWT) is a function that permits an AP to 
        define a specific time or set of times for individual stations
        (associated to this wlan) to access the medium.

        A value of 'true' indicates that 11ax TargetWaketime is 
        enabled on the WLAN.
        A value of 'false' indicates that 11ax TargetWaketime is 
        disabled on the WLAN."
    DEFVAL          { false } 
    ::= { cLWlan11axConfigEntry 5 }

cLWlan11axBssColorModeEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether 11ax Basic service set color
        mode is enabled or disabled for the WLAN.
        BSS Coloring is a method of reducing medium contention overhead
        due to overlapping basic service set (OBSS) and spatial reuse.
        802.11ax pre-amble assigns a BSS color value(0-255)to each AP 
        so that stations can differentiate between BSSs and new channel 
        access behavior will be assigned based on the color detected.
        Thereby decreasing interference.

        A value of 'true' indicates that 11ax Bss color mode is enabled
        on the WLAN.
        A value of 'false' indicates tha 11ax Bss color mode is 
        disabled on the WLAN."
    DEFVAL          { false } 
    ::= { cLWlan11axConfigEntry 6 }

cLWlan11axBssColorCode OBJECT-TYPE
    SYNTAX          Unsigned32 (0..255)
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies 11ax Basic service set color code value
        (0-255) of the WLAN.
        BSS Coloring is a method of reducing medium contention overhead 
        due to overlapping basic service set (OBSS) and spatial reuse.
        802.11ax pre-amble assigns a BSS color value(0-255)to each AP 
        so that stations can differentiate between BSSs and new channel
        access behavior will be assigned based on the color detected.
        Thereby decreasing interference." 
    ::= { cLWlan11axConfigEntry 7 }

cLWlan11axBssPartialColorEnable OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies whether 11ax Basic service set Partial
        color mode is enabled or disabled for the WLAN.
        BSS Partial Colorig is method of BSS coloring in which a
        receiving station identifies the BSS from the AP so that the
        station can use the channel access rules or reduce power 
        consumption.
        A value of 'true' indicates 11ax Bss Partial color mode is
        enabled on the WLAN.
        A value of 'false' indicates 11ax Bss Partial color mode is
        disabled on the WLAN."
    DEFVAL          { false } 
    ::= { cLWlan11axConfigEntry 8 }
 

-- ***********************************************
-- Wlan Scheduling Table
-- ***********************************************

cLPolicyWlanSchedulingTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CLPolicyWlanSchedulingEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table represents the WLAN scheduling on
        the controller.
        Rows are added or deleted by explicit 
        management actions initiated by the user from a
        network management station through the 
        cLPolicyWlanSchedulingRowStatus object."
    ::= { ciscoLwappPolicyConfig 4 }

cLPolicyWlanSchedulingEntry OBJECT-TYPE
    SYNTAX          CLPolicyWlanSchedulingEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "Each entry in this table represents the
        configuration attributes of 
        cLPolicyWlanSchedulingTable."
    INDEX           {
                        cLPolicyIndex,
                        cLPolicyWlanSchedulingDay
                    } 
    ::= { cLPolicyWlanSchedulingTable 1 }

CLPolicyWlanSchedulingEntry ::= SEQUENCE {
        cLPolicyWlanSchedulingDay       INTEGER,
        cLPolicyWlanSchedulingStatus    TruthValue,
        cLPolicyWlanSchedulingStartTime TimeTicks,
        cLPolicyWlanSchedulingEndTime   TimeTicks,
        cLPolicyWlanSchedulingRowStatus RowStatus
}

cLPolicyWlanSchedulingDay OBJECT-TYPE
    SYNTAX          INTEGER  {
                        mon(1),
                        tue(2),
                        wed(3),
                        thu(4),
                        fri(5),
                        sat(6),
                        sun(7)
                    }
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This object specifies the day for which WLAN
        scheduling is configured on the policy." 
    ::= { cLPolicyWlanSchedulingEntry 1 }

cLPolicyWlanSchedulingStatus OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies scheduling status per WLAN.
        A value of 'true' indicates that scheduling status is
        enabled on a WLAN.
        A value of 'false' indicates that scheduling status is
        disabled on a WLAN." 
    ::= { cLPolicyWlanSchedulingEntry 2 }

cLPolicyWlanSchedulingStartTime OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies a start of WLAN scheduling
        hours for a day added to a Policy." 
    ::= { cLPolicyWlanSchedulingEntry 3 }

cLPolicyWlanSchedulingEndTime OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This object specifies a end of WLAN scheduling hours
        for a day added to a Policy." 
    ::= { cLPolicyWlanSchedulingEntry 4 }

cLPolicyWlanSchedulingRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "This is the status column for this row and is
        used to create and delete specific instances 
        of rows in this table." 
    ::= { cLPolicyWlanSchedulingEntry 5 }
 

-- ********************************************************************
-- *    Compliance statements
-- ********************************************************************

ciscoLwappWlanMIBCompliances  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIBConform 1 }

ciscoLwappWlanMIBGroups  OBJECT IDENTIFIER
    ::= { ciscoLwappWlanMIBConform 2 }


ciscoLwappWlanMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS { ciscoLwappWlanConfigGroup }

    OBJECT          cLWlanRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."
    ::= { ciscoLwappWlanMIBCompliances 1 }

ciscoLwappWlanMIBComplianceRev1 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappWlanConfigGroupSup1,
                        ciscoLwappWlanConfigClientGroup
                    }

    OBJECT          cLWlanRowStatus
    SYNTAX          INTEGER  {
                        active(1),
                        createAndGo(4),
                        destroy(6)
                    }
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."
    ::= { ciscoLwappWlanMIBCompliances 2 }

ciscoLwappWlanMIBComplianceRev2 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappWlanConfigGroupSup1,
                        ciscoLwappWlanConfigClientGroup,
                        ciscoLwappWlan11uConfigGroup,
                        ciscoLwappAPGroupsVlanConfigGroup,
                        ciscoLwappWlanConfigGroupSup2,
                        ciscoLwappWlanConfigClientGroupSup1
                    }

    OBJECT          cLAPGroupsVlanConfigRowStatus
    SYNTAX          RowStatus
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."

    OBJECT          cLWlan11uOuiRowStatus
    SYNTAX          RowStatus
    DESCRIPTION
        "An implementation is only required to support
        three of the six enumerated values of the
        RowStatus textual convention, specifically,
        'active', 'createAndGo' and 'destroy'."
    ::= { ciscoLwappWlanMIBCompliances 3 }

ciscoLwappWlanMIBComplianceRev3 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappWlanConfigGroupSup1,
                        ciscoLwappWlanConfigClientGroup,
                        ciscoLwappWlan11uConfigGroup,
                        ciscoLwappAPGroupsVlanConfigGroup,
                        ciscoLwappWlanConfigGroupSup2,
                        ciscoLwappWlanConfigClientGroupSup1,
                        ciscoLwappWlanConfigGroupSup3
                    }
    ::= { ciscoLwappWlanMIBCompliances 4 }

ciscoLwappWlanMIBComplianceRev4 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappWlanConfigGroupSup1,
                        ciscoLwappWlanConfigClientGroup,
                        ciscoLwappAPGroupsVlanConfigGroup,
                        ciscoLwappWlanConfigGroupSup2,
                        ciscoLwappWlanConfigClientGroupSup1,
                        ciscoLwappWlanConfigGroupSup3,
                        ciscoLwappWlan11uConfigGroupsup1,
                        ciscoLwappWlanServiceAdvertisementConfigGroup,
                        ciscoLwappWlanHotSpot2ConfigGroup,
                        ciscoLwappWlanIosConfigGroup,
                        ciscoLwappWlanQosConfigGroup,
                        ciscoLwappWlan11uConfigGroupsup2,
                        ciscoLwappWlanConfigGroupSup4,
                        ciscoLwappWlanHotSpot2ConfigGroupSup1,
                        ciscoLwappAPGroupsVlanConfigGroupSup1,
                        cLAPGroupsVenueConfigGroup,
                        cLAPGroupsMultipleVenueGroup,
                        ciscoLwappWlanConfigClientGroupSup2
                    }
    ::= { ciscoLwappWlanMIBCompliances 5 }

ciscoLwappWlanMIBComplianceRev5 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappWlanConfigGroupSup1,
                        ciscoLwappWlanConfigClientGroup,
                        ciscoLwappAPGroupsVlanConfigGroup,
                        ciscoLwappWlanConfigGroupSup2,
                        ciscoLwappWlanConfigClientGroupSup1,
                        ciscoLwappWlanConfigGroupSup3,
                        ciscoLwappWlan11uConfigGroupsup1,
                        ciscoLwappWlanServiceAdvertisementConfigGroup,
                        ciscoLwappWlanHotSpot2ConfigGroup,
                        ciscoLwappWlanIosConfigGroup,
                        ciscoLwappWlanQosConfigGroup,
                        ciscoLwappWlan11uConfigGroupsup2,
                        ciscoLwappWlanConfigGroupSup4,
                        ciscoLwappWlanHotSpot2ConfigGroupSup1,
                        ciscoLwappAPGroupsVlanConfigGroupSup1,
                        cLAPGroupsVenueConfigGroup,
                        cLAPGroupsMultipleVenueGroup,
                        ciscoLwappWlanConfigClientGroupSup2,
                        ciscoLwappWlanConfigFlexibleNetflowGroup
                    }
    ::= { ciscoLwappWlanMIBCompliances 6 }

ciscoLwappWlanMIBComplianceRev6 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappWlanConfigGroupSup1,
                        ciscoLwappWlanConfigClientGroup,
                        ciscoLwappWlanConfigGroupSup2,
                        ciscoLwappWlanConfigClientGroupSup1,
                        ciscoLwappWlanConfigGroupSup3,
                        ciscoLwappWlan11uConfigGroupsup1,
                        ciscoLwappWlanServiceAdvertisementConfigGroup,
                        ciscoLwappWlanHotSpot2ConfigGroup,
                        ciscoLwappWlanIosConfigGroup,
                        ciscoLwappWlanQosConfigGroup,
                        ciscoLwappWlan11uConfigGroupsup2,
                        ciscoLwappWlanConfigGroupSup4,
                        ciscoLwappWlanHotSpot2ConfigGroupSup1,
                        ciscoLwappAPGroupsVlanConfigGroupSup1,
                        cLAPGroupsVenueConfigGroup,
                        cLAPGroupsMultipleVenueGroup,
                        ciscoLwappWlanConfigClientGroupSup2,
                        ciscoLwappWlanConfigFlexibleNetflowGroup,
                        ciscoLwappAPGroupsVlanConfigGroupSup2
                    }
    ::= { ciscoLwappWlanMIBCompliances 7 }

ciscoLwappWlanMIBComplianceRev7 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappWlanConfigGroupSup1,
                        ciscoLwappWlanConfigClientGroup,
                        ciscoLwappWlanConfigGroupSup2,
                        ciscoLwappWlanConfigClientGroupSup1,
                        ciscoLwappWlanConfigGroupSup3,
                        ciscoLwappWlan11uConfigGroupsup1,
                        ciscoLwappWlanServiceAdvertisementConfigGroup,
                        ciscoLwappWlanHotSpot2ConfigGroup,
                        ciscoLwappWlanIosConfigGroup,
                        ciscoLwappWlanQosConfigGroup,
                        ciscoLwappWlan11uConfigGroupsup2,
                        ciscoLwappWlanConfigGroupSup4,
                        ciscoLwappWlanHotSpot2ConfigGroupSup1,
                        ciscoLwappAPGroupsVlanConfigGroupSup1,
                        cLAPGroupsVenueConfigGroup,
                        cLAPGroupsMultipleVenueGroup,
                        ciscoLwappWlanConfigClientGroupSup2,
                        ciscoLwappWlanConfigFlexibleNetflowGroup,
                        ciscoLwappAPGroupsVlanConfigGroupSup2,
                        ciscoLwappWlanConfigGroupSup6
                    }
    ::= { ciscoLwappWlanMIBCompliances 8 }

ciscoLwappWlanMIBComplianceRev8 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappWlanConfigGroupSup1,
                        ciscoLwappWlanConfigClientGroup,
                        ciscoLwappWlanConfigGroupSup2,
                        ciscoLwappWlanConfigClientGroupSup1,
                        ciscoLwappWlanConfigGroupSup3,
                        ciscoLwappWlan11uConfigGroupsup1,
                        ciscoLwappWlanServiceAdvertisementConfigGroup,
                        ciscoLwappWlanHotSpot2ConfigGroup,
                        ciscoLwappWlanIosConfigGroup,
                        ciscoLwappWlanQosConfigGroup,
                        ciscoLwappWlan11uConfigGroupsup2,
                        ciscoLwappWlanConfigGroupSup4,
                        ciscoLwappWlanHotSpot2ConfigGroupSup1,
                        ciscoLwappAPGroupsVlanConfigGroupSup1,
                        cLAPGroupsVenueConfigGroup,
                        cLAPGroupsMultipleVenueGroup,
                        ciscoLwappWlanConfigClientGroupSup2,
                        ciscoLwappWlanConfigFlexibleNetflowGroup,
                        ciscoLwappAPGroupsVlanConfigGroupSup2,
                        ciscoLwappWlanConfigGroupSup6,
                        ciscoLwappWlanConfigGroupSup7,
                        ciscoLwappWlanConfigGroupSup8
                    }
    ::= { ciscoLwappWlanMIBCompliances 9 }

ciscoLwappWlanMIBComplianceRev9 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappWlanConfigGroupSup1,
                        ciscoLwappWlanConfigClientGroup,
                        ciscoLwappWlanConfigGroupSup2,
                        ciscoLwappWlanConfigClientGroupSup1,
                        ciscoLwappWlanConfigGroupSup3,
                        ciscoLwappWlan11uConfigGroupsup1,
                        ciscoLwappWlanServiceAdvertisementConfigGroup,
                        ciscoLwappWlanHotSpot2ConfigGroup,
                        ciscoLwappWlanIosConfigGroup,
                        ciscoLwappWlanQosConfigGroup,
                        ciscoLwappWlan11uConfigGroupsup2,
                        ciscoLwappWlanHotSpot2ConfigGroupSup1,
                        ciscoLwappAPGroupsVlanConfigGroupSup1,
                        cLAPGroupsVenueConfigGroup,
                        cLAPGroupsMultipleVenueGroup,
                        ciscoLwappWlanConfigClientGroupSup2,
                        ciscoLwappWlanConfigFlexibleNetflowGroup,
                        ciscoLwappWlanConfigGroupSup5,
                        ciscoLwappAPGroupsVlanConfigGroupSup2,
                        ciscoLwappWlanConfigGroupSup6,
                        ciscoLwappWlanConfigGroupSup7,
                        ciscoLwappWlanConfigGroupSup8,
                        ciscoLwappWlan11vConfigGroup
                    }
    ::= { ciscoLwappWlanMIBCompliances 10 }

ciscoLwappWlanMIBComplianceRev10 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappWlanConfigGroupSup1,
                        ciscoLwappWlanConfigClientGroup,
                        ciscoLwappWlanConfigGroupSup2,
                        ciscoLwappWlanConfigClientGroupSup1,
                        ciscoLwappWlanConfigGroupSup3,
                        ciscoLwappWlan11uConfigGroupsup1,
                        ciscoLwappWlanServiceAdvertisementConfigGroup,
                        ciscoLwappWlanHotSpot2ConfigGroup,
                        ciscoLwappWlanIosConfigGroup,
                        ciscoLwappWlanQosConfigGroup,
                        ciscoLwappWlan11uConfigGroupsup2,
                        ciscoLwappWlanHotSpot2ConfigGroupSup1,
                        ciscoLwappAPGroupsVlanConfigGroupSup1,
                        cLAPGroupsVenueConfigGroup,
                        cLAPGroupsMultipleVenueGroup,
                        ciscoLwappWlanConfigClientGroupSup2,
                        ciscoLwappWlanConfigFlexibleNetflowGroup,
                        ciscoLwappWlanConfigGroupSup5,
                        ciscoLwappAPGroupsVlanConfigGroupSup2,
                        ciscoLwappWlanConfigGroupSup6,
                        ciscoLwappWlanConfigGroupSup7,
                        ciscoLwappWlanConfigGroupSup8,
                        ciscoLwappWlan11vConfigGroup,
                        ciscoLwappApGroupConfigGroup,
                        ciscoLwappPolicyConfigGroup
                    }
    ::= { ciscoLwappWlanMIBCompliances 11 }

ciscoLwappWlanMIBComplianceRev11 MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappWlanConfigGroupSup1,
                        ciscoLwappWlanConfigClientGroup,
                        ciscoLwappWlanConfigGroupSup2,
                        ciscoLwappWlanConfigClientGroupSup1,
                        ciscoLwappWlanConfigGroupSup3,
                        ciscoLwappWlan11uConfigGroupsup1,
                        ciscoLwappWlanServiceAdvertisementConfigGroup,
                        ciscoLwappWlanHotSpot2ConfigGroup,
                        ciscoLwappWlanIosConfigGroup,
                        ciscoLwappWlanQosConfigGroup,
                        ciscoLwappWlan11uConfigGroupsup2,
                        ciscoLwappWlanHotSpot2ConfigGroupSup1,
                        ciscoLwappAPGroupsVlanConfigGroupSup1,
                        cLAPGroupsVenueConfigGroup,
                        cLAPGroupsMultipleVenueGroup,
                        ciscoLwappWlanConfigClientGroupSup2,
                        ciscoLwappWlanConfigFlexibleNetflowGroup,
                        ciscoLwappWlanConfigGroupSup5,
                        ciscoLwappAPGroupsVlanConfigGroupSup2,
                        ciscoLwappWlanConfigGroupSup6,
                        ciscoLwappWlanConfigGroupSup7,
                        ciscoLwappWlanConfigGroupSup8,
                        ciscoLwappWlan11vConfigGroup,
                        ciscoLwappApGroupConfigGroup,
                        ciscoLwappPolicyConfigGroup,
                        ciscoLwappWlan11kConfigGroup
                    }
    ::= { ciscoLwappWlanMIBCompliances 12 }

ciscoLwappWlanMIBComplianceRev12 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for the SNMP entities that
        implement the ciscoLwappWlanMIB module."
    MODULE          -- this module
    MANDATORY-GROUPS {
                        ciscoLwappWlanConfigGroupSup1,
                        ciscoLwappWlanConfigClientGroup,
                        ciscoLwappWlanConfigGroupSup2,
                        ciscoLwappWlanConfigClientGroupSup1,
                        ciscoLwappWlanConfigGroupSup3,
                        ciscoLwappWlan11uConfigGroupsup1,
                        ciscoLwappWlanServiceAdvertisementConfigGroup,
                        ciscoLwappWlanHotSpot2ConfigGroup,
                        ciscoLwappWlanIosConfigGroup,
                        ciscoLwappWlanQosConfigGroup,
                        ciscoLwappWlan11uConfigGroupsup2,
                        ciscoLwappWlanHotSpot2ConfigGroupSup1,
                        ciscoLwappAPGroupsVlanConfigGroupSup1,
                        cLAPGroupsVenueConfigGroup,
                        cLAPGroupsMultipleVenueGroup,
                        ciscoLwappWlanConfigClientGroupSup2,
                        ciscoLwappWlanConfigFlexibleNetflowGroup,
                        ciscoLwappWlanConfigGroupSup5,
                        ciscoLwappAPGroupsVlanConfigGroupSup2,
                        ciscoLwappWlanConfigGroupSup6,
                        ciscoLwappWlanConfigGroupSup7,
                        ciscoLwappWlanConfigGroupSup8,
                        ciscoLwappWlan11vConfigGroup,
                        ciscoLwappApGroupConfigGroup,
                        ciscoLwappPolicyConfigGroup,
                        ciscoLwappWlan11kConfigGroup,
                        ciscoLwappWlan11axConfigGroup
                    }
    ::= { ciscoLwappWlanMIBCompliances 13 }

-- ********************************************************************
-- *    Units of conformance
-- ********************************************************************

ciscoLwappWlanConfigGroup OBJECT-GROUP
    OBJECTS         { cLWlanRowStatus }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects represent the
        configuration of WLANs on the controller to be passed
        to an LWAPP AP.
        ciscoLwappWlanConfigGroup object is superseded by
        ciscoLwappWlanConfigGroupSup1."
    ::= { ciscoLwappWlanMIBGroups 1 }

ciscoLwappWlanConfigGroupSup1 OBJECT-GROUP
    OBJECTS         {
                        cLWlanRowStatus,
                        cLWlanProfileName,
                        cLWlanSsid,
                        cLWlanDiagChan,
                        cLWlanStorageType
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of WLANs on the controller to be passed
        to an LWAPP AP."
    ::= { ciscoLwappWlanMIBGroups 2 }

ciscoLwappWlanConfigClientGroup OBJECT-GROUP
    OBJECTS         { cLWlanClientAclName }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of WLANs on the controller to be passed
        to an 8021.11 clients."
    ::= { ciscoLwappWlanMIBGroups 3 }

ciscoLwappWlan11uConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLWlan11uStatus,
                        cLWlan11uInternetAccess,
                        cLWlan11uNetworkType,
                        cLWlan11uVenueGroup,
                        cLWlan11uVenueType,
                        cLWlan11uVenueName,
                        cLWlan11uOui,
                        cLWlan11uOuiIsBeacon,
                        cLWlan11uOuiRowStatus,
                        cLWlan11uOuiStorageType
                    }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects represents 802.11u
        related configuration of WLANs on the controller
        to be passed to an AP.
        ciscoLwappWlan11uConfigGroup object is superseded 
        by ciscoLwappWlan11uConfigGroupsup1."
    ::= { ciscoLwappWlanMIBGroups 4 }

ciscoLwappAPGroupsVlanConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLAPGroupsVlanMappingInterfaceName,
                        cLAPGroupNACSupport,
                        cLAPGroupsVlanConfigRowStatus,
                        cLAPGroupsVlanConfigStorageType
                    }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects represent the
        configuration of AP Groups Vlan on the controller
        to be passed to an AP.
        ciscoLwappAPGroupsVlanConfigGroup object is superseded by 
        ciscoLwappAPGroupsVlanConfigGroupSup2."
    ::= { ciscoLwappWlanMIBGroups 5 }

ciscoLwappWlanConfigGroupSup2 OBJECT-GROUP
    OBJECTS         {
                        cLWlanLoadBalancingEnable,
                        cLWlanBandSelectEnable,
                        cLWlanPassiveClientEnable,
                        cLWlanIsWired,
                        cLWlanIngressInterface,
                        cLWlanNACSupport,
                        cLWlanWepKeyChange,
                        cLWlanChdEnable,
                        cLWlan802dot11anDTIM,
                        cLWlan802dot11bgnDTIM
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of WLANs on the controller to be passed
        to an LWAPP AP."
    ::= { ciscoLwappWlanMIBGroups 6 }

ciscoLwappWlanConfigClientGroupSup1 OBJECT-GROUP
    OBJECTS         { cLWlanP2PBlocking }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of WLANs on the controller to be passed
        to an 8021.11 clients."
    ::= { ciscoLwappWlanMIBGroups 7 }

ciscoLwappWlanConfigGroupSup3 OBJECT-GROUP
    OBJECTS         {
                        cLWlanReAnchorRoamedVoiceClientsEnable,
                        cLWlanMulticastInterfaceEnable,
                        cLWlanMulticastInterface,
                        cLWlanMulticastDirectEnable,
                        cLWlanNACPostureSupport,
                        cLWlanMaxClientsAccepted,
                        cLWlanScanDeferPriority,
                        cLWlanScanDeferTime,
                        cLWlanLanSubType,
                        cLWlanWebAuthOnMacFilterFailureEnabled,
                        cLWlanStaticIpTunnelingEnabled,
                        cLWlanEapProfileName,
                        cLWlanSetEapProfileName,
                        cLWlanMaxClientsAllowedPerAP,
                        cLWlanMdnsMode
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of WLANs on the controller to be passed
        to an LWAPP AP."
    ::= { ciscoLwappWlanMIBGroups 8 }

ciscoLwappWlan11uConfigGroupsup1 OBJECT-GROUP
    OBJECTS         {
                        cLWlan11uStatus,
                        cLWlan11uInternetAccess,
                        cLWlan11uNetworkType,
                        cLWlan11uHessid,
                        cLWlan11uNetworkAuthType,
                        cLWlan11uOui,
                        cLWlan11uOuiIsBeacon,
                        cLWlan11uOuiRowStatus,
                        cLWlan11uOuiStorageType,
                        cLWlan11uRealmName,
                        cLWlan11uRealmRowStatus,
                        cLWlan11uRealmEapMethod,
                        cLWlan11uRealmEapRowStatus,
                        cLWlan11uRealmEapAuthMethod,
                        cLWlan11uRealmEapAuthParam,
                        cLWlan11uRealmEapAuthRowStatus,
                        cLWlan11uDomainName,
                        cLWlan11uDomainRowStatus,
                        cLWlan11u3gppCountryCode,
                        cLWlan11u3gppNetworkCode,
                        cLWlan11u3gppRowStatus,
                        cLWlan11uIpAddressAvailIpv4,
                        cLWlan11uIpAddressAvailIpv6
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents 802.11u
        related configuration of WLANs on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 9 }

ciscoLwappWlanServiceAdvertisementConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLWlanServiceAdvertisementStatus,
                        cLWlanServiceAdvertisementMsapServerIndex
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents 802.11u
        related configuration of WLANs on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 10 }

ciscoLwappWlanHotSpot2ConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLWlanHotSpot2OperatorName,
                        cLWlanHotSpot2OperatorLanguage,
                        cLWlanHotSpot2OperatorRowStatus,
                        cLWlanHotSpot2PortConfigIpProtocol,
                        cLWlanHotSpot2PortConfigPortNumber,
                        cLWlanHotSpot2PortConfigStatus,
                        cLWlanHotSpot2PortConfigRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents 802.11u
        related configuration of WLANs on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 11 }

ciscoLwappWlanIosConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLWlanIosAccountingMethodListName,
                        cLWlanIosAuthenticationMethodListName,
                        cLWlanIosMacFilteringMethodListName,
                        cLWlanIosWebAuthMethodListName,
                        cLWlanIosQosUpStreamProfileName,
                        cLWlanIosQosDownStreamProfileName,
                        cLWlanIngressDHCPOption82Format,
                        cLWlanIngressDHCPOption82Ascii,
                        cLWlanIngressDHCPOption82Rid,
                        cLWlanIngressDHCPOption82Enable,
                        cLWlanIosScanDeferPriority,
                        cLWlanIosWebAuthParameterMapName,
                        cLWlanIosQosClientUpStreamProfileName,
                        cLWlanIosQosClientDownStreamProfileName,
                        cLWlanIosAuthorizationMethodListName,
                        cLWlanIosWebAuthAuthorizationMethodListName,
                        cLWlanIosMacOverrideMethodListName
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents IOS
        related configuration of WLANs on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 12 }

ciscoLwappWlanQosConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLWlanClientDSAverageDataRate,
                        cLWlanClientUSAverageDataRate,
                        cLWlanClientDSBurstDataRate,
                        cLWlanClientUSBurstDataRate,
                        cLWlanClientDSAvgRealTimeDataRate,
                        cLWlanClientUSAvgRealTimeDataRate,
                        cLWlanClientDSBurstRealTimeDataRate,
                        cLWlanClientUSBurstRealTimeDataRate,
                        cLWlanSsidDSAverageDataRate,
                        cLWlanSsidUSAverageDataRate,
                        cLWlanSsidDSBurstDataRate,
                        cLWlanSsidUSBurstDataRate,
                        cLWlanSsidDSAvgRealTimeDataRate,
                        cLWlanSsidUSAvgRealTimeDataRate,
                        cLWlanSsidDSBurstRealTimeDataRate,
                        cLWlanSsidUSBurstRealTimeDataRate,
                        cLWlanWlanDSAverageDataRate,
                        cLWlanWlanUSAverageDataRate,
                        cLWlanWlanDSBurstDataRate,
                        cLWlanWlanUSBurstDataRate,
                        cLWlanWlanDSAvgRealTimeDataRate,
                        cLWlanWlanUSAvgRealTimeDataRate,
                        cLWlanWlanDSBurstRealTimeDataRate,
                        cLWlanWlanUSBurstRealTimeDataRate
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents QoS
        related configuration of WLANs on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 13 }

ciscoLwappWlanConfigGroupSup4 OBJECT-GROUP
    OBJECTS         {
                        cLWlanKtsCacSupportEnabled,
                        cLWlanWifiDirectPolicyStatus,
                        cLWlanWebAuthIPv6AclName,
                        cLWlanHotSpot2Enabled,
                        cLWlanMaxClientsAllowedPerRadio,
                        cLWlanDhcpDeviceProfiling,
                        cLWlanMacAuthOverDot1xEnabled,
                        cLWlanUserTimeout,
                        cLWlanUserIdleThreshold,
                        cLWlanHttpDeviceProfiling,
                        cLWlanHotSpotClearConfig,
                        cLWlanRadiusAuthFourthServer,
                        cLWlanRadiusAuthFifthServer,
                        cLWlanRadiusAuthSixthServer,
                        cLWlanRadiusAcctFourthServer,
                        cLWlanRadiusAcctFifthServer,
                        cLWlanRadiusAcctSixthServer,
                        cLWlanSelfAnchorEnabled
                    }
    STATUS          deprecated
    DESCRIPTION
        "This collection of objects represent the
        configuration of WLANs on the controller to be passed
        to an LWAPP AP.This object is superceded by 
        ciscoLwappWlanConfigGroupSup5.
        ciscoLwappWlanConfigGroupSup4 object is superseded by ciscoLwappWlanConfigGroupSup5."
    ::= { ciscoLwappWlanMIBGroups 14 }

ciscoLwappWlan11uConfigGroupsup2 OBJECT-GROUP
    OBJECTS         { cLWlan11uRealmEapAuthCredentialType }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents 802.11u
        related configuration of WLANs on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 15 }

ciscoLwappWlanHotSpot2ConfigGroupSup1 OBJECT-GROUP
    OBJECTS         {
                        cLWlanHotSpot2WanLinkStatus,
                        cLWlanHotSpot2WanSymLinkStatus,
                        cLWlanHotSpot2WanDownLinkSpeed,
                        cLWlanHotSpot2WanUpLinkSpeed
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents 802.11u
        related configuration of WLANs on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 16 }

ciscoLwappAPGroupsVlanConfigGroupSup1 OBJECT-GROUP
    OBJECTS         { cLAPGroupsWlanOrderIndex }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of AP Groups Vlan on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 17 }

cLAPGroupsVenueConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLAPGroupsVenueConfigVenueGroup,
                        cLAPGroupsVenueConfigVenueType,
                        cLAPGroupsVenueConfigVenueName,
                        cLAPGroupsVenueConfigLanguage,
                        cLAPGroupsOperatingClass
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of Venue groups on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 18 }

cLAPGroupsMultipleVenueGroup OBJECT-GROUP
    OBJECTS         {
                        cLAPGroupsMultipleVenueName,
                        cLAPGroupsMultipleVenueRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of Venue groups on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 19 }

ciscoLwappWlanConfigClientGroupSup2 OBJECT-GROUP
    OBJECTS         { cLWlanClientIPv6AclName }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of WLANs on the controller to be passed
        to an 8021.11 clients."
    ::= { ciscoLwappWlanMIBGroups 20 }

ciscoLwappWlanConfigFlexibleNetflowGroup OBJECT-GROUP
    OBJECTS         {
                        cLWlanFlexibleNetflowMonitorName,
                        cLWlanFlexibleNetflowRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the configuration
        of flexible netflow policy details per WLAN 
        on the conroller to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 21 }

ciscoLwappWlanConfigGroupSup5 OBJECT-GROUP
    OBJECTS         {
                        cLWlanKtsCacSupportEnabled,
                        cLWlanWifiDirectPolicyStatus,
                        cLWlanWebAuthIPv6AclName,
                        cLWlanHotSpot2Enabled,
                        cLWlanMaxClientsAllowedPerRadio,
                        cLWlanDhcpDeviceProfiling,
                        cLWlanMacAuthOverDot1xEnabled,
                        cLWlanUserTimeout,
                        cLWlanUserIdleThreshold,
                        cLWlanHttpDeviceProfiling,
                        cLWlanHotSpotClearConfig,
                        cLWlanRadiusAuthFourthServer,
                        cLWlanRadiusAuthFifthServer,
                        cLWlanRadiusAuthSixthServer,
                        cLWlanRadiusAcctFourthServer,
                        cLWlanRadiusAcctFifthServer,
                        cLWlanRadiusAcctSixthServer,
                        cLWlanSelfAnchorEnabled,
                        cLWlanUniversalAdmin
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of WLANs on the controller to be passed
        to an LWAPP AP."
    ::= { ciscoLwappWlanMIBGroups 22 }

ciscoLwappAPGroupsVlanConfigGroupSup2 OBJECT-GROUP
    OBJECTS         {
                        cLAPGroupNACSupport,
                        cLAPGroupsVlanConfigRowStatus,
                        cLAPGroupsVlanConfigStorageType,
                        cLAPGroupsVlanMappingInterfaceNameRev1
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of AP Groups Vlan on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 23 }

ciscoLwappWlanConfigGroupSup6 OBJECT-GROUP
    OBJECTS         { cLWlan11acMuMimoEnabled }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of WLANs on the controller to be passed
        to an LWAPP AP."
    ::= { ciscoLwappWlanMIBGroups 24 }

ciscoLwappWlanConfigGroupSup7 OBJECT-GROUP
    OBJECTS         {
                        cLAPGroupsHyperlocationEnable,
                        cLAPGroupsPakRssiThreshold,
                        cLAPGroupsPakRssiThresholdTrigger,
                        cLAPGroupsPakRssiNtpIpAddressType,
                        cLAPGroupsPakRssiNtpAddress
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of AP Groups HyperLocation on the 
        controller to be passed to an LWAPP AP."
    ::= { ciscoLwappWlanMIBGroups 25 }

ciscoLwappWlanConfigGroupSup8 OBJECT-GROUP
    OBJECTS         {
                        cLAPGroupsLANPortStatus,
                        cLAPGroupsLANPortPoeStatus,
                        cLAPGroupsLANPortRlanName,
                        cLAPGroupsLANPortRowStatus,
                        cLAPGroupsExtModuleStatus,
                        cLAPGroupsExtModuleRlanName
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of AP Groups LAN Port on the controller 
        to be passed to an LWAPP AP."
    ::= { ciscoLwappWlanMIBGroups 26 }

ciscoLwappWlan11vConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLWlan11vBssTransEnable,
                        cLWlan11vDisassocImmiEnable,
                        cLWlan11vDisassocTimer,
                        cLWlan11vOpRoamDisassocTimer,
                        cLWlan11vDMSEnable
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents 802.11v BSS Transistion
        related configuration of WLANs on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 27 }

ciscoLwappApGroupConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLAPGroupNasId,
                        cLApGroupPreferMode,
                        cLApGroupGlobalWebAuthConfig,
                        cLApGroupExternalWebAuthUrl,
                        cLAPGroupsPolicyIndex,
                        cLAPGroupsPolicyWlanProfile,
                        cLAPGroupsPolicyRowStatus,
                        cLAPGroupTrafficQinqEnabled,
                        cLAPGroupDhcpQinqEnabled,
                        cLAPGroupQinqServiceVlanId
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents AP group related
        configuration of WLANs on the controller."
    ::= { ciscoLwappWlanMIBGroups 28 }

ciscoLwappPolicyConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLPolicyName,
                        cLPolicyRoleName,
                        cLPolicyEapType,
                        cLPolicyAclName,
                        cLPolicyVlanId,
                        cLPolicyQosProfile,
                        cLPolicySessionTimeout,
                        cLPolicySleepTimeout,
                        cLPolicyRowStatus,
                        cLPolicyFlexAclName,
                        cLPolicyAvcProfileName,
                        cLPolicyMdnsProfileName,
                        cLPolicyFlexVlanId,
                        cLPolicyUrlAclName,
                        cLPolicyOpendnsProfileName,
                        cLPolicyDeviceName,
                        cLPolicyDeviceRowStatus,
                        cLPolicyActiveStartTime,
                        cLPolicyActiveEndTime,
                        cLPolicyActiveHoursRowStatus,
                        cLPolicyWlanSchedulingStatus,
                        cLPolicyWlanSchedulingStartTime,
                        cLPolicyWlanSchedulingEndTime,
                        cLPolicyWlanSchedulingRowStatus
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents Policy related
        configuration of WLANs on the controller."
    ::= { ciscoLwappWlanMIBGroups 29 }

ciscoLwappWlan11kConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLWlan11kAssistedRoamingEnable,
                        cLWlan11kNeighborListEnable,
                        cLWlan11kDualbandNeigListEnable
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represent the
        configuration of AP Groups 11k on the controller 
        to be passed to an LWAPP AP."
    ::= { ciscoLwappWlanMIBGroups 30 }

ciscoLwappWlan11axConfigGroup OBJECT-GROUP
    OBJECTS         {
                        cLWlan11axMuMimoUplinkEnable,
                        cLWlan11axMuMimoDownlinkEnable,
                        cLWlan11axOfdmaUplinkEnable,
                        cLWlan11axOfdmaDownlinkEnable,
                        cLWlan11axTargetWaketimeEnable,
                        cLWlan11axBssColorModeEnable,
                        cLWlan11axBssColorCode,
                        cLWlan11axBssPartialColorEnable
                    }
    STATUS          current
    DESCRIPTION
        "This collection of objects represents 802.11ax
        related configuration of WLANs on the controller
        to be passed to an AP."
    ::= { ciscoLwappWlanMIBGroups 31 }

END


-- %DNP%  MLC -Edit MLC

