-- This file was included in WWP MIB release 04-07-01-0008
LLDP-EXT-DOT3-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, TruthValue
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    lldpExtensions, lldpLocPortNum, 
    lldpRemTimeMark, lldpRemLocalPortNum, lldpRemIndex,
    lldpPortConfigEntry
        FROM LLDP-MIB;

lldpXdot3MIB MODULE-IDENTITY
    LAST-UPDATED "200505060000Z" -- May 06, 2005
    ORGANIZATION "IEEE 802.1 Working Group"
    CONTACT-INFO 
            "  WG-URL: http://grouper.ieee.org/groups/802/1/index.html
             WG-EMail: stds-802-1@ieee.org

              Contact: Paul Congdon
               Postal: Hewlett-Packard Company
                       8000 Foothills Blvd. 
                       Roseville, CA 95747
                       USA
                  Tel: +1-916-785-5753
               E-mail: paul_congdon@hp.com"
    DESCRIPTION
            "The LLDP Management Information Base extension module for
            IEEE 802.3 organizationally defined discovery information.

            In order to assure the uniqueness of the LLDP-MIB,
            lldpXdot3MIB is branched from lldpExtensions using OUI value
            as the node.  An OUI/'company_id' is a 24 bit globally unique
            assigned number referenced by various standards.

            Copyright (C) IEEE (2005).  This version of this MIB module
            is published as Annex G.6.1 of IEEE Std 802.1AB-2005;
            see the standard itself for full legal notices."
    REVISION        "200505060000Z" -- May 06, 2005
    DESCRIPTION
            "Published as part of IEEE Std 802.1AB-2005 initial version."
-- OUI for IEEE 802.3 is 4623 (00-12-0F)
   ::= { lldpExtensions 4623 } 

------------------------------------------------------------------------------
------------------------------------------------------------------------------
--
-- Organizationally Defined Information Extension - IEEE 802.3
--
------------------------------------------------------------------------------
------------------------------------------------------------------------------

lldpXdot3Objects    OBJECT IDENTIFIER ::= { lldpXdot3MIB 1 }

-- LLDP IEEE 802.3 extension MIB groups
lldpXdot3Config     OBJECT IDENTIFIER ::= { lldpXdot3Objects 1 }
lldpXdot3LocalData  OBJECT IDENTIFIER ::= { lldpXdot3Objects 2 }
lldpXdot3RemoteData OBJECT IDENTIFIER ::= { lldpXdot3Objects 3 }

-- textual conventions

LldpPowerPortClass ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
            "This TC describes the Power over Ethernet (PoE) port class."
    SYNTAX  INTEGER {
            pClassPSE(1),
            pClassPD(2)
    }

LldpLinkAggStatusMap ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
            "This TC describes the link aggregation status.

            The bit 'aggCapable(0)' indicates the link is capable of being
            aggregated. 

            The bit 'aggEnabled(1)' indicates the link is currently in
            aggregation."
    SYNTAX  BITS {
            aggCapable(0),
            aggEnabled(1)
    }

------------------------------------------------------------------------------
-- IEEE 802.3 - Configuration
------------------------------------------------------------------------------

lldpXdot3PortConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot3PortConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A table that controls selection of LLDP TLVs to be transmitted 
            on individual ports."
    ::= { lldpXdot3Config 1 }

lldpXdot3PortConfigEntry  OBJECT-TYPE
    SYNTAX      LldpXdot3PortConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "LLDP configuration information that controls the
            transmission of IEEE 802.3 organizationally defined TLVs on
            LLDP transmission capable ports.

            This configuration object augments the lldpPortConfigEntry of
            the LLDP-MIB, therefore it is only present along with the port
            configuration defined by the associated lldpPortConfigEntry
            entry.

            Each active lldpXdot3PortConfigEntry must be from non-volatile
            storage (along with the corresponding lldpPortConfigEntry)
            after a re-initialization of the management system."
    AUGMENTS { lldpPortConfigEntry }
    ::= { lldpXdot3PortConfigTable 1 }

LldpXdot3PortConfigEntry ::= SEQUENCE {
      lldpXdot3PortConfigTLVsTxEnable  BITS
}

lldpXdot3PortConfigTLVsTxEnable  OBJECT-TYPE
    SYNTAX      BITS {
            macPhyConfigStatus(0),
            powerViaMDI(1),
            linkAggregation(2),
            maxFrameSize(3)
    }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The lldpXdot3PortConfigTLVsTxEnable, defined as a bitmap,
            includes the IEEE 802.3 organizationally defined set of LLDP
            TLVs whose transmission is allowed on the local LLDP agent by
            the network management.  Each bit in the bitmap corresponds
            to an IEEE 802.3 subtype associated with a specific IEEE
            802.3 optional TLV.  The bit 0 is not used since there is
            no corresponding subtype.

            The bit 'macPhyConfigStatus(0)' indicates that LLDP agent
            should transmit 'MAC/PHY configuration/status TLV'.

            The bit 'powerViaMDI(1)' indicates that LLDP agent should
            transmit 'Power via MDI TLV'.

            The bit 'linkAggregation(2)' indicates that LLDP agent should
            transmit 'Link Aggregation TLV'.

            The bit 'maxFrameSize(3)' indicates that LLDP agent should
            transmit 'Maximum-frame-size TLV'.

            The default value for lldpXdot3PortConfigTLVsTxEnable object
            is an empty set, which means no enumerated values are set.

            The value of this object must be restored from non-volatile
            storage after a re-initialization of the management system."
    REFERENCE 
            "IEEE 802.1AB-2005 10.2.1.1"
    DEFVAL  { { } }
    ::= { lldpXdot3PortConfigEntry  1 }


------------------------------------------------------------------------------
-- IEEE 802.3 - Local Device Information 
------------------------------------------------------------------------------
---
--- lldpXdot3LocPortTable: Ethernet Port AutoNeg/Speed/Duplex
---                        Information Table
---
---
lldpXdot3LocPortTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot3LocPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one row per port of Ethernet port
            information (as a part of the LLDP 802.3 organizational
            extension) on the local system known to this agent."
    ::= { lldpXdot3LocalData 1 }

lldpXdot3LocPortEntry OBJECT-TYPE
    SYNTAX      LldpXdot3LocPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Information about a particular port component."
    INDEX   { lldpLocPortNum }
    ::= { lldpXdot3LocPortTable 1 }

LldpXdot3LocPortEntry ::= SEQUENCE {
              lldpXdot3LocPortAutoNegSupported     TruthValue,
              lldpXdot3LocPortAutoNegEnabled       TruthValue,
              lldpXdot3LocPortAutoNegAdvertisedCap OCTET STRING,
              lldpXdot3LocPortOperMauType          Integer32
} 

lldpXdot3LocPortAutoNegSupported OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value used to indicate whether the given port
            (associated with the local system) supports Auto-negotiation."
    REFERENCE 
            "IEEE 802.1AB-2005 G.2.1"
    ::= { lldpXdot3LocPortEntry 1 }

lldpXdot3LocPortAutoNegEnabled  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value used to indicate whether port
            Auto-negotiation is enabled on the given port associated
            with the local system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.2.1"
    ::= { lldpXdot3LocPortEntry 2 }

lldpXdot3LocPortAutoNegAdvertisedCap OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(2))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "This object contains the value (bitmap) of the
            ifMauAutoNegCapAdvertisedBits object (defined in IETF RFC
            3636) which is associated with the given port on the
            local system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.2.2"
    ::= { lldpXdot3LocPortEntry 3 }

lldpXdot3LocPortOperMauType  OBJECT-TYPE
    SYNTAX 	    Integer32(0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "An integer value that indicates the operational MAU type
            of the given port on the local system.

            This object contains the integer value derived from the
            list position of the corresponding dot3MauType as listed 
            in IETF RFC 3636 (or subsequent revisions) and is equal
            to the last number in the respective dot3MauType OID.
           
            For example, if the ifMauType object is dot3MauType1000BaseTHD
            which corresponds to {dot3MauType 29}, the numerical value of
            this field will be 29. For MAU types not listed in RFC 3636
            (or subsequent revisions), the value of this field shall be
            set to zero."
    REFERENCE 
            "IEEE 802.1AB-2005 G.2.3"
    ::= { lldpXdot3LocPortEntry 4 }

---
---
--- lldpXdot3LocPowerTable: Power Ethernet Information Table
---
---
lldpXdot3LocPowerTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot3LocPowerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one row per port of power ethernet 
            information (as a part of the LLDP 802.3 organizational
            extension) on the local system known to this agent."
    ::= { lldpXdot3LocalData 2 }

lldpXdot3LocPowerEntry OBJECT-TYPE
    SYNTAX      LldpXdot3LocPowerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Information about a particular port component."
    INDEX   { lldpLocPortNum }
    ::= { lldpXdot3LocPowerTable 1 }

LldpXdot3LocPowerEntry ::= SEQUENCE {
              lldpXdot3LocPowerPortClass           LldpPowerPortClass,
              lldpXdot3LocPowerMDISupported        TruthValue,
              lldpXdot3LocPowerMDIEnabled          TruthValue,
              lldpXdot3LocPowerPairControlable     TruthValue,
              lldpXdot3LocPowerPairs               Integer32,
              lldpXdot3LocPowerClass               Integer32
} 

lldpXdot3LocPowerPortClass  OBJECT-TYPE
    SYNTAX      LldpPowerPortClass
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The value that identifies the port Class of the given port
            associated with the local system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.3.1"
    ::= { lldpXdot3LocPowerEntry 1 }

lldpXdot3LocPowerMDISupported  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value used to indicate whether the MDI power is
            supported on the given port associated with the local system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.3.1"
    ::= { lldpXdot3LocPowerEntry 2 }

lldpXdot3LocPowerMDIEnabled  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value used to identify whether MDI power is
            enabled on the given port associated with the local system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.3.1"
    ::= { lldpXdot3LocPowerEntry 3 }

lldpXdot3LocPowerPairControlable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value is derived from the value of
            pethPsePortPowerPairsControlAbility object (defined in IETF
            RFC 3621) and is used to indicate whether the pair selection
            can be controlled on the given port associated with the
            local system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.3.1"
    ::= { lldpXdot3LocPowerEntry 4 }

lldpXdot3LocPowerPairs  OBJECT-TYPE
    SYNTAX      Integer32(1|2)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "This object contains the value of the pethPsePortPowerPairs
            object (defined in IETF RFC 3621) which is associated with
            the given port on the local system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.3.2"
    ::= { lldpXdot3LocPowerEntry 5 }

lldpXdot3LocPowerClass  OBJECT-TYPE
    SYNTAX      Integer32(1|2|3|4|5)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "This object contains the value of the
            pethPsePortPowerClassifications object (defined in IETF
            RFC 3621) which is associated with the given port on the
            local system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.3.3"
    ::= { lldpXdot3LocPowerEntry 6 }

---
---
--- lldpXdot3LocLinkAggTable: Link Aggregation Information Table
---
---
lldpXdot3LocLinkAggTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot3LocLinkAggEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one row per port of link aggregation 
            information (as a part of the LLDP 802.3 organizational
            extension) on the local system known to this agent."
    ::= { lldpXdot3LocalData 3 }

lldpXdot3LocLinkAggEntry OBJECT-TYPE
    SYNTAX      LldpXdot3LocLinkAggEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Link Aggregation information about a particular port
            component."
    INDEX   { lldpLocPortNum }
    ::= { lldpXdot3LocLinkAggTable 1 }

LldpXdot3LocLinkAggEntry ::= SEQUENCE {
              lldpXdot3LocLinkAggStatus       LldpLinkAggStatusMap,
              lldpXdot3LocLinkAggPortId       Integer32
} 

lldpXdot3LocLinkAggStatus OBJECT-TYPE
    SYNTAX      LldpLinkAggStatusMap
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The bitmap value contains the link aggregation capabilities
            and the current aggregation status of the link."
    REFERENCE 
            "IEEE 802.1AB-2005 G.4.1"
    ::= { lldpXdot3LocLinkAggEntry 1 }

lldpXdot3LocLinkAggPortId OBJECT-TYPE
    SYNTAX 	    Integer32(0|1..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "This object contains the IEEE 802.3 aggregated port
            identifier, aAggPortID (IEEE 802.3-2002, 30.7.2.1.1),
            derived from the ifNumber of the ifIndex for the port
            component in link aggregation.

            If the port is not in link aggregation state and/or it
            does not support link aggregation, this value should be set
            to zero."
    REFERENCE 
            "IEEE 802.1AB-2005 G.4.2"
    ::= { lldpXdot3LocLinkAggEntry 2 }

---
---
--- lldpXdot3LocMaxFrameSizeTable: Maximum Frame Size information 
---
---
lldpXdot3LocMaxFrameSizeTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot3LocMaxFrameSizeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one row per port of maximum frame 
            size information (as a part of the LLDP 802.3 organizational
            extension) on the local system known to this agent."
    ::= { lldpXdot3LocalData 4 }

lldpXdot3LocMaxFrameSizeEntry OBJECT-TYPE
    SYNTAX      LldpXdot3LocMaxFrameSizeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Maximum Frame Size information about a particular port
            component."
    INDEX   { lldpLocPortNum }
    ::= { lldpXdot3LocMaxFrameSizeTable 1 }

LldpXdot3LocMaxFrameSizeEntry ::= SEQUENCE {
              lldpXdot3LocMaxFrameSize   Integer32
} 

lldpXdot3LocMaxFrameSize OBJECT-TYPE
    SYNTAX      Integer32(0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "An integer value indicating the maximum supported frame 
             size in octets on the given port of the local system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.5.1"
    ::= { lldpXdot3LocMaxFrameSizeEntry 1 }


------------------------------------------------------------------------------
-- IEEE 802.3 - Remote Devices Information
------------------------------------------------------------------------------
---
---
--- lldpXdot3RemPortTable: Ethernet Information Table
---
---
lldpXdot3RemPortTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot3RemPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains Ethernet port information (as a part
            of the LLDP 802.3 organizational extension) of the remote
            system."
    ::= { lldpXdot3RemoteData 1 }

lldpXdot3RemPortEntry OBJECT-TYPE
    SYNTAX      LldpXdot3RemPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Information about a particular physical network connection."
    INDEX   { lldpRemTimeMark,
              lldpRemLocalPortNum,
              lldpRemIndex }
    ::= { lldpXdot3RemPortTable 1 }

LldpXdot3RemPortEntry ::= SEQUENCE {
              lldpXdot3RemPortAutoNegSupported     TruthValue,
              lldpXdot3RemPortAutoNegEnabled       TruthValue,
              lldpXdot3RemPortAutoNegAdvertisedCap OCTET STRING,
              lldpXdot3RemPortOperMauType          Integer32
} 

lldpXdot3RemPortAutoNegSupported OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value used to indicate whether the given port
            (associated with remote system) supports Auto-negotiation."
    REFERENCE 
            "IEEE 802.1AB-2005 G.2.1"
    ::= { lldpXdot3RemPortEntry 1 }

lldpXdot3RemPortAutoNegEnabled  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value used to indicate whether port
            Auto-negotiation is enabled on the given port associated
            with the remote system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.2.1"
    ::= { lldpXdot3RemPortEntry 2 }

lldpXdot3RemPortAutoNegAdvertisedCap  OBJECT-TYPE
    SYNTAX      OCTET STRING(SIZE(2))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "This object contains the value (bitmap) of the
            ifMauAutoNegCapAdvertisedBits object (defined in IETF RFC
            3636) which is associated with the given port on the
            remote system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.2.2"
    ::= { lldpXdot3RemPortEntry 3 }

lldpXdot3RemPortOperMauType OBJECT-TYPE
    SYNTAX 	    Integer32(0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "An integer value that indicates the operational MAU type
            of the sending device.

            This object contains the integer value derived from the
            list position of the corresponding dot3MauType as listed in
            in IETF RFC 3636 (or subsequent revisions) and is equal
            to the last number in the respective dot3MauType OID.
           
            For example, if the ifMauType object is dot3MauType1000BaseTHD
            which corresponds to {dot3MauType 29}, the numerical value of
            this field will be 29. For MAU types not listed in RFC 3636
            (or subsequent revisions), the value of this field shall be
            set to zero."
    REFERENCE 
            "IEEE 802.1AB-2005 G.2.3"
    ::= { lldpXdot3RemPortEntry 4 }

---
---
--- lldpXdot3RemPowerTable: Power Ethernet Information Table
---
---
lldpXdot3RemPowerTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot3RemPowerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains Ethernet power information (as a part
            of the LLDP 802.3 organizational extension) of the remote
            system."
    ::= { lldpXdot3RemoteData 2 }

lldpXdot3RemPowerEntry OBJECT-TYPE
    SYNTAX      LldpXdot3RemPowerEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Information about a particular physical network connection."
    INDEX   { lldpRemTimeMark,
              lldpRemLocalPortNum,
              lldpRemIndex }
    ::= { lldpXdot3RemPowerTable 1 }

LldpXdot3RemPowerEntry ::= SEQUENCE {
              lldpXdot3RemPowerPortClass           LldpPowerPortClass,
              lldpXdot3RemPowerMDISupported        TruthValue,
              lldpXdot3RemPowerMDIEnabled          TruthValue,
              lldpXdot3RemPowerPairControlable     TruthValue,
              lldpXdot3RemPowerPairs               Integer32,
              lldpXdot3RemPowerClass               Integer32
} 

lldpXdot3RemPowerPortClass  OBJECT-TYPE
    SYNTAX      LldpPowerPortClass
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The value that identifies the port Class of the given port
            associated with the remote system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.3.1"
    ::= { lldpXdot3RemPowerEntry 1 }

lldpXdot3RemPowerMDISupported  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value used to indicate whether the MDI power
            is supported on the given port associated with the remote
            system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.3.1"
    ::= { lldpXdot3RemPowerEntry 2 }

lldpXdot3RemPowerMDIEnabled  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value used to identify whether MDI power is
            enabled on the given port associated with the remote system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.3.1"
    ::= { lldpXdot3RemPowerEntry 3 }

lldpXdot3RemPowerPairControlable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value is derived from the value of
            pethPsePortPowerPairsControlAbility object (defined in IETF
            RFC 3621) and is used to indicate whether the pair selection
            can be controlled on the given port associated with the
            remote system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.3.1"
    ::= { lldpXdot3RemPowerEntry 4 }

lldpXdot3RemPowerPairs  OBJECT-TYPE
    SYNTAX      Integer32(1|2)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "This object contains the value of the pethPsePortPowerPairs
            object (defined in IETF RFC 3621) which is associated with
            the given port on the remote system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.3.2"
    ::= { lldpXdot3RemPowerEntry 5 }

lldpXdot3RemPowerClass  OBJECT-TYPE
    SYNTAX      Integer32(1|2|3|4|5)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "This object contains the value of the
            pethPsePortPowerClassifications object (defined in IETF
            RFC 3621) which is associated with the given port on the
            remote system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.3.3"
    ::= { lldpXdot3RemPowerEntry 6 }

---
---
--- lldpXdot3RemLinkAggTable: Link Aggregation Information Table
---
---
lldpXdot3RemLinkAggTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot3RemLinkAggEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains port link aggregation information
            (as a part of the LLDP 802.3 organizational extension)
            of the remote system."
    ::= { lldpXdot3RemoteData 3 }

lldpXdot3RemLinkAggEntry OBJECT-TYPE
    SYNTAX      LldpXdot3RemLinkAggEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Link Aggregation information about remote system's port
            component."
    INDEX   { lldpRemTimeMark,
              lldpRemLocalPortNum,
              lldpRemIndex }
    ::= { lldpXdot3RemLinkAggTable 1 }

LldpXdot3RemLinkAggEntry ::= SEQUENCE {
              lldpXdot3RemLinkAggStatus       LldpLinkAggStatusMap,
              lldpXdot3RemLinkAggPortId       Integer32
} 

lldpXdot3RemLinkAggStatus OBJECT-TYPE
    SYNTAX      LldpLinkAggStatusMap
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The bitmap value contains the link aggregation capabilities
            and the current aggregation status of the link."
    REFERENCE 
            "IEEE 802.1AB-2005 G.4.1"
    ::= { lldpXdot3RemLinkAggEntry 1 }

lldpXdot3RemLinkAggPortId OBJECT-TYPE
    SYNTAX 	    Integer32(0|1..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "This object contains the IEEE 802.3 aggregated port
            identifier, aAggPortID (IEEE 802.3-2002, 30.7.2.1.1),
            derived from the ifNumber of the ifIndex for the port
            component associated with the remote system.

            If the remote port is not in link aggregation state and/or
            it does not support link aggregation, this value should be
            zero."
    REFERENCE 
            "IEEE 802.1AB-2005 G.4.2"
    ::= { lldpXdot3RemLinkAggEntry 2 }


---
---
--- lldpXdot3RemMaxFrameSizeTable: Maximum Frame Size information 
---
---
lldpXdot3RemMaxFrameSizeTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot3RemMaxFrameSizeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one row per port of maximum frame 
            size information (as a part of the LLDP 802.3 organizational
            extension) of the remote system."
    ::= { lldpXdot3RemoteData 4 }

lldpXdot3RemMaxFrameSizeEntry OBJECT-TYPE
    SYNTAX      LldpXdot3RemMaxFrameSizeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Maximum Frame Size information about a particular port
            component."
    INDEX   { lldpRemTimeMark,
              lldpRemLocalPortNum,
              lldpRemIndex }
    ::= { lldpXdot3RemMaxFrameSizeTable 1 }

LldpXdot3RemMaxFrameSizeEntry ::= SEQUENCE {
              lldpXdot3RemMaxFrameSize   Integer32
} 

lldpXdot3RemMaxFrameSize OBJECT-TYPE
    SYNTAX      Integer32(0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "An integer value indicating the maximum supported frame 
             size in octets on the port component associated with the 
             remote system."
    REFERENCE 
            "IEEE 802.1AB-2005 G.5.1"
    ::= { lldpXdot3RemMaxFrameSizeEntry 1 }


------------------------------------------------------------------------------
-- Conformance Information
------------------------------------------------------------------------------
lldpXdot3Conformance OBJECT IDENTIFIER ::= { lldpXdot3MIB 2 }
lldpXdot3Compliances OBJECT IDENTIFIER ::= { lldpXdot3Conformance 1 }
lldpXdot3Groups      OBJECT IDENTIFIER ::= { lldpXdot3Conformance 2 }

-- compliance statements

lldpXdot3Compliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for SNMP entities which implement
            the LLDP 802.3 organizational extension MIB."
    MODULE  -- this module
        MANDATORY-GROUPS { lldpXdot3ConfigGroup, 
                           lldpXdot3LocSysGroup,
                           lldpXdot3RemSysGroup
        }
    ::= { lldpXdot3Compliances 1 }

-- MIB groupings

lldpXdot3ConfigGroup    OBJECT-GROUP
    OBJECTS {
        lldpXdot3PortConfigTLVsTxEnable
    }
    STATUS  current
    DESCRIPTION
            "The collection of objects which are used to configure the
            LLDP 802.3 organizational extension implementation behavior.

            This group is mandatory for agents which implement the 
            LLDP 802.3 organizational extension."
    ::= { lldpXdot3Groups 1 }

lldpXdot3LocSysGroup  OBJECT-GROUP
    OBJECTS {
        lldpXdot3LocPortAutoNegSupported,
        lldpXdot3LocPortAutoNegEnabled,
        lldpXdot3LocPortAutoNegAdvertisedCap,
        lldpXdot3LocPortOperMauType,
        lldpXdot3LocPowerPortClass,
        lldpXdot3LocPowerMDISupported,
        lldpXdot3LocPowerMDIEnabled,
        lldpXdot3LocPowerPairControlable,
        lldpXdot3LocPowerPairs,
        lldpXdot3LocPowerClass,
        lldpXdot3LocLinkAggStatus,
        lldpXdot3LocLinkAggPortId,
        lldpXdot3LocMaxFrameSize
    }
    STATUS  current
    DESCRIPTION
            "The collection of objects which are used to represent LLDP
            802.3 organizational extension Local Device Information.
            
            This group is mandatory for agents which implement the 
            LLDP 802.3 organizational extension in the TX mode."
    ::= { lldpXdot3Groups 2 }

lldpXdot3RemSysGroup  OBJECT-GROUP
    OBJECTS {
        lldpXdot3RemPortAutoNegSupported,
        lldpXdot3RemPortAutoNegEnabled,
        lldpXdot3RemPortAutoNegAdvertisedCap,
        lldpXdot3RemPortOperMauType,
        lldpXdot3RemPowerPortClass,
        lldpXdot3RemPowerMDISupported,
        lldpXdot3RemPowerMDIEnabled,
        lldpXdot3RemPowerPairControlable,
        lldpXdot3RemPowerPairs,
        lldpXdot3RemPowerClass,
        lldpXdot3RemLinkAggStatus,
        lldpXdot3RemLinkAggPortId,
        lldpXdot3RemMaxFrameSize
    }
    STATUS  current
    DESCRIPTION
            "The collection of objects which are used to represent LLDP
            802.3 organizational extension Local Device Information.
            
            This group is mandatory for agents which implement the 
            LLDP 802.3 organizational extension in the RX mode."
    ::= { lldpXdot3Groups 3 }

END
