-- This file was included in WWP MIB release 04-07-01-0008
 --
 -- WWP-LEOS-VLAN-TAG-MIB.my
 --

 WWP-LEOS-VLAN-TAG-MIB DEFINITIONS ::= BEGIN

 IMPORTS                
   TimeTicks, Integer32, Unsigned32, Counter32, Counter64, OBJECT-TYPE, MODULE-IDENTITY                       
        FROM SNMPv2-SMI                 
   DisplayString, MacAddress, TEXTUAL-CONVENTION, RowStatus, TruthValue, TimeStamp                 
        FROM SNMPv2-TC                                                  
   wwpModulesLeos           
        FROM WWP-SMI;

        
 wwpLeosVlanMIB MODULE-IDENTITY
            LAST-UPDATED "200709291700Z"
            ORGANIZATION "Ciena, Inc"
            CONTACT-INFO
                    "   Mib Meister
		  			115 North Sullivan Road
					Spokane Valley, WA 99037
		        	USA		 		
		        	Phone:  +1 509 242 9000
					Email:  support@ciena.com"
            DESCRIPTION
                    "This MIB module defines the managed objects for the VLAN,
                    specific for the WWP products."  
            REVISION     "200301151700Z"
            DESCRIPTION
                    "Initial creation."
            REVISION     "200709291700Z"
            DESCRIPTION
                    "Added VLAN statistics."
            ::= { wwpModulesLeos 5 }

 --
 -- Textual conventions
 --

 VlanId ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "A Vlan ID represents a Broadcast Domain."
    SYNTAX      INTEGER (1..24576)
 
 VlanTag ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "A 12-bit ID used in the VLAN Tag header."
    SYNTAX      INTEGER (1..4094)
 
 --
 -- Node definitions
 --
        
 wwpLeosVlanMIBObjects OBJECT IDENTIFIER ::= { wwpLeosVlanMIB 1 }

 wwpLeosVlan  OBJECT IDENTIFIER ::= { wwpLeosVlanMIBObjects 1 }
 
 wwpLeosVlanEPR OBJECT IDENTIFIER ::= { wwpLeosVlanMIBObjects 2 }
 
 
 -- Notifications 
  
 wwpLeosVlanMIBNotificationPrefix  OBJECT IDENTIFIER ::= { wwpLeosVlanMIB 2 } 
 wwpLeosVlanMIBNotifications       OBJECT IDENTIFIER ::=  
                       { wwpLeosVlanMIBNotificationPrefix 0 }

 -- Conformance information 
 
 wwpLeosVlanMIBConformance OBJECT IDENTIFIER ::= { wwpLeosVlanMIB 3 } 
 wwpLeosVlanMIBCompliances OBJECT IDENTIFIER ::= { wwpLeosVlanMIBConformance 1 }                
 wwpLeosVlanMIBGroups      OBJECT IDENTIFIER ::= { wwpLeosVlanMIBConformance 2 }
   
 wwpLeosMaxVlans OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The maximum number of VLANs that this device
        supports."
    ::= { wwpLeosVlan 1 }
    
 wwpLeosMaxSupportedVlanTagId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The maximum value of VLAN Tag ID that this 
        device supports."
    ::= { wwpLeosVlan 2 }
    
 wwpLeosNumVlans OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current number of VLANs that are
        configured in this device."
    ::= { wwpLeosVlan 3 }
    
 wwpLeosVlanTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosVlanEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION
            "The (conceptual) table listing the config 
            parameters for the VLAN."  
     ::= { wwpLeosVlan 4 }
                
 wwpLeosVlanEntry OBJECT-TYPE
     SYNTAX      WwpLeosVlanEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
           "An entry (conceptual row) in the wwpLeosVlanTable."
     INDEX { wwpLeosVlanId }
     ::= { wwpLeosVlanTable 1 }
                
 WwpLeosVlanEntry ::=  SEQUENCE { 
     wwpLeosVlanId                     VlanId,
     wwpLeosVlanName                   OCTET STRING,
     wwpLeosVlanStatus                 RowStatus,
     wwpLeosVlanMacLrnState            INTEGER,
     wwpLeosVlanMacLrnOperState	       INTEGER,
     wwpLeosVlanTranslationVlan        INTEGER
 }

 wwpLeosVlanId OBJECT-TYPE
     SYNTAX      VlanId
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
             "A unique identifier for the VLAN."
     ::= { wwpLeosVlanEntry 1 }
                
 wwpLeosVlanName OBJECT-TYPE
     SYNTAX       OCTET STRING (SIZE (0..32))
     MAX-ACCESS   read-create
     STATUS       current
     DESCRIPTION
             "Name associated with this VLAN Entry."
     ::= { wwpLeosVlanEntry 2 }

 wwpLeosVlanStatus OBJECT-TYPE
     SYNTAX       RowStatus
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "Used to manage the creation and deletion of the 
             conceptual rows in this table.

             To create a row in this table, a manager must
             set this object to 'createAndGo'. To delete a row in this
             table, there should not be any port/tag associated with 
             this VLAN."
     ::= { wwpLeosVlanEntry 4 }  
 
 wwpLeosVlanMacLrnState OBJECT-TYPE
     SYNTAX       INTEGER {
     				enabled(1),
     				disabled(2)
     			  }
     MAX-ACCESS   read-write
     STATUS       current      
     DESCRIPTION
             "Setting this object will enable or disable MAC learning for the VLAN."
     DEFVAL		  { enabled }
     ::= { wwpLeosVlanEntry 5 } 

 wwpLeosVlanMacLrnOperState OBJECT-TYPE
     SYNTAX       INTEGER {
     				enabled(1),
     				disabled(2),
				vsOverride(3)
     			  }
     MAX-ACCESS   read-only
     STATUS       current      
     DESCRIPTION
             "Displays the operational status of MAC learning for the VLAN."
     DEFVAL		  { enabled }
     ::= { wwpLeosVlanEntry 6 }
 
 wwpLeosVlanTranslationVlan OBJECT-TYPE
     SYNTAX       INTEGER (0..24576)
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
             "The translated VLAN for the given ingress VLAN specified by 
             wwpLeosVlanId. Setting this MIB object to 0 will result in 
             unsetting the translation VLAN for given ingress VLAN wwpLeosVlanId."
     ::= { wwpLeosVlanEntry 7 }
          
 --
 --  The VLAN Membership Table
 --

 wwpLeosVlanTagMemberTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosVlanTagMemberEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION
            "The (conceptual) table listing the configuration parameters 
            for the members of the VLANs."
    ::= { wwpLeosVlan 5 }

 wwpLeosVlanTagMemberEntry OBJECT-TYPE
    SYNTAX     WwpLeosVlanTagMemberEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "An entry (conceptual row) in the wwpLeosVlanTagMemberTable."
    INDEX      { wwpLeosVlanId, wwpLeosVlanMemberPortId, wwpLeosVlanMemberTagId }
    ::= { wwpLeosVlanTagMemberTable 1 }

 WwpLeosVlanTagMemberEntry ::= SEQUENCE {   
    wwpLeosVlanMemberPortId             INTEGER,
    wwpLeosVlanMemberTagId              VlanTag,    
    wwpLeosVlanMemberStatus             RowStatus
 }
 
 wwpLeosVlanMemberPortId   OBJECT-TYPE
     SYNTAX           INTEGER(1..65535)
     MAX-ACCESS       read-only
     STATUS           current
     DESCRIPTION
             "The port ID to be associated with this VLAN."               
     ::= { wwpLeosVlanTagMemberEntry 1 }

 wwpLeosVlanMemberTagId   OBJECT-TYPE
     SYNTAX      VlanTag
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
             "The VLAN Tag ID used by the port on this
             VLAN. If the switch is being used as a traditional 
             Layer 2 device, then the value of 
             wwpLeosVlanMemberTagId should be same as wwpLeosVlanMemberId."
     ::= { wwpLeosVlanTagMemberEntry 2 } 
     
 wwpLeosVlanMemberStatus OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
             "Used to manage the creation and deletion of the 
             conceptual rows in this table.

             To create a row in this table, a manager must
             set this object to 'createAndGo'."
     ::= { wwpLeosVlanTagMemberEntry 4 }

 --
 -- VC Table
 -- 
 wwpLeosVlanCircuitTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosVlanCircuitEntry
     MAX-ACCESS not-accessible
     STATUS     deprecated
     DESCRIPTION
            "The (conceptual) table listing the virtual circuit table."
     ::= { wwpLeosVlan 6 }
     
 wwpLeosVlanCircuitEntry  OBJECT-TYPE
     SYNTAX       WwpLeosVlanCircuitEntry
     MAX-ACCESS   not-accessible
     STATUS       deprecated
     DESCRIPTION
             "The virtual circuit table entry indexed by virtual circuit index.
              To create an entry, use the SNMP multiple set operation because 
              wwpLeosCircuitVlanId, wwpLeosCircuitName and wwpLeosCircuitType 
              are mandatory while creating entry in the table."
     INDEX { wwpLeosCircuitIndex}
     ::= { wwpLeosVlanCircuitTable 1 }
     
 WwpLeosVlanCircuitEntry ::=  SEQUENCE {
     wwpLeosCircuitIndex                        INTEGER,
     wwpLeosCircuitVlanId                       VlanId,
     wwpLeosCircuitType                         INTEGER,
     wwpLeosCircuitName                         OCTET STRING,
     wwpLeosCircuitPriority                     INTEGER,
     wwpLeosCircuitDataTunnelState              INTEGER,
     wwpLeosCircuitCtrlProtocolTunnelState      INTEGER,
     wwpLeosCircuitNumEndPoints                 INTEGER,
     wwpLeosCircuitStatus                       RowStatus
 }
 
 wwpLeosCircuitIndex OBJECT-TYPE
     SYNTAX      INTEGER (1..65535)
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "This represents the virtual circuit index in the table."
     ::= { wwpLeosVlanCircuitEntry 1 } 
  
 wwpLeosCircuitVlanId OBJECT-TYPE
     SYNTAX      VlanId
     MAX-ACCESS  read-write
     STATUS      deprecated
     DESCRIPTION
        "This represents the VLAN ID associated with virtual circuit index in the table."
     ::= { wwpLeosVlanCircuitEntry 2 }
  
 wwpLeosCircuitType OBJECT-TYPE
     SYNTAX      INTEGER {
                        ethernet(1),
                        mpls(2)
                 }
     MAX-ACCESS  read-write
     STATUS      deprecated
     DESCRIPTION
        "This represents the type of virtual circuit eth or mpls."
     ::= { wwpLeosVlanCircuitEntry 3 }

 wwpLeosCircuitName OBJECT-TYPE
     SYNTAX      OCTET STRING (SIZE (0..16))
     MAX-ACCESS  read-write
     STATUS      deprecated
     DESCRIPTION
        "This represents the name associated with the virtual circuit."
     ::= { wwpLeosVlanCircuitEntry 4 }
 
 wwpLeosCircuitPriority OBJECT-TYPE
     SYNTAX      INTEGER (0..7)
     MAX-ACCESS  read-write
     STATUS      deprecated
     DESCRIPTION
        "This represents the 802.1D priority associated with the virtual circuit."
     ::= { wwpLeosVlanCircuitEntry 5 }
 
 wwpLeosCircuitDataTunnelState OBJECT-TYPE
     SYNTAX      INTEGER {
                        on(1),
                        off(2)
                 }
     MAX-ACCESS  read-write
     STATUS      deprecated
     DESCRIPTION
        "This represents the data tunnel state associated with the virtual circuit.
         Setting to 'on' enables the tunnel for data frames. Setting to 'off' disables 
         it."
     ::= { wwpLeosVlanCircuitEntry 6 }
 
 wwpLeosCircuitCtrlProtocolTunnelState OBJECT-TYPE
     SYNTAX      INTEGER {
                        on(1),
                        off(2)
                 }
     MAX-ACCESS  read-write
     STATUS      deprecated
     DESCRIPTION
        "This represents the control frame tunnel state associated with the virtual 
        circuit. Setting to 'on' enables the tunnel for control frames. Setting to 
        'off' disables it."
     ::= { wwpLeosVlanCircuitEntry 7 }
 
 wwpLeosCircuitNumEndPoints OBJECT-TYPE
     SYNTAX      INTEGER (0..65535)
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "This represents the number of end points associated with this entry."
     ::= { wwpLeosVlanCircuitEntry 8 }

 wwpLeosCircuitStatus OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      deprecated
     DESCRIPTION
        "Setting this object to 'createAndGo' will create the entry 
         and by default will enable control frame and data frame tunnel
         .       
         Setting this object to 'destroy' will delete the entry
         from the table for given VLAN."
     ::= { wwpLeosVlanCircuitEntry 9 }

 --
 -- Vc Port Exclusive list
 --  
 wwpLeosVlanCircuitPortExclusiveTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosVlanCircuitPortExclusiveEntry
     MAX-ACCESS not-accessible
     STATUS     deprecated
     DESCRIPTION
            "The (conceptual) table listing the layer 2 control frame tunnel  
             status on a VLAN."
     ::= { wwpLeosVlan 7 }
     
 wwpLeosVlanCircuitPortExclusiveEntry  OBJECT-TYPE
     SYNTAX       WwpLeosVlanCircuitPortExclusiveEntry
     MAX-ACCESS   not-accessible
     STATUS       deprecated
     DESCRIPTION
             "The layer 2 control frame protocol tunnel entry for the VLAN."
     INDEX { wwpLeosCircuitIndex, wwpLeosPortId}
     ::= { wwpLeosVlanCircuitPortExclusiveTable 1 }
     
 WwpLeosVlanCircuitPortExclusiveEntry ::=  SEQUENCE { 
     wwpLeosPortId                      INTEGER,
     wwpLeosPortExclusiveStatus         RowStatus
 }
 
 wwpLeosPortId OBJECT-TYPE
     SYNTAX      INTEGER (1..65535)
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "This specifies the port which is the end point for in this virtual circuit."
     ::= { wwpLeosVlanCircuitPortExclusiveEntry 1 }

 wwpLeosPortExclusiveStatus OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      deprecated
     DESCRIPTION
        "Setting this object to 'createAndGo' will create the entry 
         and designate the port as the end point of the virtual circuit.     
         Setting this object to 'destroy' will delete the entry
         from the table for the given virtual circuit."
     ::= { wwpLeosVlanCircuitPortExclusiveEntry 2 }

--
-- l2 control frame protocol table
--
wwpLeosVlanCircuitCtrlProtocolTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosVlanCircuitCtrlProtocolEntry
     MAX-ACCESS not-accessible
     STATUS     deprecated
     DESCRIPTION
            "The (conceptual) table listing the layer 2 control frame protocol status 
             tunnel for a given VLAN."
     ::= { wwpLeosVlan 8 }
     
 wwpLeosVlanCircuitCtrlProtocolEntry  OBJECT-TYPE
     SYNTAX       WwpLeosVlanCircuitCtrlProtocolEntry
     MAX-ACCESS   not-accessible
     STATUS       deprecated
     DESCRIPTION
             "The layer 2 control frame protocol tunnel entry for the VLAN."
     INDEX {wwpLeosCircuitIndex, wwpLeosVlanl2ProtocolNum}
     ::= { wwpLeosVlanCircuitCtrlProtocolTable 1 }
     
 WwpLeosVlanCircuitCtrlProtocolEntry ::=  SEQUENCE { 
     wwpLeosVlanl2ProtocolNum           INTEGER,
     wwpLeosVlanl2Type                  INTEGER
 }

  wwpLeosVlanl2ProtocolNum OBJECT-TYPE
     SYNTAX      INTEGER {                     
                     l28021x(1),
                     rstp(2),
                     ciscoCdp(3),
                     ciscoDtp(4),
                     ciscoPagp(5),
                     ciscoPvst(6),
                     ciscoUplinkFast(7),
                     ciscoUdlp(8),
                     ciscoVtp(9),
                     gvrp(10),
                     lacp(11),
                     lacpMarker(12),
                     lldp(13),
                     oam(14),
                     vlanBridge(15)                  
                 }
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "This object represent the list of protocols supported by 
         the device."
     ::= { wwpLeosVlanCircuitCtrlProtocolEntry 1 }

  wwpLeosVlanl2Type OBJECT-TYPE
     SYNTAX      INTEGER {
                     discard(1),
                     peer(2),
                     tunnel(3)               
                 }
     MAX-ACCESS  read-create
     STATUS      deprecated
     DESCRIPTION
        "Setting this object to 'discard' will cause wwpLeosProtocolNum
         frames arriving at the specified UNI to be discarded.  
         Setting this to 'peer' will cause the wwpLeosProtocolNum frame
         to be processed by the provider network and cause the provider 
         network to behave as a peer.  
         Setting this to 'tunnel' will cause the wwpLeosProtocolNum frame to be 
         tunneled."
     ::= { wwpLeosVlanCircuitCtrlProtocolEntry 2 }

--
-- l2 global stats
--
wwpLeosVlanCircuitStats OBJECT IDENTIFIER ::= { wwpLeosVlan 9 }

 wwpLeosVlanl2AllRxPkts OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies total number of packets ingressed on VLAN."
     ::= { wwpLeosVlanCircuitStats 1 }

 wwpLeosVlanl2AllTunneledPkts OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the total number of packets tunneled on the VLAN."
     ::= { wwpLeosVlanCircuitStats 2 }

 wwpLeosVlanl2AllPeerPkts OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the total number of packets peered on the VLAN."
     ::= { wwpLeosVlanCircuitStats 3 }

 wwpLeosVlanl2AllDiscardedPkts OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the total number of discarded packets on the VLAN."
     ::= { wwpLeosVlanCircuitStats 4 }

 wwpLeosVlanl2AllDecodedPkts OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the total number of packets tunneled and then 
        restored on the VLAN."
     ::= { wwpLeosVlanCircuitStats 5 }

 wwpLeosVlanl2AllDecodedFailures OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the total number of packets failed to 'untunnel'
        on the VLAN."
     ::= { wwpLeosVlanCircuitStats 6 }

 wwpLeosVlanl2AllTunneledSubcriberPortPkts OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the total number of tunneled packets received 
         on the subscriber port on the VLAN."
     ::= { wwpLeosVlanCircuitStats 7 }

--
-- l2 control frame protocol table stats
--
 wwpLeosVlanCircuitProtocolStatsTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosVlanCircuitProtocolStatsEntry
     MAX-ACCESS not-accessible
     STATUS     deprecated
     DESCRIPTION
            "The (conceptual) table listing the layer 2 control frame protocol 
            statistics for a given VLAN."
     ::= { wwpLeosVlan 10 }
     
 wwpLeosVlanCircuitProtocolStatsEntry  OBJECT-TYPE
     SYNTAX       WwpLeosVlanCircuitProtocolStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       deprecated
     DESCRIPTION
             "The layer 2 control frame protocol statistics entry for the VLAN."
     INDEX { wwpLeosCircuitIndex, wwpLeosVlanl2ProtocolNum}
     ::= { wwpLeosVlanCircuitProtocolStatsTable 1 }
     
 WwpLeosVlanCircuitProtocolStatsEntry ::=  SEQUENCE { 
     wwpLeosVlanl2RxPkts                        Counter32,
     wwpLeosVlanl2TunneledPkts                  Counter32,
     wwpLeosVlanl2PeerPkts                      Counter32,
     wwpLeosVlanl2DiscardedPkts                 Counter32,
     wwpLeosVlanl2DecodedPkts                   Counter32,
     wwpLeosVlanl2DecodedFailures               Counter32,
     wwpLeosVlanl2TunneledSubcriberPortPkts     Counter32
 }

 wwpLeosVlanl2RxPkts OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the number of packets ingressed matching the protocol."
     ::= { wwpLeosVlanCircuitProtocolStatsEntry 1 }

 wwpLeosVlanl2TunneledPkts OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the number of packets tunneled."
     ::= { wwpLeosVlanCircuitProtocolStatsEntry 2 }

 wwpLeosVlanl2PeerPkts OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the number of peered packets."
     ::= { wwpLeosVlanCircuitProtocolStatsEntry 3 }

 wwpLeosVlanl2DiscardedPkts OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the number of discarded packets."
     ::= { wwpLeosVlanCircuitProtocolStatsEntry 4 }

 wwpLeosVlanl2DecodedPkts OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the number of packets tunneled and then restored."
     ::= { wwpLeosVlanCircuitProtocolStatsEntry 5 }

 wwpLeosVlanl2DecodedFailures OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the number of packets failed to 'untunnel'."
     ::= { wwpLeosVlanCircuitProtocolStatsEntry 6 }

 wwpLeosVlanl2TunneledSubcriberPortPkts OBJECT-TYPE
     SYNTAX      Counter32
     MAX-ACCESS  read-only
     STATUS      deprecated
     DESCRIPTION
        "Specifies the number of tunneled packets received 
         on the subscriber port."
     ::= { wwpLeosVlanCircuitProtocolStatsEntry 7 }

--
-- VLAN stats
--       
 wwpLeosVlanStatsTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosVlanStatsEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION
            "A list of VLAN statistics entries."
     ::= { wwpLeosVlan 11 }
                 
 wwpLeosVlanStatsEntry OBJECT-TYPE
     SYNTAX       WwpLeosVlanStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
           "An entry in the VLAN stats table."
     INDEX { wwpLeosVlanStatsVlanId }
     ::= { wwpLeosVlanStatsTable 1 }
            
 WwpLeosVlanStatsEntry ::= SEQUENCE { 
     wwpLeosVlanStatsVlanId               VlanTag,
     wwpLeosVlanStatsCreateTime           TimeStamp,
     wwpLeosVlanStatsUniOctets            Counter64,
     wwpLeosVlanStatsUniPkts              Counter32,
     wwpLeosVlanStatsNonUniOctets         Counter64,
     wwpLeosVlanStatsNonUniPkts           Counter32,
     wwpLeosVlanStatsStatus               RowStatus,
     wwpLeosVlanStatsClear                TruthValue,
     wwpLeosVlanStatsPortId               INTEGER
}

 wwpLeosVlanStatsVlanId OBJECT-TYPE
    SYNTAX        VlanTag
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
          "The VLAN ID for this statistics entry."
    ::= { wwpLeosVlanStatsEntry 1 }

 wwpLeosVlanStatsCreateTime OBJECT-TYPE
    SYNTAX       TimeStamp
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The value of sysUpTime when this control entry was last
            activated. This value can be used by the management station to
            ensure that the entry has not been deleted and recreated
            between polls."
    ::= { wwpLeosVlanStatsEntry 2 }

 wwpLeosVlanStatsUniOctets OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of unicast bytes through this VLAN."
    ::= { wwpLeosVlanStatsEntry 3 }

 wwpLeosVlanStatsUniPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of unicast packets through this VLAN."
    ::= { wwpLeosVlanStatsEntry 4 }

wwpLeosVlanStatsNonUniOctets OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of broadcast or multicast bytes through this VLAN."
    ::= { wwpLeosVlanStatsEntry 5 }

 wwpLeosVlanStatsNonUniPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of broadcast or multicast packets through this VLAN."
    ::= { wwpLeosVlanStatsEntry 6 }
    
 wwpLeosVlanStatsStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Setting this object to 'createAndGo' will enable the collection 
         of statistics on the specified VLAN, clear the initial statistics
         bucket and add the entry to the table.
         Setting this object to 'destroy' will disable the collection of
         statistics and remove the entry from the table for given VLAN."
    ::= { wwpLeosVlanStatsEntry 7 }
    
 wwpLeosVlanStatsClear OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
          "Setting this object to True will reset the statistics of the
          given VLAN. Read on this object will always return False."
    DEFVAL          { false }
    ::= { wwpLeosVlanStatsEntry 8 }

 wwpLeosVlanStatsPortId OBJECT-TYPE
     SYNTAX           INTEGER(0..65535)
     MAX-ACCESS       read-write
     STATUS           current
     DESCRIPTION
             "The port ID to be associated with this VLAN statistics entry.
              When a portId is specified, VLAN statistics gathering	is restricted
              to the specified port. A port ID of zero means no port restriction.
             Support for this object is currently not implemented."
     DEFVAL		      { 0 }
     ::= { wwpLeosVlanStatsEntry 9 }          
--
-- VLAN Total stats
--       
 wwpLeosVlanTotalStatsTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosVlanTotalStatsEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION
            "A list of VLAN statistics entries."
     ::= { wwpLeosVlan 12 }   
      
 wwpLeosVlanTotalStatsEntry OBJECT-TYPE
     SYNTAX       WwpLeosVlanTotalStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
           "An entry in the VLAN statistics table."
     INDEX { wwpLeosVlanTotalStatsVlanId }
     ::= { wwpLeosVlanTotalStatsTable 1 }   
     
  WwpLeosVlanTotalStatsEntry ::= SEQUENCE { 
     wwpLeosVlanTotalStatsVlanId               VlanTag,
     wwpLeosVlanTotalStatsCreateTime           TimeStamp,
     wwpLeosVlanTotalStatsUniOctets            Counter64,
     wwpLeosVlanTotalStatsUniPkts              Counter32,
     wwpLeosVlanTotalStatsNonUniOctets         Counter64,
     wwpLeosVlanTotalStatsNonUniPkts           Counter32,
     wwpLeosVlanTotalStatsStatus               RowStatus,
     wwpLeosVlanTotalStatsClear                TruthValue,
     wwpLeosVlanTotalStatsPortId               INTEGER
}

 wwpLeosVlanTotalStatsVlanId OBJECT-TYPE
    SYNTAX        VlanTag
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
          "The VLAN ID for this statistics entry."
    ::= { wwpLeosVlanTotalStatsEntry 1 }

 wwpLeosVlanTotalStatsCreateTime OBJECT-TYPE
    SYNTAX       TimeStamp
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The value of sysUpTime when this control entry was last
            activated. This value can be used by the management station to
            ensure that the entry has not been deleted and recreated
            between polls."
    ::= { wwpLeosVlanTotalStatsEntry 2 }

 wwpLeosVlanTotalStatsUniOctets OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of unicast bytes through this VLAN."
    ::= { wwpLeosVlanTotalStatsEntry 3 }

 wwpLeosVlanTotalStatsUniPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of unicast packets through this VLAN."
    ::= { wwpLeosVlanTotalStatsEntry 4 }

wwpLeosVlanTotalStatsNonUniOctets OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of broadcast or multicast bytes through this VLAN."
    ::= { wwpLeosVlanTotalStatsEntry 5 }

 wwpLeosVlanTotalStatsNonUniPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of broadcast or multicast packets through this VLAN."
    ::= { wwpLeosVlanTotalStatsEntry 6 }
    
 wwpLeosVlanTotalStatsStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Setting this object to 'createAndGo' will enable the collection 
         of statistics on the specified VLAN, clear the initial statistics
         bucket and add the entry to the table.
         Setting this object to 'destroy' will disable the collection of
         statistics and remove the entry from the table for given VLAN."
    ::= { wwpLeosVlanTotalStatsEntry 7 }
    
 wwpLeosVlanTotalStatsClear OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
          "Setting this object to True resets the statistics of the given VLAN.
           Read on this object will always return False."
    DEFVAL          { false }
    ::= { wwpLeosVlanTotalStatsEntry 8 }

 wwpLeosVlanTotalStatsPortId   OBJECT-TYPE
     SYNTAX           INTEGER(0..65535)
     MAX-ACCESS       read-write
     STATUS           current
     DESCRIPTION
             "The port ID to be associated with this VLAN statistics entry.
             When a portId is specified, the VLAN statistics gathering is restricted
             to the specified port. A port ID of zero means no port restriction.
             Support for this object is currently not implemented."
     DEFVAL		      { 0 }
     ::= { wwpLeosVlanTotalStatsEntry 9 } 

--
-- VLAN Translation Table.
--       
 wwpLeosVlanTranslationTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosVlanTranslationEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION
            "VLAN translation table."
     ::= { wwpLeosVlan 13 }   
      
 wwpLeosVlanTranslationEntry OBJECT-TYPE
     SYNTAX       WwpLeosVlanTranslationEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
           "An entry in the VLAN translation table."
     INDEX { wwpLeosVlanTranslationPgId, wwpLeosVlanTranslationFrameVid }
     ::= { wwpLeosVlanTranslationTable 1 }   
     
  WwpLeosVlanTranslationEntry ::= SEQUENCE { 
     wwpLeosVlanTranslationPgId               INTEGER,
     wwpLeosVlanTranslationFrameVid			  VlanTag,
     wwpLeosVlanTranslationVlanId				  VlanTag,
     wwpLeosVlanTranslationStatus		  RowStatus
    }
    
  wwpLeosVlanTranslationPgId		OBJECT-TYPE
  	SYNTAX		INTEGER (1..65535)
  	MAX-ACCESS	not-accessible
  	STATUS		current
  	DESCRIPTION
  			"Logical port interface for which the translation applies."
  	::= {wwpLeosVlanTranslationEntry 1}
  	
  wwpLeosVlanTranslationFrameVid	OBJECT-TYPE
  	SYNTAX		VlanTag
  	MAX-ACCESS	not-accessible
  	STATUS		current
  	DESCRIPTION
  		"Frame Ingres-egress vlan-id."
  	::= { wwpLeosVlanTranslationEntry 2 }
  	
  wwpLeosVlanTranslationVlanId		OBJECT-TYPE
  	SYNTAX		VlanTag
  	MAX-ACCESS	read-create
  	STATUS		current
  	DESCRIPTION	
  		"Assign/stamp to this internal VLAN."
  	::= { wwpLeosVlanTranslationEntry 3 }
  	
  wwpLeosVlanTranslationStatus		OBJECT-TYPE
  	SYNTAX		RowStatus
  	MAX-ACCESS	read-create
  	STATUS		current
  	DESCRIPTION
  		"Setting this object to CreateAndGo will create a VLAn tranlsation entry. Setting 
  		this object to destroy will delete a translation entry."
  	::= { wwpLeosVlanTranslationEntry 4 }



--
-- EPR
--
 wwpLeosVlanEPRTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosVlanEPREntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION
            "The (conceptual) table listing the egress port
            restriction parameters for the VLAN."  
     ::= { wwpLeosVlanEPR 1 }
     
 wwpLeosVlanEPREntry  OBJECT-TYPE
     SYNTAX       WwpLeosVlanEPREntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "The egress port restriction entry for a VLAN."
     INDEX { wwpLeosVlanId }
     ::= { wwpLeosVlanEPRTable 1 }
     
 WwpLeosVlanEPREntry ::=  SEQUENCE { 
     wwpLeosVlanEPRState             INTEGER    
 } 
 
 wwpLeosVlanEPRState OBJECT-TYPE
     SYNTAX      INTEGER {
                    enable(1),
                    disable(2)
                 }
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "Setting this object to 'enable' will enable the 
         egress port restriction on this VLAN. Setting this 
         object to 'disable' will disable the egress port 
         restriction on this VLAN."
      DEFVAL { disable } 
     ::= { wwpLeosVlanEPREntry 1 }
     
 --
 -- wwpLeosVlanEPRGrpMemTable
 --  
 wwpLeosVlanEPRGrpMemTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosVlanEPRGrpMemEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION
            "The (conceptual) table listing the egress port
            restriction group for the VLAN members."  
     ::= { wwpLeosVlanEPR 2 }
     
 wwpLeosVlanEPRGrpMemEntry  OBJECT-TYPE
     SYNTAX       WwpLeosVlanEPRGrpMemEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "The egress port restriction group entry for the
              VLAN members."
     INDEX { wwpLeosVlanId, wwpLeosVlanMemberPortId, wwpLeosVlanMemberTagId }
     ::= { wwpLeosVlanEPRGrpMemTable 1 }
     
 WwpLeosVlanEPRGrpMemEntry ::=  SEQUENCE {
     wwpLeosVlanEPRGrpName      INTEGER     
 }
 
 wwpLeosVlanEPRGrpName OBJECT-TYPE
     SYNTAX      INTEGER {
                    groupA(1),
                    groupB(2)
                 }
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "Setting this object will assign the specified group to 
        the given port-tag-vlan combination."      
     ::= { wwpLeosVlanEPRGrpMemEntry 1 }
      
 --
 -- wwpLeosVlanEPRGrpAccessTable
 --  
 wwpLeosVlanEPRGrpAccessTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosVlanEPRGrpAccessEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION
            "The (conceptual) table listing the group access
             for the given VLAN."  
     ::= { wwpLeosVlanEPR 3 }
     
 wwpLeosVlanEPRGrpAccessEntry  OBJECT-TYPE
     SYNTAX       WwpLeosVlanEPRGrpAccessEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Entry for the group access for the given VLAN."
     INDEX { wwpLeosVlanId }
     ::= { wwpLeosVlanEPRGrpAccessTable 1 }
     
 WwpLeosVlanEPRGrpAccessEntry ::=  SEQUENCE {
     wwpLeosVlanEPRGrpAAccess           INTEGER,
     wwpLeosVlanEPRGrpBAccess           INTEGER
 }
 
 wwpLeosVlanEPRGrpAAccess OBJECT-TYPE
     SYNTAX      INTEGER {
                    groupA(1),
                    groupB(2),
                    groupAB(3)
                 }
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "Setting this object will allow group A members for this VLAN
         to talk to specified group."      
     ::= { wwpLeosVlanEPRGrpAccessEntry 1 }
 
 wwpLeosVlanEPRGrpBAccess OBJECT-TYPE
     SYNTAX      INTEGER {
                    groupA(1),
                    groupB(2),
                    groupAB(3)
                 }
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "Setting this object will allow group B members for this VLAN
         to talk to specified group."      
     ::= { wwpLeosVlanEPRGrpAccessEntry 2 } 


 END

