-- This file was included in WWP MIB release 04-07-01-0008
 --
 -- WWP-LEOS-RSVPTE-MIB.my
 --

 WWP-LEOS-RSVPTE-MIB DEFINITIONS ::= BEGIN

 IMPORTS 		
   TimeTicks, Integer32, Unsigned32, OBJECT-TYPE, MODULE-IDENTITY			
	FROM SNMPv2-SMI			
   DisplayString, MacAddress, TEXTUAL-CONVENTION, RowStatus, TruthValue			
	FROM SNMPv2-TC							
   wwpModulesLeos		
	FROM WWP-SMI;

	
 wwpLeosRsvpteMIB MODULE-IDENTITY
	    LAST-UPDATED "200104031700Z"
	    ORGANIZATION "Ciena, Inc"
	    CONTACT-INFO
		    "   Mib Meister
		  			115 North Sullivan Road
					Spokane Valley, WA 99037
		        	USA		 		
		        	Phone:  +1 509 242 9000
					Email:  support@ciena.com"
	    DESCRIPTION
		    "This MIB module is for the RSVP-TE configuration for MPLS tunnels"
	    REVISION    "200508081700Z"
	    DESCRIPTION
		    "Initial creation."
	    ::= { wwpModulesLeos 30 }

 --
 -- Node definitions
 --
	
 wwpLeosRsvpteMIBObjects OBJECT IDENTIFIER ::= { wwpLeosRsvpteMIB 1 }
 wwpLeosRsvpteObjects    OBJECT IDENTIFIER ::= { wwpLeosRsvpteMIBObjects 1 }
 wwpLeosRsvpte           OBJECT IDENTIFIER ::= { wwpLeosRsvpteMIBObjects 2 }

 wwpLeosRsvpteAdminStatus OBJECT-TYPE
      SYNTAX      INTEGER {
                      enable(1),
                      disable(2)
                  }
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "The desired administrative state of RSVP-TE."
      ::= { wwpLeosRsvpteObjects 1 }

 wwpLeosRsvpteOperStatus OBJECT-TYPE
      SYNTAX      INTEGER {
                      up(1),          -- active
                      down(2),        -- inactive
                      goingUp(3),     -- activating
                      goingDown(4),   -- deactivating
                      actFailed(5)    -- activation failed
                  }
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "The current operational state of RSVP-TE."
      ::= { wwpLeosRsvpteObjects 2 }
      
 wwpLeosRsvpteRetryInterval OBJECT-TYPE
      SYNTAX      Unsigned32 (3..65)
      UNITS       "seconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "The persistent tunnel retry interval.
           This is the interval between the first failure of a persistent
           tunnel and the first attempt to re-establish the tunnel.
           This cannot be changed while admin status is enable or oper status is up"
      DEFVAL      { 3 }
      ::= { wwpLeosRsvpteObjects 3 }

 wwpLeosRsvpteRetryInfiniteState OBJECT-TYPE
      SYNTAX      INTEGER {
      				on(1),
      				off(2)
      				}      
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "The persistent tunnel retry infinity.
           This is the State which when on will trigger RSVP-TE to try to restore the tunnels
           infinite times. This object can only be set if RSVP-TE is globally disabled."
      DEFVAL      { on }
      ::= { wwpLeosRsvpteObjects 4 }

 wwpLeosRsvpteRetryMax OBJECT-TYPE
      SYNTAX      INTEGER (1..255)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "The maximum number of retry attempts that will be made before a
           persistent tunnel is deemed inoperable.  Once in this state,
           a management agent should set mplsTunnelAdminStatus to 'up' to
           attempt to reestablish the tunnel.
           This field is not used when wwpLeosRsvpteRetryInfiniteState is on "
      DEFVAL      { 10 }
      ::= { wwpLeosRsvpteObjects 5 }


 wwpLeosRsvpteRefreshInterval OBJECT-TYPE
      SYNTAX      Integer32
      UNITS       "milliseconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
       "This RSVP-TE value, R,  which is used to set the average
        interval between refresh path and resv messages."
      DEFVAL { 30000 }
      ::= { wwpLeosRsvpteObjects 6 }

 wwpLeosRsvpteRefreshMultiple OBJECT-TYPE
      SYNTAX      Integer32 (1..214783647)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
       "The RSVP-TE value, K, which is the number of unresponded Path
        or Resv refresh attempts which must be made, spaced by
        the refresh interval before the state is deemed to have
        timed out."
      DEFVAL { 3 }
      ::= { wwpLeosRsvpteObjects 7 }

 wwpLeosRsvpteRfrshSlewDenom OBJECT-TYPE
      SYNTAX      Integer32 (1..214783647)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
       "The denominator of the fraction, SlewMax, which is the
        maximum allowable increase in the refresh interval, R, to
        prevent state timeout while changing R.  R is increased by
        this fraction until it reaches the new desired value."
      DEFVAL { 10 }
      ::= { wwpLeosRsvpteObjects 8 }

 wwpLeosRsvpteRfrshSlewNumerator OBJECT-TYPE
      SYNTAX      Integer32 (1..214783647)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
       "The numerator of the fraction, SlewMax, which is the maximum
        allowable increase in the refresh interval, R, to prevent
        state timeout while changing R.  R is increased by this
        fraction until it reaches the new desired value."
      DEFVAL { 3 }
      ::= { wwpLeosRsvpteObjects 9 }

 wwpLeosRsvpteBlockadeMultiple OBJECT-TYPE
      SYNTAX      Integer32 (1..214783647)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
       "The RSVP-TE value, Kb, which is the number of refresh timeout
        periods after which blockade state is deleted."
      DEFVAL { 2 }
      ::= { wwpLeosRsvpteObjects 10 }

 wwpLeosRsvpteLSPSetupPriority OBJECT-TYPE
      SYNTAX      Integer32 (0..7)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
       "The setup priority to apply to LSPs which are not
        signalling this parameter.  0 represents the highest
        priority, 7 the lowest.  The value of this object must be
        numerically more or equal (so lower or equal priority)
        than the value of the holding priority object."
      DEFVAL { 4 }
      ::= { wwpLeosRsvpteObjects 11 }

 wwpLeosRsvpteLSPHoldingPriority OBJECT-TYPE
      SYNTAX      Integer32 (0..7)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
      "The holding priority to apply to LSPs which are not
       signalling this parameter.  0 represents the highest
       priority, 7 the lowest.  The value of this object must be
       numerically less or equal (so higher or equal priority)
       than the value of the holding priority object."
      DEFVAL { 3 }
      ::= { wwpLeosRsvpteObjects 12 }

 wwpLeosRsvpteUseHopByHop OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "A flag to indicate that RSVP-TE should use the hop by hop
         addressing scheme for PATH and PATH-TEAR messages it
         sends.  If set then the IP addresses used in the IP header
         of PATH messages forwarded by RSVP-TE set source as the
         local outgoing interface IP address, and destination as
         the next hop router IP address."
      DEFVAL { false }
      ::= { wwpLeosRsvpteObjects 13 }

 wwpLeosRsvpteRestartCapable OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "A flag to indicate whether the local node should advertise
           itself as restart capable."
      DEFVAL { false }
      ::= { wwpLeosRsvpteObjects 14 }

 wwpLeosRsvpteRestartTime OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "The time in milliseconds that the local node takes to
         restart RSVP-TE and the communication channel used for
         RSVP-TE communication.  This is advertised to neighbors in
         the Restart_Cap object in Hello messages.

         Only used if wwpLeosRsvpteRestartCapable is set to true."
      DEFVAL { 10000 }
      ::= { wwpLeosRsvpteObjects 15 }

 wwpLeosRsvpteRecoveryTime OBJECT-TYPE
      SYNTAX      Unsigned32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "The period of time in milliseconds that the local node
         would like neighbors to take to resyncronize RSVP-TE and
         MPLS forwarding information after the re-establishment of
         Hello connectivity.  This is advertised to neighbors in
         the Restart_Cap object in Hello messages.

         A value of zero indicates that the node does not support
         resynchronization following failure of the local node.

         A value of 0xFFFFFFFF indicates an infinite recovery time.

         Only used if wwpLeosRsvpteRestartCapable is set to true."
      DEFVAL { 10000 }
      ::= { wwpLeosRsvpteObjects 16 }

 wwpLeosRsvpteMinPeerRestart OBJECT-TYPE
      SYNTAX      Integer32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
        "The mininum period of time in milliseconds that RSVP-TE
         should wait for a restart capable neighbor to regain
         Hello connectivity before invoking procedures related to
         communication loss.

         RSVP-TE will wait for the maximum of this time and the
         restart_time advertised in the RESTART_CAP object in Hello
         messages from the neighbor."
      DEFVAL { 0 }
      ::= { wwpLeosRsvpteObjects 17 }

 wwpLeosRsvpteIfTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF WwpLeosRsvpteIfEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
          "A table of interfaces that RSVP-TE can be enabled on."
      ::= { wwpLeosRsvpte 1 }
    
 wwpLeosRsvpteIfEntry OBJECT-TYPE
      SYNTAX      WwpLeosRsvpteIfEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
          "WWP Descr."
           INDEX       { wwpLeosRsvpteIfIndex }
      ::= { wwpLeosRsvpteIfTable 1 }

 WwpLeosRsvpteIfEntry ::= SEQUENCE {
      wwpLeosRsvpteIfIndex           INTEGER,
      wwpLeosRsvpteIfName            DisplayString,
      wwpLeosRsvpteIfIpAddr          IpAddress,
      wwpLeosRsvpteIfMtu             INTEGER,
      wwpLeosRsvpteIfAdminStatus     INTEGER,
      wwpLeosRsvpteIfOperStatus      INTEGER
 }

 wwpLeosRsvpteIfName OBJECT-TYPE
      SYNTAX      DisplayString (SIZE (0..32))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "Interface Name"
      ::= { wwpLeosRsvpteIfEntry 1 }

 wwpLeosRsvpteIfIndex OBJECT-TYPE
      SYNTAX      INTEGER (1..4096)
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
          "Interface Index"
      ::= { wwpLeosRsvpteIfEntry 2 }

 wwpLeosRsvpteIfIpAddr OBJECT-TYPE
      SYNTAX      IpAddress
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "Interface IP Address"
      ::= { wwpLeosRsvpteIfEntry 3 }

 wwpLeosRsvpteIfMtu OBJECT-TYPE
      SYNTAX      INTEGER (1500..9216)
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "RSVP-TE Interface MTU"
      ::= { wwpLeosRsvpteIfEntry 4 }

 wwpLeosRsvpteIfAdminStatus OBJECT-TYPE
      SYNTAX      INTEGER {
                     enable(1),
                     disable(2)
                  }
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
          "Desired RSVP-TE status on this Interface"
      ::= { wwpLeosRsvpteIfEntry 5 }

 wwpLeosRsvpteIfOperStatus OBJECT-TYPE
      SYNTAX      INTEGER {
                     up(1),
                     down(2)
                  }
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "RSVP-TE Operational Status on this Interface"
      ::= { wwpLeosRsvpteIfEntry 6 }


 END
 
--
-- WWP-LEOS-RSVPTE-MIB
--
