-- This file was included in WWP MIB release 04-07-01-0008
-- file: IANAifType-MIB.my (RFC 1573)
-- Changes:
--     Extracted from RFC1573 - the combined IANAifType-MIB & IF-MIB
--     Added the following import: mib-2 from SNMPv2-SMI
--     Removed the following unneeded import: OBJECT-TYPE from
--         SNMPv2-SMI.
--     Added new enum values (22-apr-1998: dtp)
--
-- dperkins@snmpinfo.com: 27-dec-1997

   IANAifType-MIB DEFINITIONS ::= BEGIN

   IMPORTS
       MODULE-IDENTITY, mib-2
           FROM SNMPv2-SMI
       TEXTUAL-CONVENTION
           FROM SNMPv2-TC;

   ianaifType MODULE-IDENTITY
       LAST-UPDATED "9804220000Z"
       ORGANIZATION "IANA"
       CONTACT-INFO

                  "        Internet Assigned Numbers Authority

                   Postal: USC/Information Sciences Institute
                           4676 Admiralty Way, Marina del Rey, CA 90292

                   Tel:    +1  310 822 1511
                   E-Mail: iana@isi.edu"
       DESCRIPTION
               "The MIB module which defines the IANAifType textual
               convention, and thus the enumerated values of the
               ifType object defined in MIB-II's ifTable."
       REVISION "9804220000Z"
           DESCRIPTION "Added latest types"
       ::= { mib-2 30 }


   IANAifType ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
               "This data type is used as the syntax of the ifType
               object in the (updated) definition of MIB-II's
               ifTable.

               The definition of this textual convention with the
               addition of newly assigned values is published
               periodically by the IANA, in either the Assigned
               Numbers RFC, or some derivative of it specific to
               Internet Network Management number assignments.  (The
               latest arrangements can be obtained by contacting the
               IANA.)

               Requests for new values should be made to IANA via
               email (iana@isi.edu).

               The relationship between the assignment of ifType
               values and of OIDs to particular media-specific MIBs
               is solely the purview of IANA and is subject to change
               without notice.  Quite often, a media-specific MIB's
               OID-subtree assignment within MIB-II's 'transmission'
               subtree will be the same as its ifType value.
               However, in some circumstances this will not be the
               case, and implementors must not pre-assume any
               specific relationship between ifType values and
               transmission subtree OIDs."
       SYNTAX  INTEGER {
                   other(1),          -- none of the following
                   regular1822(2),    -- BBN Report 1822
                   hdh1822(3),        -- BBN Report 1822
                   ddnX25(4),         -- BBN Report 1822
                   rfc877x25(5),
                   ethernetCsmacd(6),
                   iso88023Csmacd(7),  -- CSMACD like Objects
                   iso88024TokenBus(8), -- Token Bus like Objects
                   iso88025TokenRing(9), -- Token Ring like Objects
                   iso88026Man(10),
                   starLan(11),
                   proteon10Mbit(12),
                   proteon80Mbit(13),
                   hyperchannel(14),
                   fddi(15),
                   lapb(16),
                   sdlc(17),
                   ds1(18),           -- DS1/E1 (RFC 1406)
                   e1(19),            -- obsolete
                   basicISDN(20),
                   primaryISDN(21),
                   propPointToPointSerial(22), -- proprietary serial
                   ppp(23),
                   softwareLoopback(24),
                   eon(25),            -- CLNP over IP (RFC 1070)
                   ethernet3Mbit(26),
                   nsip(27),           -- XNS over IP
                   slip(28),           -- generic SLIP
                   ultra(29),          -- ULTRA technologies
                   ds3(30),            -- T-3
                   sip(31),            -- SMDS
                   frameRelay(32),     -- DTE only
                   rs232(33),
                   para(34),           -- parallel-port
                   arcnet(35),         -- arcnet
                   arcnetPlus(36),     -- arcnet plus
                   atm(37),            -- ATM cells
                   miox25(38),
                   sonet(39),          -- SONET or SDH
                   x25ple(40),         -- X.25 packet level
                   iso88022llc(41),    -- 802.2 LLC
                   localTalk(42),
                   smdsDxi(43),
                   frameRelayService(44),  -- Frame relay DCE
                   v35(45),
                   hssi(46),
                   hippi(47),
                   modem(48),          -- Generic modem
                   aal5(49),           -- AAL5 over ATM
                   sonetPath(50),
                   sonetVT(51),
                   smdsIcip(52),       -- SMDS InterCarrier Interface
                   propVirtual(53),    -- proprietary virtual/internal
                   propMultiplexor(54), -- proprietary multiplexing

                   ieee80212(55),      -- 100BaseVG
                   fibreChannel(56),   -- Fibre Channel
                   hippiInterface(57), -- HIPPI interfaces     
                   frameRelayInterconnect(58), -- Obsolete use either
                                               -- frameRelay(32) or 
                                               -- frameRelayService(44).
                   aflane8023(59),     -- ATM Emulated LAN for 802.3
                   aflane8025(60),     -- ATM Emulated LAN for 802.5
                   cctEmul(61),        -- ATM Emulated circuit 
                   fastEther(62),      -- Fast Ethernet (100BaseT)
                   isdn(63),           -- ISDN and X.25
                   v11(64),            -- CCITT V.11/X.21
                   v36(65),            -- CCITT V.36
                   g703at64k(66),      -- CCITT G703 at 64Kbps
                   g703at2mb(67),      -- Obsolete see DS1-MIB
                   qllc(68),           -- SNA QLLC
                   fastEtherFX(69),    -- Fast Ethernet (100BaseFX)
                   channel(70),        -- channel
                   ieee80211(71),      -- radio spread spectrum
                   ibm370parChan(72),  -- IBM System 360/370 OEMI Channel
                   escon(73),          -- IBM Enterprise Systems Connection
                   dlsw(74),           -- Data Link Switching
                   isdns(75),          -- ISDN S/T interface
                   isdnu(76),          -- ISDN U interface
                   lapd(77),           -- Link Access Protocol D
                   ipSwitch(78),       -- IP Switching Objects
                   rsrb(79),           -- Remote Source Route Bridging
                   atmLogical(80),     -- ATM Logical Port
                   ds0(81),            -- Digital Signal Level 0
                   ds0Bundle(82),      -- group of ds0s on the same ds1
                   bsc(83),            -- Bisynchronous Protocol
                   async(84),          -- Asynchronous Protocol
                   cnr(85),            -- Combat Net Radio
                   iso88025Dtr(86),    -- ISO 802.5r DTR
                   eplrs(87),          -- Ext Pos Loc Report Sys
                   arap(88),           -- Appletalk Remote Access Protocol
                   propCnls(89),       -- Proprietary Connectionless Protocol
                   hostPad(90),        -- CCITT-ITU X.29 PAD Protocol
                   termPad(91),        -- CCITT-ITU X.3 PAD Facility
                   frameRelayMPI(92),  -- Multiproto Interconnect over FR
                   x213(93),           -- CCITT-ITU X213
                   adsl(94),           -- Asymmetric Digital Subscriber Loop
                   radsl(95),          -- Rate-Adapt. Digital Subscriber Loop
                   sdsl(96),           -- Symmetric Digital Subscriber Loop
                   vdsl(97),           -- Very H-Speed Digital Subscrib. Loop
                   iso88025CRFPInt(98), -- ISO 802.5 CRFP
                   myrinet(99),        -- Myricom Myrinet
                   voiceEM(100),       -- voice recEive and transMit
                   voiceFXO(101),      -- voice Foreign Exchange Office
                   voiceFXS(102),      -- voice Foreign Exchange Station
                   voiceEncap(103),    -- voice encapsulation
                   voiceOverIp(104),   -- voice over IP encapsulation
                   atmDxi(105),        -- ATM DXI
                   atmFuni(106),       -- ATM FUNI
                   atmIma(107),        -- ATM IMA
                   pppMultilinkBundle(108),  -- PPP Multilink Bundle
                   ipOverCdlc(109),    -- IBM ipOverCdlc
                   ipOverClaw(110),    -- IBM Common Link Access to Workstn 
                   stackToStack(111),  -- IBM stackToStack
                   virtualIpAddress(112), -- IBM VIPA 
                   mpc(113),           -- IBM multi-protocol channel support
                   ipOverAtm(114),     -- IBM ipOverAtm
                   iso88025Fiber(115), -- ISO 802.5j Fiber Token Ring
                   tdlc(116),          -- IBM twinaxial data link control
                   gigabitEthernet(117), -- Gigabit Ethernet
                   hdlc(118),          -- HDLC
                   lapf(119),          -- LAP F
                   v37(120),           -- V.37
                   x25mlp(121),        -- Multi-Link Protocol
                   x25huntGroup(122),  -- X25 Hunt Group
                   transpHdlc(123),    -- Transp HDLC
                   interleave(124),    -- Interleave channel
                   fast(125),          -- Fast channel
                   ip(126),            -- IP (for APPN HPR in IP networks)
                   docsCableMaclayer(127), -- CATV Mac Layer 
                   docsCableDownstream(128), -- CATV Downstream interface
                   docsCableUpstream(129), -- CATV Upstream interface
                   a12MppSwitch(130),  -- Avalon Parallel Processor
                   tunnel(131),        -- Encapsulation interface
                   coffee(132),        -- coffee pot
                   ces(133),           -- Circiut Emulation Service
                   atmSubInterface(134), -- ATM Sub Interface
                   l2vlan(135),        -- Layer 2 Virtual LAN using 802.1Q
                   l3ipvlan(136),      -- Layer 3 Virtual LAN - IP Protocol
                   l3ipxvlan(137)     -- Layer 3 Virtual LAN - IPX Prot.
                   }

   END

