-- This file was included in WWP MIB release 04-07-01-0008
      SNMP-COMMUNITY-MIB DEFINITIONS ::= BEGIN

      IMPORTS
          IpAddress,
          MODULE-IDENTITY,
          OBJECT-TYPE,
          Integer32,
          snmpModules
              FROM SNMPv2-SMI
          RowStatus,
          StorageType
              FROM SNMPv2-TC
          SnmpAdminString,
          SnmpEngineID
              FROM SNMP-FRAMEWORK-MIB
          SnmpTagValue,
          snmpTargetAddrEntry
              FROM SNMP-TARGET-MIB
          MODULE-COMPLIANCE,
          OBJECT-GROUP
              FROM SNMPv2-CONF;

      snmpCommunityMIB MODULE-IDENTITY
          LAST-UPDATED "200003060000Z"          -- 6 Mar 2000, midnight
          ORGANIZATION "SNMPv3 Working Group"
          CONTACT-INFO "WG-email:   snmpv3@lists.tislabs.com
                        Subscribe:  majordomo@lists.tislabs.com
                                    In msg body:  subscribe snmpv3

                        Chair:      Russ Mundy
                                    TIS Labs at Network Associates
                        Postal:     3060 Washington Rd
                                    Glenwood MD 21738
                                    USA
                        Email:      mundy@tislabs.com
                        phone:      +1-301-854-6889

                        Co-editor:  Rob Frye
                                    CoSine Communications
                        Postal:     1200 Bridge Parkway
                                    Redwood City, CA 94065
                                    USA
                        E-mail:     rfrye@cosinecom.com
                        Phone:      +1 703 725 1130

                        Co-editor:  David B. Levi
                                    Nortel Networks
                        Postal:     3505 Kesterwood Drive
                                    Knoxville, TN 37918
                        E-mail:     dlevi@nortelnetworks.com
                        Phone:      +1 423 686 0432

                        Co-editor:  Shawn A. Routhier
                                    Integrated Systems Inc.
                        Postal:     333 North Ave 4th Floor
                                    Wakefield, MA 01880
                        E-mail:     sar@epilogue.com
                        Phone:      +1 781 245 0804

                        Co-editor:  Bert Wijnen
                                    Lucent Technologies
                        Postal:     Schagen 33
                                    3461 GL Linschoten
                                    Netherlands
                        Email:      bwijnen@lucent.com
                        Phone:      +31-348-407-775
                       "

              DESCRIPTION
                  "This MIB module defines objects to help support coexistence
                   between SNMPv1, SNMPv2, and SNMPv3."
              REVISION "200003060000Z" -- 6 Mar 2000
              DESCRIPTION "This version published as RFC 2576."
              REVISION "199905130000Z" -- 13 May 1999
              DESCRIPTION "The Initial Revision"
          ::= { snmpModules 18 }

      -- Administrative assignments ****************************************

      snmpCommunityMIBObjects     OBJECT IDENTIFIER ::= { snmpCommunityMIB 1 }
      snmpCommunityMIBConformance OBJECT IDENTIFIER ::= { snmpCommunityMIB 2 }

      --
      -- The snmpCommunityTable contains a database of community strings.
      -- This table provides mappings between community strings, and the
      -- parameters required for View-based Access Control.
      --

      snmpCommunityTable OBJECT-TYPE
          SYNTAX       SEQUENCE OF SnmpCommunityEntry
          MAX-ACCESS   not-accessible
          STATUS       current
          DESCRIPTION
              "The table of community strings configured in the SNMP
               engine's Local Configuration Datastore (LCD)."
          ::= { snmpCommunityMIBObjects 1 }

      snmpCommunityEntry OBJECT-TYPE
          SYNTAX       SnmpCommunityEntry
          MAX-ACCESS   not-accessible
          STATUS       current
          DESCRIPTION
              "Information about a particular community string."
          INDEX       { IMPLIED snmpCommunityIndex }
          ::= { snmpCommunityTable 1 }

      SnmpCommunityEntry ::= SEQUENCE {
          snmpCommunityIndex               SnmpAdminString,
          snmpCommunityName                OCTET STRING,
          snmpCommunitySecurityName        SnmpAdminString,
          snmpCommunityContextEngineID     SnmpEngineID,
          snmpCommunityContextName         SnmpAdminString,
          snmpCommunityTransportTag        SnmpTagValue,
          snmpCommunityStorageType         StorageType,
          snmpCommunityStatus              RowStatus
      }

      snmpCommunityIndex OBJECT-TYPE
          SYNTAX      SnmpAdminString (SIZE(1..32))
          MAX-ACCESS  not-accessible
          STATUS      current
          DESCRIPTION
              "The unique index value of a row in this table."
          ::= { snmpCommunityEntry 1 }

      snmpCommunityName OBJECT-TYPE
          SYNTAX       OCTET STRING
          MAX-ACCESS   read-create
          STATUS       current
          DESCRIPTION
              "The community string for which a row in this table
               represents a configuration."
          ::= { snmpCommunityEntry 2 }

      snmpCommunitySecurityName OBJECT-TYPE
          SYNTAX       SnmpAdminString (SIZE(1..32))
          MAX-ACCESS   read-create
          STATUS       current
          DESCRIPTION
              "A human readable string representing the corresponding
               value of snmpCommunityName in a Security Model
               independent format."
          ::= { snmpCommunityEntry 3 }

      snmpCommunityContextEngineID OBJECT-TYPE
          SYNTAX       SnmpEngineID







          MAX-ACCESS   read-create
          STATUS       current
          DESCRIPTION
              "The contextEngineID indicating the location of the
               context in which management information is accessed
               when using the community string specified by the
               corresponding instance of snmpCommunityName.

               The default value is the snmpEngineID of the entity in
               which this object is instantiated."
          ::= { snmpCommunityEntry 4 }

      snmpCommunityContextName OBJECT-TYPE
          SYNTAX       SnmpAdminString (SIZE(0..32))
          MAX-ACCESS   read-create
          STATUS       current
          DESCRIPTION
              "The context in which management information is accessed
               when using the community string specified by the corresponding
               instance of snmpCommunityName."
          DEFVAL      { ''H }   -- the empty string
          ::= { snmpCommunityEntry 5 }

      snmpCommunityTransportTag OBJECT-TYPE
          SYNTAX       SnmpTagValue
          MAX-ACCESS   read-create
          STATUS       current
          DESCRIPTION
              "This object specifies a set of transport endpoints
               from which an agent will accept management requests.
               If a management request containing this community
               is received on a transport endpoint other than the
               transport endpoints identified by this object, the
               request is deemed unauthentic.

               The transports identified by this object are specified
               in the snmpTargetAddrTable.  Entries in that table
               whose snmpTargetAddrTagList contains this tag value
               are identified.

               If the value of this object has zero-length, transport
               endpoints are not checked when authenticating messages
               containing this community string."
          DEFVAL      { ''H }   -- the empty string
          ::= { snmpCommunityEntry 6 }

      snmpCommunityStorageType OBJECT-TYPE







          SYNTAX       StorageType
          MAX-ACCESS   read-create
          STATUS       current
          DESCRIPTION
              "The storage type for this conceptual row in the
               snmpCommunityTable.  Conceptual rows having the value
               'permanent' need not allow write-access to any
               columnar object in the row."
          ::= { snmpCommunityEntry 7 }

      snmpCommunityStatus OBJECT-TYPE
          SYNTAX       RowStatus
          MAX-ACCESS   read-create
          STATUS       current
          DESCRIPTION
              "The status of this conceptual row in the snmpCommunityTable.

               An entry in this table is not qualified for activation
               until instances of all corresponding columns have been
               initialized, either through default values, or through
               Set operations.  The snmpCommunityName and
               snmpCommunitySecurityName objects must be explicitly set.

               There is no restriction on setting columns in this table
               when the value of snmpCommunityStatus is active(1)."
          ::= { snmpCommunityEntry 8 }

      --
      -- The snmpTargetAddrExtTable
      --

      snmpTargetAddrExtTable OBJECT-TYPE
          SYNTAX       SEQUENCE OF SnmpTargetAddrExtEntry
          MAX-ACCESS   not-accessible
          STATUS       current
          DESCRIPTION
              "The table of mask and mms values associated with the
               snmpTargetAddrTable.

               The snmpTargetAddrExtTable augments the
               snmpTargetAddrTable with a transport address mask value
               and a maximum message size value.  The transport address
               mask allows entries in the snmpTargetAddrTable to define
               a set of addresses instead of just a single address.
               The maximum message size value allows the maximum
               message size of another SNMP entity to be configured for
               use in SNMPv1 (and SNMPv2c) transactions, where the
               message format does not specify a maximum message size."
          ::= { snmpCommunityMIBObjects 2 }

      snmpTargetAddrExtEntry OBJECT-TYPE
          SYNTAX       SnmpTargetAddrExtEntry
          MAX-ACCESS   not-accessible







          STATUS       current
          DESCRIPTION
              "Information about a particular mask and mms value."
          AUGMENTS       { snmpTargetAddrEntry }
          ::= { snmpTargetAddrExtTable 1 }

      SnmpTargetAddrExtEntry ::= SEQUENCE {
          snmpTargetAddrTMask              OCTET STRING,
          snmpTargetAddrMMS                Integer32
      }

      snmpTargetAddrTMask OBJECT-TYPE
          SYNTAX      OCTET STRING (SIZE (0..255))
          MAX-ACCESS  read-create
          STATUS      current
          DESCRIPTION
              "The mask value associated with an entry in the
               snmpTargetAddrTable.  The value of this object must
               have the same length as the corresponding instance of
               snmpTargetAddrTAddress, or must have length 0.  An
               attempt to set it to any other value will result in
               an inconsistentValue error.

               The value of this object allows an entry in the
               snmpTargetAddrTable to specify multiple addresses.
               The mask value is used to select which bits of
               a transport address must match bits of the corresponding
               instance of snmpTargetAddrTAddress, in order for the
               transport address to match a particular entry in the
               snmpTargetAddrTable.  Bits which are 1 in the mask
               value indicate bits in the transport address which
               must match bits in the snmpTargetAddrTAddress value.
               Bits which are 0 in the mask indicate bits in the
               transport address which need not match.  If the
               length of the mask is 0, the mask should be treated
               as if all its bits were 1 and its length were equal
               to the length of the corresponding value of
               snmpTargetAddrTable.

               This object may not be modified while the value of the
               corresponding instance of snmpTargetAddrRowStatus is
               active(1).  An attempt to set this object in this case
               will result in an inconsistentValue error."
          DEFVAL { ''H }
          ::= { snmpTargetAddrExtEntry 1 }

      snmpTargetAddrMMS OBJECT-TYPE
          SYNTAX      Integer32 (484..65535)
          MAX-ACCESS  read-create
          STATUS      current
          DESCRIPTION
              "The maximum message size value associated with an entry
               in the snmpTargetAddrTable."
          DEFVAL { 2048 }
          ::= { snmpTargetAddrExtEntry 2 }

      --
      -- The snmpTrapAddress and snmpTrapCommunity objects are included
      -- in notifications that are forwarded by a proxy, which were
      -- originally received as SNMPv1 Trap messages.
      --

      snmpTrapAddress OBJECT-TYPE
          SYNTAX      IpAddress
          MAX-ACCESS  accessible-for-notify
          STATUS      current
          DESCRIPTION
              "The value of the agent-addr field of a Trap PDU which
               is forwarded by a proxy forwarder application using
               an SNMP version other than SNMPv1.  The value of this







               object SHOULD contain the value of the agent-addr field
               from the original Trap PDU as generated by an SNMPv1
               agent."
          ::= { snmpCommunityMIBObjects 3 }

      snmpTrapCommunity OBJECT-TYPE
          SYNTAX      OCTET STRING
          MAX-ACCESS  accessible-for-notify
          STATUS      current
          DESCRIPTION
              "The value of the community string field of an SNMPv1
               message containing a Trap PDU which is forwarded by
               a proxy forwarder application using an SNMP version
               other than SNMPv1.  The value of this object SHOULD
               contain the value of the community string field from
               the original SNMPv1 message containing a Trap PDU as
               generated by an SNMPv1 agent."
          ::= { snmpCommunityMIBObjects 4 }

      -- Conformance Information *******************************************

      snmpCommunityMIBCompliances OBJECT IDENTIFIER
                                  ::= { snmpCommunityMIBConformance 1 }
      snmpCommunityMIBGroups      OBJECT IDENTIFIER
                                  ::= { snmpCommunityMIBConformance 2 }

      -- Compliance statements

      snmpCommunityMIBCompliance MODULE-COMPLIANCE
          STATUS       current
          DESCRIPTION
              "The compliance statement for SNMP engines which
               implement the SNMP-COMMUNITY-MIB."

          MODULE       -- this module
              MANDATORY-GROUPS { snmpCommunityObjectGroup }

              OBJECT           snmpCommunityName
              MIN-ACCESS       read-only
              DESCRIPTION     "Write access is not required."

              OBJECT           snmpCommunitySecurityName
              MIN-ACCESS       read-only
              DESCRIPTION     "Write access is not required."

              OBJECT           snmpCommunityContextEngineID
              MIN-ACCESS       read-only
              DESCRIPTION     "Write access is not required."

              OBJECT           snmpCommunityContextName
              MIN-ACCESS       read-only
              DESCRIPTION     "Write access is not required."

              OBJECT           snmpCommunityTransportTag
              MIN-ACCESS       read-only
              DESCRIPTION     "Write access is not required."

              OBJECT           snmpCommunityStorageType
              MIN-ACCESS       read-only
              DESCRIPTION     "Write access is not required."

              OBJECT           snmpCommunityStatus
              MIN-ACCESS       read-only
              DESCRIPTION     "Write access is not required."

          ::= { snmpCommunityMIBCompliances 1 }

      snmpProxyTrapForwardCompliance MODULE-COMPLIANCE
          STATUS       current
          DESCRIPTION
              "The compliance statement for SNMP engines which
               contain a proxy forwarding application which is
               capable of forwarding SNMPv1 traps using SNMPv2c
               or SNMPv3."
          MODULE       -- this module
              MANDATORY-GROUPS { snmpProxyTrapForwardGroup }
          ::= { snmpCommunityMIBCompliances 2 }

      snmpCommunityObjectGroup OBJECT-GROUP
          OBJECTS {
              snmpCommunityIndex,
              snmpCommunityName,
              snmpCommunitySecurityName,
              snmpCommunityContextEngineID,
              snmpCommunityContextName,
              snmpCommunityTransportTag,
              snmpCommunityStorageType,
              snmpCommunityStatus,
              snmpTargetAddrTMask,
              snmpTargetAddrMMS
          }
          STATUS       current
          DESCRIPTION
              "A collection of objects providing for configuration
               of community strings for SNMPv1 (and SNMPv2c) usage."
          ::= { snmpCommunityMIBGroups 1 }

      snmpProxyTrapForwardGroup OBJECT-GROUP
          OBJECTS {
              snmpTrapAddress,
              snmpTrapCommunity
          }
          STATUS       current
          DESCRIPTION
              "Objects which are used by proxy forwarding applications
               when translating traps between SNMP versions.  These are
               used to preserve SNMPv1-specific information when
               translating to SNMPv2c or SNMPv3."
          ::= { snmpCommunityMIBGroups 3 }

      END
