-- This file was included in WWP MIB release 04-07-01-0008
LLDP-EXT-DOT1-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32
        FROM SNMPv2-SMI
    TruthValue
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    lldpExtensions, lldpLocPortNum, 
    lldpRemTimeMark, lldpRemLocalPortNum, lldpRemIndex, 
    lldpPortConfigEntry
        FROM LLDP-MIB
   VlanId
        FROM Q-BRIDGE-MIB;

lldpXdot1MIB MODULE-IDENTITY
    LAST-UPDATED "200505060000Z" -- May 06, 2005
    ORGANIZATION "IEEE 802.1 Working Group"
    CONTACT-INFO 
            "  WG-URL: http://grouper.ieee.org/groups/802/1/index.html
             WG-EMail: stds-802-1@ieee.org

              Contact: Paul Congdon
               Postal: Hewlett-Packard Company
                       8000 Foothills Blvd. 
                       Roseville, CA 95747
                       USA
                  Tel: +1-916-785-5753
               E-mail: paul_congdon@hp.com"
    DESCRIPTION
            "The LLDP Management Information Base extension module for
            IEEE 802.1 organizationally defined discovery information.

            In order to assure the uniqueness of the LLDP-MIB,
            lldpXdot1MIB is branched from lldpExtensions using OUI value
            as the node.  An OUI/'company_id' is a 24 bit globally unique
            assigned number referenced by various standards.

            Copyright (C) IEEE (2005).  This version of this MIB module
            is published as Annex F.7.1 of IEEE Std 802.1AB-2005;
            see the standard itself for full legal notices."
    REVISION        "200505060000Z" -- May 06, 2005
    DESCRIPTION
            "Published as part of IEEE Std 802.1AB-2005 initial version."
-- OUI for IEEE 802.1 is 32962 (00-80-C2) 
   ::= { lldpExtensions 32962 }

------------------------------------------------------------------------------
------------------------------------------------------------------------------
--
-- Organizationally Defined Information Extension - IEEE 802.1
--
------------------------------------------------------------------------------
------------------------------------------------------------------------------

lldpXdot1Objects    OBJECT IDENTIFIER ::= { lldpXdot1MIB 1 }

-- LLDP IEEE 802.1 extension MIB groups
lldpXdot1Config     OBJECT IDENTIFIER ::= { lldpXdot1Objects 1 }
lldpXdot1LocalData  OBJECT IDENTIFIER ::= { lldpXdot1Objects 2 }
lldpXdot1RemoteData OBJECT IDENTIFIER ::= { lldpXdot1Objects 3 }

------------------------------------------------------------------------------
-- IEEE 802.1 - Configuration
------------------------------------------------------------------------------
--
-- lldpXdot1ConfigPortVlanTable : configure the transmission of the 
--                                Port VLAN-ID TLVs on set of ports.
--

lldpXdot1ConfigPortVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot1ConfigPortVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A table that controls selection of LLDP Port VLAN-ID TLVs
            to be transmitted on individual ports."
    ::= { lldpXdot1Config 1 }

lldpXdot1ConfigPortVlanEntry  OBJECT-TYPE
    SYNTAX      LldpXdot1ConfigPortVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "LLDP configuration information that controls the
            transmission of IEEE 802.1 organizationally defined Port
            VLAN-ID TLV on LLDP transmission capable ports.

            This configuration object augments the lldpPortConfigEntry of
            the LLDP-MIB, therefore it is only present along with the port
            configuration defined by the associated lldpPortConfigEntry
            entry.

            Each active lldpConfigEntry must be restored from non-volatile
            storage (along with the corresponding lldpPortConfigEntry)
            after a re-initialization of the management system."
    AUGMENTS { lldpPortConfigEntry }
    ::= { lldpXdot1ConfigPortVlanTable 1 }

LldpXdot1ConfigPortVlanEntry ::= SEQUENCE {
      lldpXdot1ConfigPortVlanTxEnable  TruthValue
}

lldpXdot1ConfigPortVlanTxEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The lldpXdot1ConfigPortVlanTxEnable, which is defined as
            a truth value and configured by the network management,
            determines whether the IEEE 802.1 organizationally defined
            port VLAN TLV transmission is allowed on a given LLDP
            transmission capable port.

            The value of this object must be restored from non-volatile
            storage after a re-initialization of the management system."
    REFERENCE 
            "IEEE 802.1AB-2005 10.2.1.1"
    DEFVAL  { false }
    ::= { lldpXdot1ConfigPortVlanEntry 1 }
               
--
-- lldpXdot1ConfigVlanNameTable : configure the transmission of the 
--                                VLAN name instances on set of ports.
--

lldpXdot1ConfigVlanNameTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot1ConfigVlanNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The table that controls selection of LLDP VLAN name TLV
            instances to be transmitted on individual ports."
    ::= { lldpXdot1Config 2 }

lldpXdot1ConfigVlanNameEntry  OBJECT-TYPE
    SYNTAX      LldpXdot1ConfigVlanNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "LLDP configuration information that specifies the set of
            ports (represented as a PortList) on which the Local System
            VLAN name instance will be transmitted.

            This configuration object augments the lldpLocVlanEntry,
            therefore it is only present along with the VLAN Name instance
            contained in the associated lldpLocVlanNameEntry entry.

            Each active lldpXdot1ConfigVlanNameEntry must be restored
            from non-volatile storage (along with the corresponding
            lldpXdot1LocVlanNameEntry) after a re-initialization of the
            management system."
    AUGMENTS { lldpXdot1LocVlanNameEntry }
    ::= { lldpXdot1ConfigVlanNameTable 1 }

LldpXdot1ConfigVlanNameEntry ::= SEQUENCE {
      lldpXdot1ConfigVlanNameTxEnable  TruthValue 
}

lldpXdot1ConfigVlanNameTxEnable  OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
            "The boolean value that indicates whether the corresponding
            Local System VLAN name instance will be transmitted on the
            port defined by the given lldpXdot1LocVlanNameEntry.

            The value of this object must be restored from non-volatile
            storage after a re-initialization of the management system."
    REFERENCE 
            "IEEE 802.1AB-2005 10.2.1.1"
    DEFVAL  { false }
    ::= { lldpXdot1ConfigVlanNameEntry 1 }

--
-- lldpXdot1ConfigProtoVlanTable : configure the transmission of the 
--                                 protocol VLAN instances on set
--                                 of ports.
--

lldpXdot1ConfigProtoVlanTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot1ConfigProtoVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The table that controls selection of LLDP Port and Protocol
            VLAN ID TLV instances to be transmitted on individual ports."
    ::= { lldpXdot1Config 3 }

lldpXdot1ConfigProtoVlanEntry  OBJECT-TYPE
    SYNTAX      LldpXdot1ConfigProtoVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "LLDP configuration information that specifies the set of
            ports (represented as a PortList) on which the Local System
            Protocol VLAN instance will be transmitted.

            This configuration object augments the lldpXdot1LocVlanEntry,
            therefore it is only present along with the Port and
            Protocol VLAN ID instance contained in the associated
            lldpXdot1LocVlanEntry entry.

            Each active lldpXdot1ConfigProtoVlanEntry must be restored
            from non-volatile storage (along with the corresponding
            lldpXdot1LocProtoVlanEntry) after a re-initialization of
            the management system."

    AUGMENTS { lldpXdot1LocProtoVlanEntry }
    ::= { lldpXdot1ConfigProtoVlanTable 1 }

LldpXdot1ConfigProtoVlanEntry ::= SEQUENCE {
      lldpXdot1ConfigProtoVlanTxEnable   TruthValue
}

lldpXdot1ConfigProtoVlanTxEnable OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
            "The boolean value that indicates whether the corresponding
            Local System Port and Protocol VLAN instance will
            be transmitted on the port defined by the given
            lldpXdot1LocProtoVlanEntry.

            The value of this object must be restored from non-volatile
            storage after a re-initialization of the management system."
    REFERENCE 
            "IEEE 802.1AB-2005 10.2.1.1"
    DEFVAL  { false }
    ::= { lldpXdot1ConfigProtoVlanEntry 1 }

--
-- lldpXdot1ConfigProtocolTable : configure the transmission of the 
--                                protocol instances on set
--                                of ports.
--

lldpXdot1ConfigProtocolTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot1ConfigProtocolEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The table that controls selection of LLDP Protocol 
            TLV instances to be transmitted on individual ports."
    ::= { lldpXdot1Config 4 }

lldpXdot1ConfigProtocolEntry  OBJECT-TYPE
    SYNTAX      LldpXdot1ConfigProtocolEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "LLDP configuration information that specifies the set of
            ports (represented as a PortList) on which the Local System
            Protocol instance will be transmitted.

            This configuration object augments the lldpXdot1LocProtoEntry,
            therefore it is only present along with the Protocol instance
            contained in the associated lldpXdot1LocProtoEntry entry.

            Each active lldpXdot1ConfigProtocolEntry must be restored
            from non-volatile storage (along with the corresponding
            lldpXdot1LocProtocolEntry) after a re-initialization of the
            management system."
    AUGMENTS { lldpXdot1LocProtocolEntry }
    ::= { lldpXdot1ConfigProtocolTable 1 }

LldpXdot1ConfigProtocolEntry ::= SEQUENCE {
      lldpXdot1ConfigProtocolTxEnable   TruthValue
}

lldpXdot1ConfigProtocolTxEnable  OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
            "The boolean value that indicates whether the corresponding
            Local System Protocol Identity instance will be transmitted
            on the port defined by the given lldpXdot1LocProtocolEntry.

            The value of this object must be restored from non-volatile
            storage after a re-initialization of the management system."
    REFERENCE 
            "IEEE 802.1AB-2005 10.2.1.1"
    DEFVAL  { false }
    ::= { lldpXdot1ConfigProtocolEntry 1 }

------------------------------------------------------------------------------
-- IEEE 802.1 - Local System Information
------------------------------------------------------------------------------
lldpXdot1LocTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot1LocEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one row per port for IEEE 802.1
            organizationally defined LLDP extension on the local system
            known to this agent."
    ::= { lldpXdot1LocalData 1 }

lldpXdot1LocEntry  OBJECT-TYPE
    SYNTAX      LldpXdot1LocEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Information about IEEE 802.1 organizationally defined
            LLDP extension."
    INDEX   { lldpLocPortNum }
    ::= { lldpXdot1LocTable 1 }

LldpXdot1LocEntry ::= SEQUENCE {
              lldpXdot1LocPortVlanId         Integer32
} 

lldpXdot1LocPortVlanId OBJECT-TYPE
    SYNTAX      Integer32(0|1..4094)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The integer value used to identify the port's VLAN identifier
            associated with the local system.   A value of zero shall
            be used if the system either does not know the PVID or does
            not support port-based VLAN operation."
    REFERENCE 
            "IEEE 802.1AB-2005 F.2.1"
    ::= { lldpXdot1LocEntry 1 }

--
-- lldpXdot1LocProtoVlanTable: Port and Protocol VLAN information 
--

lldpXdot1LocProtoVlanTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot1LocProtoVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one or more rows per Port and Protocol
            VLAN information about the local system."
    ::= { lldpXdot1LocalData 2 }

lldpXdot1LocProtoVlanEntry OBJECT-TYPE
    SYNTAX      LldpXdot1LocProtoVlanEntry 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Port and protocol VLAN ID Information about a particular
            port component.  There may be multiple port and protocol VLANs,
            identified by a particular lldpXdot1LocProtoVlanId, configured
            on the given port."
    INDEX   { lldpLocPortNum,
              lldpXdot1LocProtoVlanId }
    ::= { lldpXdot1LocProtoVlanTable 1 }

LldpXdot1LocProtoVlanEntry ::= SEQUENCE {
      lldpXdot1LocProtoVlanId        Integer32,
      lldpXdot1LocProtoVlanSupported TruthValue,
      lldpXdot1LocProtoVlanEnabled   TruthValue
}

lldpXdot1LocProtoVlanId  OBJECT-TYPE
    SYNTAX      Integer32(0|1..4094)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The integer value used to identify the port and protocol
            VLANs associated with the given port associated with the
            local system.  A value of zero shall be used if the system
            either does not know the protocol VLAN ID (PPVID) or does
            not support port and protocol VLAN operation."
    REFERENCE 
            "IEEE 802.1AB-2005 F.3.2"
    ::= { lldpXdot1LocProtoVlanEntry 1 }

lldpXdot1LocProtoVlanSupported  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value used to indicate whether the given port
            (associated with the local system) supports port and protocol
            VLANs."
    REFERENCE 
            "IEEE 802.1AB-2005 F.3.1"
    ::= { lldpXdot1LocProtoVlanEntry 2 }

lldpXdot1LocProtoVlanEnabled  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value used to indicate whether the port and
            protocol VLANs are enabled on the given port associated with
            the local system."
    REFERENCE 
            "IEEE 802.1AB-2005 F.3.1"
    ::= { lldpXdot1LocProtoVlanEntry 3 }

--
-- lldpXdot1LocVlanNameTable : VLAN name information about the local system
--

lldpXdot1LocVlanNameTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot1LocVlanNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one or more rows per IEEE 802.1Q VLAN
            name information on the local system known to this agent."
    ::= { lldpXdot1LocalData 3 }

lldpXdot1LocVlanNameEntry OBJECT-TYPE
    SYNTAX      LldpXdot1LocVlanNameEntry 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "VLAN name Information about a particular port component.
            There may be multiple VLANs, identified by a particular
            lldpXdot1LocVlanId, configured on the given port."
    INDEX   { lldpLocPortNum,
              lldpXdot1LocVlanId }
    ::= { lldpXdot1LocVlanNameTable 1 }

LldpXdot1LocVlanNameEntry ::= SEQUENCE {
      lldpXdot1LocVlanId     VlanId,
      lldpXdot1LocVlanName   SnmpAdminString
}

lldpXdot1LocVlanId  OBJECT-TYPE
    SYNTAX      VlanId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The integer value used to identify the IEEE 802.1Q 
            VLAN IDs with which the given port is compatible."
    REFERENCE 
            "IEEE 802.1AB-2005 F.4.2"
    ::= { lldpXdot1LocVlanNameEntry 1 }

lldpXdot1LocVlanName  OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The string value used to identify VLAN name identified by the
            Vlan Id associated with the given port on the local system.

            This object should contain the value of the dot1QVLANStaticName
            object (defined in IETF RFC 2674) identified with the given
            lldpXdot1LocVlanId."
    REFERENCE 
            "IEEE 802.1AB-2005 F.4.4"
    ::= { lldpXdot1LocVlanNameEntry 2 }

--
-- lldpXdot1LocProtocolTable : Protocol Identity information 
--

lldpXdot1LocProtocolTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot1LocProtocolEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one or more rows per protocol identity
            information on the local system known to this agent."
    REFERENCE 
            "IEEE 802.1AB-2005 F.5"
    ::= { lldpXdot1LocalData 4 }

lldpXdot1LocProtocolEntry  OBJECT-TYPE
    SYNTAX      LldpXdot1LocProtocolEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Information about particular protocols that are accessible
            through the given port component.

            There may be multiple protocols, identified by particular
            lldpXdot1ProtocolIndex, and lldpLocPortNum."
    REFERENCE 
            "IEEE 802.1AB-2005 F.5"
    INDEX   { lldpLocPortNum,
              lldpXdot1LocProtocolIndex }
    ::= { lldpXdot1LocProtocolTable 1 }

LldpXdot1LocProtocolEntry ::= SEQUENCE {
      lldpXdot1LocProtocolIndex Integer32,
      lldpXdot1LocProtocolId    OCTET STRING
}

lldpXdot1LocProtocolIndex  OBJECT-TYPE
    SYNTAX      Integer32(1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This object represents an arbitrary local integer value used
            by this agent to identify a particular protocol identity."
    ::= { lldpXdot1LocProtocolEntry 1 }

lldpXdot1LocProtocolId  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (1..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The octet string value used to identify the protocols
            associated with the given port of the local system."
    REFERENCE 
            "IEEE 802.1AB-2005 F.5.3"
    ::= { lldpXdot1LocProtocolEntry 2 }


------------------------------------------------------------------------------
-- IEEE 802.1 - Remote System Information
------------------------------------------------------------------------------
lldpXdot1RemTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot1RemEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one or more rows per physical network
            connection known to this agent.  The agent may wish to
            ensure that only one lldpXdot1RemEntry is present for
            each local port, or it may choose to maintain multiple
            lldpXdot1RemEntries for the same local port."
    ::= { lldpXdot1RemoteData 1 }

lldpXdot1RemEntry OBJECT-TYPE
    SYNTAX      LldpXdot1RemEntry 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Information about a particular port component."
    INDEX   { lldpRemTimeMark,
              lldpRemLocalPortNum,
              lldpRemIndex }
    ::= { lldpXdot1RemTable 1 }

LldpXdot1RemEntry ::= SEQUENCE {
              lldpXdot1RemPortVlanId         Integer32
}

lldpXdot1RemPortVlanId OBJECT-TYPE
    SYNTAX      Integer32(0|1..4094)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The integer value used to identify the port's VLAN identifier
            associated with the remote system.  if the remote system
            either does not know the PVID or does not support port-based
            VLAN operation, the value of lldpXdot1RemPortVlanId should
            be zero."
    REFERENCE 
            "IEEE 802.1AB-2005 F.2.1"
    ::= { lldpXdot1RemEntry 1 }

lldpXdot1RemProtoVlanTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot1RemProtoVlanEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one or more rows per Port and Protocol
            VLAN information about the remote system, received on the
            given port."
    ::= { lldpXdot1RemoteData 2 }

lldpXdot1RemProtoVlanEntry OBJECT-TYPE
    SYNTAX      LldpXdot1RemProtoVlanEntry 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Port and protocol VLAN name Information about a particular
            port component.  There may be multiple protocol VLANs,
            identified by a particular lldpXdot1RemProtoVlanId, configured
            on the remote system."
    INDEX   { lldpRemTimeMark,
              lldpRemLocalPortNum,
              lldpRemIndex,
              lldpXdot1RemProtoVlanId }
    ::= { lldpXdot1RemProtoVlanTable 1 }

LldpXdot1RemProtoVlanEntry ::= SEQUENCE {
      lldpXdot1RemProtoVlanId        Integer32,
      lldpXdot1RemProtoVlanSupported TruthValue,
      lldpXdot1RemProtoVlanEnabled   TruthValue
}

lldpXdot1RemProtoVlanId  OBJECT-TYPE
    SYNTAX      Integer32(0|1..4094)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The integer value used to identify the port and protocol
            VLANs associated with the given port associated with the
            remote system.

            If port and protocol VLANs are not supported on the given
            port associated with the remote system, or if the port is
            not enabled with any port and protocol VLAN, the value of
            lldpXdot1RemProtoVlanId should be zero."
    REFERENCE 
            "IEEE 802.1AB-2005 F.3.2"
    ::= { lldpXdot1RemProtoVlanEntry 1 }

lldpXdot1RemProtoVlanSupported  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value used to indicate whether the given port
            (associated with the remote system) is capable of supporting
            port and protocol VLANs."
    REFERENCE 
            "IEEE 802.1AB-2005 F.3.1"
    ::= { lldpXdot1RemProtoVlanEntry 2 }

lldpXdot1RemProtoVlanEnabled  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The truth value used to indicate whether the port and
            protocol VLANs are enabled on the given port associated with
            the remote system."
    REFERENCE 
            "IEEE 802.1AB-2005 F.3.1"
    ::= { lldpXdot1RemProtoVlanEntry 3 }


-- 
-- lldpXdot1RemVlanNameTable : VLAN name information of the remote 
--                             systems
--

lldpXdot1RemVlanNameTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot1RemVlanNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one or more rows per IEEE 802.1Q VLAN
            name information about the remote system, received on the
            given port."
    REFERENCE 
            "IEEE 802.1AB-2005 F.4"
    ::= { lldpXdot1RemoteData 3 }

lldpXdot1RemVlanNameEntry OBJECT-TYPE
    SYNTAX      LldpXdot1RemVlanNameEntry 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "VLAN name Information about a particular port component.
            There may be multiple VLANs, identified by a particular
            lldpXdot1RemVlanId, received on the given port."
    INDEX   { lldpRemTimeMark,
              lldpRemLocalPortNum,
              lldpRemIndex,
              lldpXdot1RemVlanId }
    ::= { lldpXdot1RemVlanNameTable 1 }

LldpXdot1RemVlanNameEntry ::= SEQUENCE {
      lldpXdot1RemVlanId     VlanId,
      lldpXdot1RemVlanName   SnmpAdminString
}

lldpXdot1RemVlanId  OBJECT-TYPE
    SYNTAX      VlanId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The integer value used to identify the IEEE 802.1Q 
            VLAN IDs with which the given port of the remote system
            is compatible."
    REFERENCE 
            "IEEE 802.1AB-2005 F.4.2"
    ::= { lldpXdot1RemVlanNameEntry 1 }

lldpXdot1RemVlanName  OBJECT-TYPE
    SYNTAX      SnmpAdminString (SIZE(1..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The string value used to identify VLAN name identified by the 
            VLAN Id associated with the remote system."
    REFERENCE 
            "IEEE 802.1AB-2005 F.4.4"
    ::= { lldpXdot1RemVlanNameEntry 2 }

--
-- lldpXdot1RemProtocolTable : Protocol information of the remote systems
--

lldpXdot1RemProtocolTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF LldpXdot1RemProtocolEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains one or more rows per protocol information
            about the remote system, received on the given port."
    ::= { lldpXdot1RemoteData 4 }

lldpXdot1RemProtocolEntry  OBJECT-TYPE
    SYNTAX      LldpXdot1RemProtocolEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Protocol information about a particular port component.
            There may be multiple protocols, identified by a particular
            lldpXdot1ProtocolIndex, received on the given port."
    INDEX   { lldpRemTimeMark,
              lldpRemLocalPortNum,
              lldpRemIndex,
              lldpXdot1RemProtocolIndex }
    ::= { lldpXdot1RemProtocolTable 1 }

LldpXdot1RemProtocolEntry ::= SEQUENCE {
      lldpXdot1RemProtocolIndex Integer32,
      lldpXdot1RemProtocolId    OCTET STRING
}

lldpXdot1RemProtocolIndex  OBJECT-TYPE
    SYNTAX      Integer32(1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This object represents an arbitrary local integer value used
            by this agent to identify a particular protocol identity."
    ::= { lldpXdot1RemProtocolEntry 1 }

lldpXdot1RemProtocolId  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (1..255))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The octet string value used to identify the protocols
            associated with the given port of remote system."
    REFERENCE 
            "IEEE 802.1AB-2005 F.5.3"
    ::= { lldpXdot1RemProtocolEntry 2 }


------------------------------------------------------------------------------
-- Conformance Information
------------------------------------------------------------------------------

lldpXdot1Conformance OBJECT IDENTIFIER ::= { lldpXdot1MIB 2 }
lldpXdot1Compliances OBJECT IDENTIFIER ::= { lldpXdot1Conformance 1 }
lldpXdot1Groups      OBJECT IDENTIFIER ::= { lldpXdot1Conformance 2 }

-- compliance statements

lldpXdot1Compliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for SNMP entities which implement
            the IEEE 802.1 organizationally defined LLDP extension MIB."
    MODULE  -- this module
        MANDATORY-GROUPS { lldpXdot1ConfigGroup, 
                           lldpXdot1LocSysGroup,
                           lldpXdot1RemSysGroup
        }
    ::= { lldpXdot1Compliances 1 }

-- MIB groupings

lldpXdot1ConfigGroup    OBJECT-GROUP
    OBJECTS {
        lldpXdot1ConfigPortVlanTxEnable,
        lldpXdot1ConfigVlanNameTxEnable,
        lldpXdot1ConfigProtoVlanTxEnable,
        lldpXdot1ConfigProtocolTxEnable
    }
    STATUS  current
    DESCRIPTION
            "The collection of objects which are used to configure the
            IEEE 802.1 organizationally defined LLDP extension
            implementation behavior.

            This group is mandatory for agents which implement the 
            IEEE 802.1 organizationally defined LLDP extension."
    ::= { lldpXdot1Groups 1 }

lldpXdot1LocSysGroup  OBJECT-GROUP
    OBJECTS {
        lldpXdot1LocPortVlanId,
        lldpXdot1LocProtoVlanSupported,
        lldpXdot1LocProtoVlanEnabled,
        lldpXdot1LocVlanName,
        lldpXdot1LocProtocolId 
    }
    STATUS  current
    DESCRIPTION
            "The collection of objects which are used to represent 
            IEEE 802.1 organizationally defined LLDP extension associated
            with the Local Device Information.
            
            This group is mandatory for agents which implement the 
            IEEE 802.1 organizationally defined LLDP extension in the
            TX mode."
    ::= { lldpXdot1Groups 2 }

lldpXdot1RemSysGroup  OBJECT-GROUP
    OBJECTS {
        lldpXdot1RemPortVlanId,
        lldpXdot1RemProtoVlanSupported,
        lldpXdot1RemProtoVlanEnabled,
        lldpXdot1RemVlanName,
        lldpXdot1RemProtocolId 
    }
    STATUS  current
    DESCRIPTION
            "The collection of objects which are used to represent LLDP
            802.1 organizational extension Local Device Information.
            
            This group is mandatory for agents which implement the 
            LLDP 802.1 organizational extension in the RX mode."
    ::= { lldpXdot1Groups 3 }

END
