-- This file was included in WWP MIB release 04-07-01-0008
 --
 -- WWP-LEOS-TABLE-CHG-NOTIF-MIB.my
 --
 --

 WWP-LEOS-TABLE-CHG-NOTIF-MIB DEFINITIONS ::= BEGIN

 IMPORTS 		
   Integer32, Unsigned32, OBJECT-TYPE, MODULE-IDENTITY			
	FROM SNMPv2-SMI			
   DisplayString, MacAddress, RowStatus, TEXTUAL-CONVENTION, TruthValue			
	FROM SNMPv2-TC
   AddressFamilyNumbers
	FROM IANA-ADDRESS-FAMILY-NUMBERS-MIB
   wwpModules, wwpModulesLeos		
	FROM WWP-SMI;

	
 wwpLeosTableChgNotifMIB MODULE-IDENTITY
	 LAST-UPDATED "200203120000Z"
	 ORGANIZATION "Ciena, Inc"
	 CONTACT-INFO
		  "   Mib Meister
		  			115 North Sullivan Road
					Spokane Valley, WA 99037
		        	USA		 		
		        	Phone:  +1 509 242 9000
					Email:  support@ciena.com"
	  DESCRIPTION
	          "This MIB module is used to maintain the table of (Table, Ems IP)"
	  REVISION    "200203120000Z"
	  DESCRIPTION
      	          "Initial creation."
	  ::= { wwpModulesLeos 9}

 
 --
 -- Node definitions
 --

 wwpLeosTableChgNotifMIBObjects OBJECT IDENTIFIER ::= { wwpLeosTableChgNotifMIB 1 }

 wwpLeosTableChgNotif  OBJECT IDENTIFIER ::= {  wwpLeosTableChgNotifMIBObjects 7 }

 -- Notifications 
  
 wwpLeosTableChgNotifMIBNotificationPrefix  OBJECT IDENTIFIER ::= { wwpLeosTableChgNotifMIB 2 } 
 
 wwpLeosTableChgNotifMIBNotifications       OBJECT IDENTIFIER ::=  { wwpLeosTableChgNotifMIBNotificationPrefix 0 }

 -- Conformance information 
 
 wwpLeosTableChgNotifMIBConformance OBJECT IDENTIFIER ::= { wwpLeosTableChgNotifMIB 3 } 
 wwpLeosTableChgNotifMIBCompliances OBJECT IDENTIFIER ::= { wwpLeosTableChgNotifMIBConformance 1 } 		
 wwpLeosTableChgNotifMIBGroups      OBJECT IDENTIFIER ::= { wwpLeosTableChgNotifMIBConformance 2 } 
 
 wwpLeosTableTrapNotifTimer   OBJECT-TYPE
     SYNTAX		      INTEGER (30..3600)
     MAX-ACCESS		  read-write
     STATUS		      current
     DESCRIPTION
	     "Setting this value will set the trap timer. Device will 
	      send the trap notification after every wwpLeosTableTrapNotifTimer 
	      seconds if any of the table changes."
     ::= { wwpLeosTableChgNotifMIBObjects 1 }

 wwpLeosListenerRefreshTimer   OBJECT-TYPE
     SYNTAX		       INTEGER (30..1000)
     MAX-ACCESS		   read-write
     STATUS		       current
     DESCRIPTION
	     "Setting this value will set the listener refresh timer. Device will 
	      send the trap notification 'wwpLeosTableRefreshTrap' after every 
	      'wwpLeosListenerRefreshTimer' seconds if count value associated with 
	      'wwpLeosListenerEntry' becomes 20 or 10 or 5. Device will delete entry 
	       from wwpLeosListenerEntry once count = 0. Minimum value is 30 seconds and 
	       maximum = 1000 seconds."
     ::= { wwpLeosTableChgNotifMIBObjects 2 }
 
 wwpLeosTableChgNotifTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTableChgNotifEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "Table of Ems."
     ::= { wwpLeosTableChgNotifMIBObjects 4 }
		
 wwpLeosTableChgNotifEntry OBJECT-TYPE
     SYNTAX       WwpLeosTableChgNotifEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "Ems Entry in the ems Port Table."
     INDEX { wwpLeosTableChgNotifIndex}
     ::= { wwpLeosTableChgNotifTable 1 } 

 WwpLeosTableChgNotifEntry ::= SEQUENCE { 
     wwpLeosTableChgNotifIndex         INTEGER,     
     wwpLeosTableChgNotifOid           OBJECT IDENTIFIER,     
     wwpLeosTableChgNotifNumChanges    Counter32
  }

 wwpLeosTableChgNotifIndex   OBJECT-TYPE
     SYNTAX         INTEGER (1..100)
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This is the index used for this table."	      
     ::= { wwpLeosTableChgNotifEntry 1 }
 
 wwpLeosTableChgNotifOid   OBJECT-TYPE
     SYNTAX         OBJECT IDENTIFIER
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This is the OID of the table for which device will send trap
	      if anything changed in this table."
     ::= { wwpLeosTableChgNotifEntry 2 }
                         
 wwpLeosTableChgNotifNumChanges   OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This variables returns the counter value which keeps track of
	      how many times wwpLeosTableChgNotifOid has changed. This counter is
	      32 bit counter and will never reset, except if device is rebooted."
     ::= { wwpLeosTableChgNotifEntry 3 } 
 
 -- 
 -- Listener table index by ip
 -- 
 wwpLeosListenerTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosListenerEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "Table of EMS/NMS IP's. This table uses Multiple Set operation to create 
	      entry in the table."
     ::= { wwpLeosTableChgNotifMIBObjects 5 }
		
 wwpLeosListenerEntry OBJECT-TYPE
     SYNTAX       WwpLeosListenerEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "Entry of each EMS/NMS who is interested to receive
	      table change notification."
     INDEX { wwpLeosListenerIndex }
     ::= { wwpLeosListenerTable 1 } 

 WwpLeosListenerEntry ::= SEQUENCE { 
     wwpLeosListenerIndex	INTEGER,     
     wwpLeosListenerAddr        DisplayString,
     wwpLeosListenerResolvedIp  IpAddress,    
     wwpLeosListenerStatus      RowStatus
  }

 wwpLeosListenerIndex   OBJECT-TYPE
     SYNTAX         INTEGER (1..10)
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "Specifies the unique index in the wwpLeosListenerTable."	      
     ::= { wwpLeosListenerEntry 1 }
 
 wwpLeosListenerAddr   OBJECT-TYPE
     SYNTAX         DisplayString
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "This is the host name or ip address of the EMS/NMS."	      
     ::= { wwpLeosListenerEntry 2 } 
 
 wwpLeosListenerResolvedIp   OBJECT-TYPE
     SYNTAX         IpAddress
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This shows the resolved IP address of the host name specified in 
	      wwpLeosListenerAddr. If wwpLeosListenerAddr is set to IpV4 type then
	      wwpLeosListenerResolvedIp is equal to wwpLeosListenerAddr.
	      If wwpLeosListenerAddr is set to DNS type then
	      wwpLeosListenerResolvedIp is equal to 0 if it is unresolved 
	      or is equal to resolved IP address."	      
     ::= { wwpLeosListenerEntry 3 }

 wwpLeosListenerStatus   OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "Used to manage the creation and deletion of the 
	     conceptual rows in this table.

             To create a row in this table, a manager must
             set this object to 'createAndGo'.

	     Setting this object to 'active' if it is already active 
	     will result in refreshing this entry.

	     Setting this object to 'create and go' if this entry is already active 
	     will result in refreshing this entry.
	     
	     This table uses Multiple Set operation to create 
	     entry in the table.
	     wwpLeosListenerAddr and wwpLeosListenerStatus and index are mandatory objects that need 
	     to be set when creating entry.
	     When deleting an entry only the index needs to be specified.
	     "
     ::= { wwpLeosListenerEntry 4 }

 --
 -- Notifications
 -- 
 
 wwpLeosTableChgNotifIndexStr   OBJECT-TYPE
     SYNTAX         DisplayString (SIZE (0..255))
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This variable contains the string of indexes that changed 
	      corresponding to table wwpLeosTableChgNotifOid. This variable 
	      is sent in the trap 'wwpLeosTableChgTrap'."
     ::= { wwpLeosTableChgNotif 1 }
 
 wwpLeosListenerRefreshCount   OBJECT-TYPE
     SYNTAX		   INTEGER (30..1000)
     MAX-ACCESS		   read-only
     STATUS		   current
     DESCRIPTION
	     "This is the count value for each listener entry. when this count value 
	      becomes zero, the listener entry corresponding to this value will be deleted.
	      This count value is sent in the trap."
     ::= { wwpLeosTableChgNotif 2 }  

 wwpLeosTableChgTrap  NOTIFICATION-TYPE
        OBJECTS	   {	
	                wwpLeosTableChgNotifOid, 
                        wwpLeosTableChgNotifNumChanges,
			wwpLeosTableChgNotifIndexStr
		   }
	STATUS	   current
	DESCRIPTION
		"A notification is sent whenever the table has changed.
                 OID of the table and the counter associated with this table is 
		 sent in the trap."
	::= { wwpLeosTableChgNotifMIBNotifications 1 }
 
 wwpLeosTableRefreshTrap  NOTIFICATION-TYPE
        OBJECTS	   {wwpLeosListenerRefreshCount}
	STATUS	   current
	DESCRIPTION
		"A notification is sent whenever the listener table entry needs
                 to be refreshed."
	::= { wwpLeosTableChgNotifMIBNotifications 2 }
 END
 
