-- This file was included in WWP MIB release 04-07-01-0008
 --
 -- WWP-LEOS-DHCP-CLIENT-MIB.my
 --
           
 WWP-LEOS-DHCP-CLIENT-MIB DEFINITIONS ::= BEGIN

 IMPORTS 		
   Unsigned32, OBJECT-TYPE, MODULE-IDENTITY			
	    FROM SNMPv2-SMI			
   DisplayString, TruthValue, RowStatus			
	    FROM SNMPv2-TC						
   wwpModules, wwpModulesLeos			
	    FROM WWP-SMI;
	
	
 wwpLeosDhcpClientMIB MODULE-IDENTITY
	    LAST-UPDATED "200104031700Z"
	    ORGANIZATION "Ciena, Inc"
	    CONTACT-INFO
		    "   Mib Meister
		  		115 North Sullivan Road
				Spokane Valley, WA 99037
		        USA		 		
		        Phone:  +1 509 242 9000
				Email:  support@ciena.com"
	    DESCRIPTION
		    "The MIB module to manage DHCP client on WWP LEOS products."
	    REVISION    "200211011700Z"
	    DESCRIPTION
		    "Initial creation."
		REVISION    "200604181700Z"
		DESCRIPTION
        	"Add new tables to support DHCP relay agent functionality.
        	 Range of wwpLeosDhcpRelayAgentInterfaceIpAddr limited to 1..15."                                 
	    ::= { wwpModulesLeos 17 }
						
 --
 -- Node definitions
 --
	
 wwpLeosDhcpClientMIBObjects OBJECT IDENTIFIER ::= { wwpLeosDhcpClientMIB 1 }
 
 wwpLeosDhcpClient OBJECT IDENTIFIER ::= { wwpLeosDhcpClientMIBObjects 1 }

 wwpLeosDhcpRelayAgent OBJECT IDENTIFIER ::= { wwpLeosDhcpClientMIBObjects 2 }

 wwpLeosDhcpRelayAgentGlobalAttrs OBJECT IDENTIFIER ::= { wwpLeosDhcpRelayAgent 1 }
		
 -- Notifications 
  
 wwpLeosDhcpClientMIBNotificationPrefix  OBJECT IDENTIFIER ::= { wwpLeosDhcpClientMIB 2 } 
 wwpLeosDhcpClientMIBNotifications       OBJECT IDENTIFIER ::= { wwpLeosDhcpClientMIBNotificationPrefix 0 }

 -- Conformance information 
 
 wwpLeosDhcpClientMIBConformance OBJECT IDENTIFIER ::= { wwpLeosDhcpClientMIB 3 } 
 wwpLeosDhcpClientMIBCompliances OBJECT IDENTIFIER ::= { wwpLeosDhcpClientMIBConformance 1 } 		
 wwpLeosDhcpClientMIBGroups      OBJECT IDENTIFIER ::= { wwpLeosDhcpClientMIBConformance 2 }

 -- the DHCP client table
 
 wwpLeosDhcpIfName   OBJECT-TYPE
     SYNTAX			DisplayString(SIZE (0..32))
     MAX-ACCESS		read-write
     STATUS			current
     DESCRIPTION
		"The ifDesc associated with the DHCP client.
	     it can be set to 'remote' or 'local'"
     ::= { wwpLeosDhcpClient 1 }
     
 wwpLeosDhcpStatus     OBJECT-TYPE
     SYNTAX			INTEGER {
                        enable(1),
		         		disable(2)
		     		}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
    	"Setting this object to 'enable' will enable the 
	     DHCP client on this interface."        
     ::= { wwpLeosDhcpClient 2 } 
     
 wwpLeosDhcpState     OBJECT-TYPE
     SYNTAX			INTEGER {
 						bound(1),
		         		disabled(2),
		         		inform(3),
		         		init(4),
		         		rebinding(5),
		         		renewing(6),
		         		requesting(7),
		         		selecting(8),
		         		unknown(9)  
		     		}
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
     	"The current state of the DHCP client on this 
	     interface as per RFC2131."        
     ::= { wwpLeosDhcpClient 3 }       			 		 
      
 wwpLeosDhcpLeaseOffered  OBJECT-TYPE
     SYNTAX          Integer32(0..2147483647)
     UNITS           "seconds"
     MAX-ACCESS      read-only
     STATUS          current     
     DESCRIPTION
     	"The lease time authorized by the server."
     ::= { wwpLeosDhcpClient 5 }
     
 wwpLeosDhcpLeaseRemaining  OBJECT-TYPE
     SYNTAX          Integer32(0..2147483647)
     UNITS           "seconds"
     MAX-ACCESS      read-only
     STATUS          current     
     DESCRIPTION
     	"The time remaining for the lease to expire."
     ::= { wwpLeosDhcpClient 6 }
 
 wwpLeosDhcpDiscoveryMsgInterval  OBJECT-TYPE
     SYNTAX         Integer32(0..2147483647)
     UNITS          "seconds"
     MAX-ACCESS     read-write
     STATUS         current     
     DESCRIPTION
     	"The time interval for discovery messages issued
     	 before the client receives the first reply."
     DEFVAL  		{ 30 }
     ::= { wwpLeosDhcpClient 7 }
     
 wwpLeosDhcpRenewalTime  OBJECT-TYPE
     SYNTAX          Integer32(0..2147483647)
     UNITS           "seconds"
     MAX-ACCESS      read-only
     STATUS          current     
     DESCRIPTION
     	"The number of seconds before the client begins to renew its 
	     address lease with the DHCP server. This time is a function typically 
	     50% of the full configured duration (or lease time) for a client lease.
	     Referred to as T1 in RFC2131."
     ::= { wwpLeosDhcpClient 8 }
 
 wwpLeosDhcpRebindingTime  OBJECT-TYPE
     SYNTAX          Integer32(0..2147483647)
     UNITS           "seconds"
     MAX-ACCESS      read-only
     STATUS          current     
     DESCRIPTION
     	"The number of seconds before the client enters the rebinding state 
	     if it has not renewed its current address lease with the DHCP server. 
         This time is a function (typically, 87.5%) of the full configured 
	     duration (or lease time) for a client lease. 
	     Referred to as T2 in RFC2131."
     ::= { wwpLeosDhcpClient 9 }
     
 wwpLeosDhcpServerAddress  OBJECT-TYPE
     SYNTAX          IpAddress
     MAX-ACCESS      read-only
     STATUS          current     
     DESCRIPTION
     	"The IP address that identifies the DHCP server."
     ::= { wwpLeosDhcpClient 10 }
     
 wwpLeosDhcpRenewLease   OBJECT-TYPE
     SYNTAX         TruthValue
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
		"Setting this object to true will force the DHCP 
	     client to renew its lease."
     DEFVAL			{ false }                
     ::= { wwpLeosDhcpClient 11 }
     
 wwpLeosDhcpReleaseLease OBJECT-TYPE
     SYNTAX         TruthValue
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
   		"Setting this object to true will force the DHCP
	     client to release its lease, if the client DHCP
	     is in the bound state"
     DEFVAL			{ false }                
     ::= { wwpLeosDhcpClient 12 }
     
 --
 -- DHCPOption List
 --
 -- the Multi DHCP client Table

 wwpLeosDhcpClientOptionTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF WwpLeosDhcpClientOptionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "List of options supported by the DHCP client."
    ::= { wwpLeosDhcpClient 13 }

 wwpLeosDhcpClientOptionEntry OBJECT-TYPE
    SYNTAX      WwpLeosDhcpClientOptionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "An entry containing list of options supported by DHCP client."
    INDEX   { wwpLeosDhcpOptionCodeIndex }
    ::= { wwpLeosDhcpClientOptionTable 1 }

 WwpLeosDhcpClientOptionEntry ::=
    SEQUENCE {
    	wwpLeosDhcpOptionCodeIndex		INTEGER,
        wwpLeosDhcpOptionDesc			DisplayString,
		wwpLeosDhcpOptionCode			INTEGER,
        wwpLeosDhcpOptionState			TruthValue
    }

 wwpLeosDhcpOptionCodeIndex OBJECT-TYPE
     SYNTAX			INTEGER (1..65535)
     MAX-ACCESS		read-only
     STATUS			current
     DESCRIPTION
             "Specifies the index used for this entry."
 	::= { wwpLeosDhcpClientOptionEntry 1 }

 wwpLeosDhcpOptionDesc OBJECT-TYPE
     SYNTAX			DisplayString
     MAX-ACCESS		read-only
     STATUS			current
     DESCRIPTION
             "Specifies the description for the given DHCP option code."
 	::= { wwpLeosDhcpClientOptionEntry 2 }

 wwpLeosDhcpOptionCode OBJECT-TYPE
     SYNTAX			INTEGER (0..4294967295)
     MAX-ACCESS		read-only
     STATUS			current
     DESCRIPTION
             "Specifies the option code specified by RFC specification."
 	::= { wwpLeosDhcpClientOptionEntry 3 }

 wwpLeosDhcpOptionState OBJECT-TYPE
     SYNTAX			INTEGER {
						disabled(1),
						enabled(2)
                    }
     MAX-ACCESS		read-write
     STATUS			current
     DESCRIPTION
             "Specifies if the given option is enabled/disabled."
 	::= { wwpLeosDhcpClientOptionEntry 4 }
 
 --
 -- DHCP Relay Agent Functionality
 --                               
 wwpLeosDhcpRelayAgentCircuitId OBJECT-TYPE
     SYNTAX			INTEGER {
						slotAndPort(1),
						slotAndPortAndVlan(2)
                   	}
     MAX-ACCESS		read-write
     STATUS			current
     DESCRIPTION
             "Specifies what circuit ID should be used by DHCP relay agent."
 	::= { wwpLeosDhcpRelayAgentGlobalAttrs 1 }

 wwpLeosDhcpRelayAgentRemoteId OBJECT-TYPE
     SYNTAX			INTEGER {     			
						macAddress(1),
						hostName(2)				
                    }
     MAX-ACCESS		read-write
     STATUS			current
     DESCRIPTION
             "This object specifies what remote agent ID is used by DHCP relay agent.
              it can be set to macAddress or hostName."
 	::= { wwpLeosDhcpRelayAgentGlobalAttrs 2 }
 
 wwpLeosDhcpRelayAgentL2State OBJECT-TYPE
     SYNTAX			INTEGER {
						disabled(1),
						enabled(2)
                    }
     MAX-ACCESS		read-write
     STATUS			current
     DESCRIPTION
             "Specifies the global state of DHCP L2 relay agent."
 ::= { wwpLeosDhcpRelayAgentGlobalAttrs 3 }
 
 wwpLeosDhcpRelayAgentL3State OBJECT-TYPE
     SYNTAX			INTEGER {
						disabled(1),
						enabled(2)
                    }
     MAX-ACCESS		read-write
     STATUS			current
     DESCRIPTION
             "Specifies the global state of DHCP L3 relay agent."
 ::= { wwpLeosDhcpRelayAgentGlobalAttrs 4 }
 
 --
 -- Table to control DHCP relay agent functionality on each L2 VLAN
 --                                                                   
 wwpLeosDhcpRelayAgentL2StateTable OBJECT-TYPE
     SYNTAX       	SEQUENCE OF WwpLeosDhcpRelayAgentL2StateEntry
     MAX-ACCESS   	not-accessible
     STATUS       	current
     DESCRIPTION
             "Tables allows changing configuration of DHCP relay agent functionality for
              each wwpLeosDhcpRelayAgentVlan."
     ::= { wwpLeosDhcpRelayAgent 2 }
                
 wwpLeosDhcpRelayAgentL2StateEntry OBJECT-TYPE
     SYNTAX       	WwpLeosDhcpRelayAgentL2StateEntry
     MAX-ACCESS   	not-accessible
     STATUS       	current
     DESCRIPTION
             "Entry in the table to configure DHCP relay agent functionality."
     INDEX { wwpLeosDhcpRelayAgentVlan }
     ::= { wwpLeosDhcpRelayAgentL2StateTable 1 } 

 WwpLeosDhcpRelayAgentL2StateEntry ::= SEQUENCE { 
     wwpLeosDhcpRelayAgentVlan 	    		INTEGER,
     wwpLeosDhcpRelayAgentL2AdminState		INTEGER,
     wwpLeosDhcpRelayAgentL2OperState		INTEGER, 
     wwpLeosDhcpRelayAgentL2StatsClear		TruthValue,    
     wwpLeosDhcpRelayAgentL2RowStatus		RowStatus     
  } 

 wwpLeosDhcpRelayAgentVlan   OBJECT-TYPE
     SYNTAX         INTEGER (1..24576)
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This mib object specifies the VLAN on which DHCP relay agent is configured."
     ::= { wwpLeosDhcpRelayAgentL2StateEntry 1 } 
                                                  
 wwpLeosDhcpRelayAgentL2AdminState   OBJECT-TYPE
     SYNTAX         INTEGER {
     					disabled(1),
     					enabled(2)
     				} 
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
             "This object allows to disable or enable DHCP relay agent functionality on 
              the given VLAN specified by wwpLeosDhcpRelayAgentVlan."
     ::= { wwpLeosDhcpRelayAgentL2StateEntry 2 }                                            
 
 wwpLeosDhcpRelayAgentL2OperState   OBJECT-TYPE
     SYNTAX         INTEGER {
     					disabled(1),
     					enabled(2)
     				} 
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This object shows the operational status of the DHCP relay agent on given VLAN."
     ::= { wwpLeosDhcpRelayAgentL2StateEntry 3 }                                            
 
 wwpLeosDhcpRelayAgentL2StatsClear OBJECT-TYPE
     SYNTAX			TruthValue
     MAX-ACCESS		read-write
     STATUS			current
     DESCRIPTION
             "This mib object when set to 'true' clears DHCP relay agent stats for given VLAN."
 ::= { wwpLeosDhcpRelayAgentL2StateEntry 4 }
     
 wwpLeosDhcpRelayAgentL2RowStatus   OBJECT-TYPE
     SYNTAX         RowStatus 
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
             "Set this MIB object to 'Destroy' to terminate DHCP L2 Relaying
              on the VLAN specified by wwpLeosDhcpRelayAgentVlan.
              
              Set this MIB object to 'CreateAndGo' to enable DHCP L2 Relaying
              on the VLAN specified by wwpLeosDhcpRelayAgentVlan."
     ::= { wwpLeosDhcpRelayAgentL2StateEntry 5 }
 
 --
 -- L3 State Table
 --
 wwpLeosDhcpRelayAgentL3StateTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosDhcpRelayAgentL3StateEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Tables allows changing configuration
              of DHCP relay agent functionality for
              each wwpLeosDhcpRelayAgentInterfaceIndex."
     ::= { wwpLeosDhcpRelayAgent 3 }
                
 wwpLeosDhcpRelayAgentL3StateEntry OBJECT-TYPE
     SYNTAX       WwpLeosDhcpRelayAgentL3StateEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Entry in the table to configure DHCP relay agent functionality."
     INDEX { wwpLeosDhcpRelayAgentInterfaceIndex }
     ::= { wwpLeosDhcpRelayAgentL3StateTable 1 } 

 WwpLeosDhcpRelayAgentL3StateEntry ::= SEQUENCE { 
     wwpLeosDhcpRelayAgentInterfaceIndex	   	INTEGER,
     wwpLeosDhcpRelayAgentL3AdminState			INTEGER,
     wwpLeosDhcpRelayAgentL3OperState			INTEGER,
     wwpLeosDhcpRelayAgentL3RowStatus			RowStatus          
  } 
 
 wwpLeosDhcpRelayAgentInterfaceIndex   OBJECT-TYPE
     SYNTAX         INTEGER (1..65535)
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This mib object specifies the value of the mib object wwpLeosDhcpRelayAgentIndexType.
              So if wwpLeosDhcpRelayAgentIndexType = interface then this object represents the interface index.
              if it is set to VLAN then this object represents the VLAN id and so on."
     ::= { wwpLeosDhcpRelayAgentL3StateEntry 1 } 
                                                  
 wwpLeosDhcpRelayAgentL3AdminState   OBJECT-TYPE
     SYNTAX         INTEGER {
     					disabled(1),
     					enabled(2)
     				} 
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
             "This object allows to disable or enable DHCP relay agent functionality 
              for each wwpLeosDhcpRelayAgentIndexType."
     ::= { wwpLeosDhcpRelayAgentL3StateEntry 2 }                                        
 
 wwpLeosDhcpRelayAgentL3OperState   OBJECT-TYPE
     SYNTAX         INTEGER {
     					disabled(1),
     					enabled(2)
     				} 
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This object shows the operational status of the DHCP relay agent on the given interface."
     ::= { wwpLeosDhcpRelayAgentL3StateEntry 3 } 
     
 wwpLeosDhcpRelayAgentL3RowStatus   OBJECT-TYPE
     SYNTAX         RowStatus 
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
             "Set this MIB object to 'Destroy' to terminate DHCP L3 Relaying
              on the VLAN specified by wwpLeosDhcpRelayAgentInterfaceIndex.
              
              Set this MIB object to 'CreateAndGo' to enable DHCP L3 Relaying
              on the VLAN specified by wwpLeosDhcpRelayAgentInterfaceIndex."
     ::= { wwpLeosDhcpRelayAgentL3StateEntry 4 }                                       
     
 --
 -- DHCP Relay Agent Interface IP Table
 --                                 
 wwpLeosDhcpRelayAgentInterfaceIpTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosDhcpRelayAgentInterfaceIpEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "This table can be used to add the trusted IP addresses 
              or host names on each interface."
     ::= { wwpLeosDhcpRelayAgent 4 }
                
 wwpLeosDhcpRelayAgentInterfaceIpEntry OBJECT-TYPE
     SYNTAX       WwpLeosDhcpRelayAgentInterfaceIpEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Each entry in this table represents the trusted DHCP server IP address
              on each interface.              "
     INDEX { wwpLeosDhcpRelayAgentInterfaceIpIndex }
     ::= { wwpLeosDhcpRelayAgentInterfaceIpTable 1 } 

 WwpLeosDhcpRelayAgentInterfaceIpEntry ::= SEQUENCE { 
     wwpLeosDhcpRelayAgentInterfaceIpIndex			INTEGER,     
     wwpLeosDhcpRelayAgentInterfaceIpAddr			IpAddress,     
     wwpLeosDhcpRelayAgentInterfaceIpRowStatus    	RowStatus
  } 

 wwpLeosDhcpRelayAgentInterfaceIpIndex   OBJECT-TYPE
     SYNTAX         INTEGER (1..10)
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This mib object is used as an index in the table 
             and represents the unique index of the IP address 
             for a given wwpLeosDhcpRelayAgentInterfaceIndex."
     ::= { wwpLeosDhcpRelayAgentInterfaceIpEntry 1 } 
                                                  
 wwpLeosDhcpRelayAgentInterfaceIpAddr   OBJECT-TYPE
     SYNTAX         IpAddress
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
             "This mib object is used to specify the IP address of the DHCP server which is trusted IP
              address. This object cannot be modified once entry is created with some IP."
     ::= { wwpLeosDhcpRelayAgentInterfaceIpEntry 2 }                                              
     
 wwpLeosDhcpRelayAgentInterfaceIpRowStatus   OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	         "Used to manage the creation and deletion of the 
	          conceptual rows in this table.
	          
              To create a row in this table set this object 
              to 'createAndGo'.
              
              To delete a row in this table set this object
              to 'destroy'."
     ::= { wwpLeosDhcpRelayAgentInterfaceIpEntry 3 }

 --
 -- DHCP Relay Agent Trust Table
 --                                 
 wwpLeosDhcpRelayAgentTrustTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosDhcpRelayAgentTrustEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "This table can be used to specify what slot / ports and vlans  
              DHCP relay agent can trust."
     ::= { wwpLeosDhcpRelayAgent 5 }
                
 wwpLeosDhcpRelayAgentTrustEntry OBJECT-TYPE
     SYNTAX       WwpLeosDhcpRelayAgentTrustEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Each entry in this table can be used to specify the slot / port and VLAN to be trusted."
     INDEX { wwpLeosDhcpRelayAgentVlan, wwpLeosDhcpRelayAgentPort }
     ::= { wwpLeosDhcpRelayAgentTrustTable 1 } 

 WwpLeosDhcpRelayAgentTrustEntry ::= SEQUENCE { 
     wwpLeosDhcpRelayAgentPort			INTEGER,
     wwpLeosDhcpRelayAgentTrustMode		INTEGER
  } 
                                      
 wwpLeosDhcpRelayAgentPort   OBJECT-TYPE
     SYNTAX         INTEGER (1..65535)
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This mib object is used as index in the table and is used to specify the port."
     ::= { wwpLeosDhcpRelayAgentTrustEntry 1 }                                            
  
  wwpLeosDhcpRelayAgentTrustMode   OBJECT-TYPE
     SYNTAX         INTEGER {
     				 clientTrust(1),    
     				 serverTrust(2),           
     				 dualRoleTrust(3),           
     				 unTrust(4)
     				 }     				
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
             "This mib object can be used to set the port as client trusted, server trusted or not trusted."
     ::= { wwpLeosDhcpRelayAgentTrustEntry 2 }   
 
 --
 -- Dhcp relay agent L2 stats
 --  
 wwpLeosDhcpRelayAgentL2StatsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosDhcpRelayAgentL2StatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Tables to display L2 statistics for each wwpLeosDhcpRelayAgentVlan."
     ::= { wwpLeosDhcpRelayAgent 6 }
                
 wwpLeosDhcpRelayAgentL2StatsEntry OBJECT-TYPE
     SYNTAX       WwpLeosDhcpRelayAgentL2StatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Entry in the table to display l2 stats."
     INDEX { wwpLeosDhcpRelayAgentVlan }
     ::= { wwpLeosDhcpRelayAgentL2StatsTable 1 } 

 WwpLeosDhcpRelayAgentL2StatsEntry ::= SEQUENCE {      
     wwpLeosDhcpRelayAgentL2IpSecHeaders                        Counter32,
     wwpLeosDhcpRelayAgentL2Option82Added			Counter32, 
     wwpLeosDhcpRelayAgentL2Option82Removed			Counter32,    
     wwpLeosDhcpRelayAgentL2UntrustedClientPortPktsRx		Counter32,    
     wwpLeosDhcpRelayAgentL2UntrustedServerPortPktsRx		Counter32,    
     wwpLeosDhcpRelayAgentL2SpoofedDhcpPkts			Counter32,    
     wwpLeosDhcpRelayAgentL2Option82ExceedMTU			Counter32,
     wwpLeosDhcpRelayAgentL2NoTrustedServerPktDrop		Counter32,
     wwpLeosDhcpRelayAgentL2NoTrustedClientPktDrop		Counter32          
  } 

 wwpLeosDhcpRelayAgentL2IpSecHeaders   OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This MIB object specifies the number of packets that include IP Sec Headers."
     ::= { wwpLeosDhcpRelayAgentL2StatsEntry 1 } 
                                                  
 wwpLeosDhcpRelayAgentL2Option82Added   OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This MIB object specifies the number of packets that have had option 82 added."
     ::= { wwpLeosDhcpRelayAgentL2StatsEntry 2 }                                            
 
 wwpLeosDhcpRelayAgentL2Option82Removed   OBJECT-TYPE
     SYNTAX         Counter32 
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This MIB object specifies the number of packets that have had option 82 removed."
     ::= { wwpLeosDhcpRelayAgentL2StatsEntry 3 }                                            
 
 wwpLeosDhcpRelayAgentL2UntrustedClientPortPktsRx OBJECT-TYPE
     SYNTAX		Counter32
     MAX-ACCESS	read-only
     STATUS		current
     DESCRIPTION
             "This MIB object specifies the number of packets received on untrusted client ports."
 ::= { wwpLeosDhcpRelayAgentL2StatsEntry 4 }
     
 wwpLeosDhcpRelayAgentL2UntrustedServerPortPktsRx OBJECT-TYPE
     SYNTAX		Counter32
     MAX-ACCESS	read-only
     STATUS		current
     DESCRIPTION
             "This MIB object specifies the number of packets received from untrusted server ports."
 ::= { wwpLeosDhcpRelayAgentL2StatsEntry 5 } 
 
 wwpLeosDhcpRelayAgentL2SpoofedDhcpPkts OBJECT-TYPE
     SYNTAX		Counter32
     MAX-ACCESS	read-only
     STATUS		current
     DESCRIPTION
             "This MIB object specifies the number of spoofed DHCP packets."
 ::= { wwpLeosDhcpRelayAgentL2StatsEntry 6 }
 
 wwpLeosDhcpRelayAgentL2Option82ExceedMTU OBJECT-TYPE
     SYNTAX		Counter32
     MAX-ACCESS	read-only
     STATUS		current
     DESCRIPTION
             "This MIB object specifies the number of packets with DHCP option 82 that exceed option 82."
 ::= { wwpLeosDhcpRelayAgentL2StatsEntry 7 }
 
 wwpLeosDhcpRelayAgentL2NoTrustedServerPktDrop OBJECT-TYPE
     SYNTAX		Counter32
     MAX-ACCESS	read-only
     STATUS		current
     DESCRIPTION
             "This MIB object specifies the number of DHCP packets dropped because there are no server trusted ports configured."
 ::= { wwpLeosDhcpRelayAgentL2StatsEntry 8 }                                   
 
 wwpLeosDhcpRelayAgentL2NoTrustedClientPktDrop OBJECT-TYPE
     SYNTAX		Counter32
     MAX-ACCESS	read-only
     STATUS		current
     DESCRIPTION
             "This MIB object specifies the number of DHCP packets dropped because there are no client trusted ports configured."
 ::= { wwpLeosDhcpRelayAgentL2StatsEntry 9 } 
  --
 -- DHCP Relay Agent CID String Table
 --                                 
 wwpLeosDhcpRelayAgentCidStringTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosDhcpRelayAgentCidStringEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "This table can be used to specify cid strings for slot / ports and vlans  
              dhcp relay agent can specify in Option 82 CID information."
     ::= { wwpLeosDhcpRelayAgent 7 }
                
 wwpLeosDhcpRelayAgentCidStringEntry OBJECT-TYPE
     SYNTAX       WwpLeosDhcpRelayAgentCidStringEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Each entry in this table can be used to specify a cid string for slot / port and vlan combinations."
     INDEX { wwpLeosDhcpRelayAgentVlan, wwpLeosDhcpRelayAgentCidStringPort }
     ::= { wwpLeosDhcpRelayAgentCidStringTable 1 } 

 WwpLeosDhcpRelayAgentCidStringEntry ::= SEQUENCE { 
     wwpLeosDhcpRelayAgentCidStringPort				INTEGER,
     wwpLeosDhcpRelayAgentCidString					DisplayString,
     wwpLeosDhcpRelayAgentCidStringRowStatus		RowStatus
  } 
                                      
 wwpLeosDhcpRelayAgentCidStringPort   OBJECT-TYPE
     SYNTAX         INTEGER (1..65535)
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "This mib object is used as index in the table and is used to specify the port."
     ::= { wwpLeosDhcpRelayAgentCidStringEntry 1 }                                            
  
  wwpLeosDhcpRelayAgentCidString   OBJECT-TYPE
     SYNTAX         DisplayString     				
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
             "This mib object can be used to set the cid string for the port."
     ::= { wwpLeosDhcpRelayAgentCidStringEntry 2 }
  
  wwpLeosDhcpRelayAgentCidStringRowStatus   OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	         "Used to manage the creation and deletion of the 
	          conceptual rows in this table.
	          
              To create a row in this table set this object 
              to 'createAndGo'.
              
              To delete a row in this table set this object
              to 'destroy'."
     ::= { wwpLeosDhcpRelayAgentCidStringEntry 3 }

 --
 -- Notifications
 --
 wwpLeosDhcpClientOptionDisabledNotification NOTIFICATION-TYPE	
        OBJECTS	   {
	              wwpLeosDhcpOptionCode 
		   }
	STATUS	current
	DESCRIPTION
		"A wwpLeosDhcpClientOptionDisabledNotification is sent 
		 whenever device receives DHCP option which is disabled
		 on the device."
	::= { wwpLeosDhcpClientMIBNotifications 1 }
 END

 --
 -- WWP-LEOS-DHCP-CLIENT-MIB.my
 --
