-- This file was included in WWP MIB release 04-07-01-0008
 --
 -- WWP-LEOS-TRAFFIC-PROFILE-MIB.my
 --

 WWP-LEOS-TRAFFIC-PROFILE-MIB DEFINITIONS ::= BEGIN

 IMPORTS 		
   Integer32, IpAddress, OBJECT-TYPE, MODULE-IDENTITY			
	    FROM SNMPv2-SMI
   RowStatus, DisplayString, MacAddress, TruthValue 
            FROM SNMPv2-TC				
   wwpModules, 	wwpModulesLeos	
	    FROM WWP-SMI;
	
 wwpLeosTrafficProfileMIB MODULE-IDENTITY
	    LAST-UPDATED "200203250000Z"
	    ORGANIZATION "Ciena, Inc"
	    CONTACT-INFO
		    "   Mib Meister
		  			115 North Sullivan Road
					Spokane Valley, WA 99037
		        	USA		 		
		        	Phone:  +1 509 242 9000
					Email:  support@ciena.com" 
		DESCRIPTION 
			"Added modes hierarchicalVlan(12), hierarchicalPort(13) to wwpLeosTrafficProfileMode 
			under wwpLeosTrafficProfilePortEntry.
			Added  wwpLeosTrafficProfileStdDefaultProfile, wwpLeosTrafficProfileStdDrop,
			wwpLeosTrafficProfileStdParentIndex, wwpLeosTrafficProfileStdChildMode under wwpLeosTrafficProfileStdTable"
		REVISION "200908251700Z"
		DESCRIPTION
			"Added modes stdVlanDot1dPri, stdVlanIpp, stdDscp to wwpLeosTrafficProfileMode under wwpLeosTrafficProfilePortEntry.
			Added objects wwpLeosTrafficProfileStdCbs, wwpLeosTrafficProfileEbs, wwpLeosTrafficProfileStdDscpRemarkPolicy, 
			wwpLeosTrafficProfileStdFixedDscp to wwpLeosTrafficProfileStdEntryTable"
		REVISION	"200811141700Z"
		DESCRIPTION
			"Added wwpLeosTrafficProfileMeterPoolTable under wwpLeosTrafficProfile
			wwpLeosTrafficProfileStdIndx mib object value has been changed from 1..32 to 1..64 
			Added wwpLeosTrafficProfileMeterPool mib object under wwpLeosTrafficProfilePortEntry."
		REVISION  "200807281700Z"
		DESCRIPTION
	        "Added additional trafficPorfileMode stdDscp.
	         Profile Index changed for following mib object from 1 through 8 to 1 through 32
	         	wwpLeosTrafficProfileStdIndx,
	         	wwpLeosTrafficProfileStdDot1dTpProfile,
	         	wwpLeosTrafficProfileStdIpPrecToProfile,
	         	wwpLeosTrafficProfileStdPhbToProfile.
	         Added new wwpLeosTrafficProfileStdDscpTable.
	         Added new wwpLeosTrafficProfileStdVlanTable."
	    REVISION   "200806281700Z"
        DESCRIPTION
                    "added value in cascaded enumerations for deprecated values"
        REVISION    "200806161700Z"  
        DESCRIPTION
                    "added entries related to tos-stamping"
        REVISION    "200806131700Z"
        DESCRIPTION
		   "changed description of entries relating to cascaded profiling"
     	REVISION    "200806041700Z"    
        DESCRIPTION
		    "deprecated all entries related to cascaded traffic profiling."
     	REVISION    "200805211700Z"
	    DESCRIPTION
		    "Added Total Statistics."
     	REVISION    "200805151700Z"
	    DESCRIPTION
		    "The MIB module for the WWP leos traffic profiling specific information."
	    REVISION    "200104031700Z"
	    DESCRIPTION
		    "Initial creation."
	    ::= { wwpModulesLeos 27 }	
 				
 --
 -- Node definitions
 --
	
 wwpLeosTrafficProfileObjects OBJECT IDENTIFIER ::= { wwpLeosTrafficProfileMIB 1 }
 
 wwpLeosTrafficProfile OBJECT IDENTIFIER ::= { wwpLeosTrafficProfileObjects 1 }

 -- Notifications 
  
 wwpLeosTrafficProfileNotificationPrefix     OBJECT IDENTIFIER ::= { wwpLeosTrafficProfileMIB 2 } 
 wwpLeosTrafficProfileNotifications          OBJECT IDENTIFIER ::=  { wwpLeosTrafficProfileNotificationPrefix 0 }

 -- Conformance information 
 
 wwpLeosTrafficProfileMIBConformance OBJECT IDENTIFIER ::= { wwpLeosTrafficProfileMIB 3 } 
 wwpLeosTrafficProfileMIBCompliances OBJECT IDENTIFIER ::= { wwpLeosTrafficProfileMIBConformance 1 } 		
 wwpLeosTrafficProfileMIBGroups      OBJECT IDENTIFIER ::= { wwpLeosTrafficProfileMIBConformance 2 }  

 -- global attributes for flow
 wwpLeosTrafficProfileGlobalAttrs	   OBJECT IDENTIFIER ::= { wwpLeosTrafficProfile 1 }  
 
 -- 
 -- Global Attributes
 -- 
 wwpLeosTrafficProfileGlobalState    OBJECT-TYPE
     SYNTAX         INTEGER {
			enabled(1),
			disabled(2)
			}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "Setting this object to 'enabled' will enable traffic profile globally. 
	      Setting this object to 'disabled' will disable traffic profile globally."
     ::= { wwpLeosTrafficProfileGlobalAttrs 1 }    
     
 --
 -- Traffic profiling on per port basis.
 -- 
 wwpLeosTrafficProfilePortTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfilePortEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of traffic profile port entries."
     ::= { wwpLeosTrafficProfile 2 }
		
 wwpLeosTrafficProfilePortEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfilePortEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A traffic profile entry in the wwpLeosTrafficProfilePortTable."
     INDEX { wwpLeosTrafficProfilePort }    
     ::= { wwpLeosTrafficProfilePortTable 1 }
     
 WwpLeosTrafficProfilePortEntry ::= SEQUENCE {
     wwpLeosTrafficProfilePort			               INTEGER,
     wwpLeosTrafficProfileAdminState			         INTEGER,
     wwpLeosTrafficProfileOperState			            INTEGER,
     wwpLeosTrafficProfileMode				            INTEGER,
     wwpLeosTrafficProfileNonConformCascadedProfile	INTEGER,
     wwpLeosTrafficProfileNonConformStdProfile		   INTEGER,
     wwpLeosTrafficProfileArpCascadedProfile		      INTEGER,
     wwpLeosTrafficProfileArpStdProfile			      INTEGER,
     wwpLeosTrafficProfileMeterPool					  INTEGER
 }    
     
 wwpLeosTrafficProfilePort    OBJECT-TYPE
     SYNTAX         INTEGER (1..65535)
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies the port number also used as index in 
	      the table."
     ::= { wwpLeosTrafficProfilePortEntry 1 }     
     
 wwpLeosTrafficProfileAdminState    OBJECT-TYPE
     SYNTAX         INTEGER {
			enabled(1),
			disabled(2)
			}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "Setting this object to 'enabled' will administratively enable traffic profiling on the given port. 
	      Setting this object to 'disabled' will administratively disable traffic profiling on the given port."
     ::= { wwpLeosTrafficProfilePortEntry 2 }  
 
 wwpLeosTrafficProfileOperState    OBJECT-TYPE
     SYNTAX         INTEGER {
			enabled(1),
			disabled(2)
			}
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies operational state of the traffic profiling for a given port
	      on the device."
     ::= { wwpLeosTrafficProfilePortEntry 3 }

 wwpLeosTrafficProfileMode    OBJECT-TYPE
     SYNTAX         INTEGER {
			cascadedDot1dPri(1),
			cascadedDscp(2),
			cascadedIpPrec(3),
			stdDot1(4),
			stdDiffServ(5),
			stdIpPrec(6),
			stdVlan(7),
			stdDscp(8),
			stdVlanDot1DPri(9),
			stdVlanIpp(10),
			stdVlanDscp(11),
			hierarchicalVlan(12),
			hierarchicalPort(13),
			none(14)
			}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the mode of traffic profiling for a given port."
     ::= { wwpLeosTrafficProfilePortEntry 4 }
 
 wwpLeosTrafficProfileNonConformCascadedProfile    OBJECT-TYPE
     SYNTAX         INTEGER {
			drop(0),
			profile1(1),
			profile2(2),
			profile3(3),
            deprecated(4)			
			}
     MAX-ACCESS     read-write
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies that the device should map non-conformance traffic ingressing
	      on a given port to cascaded profile specified by 
	      wwpLeosTrafficProfileNonConformCascadedProfile. This object will become effective
	      only if device is running in cascaded profile mode. This object will be set to drop
              if using on a device that does not have cascaded-profiling"
     ::= { wwpLeosTrafficProfilePortEntry 5 }
 
 wwpLeosTrafficProfileNonConformStdProfile    OBJECT-TYPE
     SYNTAX         INTEGER (0..32) 
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies that the device should map non-conformance traffic ingressing
	      on a given port to standard profile specified by 
	      wwpLeosTrafficProfileNonConformStdProfile. This object will become effective
	      only if device is running in standard profile mode."
     ::= { wwpLeosTrafficProfilePortEntry 6 }
 
 wwpLeosTrafficProfileArpCascadedProfile    OBJECT-TYPE
     SYNTAX         INTEGER {
			bypass(0),
			profile1(1),
			profile2(2),
			profile3(3),
            deprecated(4)			
			}
     MAX-ACCESS     read-write
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies that the device should map ARP frames ingressing
	      on a given port to cascaded profile specified by 
	      wwpLeosTrafficProfileArpCascadedProfile. This object will be set to bypass
              if using on a device that does not have cascaded-profiling."
     ::= { wwpLeosTrafficProfilePortEntry 7 }
 
 wwpLeosTrafficProfileArpStdProfile    OBJECT-TYPE
     SYNTAX         INTEGER (0..32)
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies that the device should map ARP frames ingressing
	      on a given port to standard profile specified by 
	      wwpLeosTrafficProfileArpStdProfile. This object will become effective
	      only if device is running in standard profile mode."
     ::= { wwpLeosTrafficProfilePortEntry 8 } 
     
  wwpLeosTrafficProfileMeterPool 	OBJECT-TYPE
      SYNTAX     INTEGER(1..8)
      MAX-ACCESS read-write
      STATUS 	current
      DESCRIPTION
      	"This object specifies the Meter Pool Index for a port."
      ::= { wwpLeosTrafficProfilePortEntry 9}	
  

 --
 -- Cascaded profile
 -- 
 wwpLeosTrafficProfileCascadedTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileCascadedEntry
     MAX-ACCESS   not-accessible
     STATUS       deprecated
     DESCRIPTION
	     "A table of cascaded traffic profile entries.
	      To create an entry in this table the following criteria must be met.
	      - All indexes must be specified.
	      - wwpLeosTrafficProfileCascadedCir must be specified
	      - if wwpLeosTrafficProfileCascadedPir is not specified or is specified and is < wwpLeosTrafficProfileCascadedCir
	        then device will make wwpLeosTrafficProfileCascadedPir = wwpLeosTrafficProfileCascadedCir
	      - wwpLeosTrafficProfileCascadedStatus must be set to createandgo"	      
     ::= { wwpLeosTrafficProfile 3 }
		
 wwpLeosTrafficProfileCascadedEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileCascadedEntry
     MAX-ACCESS   not-accessible
     STATUS       deprecated
     DESCRIPTION
	     "A cascaded traffic profile entry in the wwpLeosTrafficProfileCascadedTable."
     INDEX { wwpLeosTrafficProfilePort , wwpLeosTrafficProfileCascadedIndx}    
     ::= { wwpLeosTrafficProfileCascadedTable 1 }
     
 WwpLeosTrafficProfileCascadedEntry ::= SEQUENCE {     
     wwpLeosTrafficProfileCascadedIndx				INTEGER,
     wwpLeosTrafficProfileCascadedCir				Integer32,
     wwpLeosTrafficProfileCascadedPir				Integer32,     
     wwpLeosTrafficProfileCascadedStatus		   	RowStatus
 }   
 
 wwpLeosTrafficProfileCascadedIndx    OBJECT-TYPE
     SYNTAX         INTEGER (1..3)
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object is used as index in the table and it represents 
	      profile index which can be 1 or 2 or 3."
     ::= { wwpLeosTrafficProfileCascadedEntry 1 }  
 wwpLeosTrafficProfileCascadedCir    OBJECT-TYPE
     SYNTAX         Integer32
     UNITS	    	"kbps"
     MAX-ACCESS     read-write
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the cir associated with a given cascaded traffic profile.
	      Units are kbps."
     ::= { wwpLeosTrafficProfileCascadedEntry 2 }

 wwpLeosTrafficProfileCascadedPir    OBJECT-TYPE
     SYNTAX         Integer32
     UNITS	    	"kbps"
     MAX-ACCESS     read-write
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the pir associated with a given cascaded traffic profile.
	      Units are kbps."
     ::= { wwpLeosTrafficProfileCascadedEntry 3 }
     
 wwpLeosTrafficProfileCascadedStatus    OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         deprecated
     DESCRIPTION
	     "Setting this object to 'createandgo' along with wwpLeosTrafficProfileCascadedCir
	      and wwpLeosTrafficProfileCascadedPir will result in creating an cascaded traffic profile entry.
	      Setting this object to 'destroy' will delete the entry from the table."
     ::= { wwpLeosTrafficProfileCascadedEntry 5 }
    
 --
 -- Std profile
 -- 
 wwpLeosTrafficProfileStdTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileStdEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of Std traffic profile entries.
	      To create entry in this table following criteria must be met.
	      - All indexes must be specified.
	      - wwpLeosTrafficProfileStdCir must be specified
	      - if wwpLeosTrafficProfileStdPir is not specified or is specified and is < wwpLeosTrafficProfileStdCir
	        then device will make wwpLeosTrafficProfileStdPir = wwpLeosTrafficProfileStdCir
	      - wwpLeosTrafficProfileStdStatus must be set to createandgo"
     ::= { wwpLeosTrafficProfile 4 }
		
 wwpLeosTrafficProfileStdEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileStdEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A standard traffic profile entry in the wwpLeosTrafficProfileStdTable."
     INDEX { wwpLeosTrafficProfilePort , wwpLeosTrafficProfileStdIndx}    
     ::= { wwpLeosTrafficProfileStdTable 1 }
     
 WwpLeosTrafficProfileStdEntry ::= SEQUENCE {
     wwpLeosTrafficProfileStdIndx			INTEGER,
     wwpLeosTrafficProfileStdCir			Integer32,
     wwpLeosTrafficProfileStdPir			Integer32,
     wwpLeosTrafficProfileStdName			DisplayString,
     wwpLeosTrafficProfileStdStatus			RowStatus,
     wwpLeosTrafficProfileStdVlan			INTEGER,
     wwpLeosTrafficProfileStdCbs            Unsigned32,
     wwpLeosTrafficProfileStdEbs            Unsigned32,
     wwpLeosTrafficProfileStdDscpRemarkPolicy INTEGER,
     wwpLeosTrafficProfileStdFixedDscp		INTEGER,
     wwpLeosTrafficProfileStdUnsetVlan		INTEGER,
     wwpLeosTrafficProfileStdDefaultProfile	INTEGER,
     wwpLeosTrafficeProfileStdDrop			INTEGER,
     wwpLeosTrafficProfileStdParentIndex	INTEGER,
     wwpLeosTrafficProfileStdChildMode		INTEGER, 
     wwpLeosTrafficProfileStdStatsMonitor		INTEGER
   } 
 
 wwpLeosTrafficProfileStdIndx    OBJECT-TYPE
     SYNTAX         INTEGER (1..512)
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object is used as index in the table and it represents 
	      profile index which can be 1 through 64."
     ::= { wwpLeosTrafficProfileStdEntry 1 }  
 
 wwpLeosTrafficProfileStdCir    OBJECT-TYPE
     SYNTAX         Integer32
     UNITS			"kbps"
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the cir associated with a given standard traffic profile."
     ::= { wwpLeosTrafficProfileStdEntry 2 }

 wwpLeosTrafficProfileStdPir    OBJECT-TYPE
     SYNTAX         Integer32
     UNITS			"kbps"
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the pir associated with a given standard traffic profile."
     ::= { wwpLeosTrafficProfileStdEntry 3 }
     
 wwpLeosTrafficProfileStdName  OBJECT-TYPE
     SYNTAX       DisplayString(SIZE (0..15))
     MAX-ACCESS   read-create
     STATUS       current
     DESCRIPTION
	     "The name associated with this profile.  This must be unique per port.
         The name does not have to be set on create.  However, when updating the name,
         it must have some value - zero-string not support." 
     ::= { wwpLeosTrafficProfileStdEntry 4 }	
 
 wwpLeosTrafficProfileStdStatus    OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "Setting this object to 'createandgo' along with wwpLeosTrafficProfileStdCir
	      and or wwpLeosTrafficProfileStdPir will result in creating an standard traffic profile entry.
	      Setting this object to 'destroy' will delete the entry from the table."
     ::= { wwpLeosTrafficProfileStdEntry 5 }

 wwpLeosTrafficProfileStdVlan    OBJECT-TYPE
     SYNTAX         INTEGER (1..4096)
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the VLAN associated with a profile."
     ::= { wwpLeosTrafficProfileStdEntry 6 }
 wwpLeosTrafficProfileStdCbs    OBJECT-TYPE
     SYNTAX       Unsigned32 
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the Commited burst size associated with a given 
              standard traffic profile."
     DEFVAL { 2 }
     ::= { wwpLeosTrafficProfileStdEntry 7 }

 wwpLeosTrafficProfileStdEbs    OBJECT-TYPE
     SYNTAX       Unsigned32      
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the Excess burst size associated with a given 
              standard traffic profile."
     DEFVAL { 2 }
     ::= { wwpLeosTrafficProfileStdEntry 8 }
 
 wwpLeosTrafficProfileStdDscpRemarkPolicy OBJECT-TYPE
 	  SYNTAX		INTEGER {
 	  						leave(1),
 	  						fixed(2)
 	  			}
 	  MAX-ACCESS	read-write
 	  STATUS		current
 	  DESCRIPTION
 	  	"Leave => Don't remark the frame. 
 	  	Fixed => Remark the DSCP of a frame with the fixed-dscp value for IP frames 
 	  	which classify to the Traffic Profile"
 	  ::= { wwpLeosTrafficProfileStdEntry 9 }
 	   
 wwpLeosTrafficProfileStdFixedDscp OBJECT-TYPE
 	  SYNTAX		INTEGER (0..63)
 	  MAX-ACCESS	read-write
 	  STATUS		current
 	  DESCRIPTION
 	  	"Fixed DSCP value to use for frames classifying to a Traffic Profile 
 	  	when the dscp-remark-policy id 'Fixed"
 	   ::= { wwpLeosTrafficProfileStdEntry 10 } 
 
 wwpLeosTrafficProfileStdUnsetVlan	OBJECT-TYPE
      SYNTAX		INTEGER {
      						 none(0),
      						 unset(1)
      						 }
 	  MAX-ACCESS	read-write
 	  STATUS		current
 	  DESCRIPTION
 	  	"Setting This object to unset(1) unsets the VLAN associated with a profile.
		 This object returns a value of none(0) on get."
 	   ::= { wwpLeosTrafficProfileStdEntry 11 } 
 
 wwpLeosTrafficProfileStdDefaultProfile   OBJECT-TYPE
 	SYNTAX    	INTEGER {
 				 true(1),
 				 false(2)
 				}
	MAX-ACCESS	read-create
 	STATUS		current
 	DESCRIPTION
 	  	"Setting this object to true(1) during createAndGo(4) will create Tier-1 default profile."
 	   ::= { wwpLeosTrafficProfileStdEntry 12 } 
  
  wwpLeosTrafficeProfileStdDrop		OBJECT-TYPE
  	SYNTAX    	INTEGER {
 				 true(1),
 				 false(2)
 				}
	MAX-ACCESS	read-create
 	STATUS		current
 	DESCRIPTION
 	  	"Setting this value to true causes metering to cease and all traffic to drop."
 	   ::= { wwpLeosTrafficProfileStdEntry 13 } 
	
	wwpLeosTrafficProfileStdParentIndex	OBJECT-TYPE
		SYNTAX	INTEGER
		MAX-ACCESS read-create
		STATUS current
		DESCRIPTION 
		"This mib object is set when creating Child traffic profile to specify the parent index"
		::= { wwpLeosTrafficProfileStdEntry 14 }

	wwpLeosTrafficProfileStdChildMode 	OBJECT-TYPE
		SYNTAX INTEGER {  
			dot1dPri(1),
			ipprec(2),
			dscp(3),
			vlan(4),
			none(99)
		}      
		MAX-ACCESS read-create
		STATUS     current
		DESCRIPTION
			"When the port mode is hierarchical-vlan, then the valid child-modes are dot1dPri, ipprec, dscp. 
			When the port mode is hierarchical-port then the valid childModes is dot1dPri, ipprec, dscp and vlan(4)."
		::= { wwpLeosTrafficProfileStdEntry 15}
   

 wwpLeosTrafficProfileStdStatsMonitor OBJECT-TYPE
 	SYNTAX   INTEGER {
 				on(1),
 				off(2)
 			}
 	MAX-ACCESS read-write
 	STATUS current
 	DESCRIPTION
 		"To disable stats collection, set this object to off(2).
 		To enable stats collection, set this object to on(1)."
 ::= { wwpLeosTrafficProfileStdEntry  16}

     
 --
 -- Std profile dot1d table
 -- 
 wwpLeosTrafficProfileStdDot1dTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileStdDot1dEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of Std dot1d traffic profile entries.	      
	      To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdDot1dStatus to 'createandgo'. 
	      - set wwpLeosTrafficProfileStdDot1dToProfile to valid profile.
	      
	      To delete entry set wwpLeosTrafficProfileStdDot1dStatus to destroy."
     ::= { wwpLeosTrafficProfile 5 }
		
 wwpLeosTrafficProfileStdDot1dEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileStdDot1dEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A standard dot1d traffic profile entry in the wwpLeosTrafficProfileStdDot1dTable."
     INDEX { wwpLeosTrafficProfilePort , wwpLeosTrafficProfileStdDot1d}    
     ::= { wwpLeosTrafficProfileStdDot1dTable 1 }
     
 WwpLeosTrafficProfileStdDot1dEntry ::= SEQUENCE {
     wwpLeosTrafficProfileStdDot1d				INTEGER,
     wwpLeosTrafficProfileStdDot1dToProfile		INTEGER,         
     wwpLeosTrafficProfileStdDot1dStatus			RowStatus
 } 
 
 wwpLeosTrafficProfileStdDot1d    OBJECT-TYPE
     SYNTAX         INTEGER (0..7)
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies the dot1d priority for the associated
	      standard profile entry in the wwpLeosTrafficProfileStdDot1dTable
	      table."
     ::= { wwpLeosTrafficProfileStdDot1dEntry 1 }  
     
 wwpLeosTrafficProfileStdDot1dToProfile    OBJECT-TYPE
     SYNTAX         INTEGER (1..512)
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the profile to which wwpLeosTrafficProfileStdDot1d 
	      must be mapped to."
     ::= { wwpLeosTrafficProfileStdDot1dEntry 2 }
 
 wwpLeosTrafficProfileStdDot1dStatus    OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdDot1dStatus to 'createandgo'. 
	      - set wwpLeosTrafficProfileStdDot1dToProfile to valid profile.
	      
	      To delete entry set wwpLeosTrafficProfileStdDot1dStatus to destroy."
     ::= { wwpLeosTrafficProfileStdDot1dEntry 3 }
 
 --
 -- Std profile IP Prec table
 -- 
 wwpLeosTrafficProfileStdIpPrecTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileStdIpPrecEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of standard ip precedence traffic profile entries.
	      To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdIpPrecStatus to 'createandgo'. 
	      - set wwpLeosTrafficProfileStdIpPrecToProfile to valid profile.
	      
	      To delete entry set wwpLeosTrafficProfileStdIpPrecStatus to destroy."
     ::= { wwpLeosTrafficProfile 6 }
		
 wwpLeosTrafficProfileStdIpPrecEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileStdIpPrecEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A standard ip precedence traffic profile entry in the wwpLeosTrafficProfileStdTable."
     INDEX { wwpLeosTrafficProfilePort , wwpLeosTrafficProfileStdIpPrec}    
     ::= { wwpLeosTrafficProfileStdIpPrecTable 1 }
     
 WwpLeosTrafficProfileStdIpPrecEntry ::= SEQUENCE {
     wwpLeosTrafficProfileStdIpPrec				INTEGER,
     wwpLeosTrafficProfileStdIpPrecToProfile		INTEGER,     
     wwpLeosTrafficProfileStdIpPrecStatus		RowStatus
 } 
 
 wwpLeosTrafficProfileStdIpPrec    OBJECT-TYPE
     SYNTAX         INTEGER (0..7)
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies the ip precedence for the associated
	      standard profile entry in wwpLeosTrafficProfileStdTable."
     ::= { wwpLeosTrafficProfileStdIpPrecEntry 1 }  
     
 wwpLeosTrafficProfileStdIpPrecToProfile    OBJECT-TYPE
     SYNTAX         INTEGER (1..512)
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the profile to which wwpLeosTrafficProfileStdIpPrec 
	      must be mapped to."
     ::= { wwpLeosTrafficProfileStdIpPrecEntry 2 }
 
 wwpLeosTrafficProfileStdIpPrecStatus    OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdIpPrecStatus to 'createandgo'. 
	      - set wwpLeosTrafficProfileStdIpPrecToProfile to valid profile.
	      
	      To delete entry set wwpLeosTrafficProfileStdIpPrecStatus to destroy."
     ::= { wwpLeosTrafficProfileStdIpPrecEntry 3 }
 
 --
 -- Std profile phb table
 -- 
 wwpLeosTrafficProfileStdPhbTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileStdPhbEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of standard phb traffic profile entries.
	      To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdPhbStatus to 'createandgo'. 
	      - set wwpLeosTrafficProfileStdPhbToProfile to valid profile.
	      
	      To delete entry set wwpLeosTrafficProfileStdPhbStatus to destroy."
     ::= { wwpLeosTrafficProfile 7 }
		
 wwpLeosTrafficProfileStdPhbEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileStdPhbEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A standard Phb traffic profile entry in the wwpLeosTrafficProfileStdTable."
     INDEX { wwpLeosTrafficProfilePort , wwpLeosTrafficProfileStdPhb}    
     ::= { wwpLeosTrafficProfileStdPhbTable 1 }
     
 WwpLeosTrafficProfileStdPhbEntry ::= SEQUENCE {
     wwpLeosTrafficProfileStdPhb					INTEGER,
     wwpLeosTrafficProfileStdPhbToProfile		INTEGER,     
     wwpLeosTrafficProfileStdPhbStatus			RowStatus
 } 
 
 wwpLeosTrafficProfileStdPhb    OBJECT-TYPE
     SYNTAX         INTEGER  {
			cs0(1),
			cs1(2),
			cs2(3),
			cs3(4),
			cs4(5),
			cs5(6),
			cs6(7),
			cs7(8),
			af1(9),
			af2(10),
			af3(11),
			af4(12),
			ef(13)
		    }
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies the diff-serv values for the associated
	      standard profile entry in wwpLeosTrafficProfileStdTable."
     ::= { wwpLeosTrafficProfileStdPhbEntry 1 }
     
 wwpLeosTrafficProfileStdPhbToProfile    OBJECT-TYPE
     SYNTAX         INTEGER (1..32)
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the profile to which wwpLeosTrafficProfileStdPhb 
	      must be mapped to."
     ::= { wwpLeosTrafficProfileStdPhbEntry 2 }  
 
 wwpLeosTrafficProfileStdPhbStatus    OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdPhbStatus to 'createandgo'. 
	      - set wwpLeosTrafficProfileStdPhbToProfile to valid profile.
	      
	      To delete entry set wwpLeosTrafficProfileStdPhbStatus to destroy."
     ::= { wwpLeosTrafficProfileStdPhbEntry 3 } 
     
  --
  -- Cascaded Profile Stats 
  -- 
  wwpLeosTrafficProfileCascadedStatsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileCascadedStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       deprecated
     DESCRIPTION
	     "A table of cascaded profile stats."
     ::= { wwpLeosTrafficProfile 8 }
		
 wwpLeosTrafficProfileCascadedStatsEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileCascadedStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       deprecated
     DESCRIPTION
	     "A cascaded traffic profile entry in the wwpLeosTrafficProfileCascadedStatsTable."
     INDEX { wwpLeosTrafficProfilePort , wwpLeosTrafficProfileCascadedIndx }    
     ::= { wwpLeosTrafficProfileCascadedStatsTable 1 }
     
 WwpLeosTrafficProfileCascadedStatsEntry ::= SEQUENCE {
     wwpLeosTrafficProfileCascadedAcceptedBytesHi	Counter32,
     wwpLeosTrafficProfileCascadedAcceptedBytesLo	Counter32,
     wwpLeosTrafficProfileCascadedDroppedBytesHi	Counter32,
     wwpLeosTrafficProfileCascadedDroppedBytesLo	Counter32,
     wwpLeosTrafficProfileCascadedRemarkedBytesHi	Counter32,
     wwpLeosTrafficProfileCascadedRemarkedBytesLo	Counter32
 }
 
 wwpLeosTrafficProfileCascadedAcceptedBytesHi    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the higher bytes of accepted frames of 
	      given cascaded profile."
     ::= { wwpLeosTrafficProfileCascadedStatsEntry 1 }  
 
 wwpLeosTrafficProfileCascadedAcceptedBytesLo    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the lower bytes of accepted frames of 
	      given cascaded profile."
     ::= { wwpLeosTrafficProfileCascadedStatsEntry 2 }

 wwpLeosTrafficProfileCascadedDroppedBytesHi    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the higher bytes of dropped frames of 
	      given cascaded profile."
     ::= { wwpLeosTrafficProfileCascadedStatsEntry 3 }
  
 wwpLeosTrafficProfileCascadedDroppedBytesLo    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the lower bytes of dropped frames of 
	      given cascaded profile."
     ::= { wwpLeosTrafficProfileCascadedStatsEntry 4 }

  wwpLeosTrafficProfileCascadedRemarkedBytesHi    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the higher bytes of remarked frames of 
	      given cascaded profile."
     ::= { wwpLeosTrafficProfileCascadedStatsEntry 5 }

  wwpLeosTrafficProfileCascadedRemarkedBytesLo    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the lower bytes of remarked frames of 
	      given cascaded profile."
     ::= { wwpLeosTrafficProfileCascadedStatsEntry 6 }  
 
  --
  -- Standard Profile Stats 
  -- 
  wwpLeosTrafficProfileStdStatsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileStdStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of standard profile stats."
     ::= { wwpLeosTrafficProfile 9 }
		
 wwpLeosTrafficProfileStdStatsEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileStdStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "The entry in wwpLeosTrafficProfileStdStatsTable."
     INDEX { wwpLeosTrafficProfilePort , wwpLeosTrafficProfileStdIndx  }    
     ::= { wwpLeosTrafficProfileStdStatsTable 1 }
     
 WwpLeosTrafficProfileStdStatsEntry ::= SEQUENCE {
     wwpLeosTrafficProfileStdAcceptedBytesHi	Counter32,
     wwpLeosTrafficProfileStdAcceptedBytesLo	Counter32,
     wwpLeosTrafficProfileStdDroppedBytesHi	Counter32,
     wwpLeosTrafficProfileStdDroppedBytesLo	Counter32     
 }
 
 wwpLeosTrafficProfileStdAcceptedBytesHi    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies the higher bytes of accepted frames of 
	      given standard profile."
     ::= { wwpLeosTrafficProfileStdStatsEntry 1 }  
 
 wwpLeosTrafficProfileStdAcceptedBytesLo    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies the lower bytes of accepted frames of 
	      given standard profile."
     ::= { wwpLeosTrafficProfileStdStatsEntry 2 }

 wwpLeosTrafficProfileStdDroppedBytesHi    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies the higher bytes of dropped frames of 
	      given standard profile."
     ::= { wwpLeosTrafficProfileStdStatsEntry 3 }
  
 wwpLeosTrafficProfileStdDroppedBytesLo    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies the higher bytes of dropped frames of 
	      given standard profile."
     ::= { wwpLeosTrafficProfileStdStatsEntry 4 }
 
 --
-- cascaded traffic profile global table
-- 
 wwpLeosTrafficProfileCascadedGlobalTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileCascadedGlobalEntry
     MAX-ACCESS   not-accessible
     STATUS       deprecated
     DESCRIPTION
	     "A table of global attributes used by cascaded traffic profile table.
	      To create entry in this table following criteria must be met.
	      - All indexes must be specified.
	      - wwpLeosTrafficProfileCascadedGlobalDot1d,wwpLeosTrafficProfileCascadedGlobalIpPrec and 
	        wwpLeosTrafficProfileCascadedGlobalDscp may be specified.
	      - wwpLeosTrafficProfileCascadedGlobalName may be specified.
	      - wwpLeosTrafficProfileCascadedGlobalStatus must be set to createandgo"	      
     ::= { wwpLeosTrafficProfile 10 }
		
 wwpLeosTrafficProfileCascadedGlobalEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileCascadedGlobalEntry
     MAX-ACCESS   not-accessible
     STATUS       deprecated
     DESCRIPTION
	     "A global cascaded traffic profile entry in the wwpLeosTrafficProfileCascadedGlobalTable."
     INDEX {wwpLeosTrafficProfileCascadedIndx}    
     ::= { wwpLeosTrafficProfileCascadedGlobalTable 1 }
     
 WwpLeosTrafficProfileCascadedGlobalEntry ::= SEQUENCE {
     wwpLeosTrafficProfileCascadedGlobalDot1d		INTEGER,
     wwpLeosTrafficProfileCascadedGlobalIpPrec		INTEGER,
     wwpLeosTrafficProfileCascadedGlobalDscp		INTEGER,
     wwpLeosTrafficProfileCascadedGlobalName		DisplayString,     
     wwpLeosTrafficProfileCascadedGlobalStatus		RowStatus
 }
 
     
 wwpLeosTrafficProfileCascadedGlobalDot1d    OBJECT-TYPE
     SYNTAX         INTEGER (-1..7)
     MAX-ACCESS     read-write
     STATUS         deprecated
     DESCRIPTION
	     "This specifies the dot1d priority for a given cascaded traffic profile.
	      If this object returns -1 then it means the value was not set by user
	      and thus doesn't care."
     ::= { wwpLeosTrafficProfileCascadedGlobalEntry 1 }

 wwpLeosTrafficProfileCascadedGlobalIpPrec    OBJECT-TYPE
     SYNTAX         INTEGER (-1..7)
     MAX-ACCESS     read-write
     STATUS         deprecated
     DESCRIPTION
	     "This specifies the ip precedence value for a given cascaded traffic profile.
	      If this object returns -1 then it means the value was not set by user
	      and thus doesn't care."
     ::= { wwpLeosTrafficProfileCascadedGlobalEntry 2 }

  wwpLeosTrafficProfileCascadedGlobalDscp    OBJECT-TYPE
     SYNTAX         INTEGER (-1..63)
     MAX-ACCESS     read-write
     STATUS         deprecated
     DESCRIPTION
	     "This specifies the dscp value for a given cascaded traffic profile.
	      If this object returns -1 then it means the value was not set by user
	      and thus doesn't care."
     ::= { wwpLeosTrafficProfileCascadedGlobalEntry 3 }
  
  wwpLeosTrafficProfileCascadedGlobalName  OBJECT-TYPE
     SYNTAX       DisplayString(SIZE (0..15))
     MAX-ACCESS   read-write
     STATUS       deprecated
     DESCRIPTION
	     "The name associated with this profile.  This must be unique name per profile.
         The name does not have to be set on create.  However, when updating the name,
         it must have some value - zero-string not support." 
     ::= { wwpLeosTrafficProfileCascadedGlobalEntry 4 }  

  wwpLeosTrafficProfileCascadedGlobalStatus    OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         deprecated
     DESCRIPTION
	     "Setting this object to 'createandgo' will result in creating an global 
	      cascaded traffic profile entry.
	      Setting this object to 'destroy' will delete the entry from the table."
     ::= { wwpLeosTrafficProfileCascadedGlobalEntry 5 }  
  --
  -- Cascaded Profile  Total Stats 
  -- 
  wwpLeosTrafficProfileCascadedTotalStatsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileCascadedTotalStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       deprecated
     DESCRIPTION
	     "A table of cascaded profile stats."
     ::= { wwpLeosTrafficProfile 11 }
		
 wwpLeosTrafficProfileCascadedTotalStatsEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileCascadedTotalStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       deprecated
     DESCRIPTION
	     "A cascaded traffic profile entry in the wwpLeosTrafficProfileCascadedTotalStatsTable."
     INDEX { wwpLeosTrafficProfilePort , wwpLeosTrafficProfileCascadedIndx }    
     ::= { wwpLeosTrafficProfileCascadedTotalStatsTable 1 }
     
 WwpLeosTrafficProfileCascadedTotalStatsEntry ::= SEQUENCE {
     wwpLeosTrafficProfileCascadedTotalAcceptedBytesHi	Counter32,
     wwpLeosTrafficProfileCascadedTotalAcceptedBytesLo	Counter32,
     wwpLeosTrafficProfileCascadedTotalDroppedBytesHi	Counter32,
     wwpLeosTrafficProfileCascadedTotalDroppedBytesLo	Counter32,
     wwpLeosTrafficProfileCascadedTotalRemarkedBytesHi	Counter32,
     wwpLeosTrafficProfileCascadedTotalRemarkedBytesLo	Counter32
 }
 
 wwpLeosTrafficProfileCascadedTotalAcceptedBytesHi    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the higher bytes of accepted frames of 
	      given cascaded profile."
     ::= { wwpLeosTrafficProfileCascadedTotalStatsEntry 1 }  
 
 wwpLeosTrafficProfileCascadedTotalAcceptedBytesLo    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the lower bytes of accepted frames of 
	      given cascaded profile."
     ::= { wwpLeosTrafficProfileCascadedTotalStatsEntry 2 }

 wwpLeosTrafficProfileCascadedTotalDroppedBytesHi    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the higher bytes of dropped frames of 
	      given cascaded profile."
     ::= { wwpLeosTrafficProfileCascadedTotalStatsEntry 3 }
  
 wwpLeosTrafficProfileCascadedTotalDroppedBytesLo    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the lower bytes of dropped frames of 
	      given cascaded profile."
     ::= { wwpLeosTrafficProfileCascadedTotalStatsEntry 4 }

  wwpLeosTrafficProfileCascadedTotalRemarkedBytesHi    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the higher bytes of remarked frames of 
	      given cascaded profile."
     ::= { wwpLeosTrafficProfileCascadedTotalStatsEntry 5 }

  wwpLeosTrafficProfileCascadedTotalRemarkedBytesLo    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         deprecated
     DESCRIPTION
	     "This object specifies the lower bytes of remarked frames of 
	      given cascaded profile."
     ::= { wwpLeosTrafficProfileCascadedTotalStatsEntry 6 }  
 
  --
  -- Standard Profile Total Stats 
  -- 
  wwpLeosTrafficProfileStdTotalStatsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileStdTotalStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of standard profile stats."
     ::= { wwpLeosTrafficProfile 12 }
		
 wwpLeosTrafficProfileStdTotalStatsEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileStdTotalStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "The entry in wwpLeosTrafficProfileStdTotalStatsTable."
     INDEX { wwpLeosTrafficProfilePort , wwpLeosTrafficProfileStdIndx  }    
     ::= { wwpLeosTrafficProfileStdTotalStatsTable 1 }
     
 WwpLeosTrafficProfileStdTotalStatsEntry ::= SEQUENCE {
     wwpLeosTrafficProfileStdTotalAcceptedBytesHi	Counter32,
     wwpLeosTrafficProfileStdTotalAcceptedBytesLo	Counter32,
     wwpLeosTrafficProfileStdTotalDroppedBytesHi	Counter32,
     wwpLeosTrafficProfileStdTotalDroppedBytesLo	Counter32     
 }
 
 wwpLeosTrafficProfileStdTotalAcceptedBytesHi    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies the higher bytes of accepted frames of 
	      given standard profile."
     ::= { wwpLeosTrafficProfileStdTotalStatsEntry 1 }  
 
 wwpLeosTrafficProfileStdTotalAcceptedBytesLo    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies the lower bytes of accepted frames of 
	      given standard profile."
     ::= { wwpLeosTrafficProfileStdTotalStatsEntry 2 }

 wwpLeosTrafficProfileStdTotalDroppedBytesHi    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies the higher bytes of dropped frames of 
	      given standard profile."
     ::= { wwpLeosTrafficProfileStdTotalStatsEntry 3 }
  
 wwpLeosTrafficProfileStdTotalDroppedBytesLo    OBJECT-TYPE
     SYNTAX         Counter32
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
	     "This object specifies the higher bytes of dropped frames of 
	      given standard profile."
     ::= { wwpLeosTrafficProfileStdTotalStatsEntry 4 }
 
  -- Std Profile Vlan Table
 
  wwpLeosTrafficProfileStdVlanTable  OBJECT-TYPE
    SYNTAX  SEQUENCE OF WwpLeosTrafficProfileStdVlanEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
    	"A table of Std Vlan Traffic Profile Entries.
    	 To create entry in the table following criteria must be met
    	 -- set wwpLeosTrafficProfileStdVlanStatus to 'createandgo'.
    	 -- set wwpLeosTrafficProfileStdVlan to valid profile.
    	 
    	 To delete entry set wwpLeosTrafficProfileStdVlanStatus to destroy."
    ::= { wwpLeosTrafficProfile 14 }
   
   wwpLeosTrafficProfileStdVlanEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileStdVlanEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A standard Dscp traffic profile entry in the wwpLeosTrafficProfileStdTable."
     INDEX { wwpLeosTrafficProfilePort , wwpLeosTrafficProfileStdVlanIndex}    
     ::= { wwpLeosTrafficProfileStdVlanTable 1 }
     
 WwpLeosTrafficProfileStdVlanEntry ::= SEQUENCE {
     wwpLeosTrafficProfileStdVlanIndex				INTEGER,
     wwpLeosTrafficProfileStdVlanToProfile		INTEGER,     
     wwpLeosTrafficProfileStdVlanStatus		    RowStatus
 } 
 
 wwpLeosTrafficProfileStdVlanIndex    OBJECT-TYPE
     SYNTAX         INTEGER (1..4094)
     MAX-ACCESS     not-accessible
     STATUS         current
     DESCRIPTION
	     "This object specifies the Vlan for the associated
	      standard profile entry in wwpLeosTrafficProfileStdTable."
     ::= { wwpLeosTrafficProfileStdVlanEntry 1 }  
     
 wwpLeosTrafficProfileStdVlanToProfile    OBJECT-TYPE
     SYNTAX         INTEGER (1..512)
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "This object specifies the profile to which wwpLeosTrafficProfileStdVlan 
	      must be mapped to."
     ::= { wwpLeosTrafficProfileStdVlanEntry 2 }
 
 wwpLeosTrafficProfileStdVlanStatus    OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdVlanStatus to 'createandgo'. 
	      - set wwpLeosTrafficProfileStdVlanToProfile to valid profile.
	      
	      To delete entry set wwpLeosTrafficProfileStdVlanStatus to destroy."
     ::= { wwpLeosTrafficProfileStdVlanEntry 3 }     
  
 --
 -- Std profile DSCP table
 --                 
 
   wwpLeosTrafficProfileStdDscpTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileStdDscpEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of standard Dscp traffic profile entries.
	      To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdDscpStatus to 'createandgo'. 
	      - set wwpLeosTrafficProfileStdDscpToProfile to valid profile.
	      
	      To delete entry set wwpLeosTrafficProfileStdDscpStatus to destroy."
     ::= { wwpLeosTrafficProfile 15 }
		
 wwpLeosTrafficProfileStdDscpEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileStdDscpEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A standard Dscp traffic profile entry in the wwpLeosTrafficProfileStdTable."
     INDEX { wwpLeosTrafficProfilePort , wwpLeosTrafficProfileStdDscp}    
     ::= { wwpLeosTrafficProfileStdDscpTable 1 }
     
 WwpLeosTrafficProfileStdDscpEntry ::= SEQUENCE {
     wwpLeosTrafficProfileStdDscp				INTEGER,
     wwpLeosTrafficProfileStdDscpToProfile		INTEGER,     
     wwpLeosTrafficProfileStdDscpStatus		RowStatus
 } 
 
 wwpLeosTrafficProfileStdDscp    OBJECT-TYPE
     SYNTAX         INTEGER (0..63)
     MAX-ACCESS     not-accessible
     STATUS         current
     DESCRIPTION
	     "This object specifies the Dscp for the associated
	      standard profile entry in wwpLeosTrafficProfileStdTable."
     ::= { wwpLeosTrafficProfileStdDscpEntry 1 }  
     
 wwpLeosTrafficProfileStdDscpToProfile    OBJECT-TYPE
     SYNTAX         INTEGER (1..512)
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "This object specifies the profile to which wwpLeosTrafficProfileStdDscp 
	      must be mapped to."
     ::= { wwpLeosTrafficProfileStdDscpEntry 2 }
 
 wwpLeosTrafficProfileStdDscpStatus    OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdDscpStatus to 'createandgo'. 
	      - set wwpLeosTrafficProfileStdDscpToProfile to valid profile.
	      
	      To delete entry set wwpLeosTrafficProfileStdDscpStatus to destroy."
     ::= { wwpLeosTrafficProfileStdDscpEntry 3 }  
     
 --
 -- Meter-Pool Table
 --
 wwpLeosTrafficProfileMeterPoolTable   OBJECT-TYPE
    SYNTAX  SEQUENCE OF WwpLeosTrafficProfileMeterPoolEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
       " A Table of Meter Pool"
    ::= { wwpLeosTrafficProfile 16 } 
    
  wwpLeosTrafficProfileMeterPoolEntry OBJECT-TYPE
     SYNTAX      WwpLeosTrafficProfileMeterPoolEntry
     MAX-ACCESS not-accessible
     STATUS current
     DESCRIPTION
        " A Meter Pool Entry in wwpLeosTrafficProfileMeterPoolTable"
     INDEX { wwpLeosTrafficProfileMeterPoolIndex }
   ::= {wwpLeosTrafficProfileMeterPoolTable 1 }
        
 WwpLeosTrafficProfileMeterPoolEntry ::= SEQUENCE {
     wwpLeosTrafficProfileMeterPoolIndex  INTEGER,
     wwpLeosTrafficProfileMeterPoolName   DisplayString,
     wwpLeosTrafficProfileMeterPoolNumOfMeters  INTEGER,
     wwpLeosTrafficProfileMeterPoolMetersUsed   INTEGER,
     wwpLeosTrafficProfileMeterPoolNumOfStats  INTEGER,
     wwpLeosTrafficProfileMeterPoolStatsUsed   INTEGER,
     wwpLeosTrafficProfileMeterPoolNumOfClassifiers  INTEGER,
     wwpLeosTrafficProfileMeterPoolClassifiersUsed   INTEGER
  }
  wwpLeosTrafficProfileMeterPoolIndex OBJECT-TYPE
     SYNTAX 	INTEGER(1..8)  
     MAX-ACCESS    not-accessible
     STATUS 		current
     DESCRIPTION 
     	" A Meter Pool Index"
   ::= { wwpLeosTrafficProfileMeterPoolEntry 1}
   
  wwpLeosTrafficProfileMeterPoolName OBJECT-TYPE
     SYNTAX  DisplayString(SIZE (0..15))
     MAX-ACCESS read-only
     STATUS current
     DESCRIPTION
        "A Meter Pool Name"
  ::= { wwpLeosTrafficProfileMeterPoolEntry 2}
  
  wwpLeosTrafficProfileMeterPoolNumOfMeters OBJECT-TYPE
     SYNTAX INTEGER
     MAX-ACCESS read-only
     STATUS current
     DESCRIPTION 
     	"Number of Meters for a pool"
  ::= {wwpLeosTrafficProfileMeterPoolEntry 3}
  
  wwpLeosTrafficProfileMeterPoolMetersUsed OBJECT-TYPE
     SYNTAX INTEGER
     MAX-ACCESS  read-only
     STATUS current
     DESCRIPTION
     	"Number of Used Meters in a Pool"
  ::= {wwpLeosTrafficProfileMeterPoolEntry 4}  
  
  wwpLeosTrafficProfileMeterPoolNumOfStats OBJECT-TYPE
     SYNTAX INTEGER
     MAX-ACCESS read-only
     STATUS current
     DESCRIPTION 
     	"Number of Stats Counters for a pool"
  ::= {wwpLeosTrafficProfileMeterPoolEntry 5}
  
  wwpLeosTrafficProfileMeterPoolStatsUsed OBJECT-TYPE
     SYNTAX INTEGER
     MAX-ACCESS  read-only
     STATUS current
     DESCRIPTION
     	"Number of Used Stats Counters in a Pool"
  ::= {wwpLeosTrafficProfileMeterPoolEntry 6}  

  wwpLeosTrafficProfileMeterPoolNumOfClassifiers OBJECT-TYPE
     SYNTAX INTEGER
     MAX-ACCESS read-only
     STATUS current
     DESCRIPTION 
     	"Number of Classifiers for a pool"
  ::= {wwpLeosTrafficProfileMeterPoolEntry 7}
  
  wwpLeosTrafficProfileMeterPoolClassifiersUsed OBJECT-TYPE
     SYNTAX INTEGER
     MAX-ACCESS  read-only
     STATUS current
     DESCRIPTION
     	"Number of Used Classifiers in a Pool"
  ::= {wwpLeosTrafficProfileMeterPoolEntry 8}  
     	   
     
--
-- Tos Stamp
-- 
  wwpLeosTrafficProfileTosStampTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileTosStampEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of TosStamps entries."
     ::= { wwpLeosTrafficProfile 20 }
 
 wwpLeosTrafficProfileTosStampEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileTosStampEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "The entry in wwpLeosTrafficProfileTosStampTable."
     INDEX { wwpLeosTrafficProfilePort  }    
     ::= { wwpLeosTrafficProfileTosStampTable 1 }
      
 WwpLeosTrafficProfileTosStampEntry ::= SEQUENCE {
     wwpLeosTrafficProfileTosStampState         	INTEGER,
     wwpLeosTrafficProfileTosStampValue     	INTEGER    
 }
 wwpLeosTrafficProfileTosStampState    OBJECT-TYPE
     SYNTAX         INTEGER {
                             on(1),
                             off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the TOS Stamp on a port"
     ::= { wwpLeosTrafficProfileTosStampEntry 1 }

 wwpLeosTrafficProfileTosStampValue    OBJECT-TYPE
     SYNTAX         INTEGER(0..63)
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the Value of the TOS Stamp. For IP 
             prec left shift the value by 3 bits."
     ::= { wwpLeosTrafficProfileTosStampEntry  2}

--
-- IP/DSCP enable disable
-- 
  wwpLeosTrafficProfileIpDscpTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileIpDscpEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of IpDscp entries."
     ::= { wwpLeosTrafficProfile 21 }
 
 wwpLeosTrafficProfileIpDscpEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileIpDscpEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "The entry in wwpLeosTrafficProfileIpDscpTable."
     INDEX { wwpLeosTrafficProfilePort  }    
     ::= { wwpLeosTrafficProfileIpDscpTable 1 }
      
 WwpLeosTrafficProfileIpDscpEntry ::= SEQUENCE {
     wwpLeosTrafficProfileIpp0Cs0State         	INTEGER,
     wwpLeosTrafficProfileIpp1Cs1State     	INTEGER,
     wwpLeosTrafficProfileIpp2Cs2State         	INTEGER,    
     wwpLeosTrafficProfileIpp3Cs3State         	INTEGER,
     wwpLeosTrafficProfileIpp4Cs4State         	INTEGER,
     wwpLeosTrafficProfileIpp5Cs5State         	INTEGER,
     wwpLeosTrafficProfileIpp6Cs6State         	INTEGER,
     wwpLeosTrafficProfileIpp7Cs7State         	INTEGER,
     wwpLeosTrafficProfileAf1State              INTEGER,
     wwpLeosTrafficProfileAf2State              INTEGER,
     wwpLeosTrafficProfileAf3State              INTEGER,
     wwpLeosTrafficProfileAf4State              INTEGER,
     wwpLeosTrafficProfileEfState               INTEGER
 }
 wwpLeosTrafficProfileIpp0Cs0State    OBJECT-TYPE
     SYNTAX        INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Ipp0 or cs0 enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 1 }

 wwpLeosTrafficProfileIpp1Cs1State    OBJECT-TYPE
     SYNTAX          INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Ipp1 or cs1 enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 2 }

 wwpLeosTrafficProfileIpp2Cs2State    OBJECT-TYPE
     SYNTAX          INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Ipp0 or cs0 enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 3 }

 wwpLeosTrafficProfileIpp3Cs3State    OBJECT-TYPE
     SYNTAX          INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Ipp3 or cs3 enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 4 }

 wwpLeosTrafficProfileIpp4Cs4State    OBJECT-TYPE
     SYNTAX          INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Ipp4 or cs4 enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 5 }

 wwpLeosTrafficProfileIpp5Cs5State    OBJECT-TYPE
     SYNTAX          INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Ipp5 or cs5 enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 6 }

 wwpLeosTrafficProfileIpp6Cs6State    OBJECT-TYPE
     SYNTAX          INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Ipp6 or cs6 enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 7 }

 wwpLeosTrafficProfileIpp7Cs7State    OBJECT-TYPE
     SYNTAX          INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Ipp7 or cs7 enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 8 }

 wwpLeosTrafficProfileAf1State    OBJECT-TYPE
     SYNTAX          INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Af1 enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 9 }

 wwpLeosTrafficProfileAf2State    OBJECT-TYPE
     SYNTAX          INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Af2 enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 10 }

 wwpLeosTrafficProfileAf3State    OBJECT-TYPE
     SYNTAX          INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Af3 enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 11}

 wwpLeosTrafficProfileAf4State    OBJECT-TYPE
     SYNTAX          INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Af4 enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 12 }

 wwpLeosTrafficProfileEfState    OBJECT-TYPE
     SYNTAX          INTEGER {
                    on(1),
                    off(2)}
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object specifies the state of the Ef enable disable on a port"
     ::= { wwpLeosTrafficProfileIpDscpEntry 13 }
 
 
 --
 -- Std profile stdVlanDot1DPri table
 -- 
 wwpLeosTrafficProfileStdVlanDot1dTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileStdVlanDot1dEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of Std Vlan dot1d traffic profile entries.	      
	      To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdDot1dStatus to 'createandgo'.
	      
	      To delete entry set wwpLeosTrafficProfileStdDot1dStatus to destroy."
     ::= { wwpLeosTrafficProfile 40 }
		
 wwpLeosTrafficProfileStdVlanDot1dEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileStdVlanDot1dEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A standard dot1d traffic profile entry in the wwpLeosTrafficProfileStdDot1dTable."
     INDEX { wwpLeosTrafficProfilePort, wwpLeosTrafficProfileStdDot1d, wwpLeosTrafficProfileStdIndx}    
     ::= { wwpLeosTrafficProfileStdVlanDot1dTable 1 }
     
 WwpLeosTrafficProfileStdVlanDot1dEntry ::= SEQUENCE {
     wwpLeosTrafficProfileStdVlanDot1dStatus			RowStatus
 } 
 
 wwpLeosTrafficProfileStdVlanDot1dStatus    OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdDot1dStatus to 'createandgo'.
	      
	      To delete entry set wwpLeosTrafficProfileStdDot1dStatus to destroy."
     ::= { wwpLeosTrafficProfileStdVlanDot1dEntry 1 }


--
 -- Std profile stdVlanIpPrec table
 -- 
 wwpLeosTrafficProfileStdVlanIpPrecTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileStdVlanIpPrecEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of Std Vlan-Ip prec traffic profile entries.	      
	      To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdVlanIpPrecStatus to 'createandgo'.	      
	      To delete entry set wwpLeosTrafficProfileStdVlanIpPrecStatus to destroy."
     ::= { wwpLeosTrafficProfile 41 }
		
 wwpLeosTrafficProfileStdVlanIpPrecEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileStdVlanIpPrecEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A standard vlan-Ip prec traffic profile entry in the wwpLeosTrafficProfileStdVlanIpPrecTable."
     INDEX { wwpLeosTrafficProfilePort ,wwpLeosTrafficProfileStdIpPrec, wwpLeosTrafficProfileStdIndx}    
     ::= { wwpLeosTrafficProfileStdVlanIpPrecTable 1 }
     
 WwpLeosTrafficProfileStdVlanIpPrecEntry ::= SEQUENCE {
     wwpLeosTrafficProfileStdVlanIpPrecStatus			RowStatus
 } 
 
  
 wwpLeosTrafficProfileStdVlanIpPrecStatus    OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdVlanIpPrecStatus to 'createandgo'.	      
	      To delete entry set wwpLeosTrafficProfileStdVlanIpPrecStatus to destroy."
     ::= { wwpLeosTrafficProfileStdVlanIpPrecEntry 1 }

 
 --
 -- Std profile stdVlanDscp table
 -- 
 wwpLeosTrafficProfileStdVlanDscpTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTrafficProfileStdVlanDscpEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A table of Std Vlan-dscp traffic profile entries.	      
	      To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdVlanDscpStatus to 'createandgo'.
	      
	      To delete entry set wwpLeosTrafficProfileStdVlanDscpStatus to destroy."
     ::= { wwpLeosTrafficProfile 42 }
		
 wwpLeosTrafficProfileStdVlanDscpEntry  OBJECT-TYPE
     SYNTAX       WwpLeosTrafficProfileStdVlanDscpEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
	     "A standard vlan-dscp traffic profile entry in the wwpLeosTrafficProfileStdVlanDscpTable."
     INDEX { wwpLeosTrafficProfilePort , wwpLeosTrafficProfileStdDscp, wwpLeosTrafficProfileStdIndx }    
     ::= { wwpLeosTrafficProfileStdVlanDscpTable 1 }
     
 WwpLeosTrafficProfileStdVlanDscpEntry ::= SEQUENCE {
     wwpLeosTrafficProfileStdVlanDscpStatus			RowStatus
 } 
 
  
 wwpLeosTrafficProfileStdVlanDscpStatus    OBJECT-TYPE
     SYNTAX         RowStatus
     MAX-ACCESS     read-create
     STATUS         current
     DESCRIPTION
	     "To create entry in the table following criteria must be met
	      - set wwpLeosTrafficProfileStdVlanDscpStatus to 'createandgo'.
	      
	      To delete entry set wwpLeosTrafficProfileStdVlanDscpStatus to destroy."
     ::= { wwpLeosTrafficProfileStdVlanDscpEntry 2 }

    
 END
 --
 -- WWP-LEOS-TRAFFIC-PROFILE-MIB
 --

 
 
 
 
 
  

