-- This file was included in WWP MIB release 04-07-01-0008
 --
 -- WWP-LEOS-PORT-XCVR-MIB.my
 --
 -- NOTE WELL
 -- Starting from LE21X 2.0, the object wwpXcvrPortHoldDownTime mentioned 
 -- in this MIB has been deprecated.
 -- NOTE WELL

 WWP-LEOS-PORT-XCVR-MIB DEFINITIONS ::= BEGIN

 IMPORTS 		
   Integer32, OBJECT-TYPE, MODULE-IDENTITY			
	    FROM SNMPv2-SMI			
   DisplayString, TruthValue
	    FROM SNMPv2-TC						
   wwpModules, wwpModulesLeos		
	    FROM WWP-SMI;
	
	
 wwpLeosPortXcvrMIB MODULE-IDENTITY
	    LAST-UPDATED "200603150000Z"
	    ORGANIZATION "Ciena, Inc"
	    CONTACT-INFO
		    "   Mib Meister
		  			115 North Sullivan Road
					Spokane Valley, WA 99037
		        	USA		 		
		        	Phone:  +1 509 242 9000
					Email:  support@ciena.com"
	    DESCRIPTION
		    "The MIB module for the WWP System physical transceiver devices."
		REVISION    "200603150000Z"
		DESCRIPTION
		    "Added notification wwpLeosPortXcvrSpeedInfoMissingNotification."
	    REVISION    "200104031700Z"
	    DESCRIPTION
		    "Initial creation."
	    ::= { wwpModulesLeos 4}
						
 --
 -- Node definitions
 --
	
 wwpLeosPortXcvrMIBObjects OBJECT IDENTIFIER ::= { wwpLeosPortXcvrMIB 1 }
 
 wwpLeosPortXcvr  OBJECT IDENTIFIER ::= { wwpLeosPortXcvrMIBObjects 1 }

 wwpLeosPortXcvrNotif  OBJECT IDENTIFIER ::= { wwpLeosPortXcvrMIBObjects 2 }

 -- Notifications 
  
 wwpLeosPortXcvrMIBNotificationPrefix  OBJECT IDENTIFIER ::= { wwpLeosPortXcvrMIB 2 } 
 wwpLeosPortXcvrMIBNotifications       OBJECT IDENTIFIER ::=  
                       { wwpLeosPortXcvrMIBNotificationPrefix 0 }

 -- Conformance information 
 
 wwpLeosPortXcvrMIBConformance OBJECT IDENTIFIER ::= { wwpLeosPortXcvrMIB 3 } 
 wwpLeosPortXcvrMIBCompliances OBJECT IDENTIFIER ::= { wwpLeosPortXcvrMIBConformance 1 } 		
 wwpLeosPortXcvrMIBGroups      OBJECT IDENTIFIER ::= { wwpLeosPortXcvrMIBConformance 2 }

		
 wwpLeosPortXcvrTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF WwpLeosPortXcvrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
	    "This table contains descriptions and settings for each of the 
	     physical transceiver devices."
    ::= { wwpLeosPortXcvr 1 }
		 
 wwpLeosPortXcvrEntry OBJECT-TYPE
    SYNTAX        WwpLeosPortXcvrEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION 
    	"The Transceiver Device Entry."
    INDEX { wwpLeosPortXcvrId }
    ::= { wwpLeosPortXcvrTable 1 }

 WwpLeosPortXcvrEntry ::= SEQUENCE {     
    wwpLeosPortXcvrId                INTEGER,    
    wwpLeosPortXcvrOperState         INTEGER,
    wwpLeosPortXcvrIdentiferType     INTEGER,
    wwpLeosPortXcvrExtIdentiferType  INTEGER,
    wwpLeosPortXcvrConnectorType     INTEGER,
    wwpLeosPortXcvrType		 INTEGER,
    wwpLeosPortXcvrVendorName	 	 DisplayString,
    wwpLeosPortXcvrVendorOUI	 	 OCTET STRING(SIZE(0..255)),
    wwpLeosPortXcvrVendorPN          DisplayString,    
    wwpLeosPortXcvrRevNum            DisplayString,
    wwpLeosPortXcvrSerialNum	     DisplayString,
    wwpLeosPortXcvrEncodingType	     INTEGER,
    wwpLeosPortXcvrMfgDate		     DisplayString,    
    wwpLeosPortXcvrComplianceVer     INTEGER,
    wwpLeosPortXcvrWaveLength	     INTEGER,
    wwpLeosPortXcvrTemperature	     INTEGER, 
    wwpLeosPortXcvrVcc				 INTEGER,
    wwpLeosPortXcvrBias				 INTEGER,
    wwpLeosPortXcvrRxPower		 	 INTEGER,
    wwpLeosPortXcvrTxState           INTEGER,
    wwpLeosPortXcvrTxFaultStatus     INTEGER,
    wwpLeosPortXcvrRxRateStatus      INTEGER,
    wwpLeosPortXcvr9by125um	 INTEGER,
    wwpLeosPortXcvr50by125um		 INTEGER,
    wwpLeosPortXcvr62dot5by125um	 INTEGER,
    wwpLeosPortXcvrCu				 INTEGER,
    wwpLeosPortXcvrTxOutputPw	 INTEGER,    
    wwpLeosPortXcvrLosState		 TruthValue,
    wwpLeosPortXcvrDiagSupported	 TruthValue,
    wwpLeosPortXcvrEnhDiagAlarmSupported	 TruthValue,
    wwpLeosPortXcvrEnhDiagSoftTxDisableSupported	 TruthValue,
    wwpLeosPortXcvrEnhDiagSoftTxFaultSupported	 TruthValue,
    wwpLeosPortXcvrEnhDiagRxLosSupported	 TruthValue,    
    wwpLeosPortXcvrHighTempAlarmThreshold	 Integer32,
    wwpLeosPortXcvrLowTempAlarmThreshold	 Integer32,
    wwpLeosPortXcvrHighVccAlarmThreshold	 Integer32,
    wwpLeosPortXcvrLowVccAlarmThreshold	 Integer32,
    wwpLeosPortXcvrHighBiasAlarmThreshold	 Integer32,
    wwpLeosPortXcvrLowBiasAlarmThreshold	 Integer32,
    wwpLeosPortXcvrHighTxPwAlarmThreshold	 Integer32,
    wwpLeosPortXcvrLowTxPwAlarmThreshold	 Integer32,
    wwpLeosPortXcvrHighRxPwAlarmThreshold	 Integer32,
    wwpLeosPortXcvrLowRxPwAlarmThreshold	 Integer32,
    wwpLeosPortXcvrLowRxPwAlarmThreshold	 Integer32,
    wwpLeosPortXcvrLowRxPwAlarmThreshold	 Integer32,
    wwpLeosPortXcvrEnhDiagRateSelectSupported	 TruthValue,
    wwpLeosPortXcvrAdminState			 INTEGER,
    wwpLeosPortXcvrXfpMinBitRate                     INTEGER,
    wwpLeosPortXcvrXfpMaxBitRate                     INTEGER,
    wwpLeosPortXcvrXfpLinkLenSmf1km                  INTEGER,
    wwpLeosPortXcvrXfpLinkLenE50u2m                  INTEGER,
    wwpLeosPortXcvrXfpLinkLen50u1m                   INTEGER,
    wwpLeosPortXcvrXfpLinkLen62dot5u1m               INTEGER,
    wwpLeosPortXcvrXfpLinkLenCopper1m                INTEGER,
    wwpLeosPortXcvrXfpDevTech                        INTEGER,
    wwpLeosPortXcvrXfpTransmitterTech                INTEGER,
    wwpLeosPortXcvrXfpCdrSupport                     INTEGER,
    wwpLeosPortXcvrXfpWaveLengthTol                  INTEGER,
    wwpLeosPortXcvrXfpMaxCaseTemp                    INTEGER,
    wwpLeosPortXcvrXfpMaxPower                       INTEGER,
    wwpLeosPortXcvrXfpMax5vCurrent                   INTEGER,
    wwpLeosPortXcvrXfpMax3p3vCurrent                 INTEGER,
    wwpLeosPortXcvrXfpMax1p8vCurrent                 INTEGER,
    wwpLeosPortXcvrXfpMaxNeg5p2vCurrent              INTEGER,
    wwpLeosPortXcvrXfpDiagMonitorType                INTEGER,
    wwpLeosPortXcvrXfpEnhancedOptions                INTEGER,
    wwpLeosPortXcvrXfpAuxMonitoringInput1            INTEGER,
    wwpLeosPortXcvrXfpAuxMonitoringInput2            INTEGER,
    wwpLeosPortXcvrAdminFrequency                    Unsigned32,
    wwpLeosPortXcvrXfpLaserFirstFrequency            Unsigned32,
    wwpLeosPortXcvrXfpLaserLastFrquency              Unsigned32,
    wwpLeosPortXcvrXfpMaxGridScacing                 INTEGER,
    wwpLeosPortXcvrXfpChannelNum                     INTEGER,
    wwpLeosPortXcvrXfpFrequencyError                 INTEGER,
    wwpLeosPortXcvrAdminWavelength                   Unsigned32,
    wwpLeosPortXcvrAdminChannel                      Unsigned32,
    wwpLeosPortXcvrXfpLaserFirstWavelenth            Unsigned32,
    wwpLeosPortXcvrXfpLaserLastWavelength            Unsigned32,
    wwpLeosPortXcvrXfpLaserFirstChannel              Unsigned32,
    wwpLeosPortXcvrXfpLaserLastChannel               Unsigned32,
    wwpLeosPortXcvrOperFrequency                     Unsigned32,
    wwpLeosPortXcvrOperWavelength                    Unsigned32
 }

 wwpLeosPortXcvrId OBJECT-TYPE
    SYNTAX           INTEGER (1..65535)
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
	    "The ID for the transceiver."
    ::= { wwpLeosPortXcvrEntry 1 } 

 wwpLeosPortXcvrOperState OBJECT-TYPE
    SYNTAX           INTEGER {
                        disabled(1),
                        enabled(2),
                        loopback(3),
                        notPresent(4),
                        faulted(5)
                     }
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
	    "The operational state of the transceiver."
    ::= { wwpLeosPortXcvrEntry 2 }

 wwpLeosPortXcvrIdentiferType OBJECT-TYPE
    SYNTAX           INTEGER {
                       unknown(1),
		       gbic(2),
		       solderedType(3),
		       sfp(4),
		       reserved(5),
		       vendorSpecific(6),
                       xbi(7),
                       xenpak(8),
                       xfp(9),
                       xff(10),
                       xfpe(11),
                       xpak(12),
                       x2(13)
                     }
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
	    "Type for the transceiver."
    ::= { wwpLeosPortXcvrEntry 3 }
   
 wwpLeosPortXcvrExtIdentiferType OBJECT-TYPE
    SYNTAX           INTEGER {
			   unknown(1),
			   sfp-gbic(2)
			}
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
	    "Extended identifier type for this transceiver."
    ::= { wwpLeosPortXcvrEntry 4 }

 wwpLeosPortXcvrConnectorType OBJECT-TYPE
    SYNTAX     		 INTEGER (1..65535)
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
	    "Type of connector.
	    	   unknown(1),
		       sc(2),
		       fiberChannelStyle1(3),
		       fiberChannelStyle2(4),
		       bnc/tnc(5),
		       coaxialHeader(6),
		       fiberJack(7),
		       lc(8),
		       mt-rj(9),
		       mu(10),
		       sg(11),
		       opticalPitTail(12),
		       reserved(13..32),
		       hssdc(33),
		       copperPitTail(34),
		       reserved(35..128),
		       vendorSpecific(129..256)."
    ::= { wwpLeosPortXcvrEntry 5 }

 wwpLeosPortXcvrType OBJECT-TYPE
    SYNTAX           INTEGER (1..65535)
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
	    "Type of Transceiver."
    ::= { wwpLeosPortXcvrEntry 6 }

 wwpLeosPortXcvrVendorName OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "String containing this transceiver's vendor name."
    ::= { wwpLeosPortXcvrEntry 7 }

 wwpLeosPortXcvrVendorOUI OBJECT-TYPE
    SYNTAX        OCTET STRING(SIZE(0..255))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "String containing this transceiver's vendor OUI."
    ::= { wwpLeosPortXcvrEntry 8 }

 wwpLeosPortXcvrVendorPN OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "String containing this transceiver's vendor OUI."
    ::= { wwpLeosPortXcvrEntry 9 }
 	
 wwpLeosPortXcvrRevNum   OBJECT-TYPE
    SYNTAX         DisplayString
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
	    "String containing this transceiver's part revision number."
    ::= { wwpLeosPortXcvrEntry 10 }

 wwpLeosPortXcvrSerialNum   OBJECT-TYPE
    SYNTAX         DisplayString
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
	    "String containing this transceiver's part serial number."
    ::= { wwpLeosPortXcvrEntry 11 } 		
  
 wwpLeosPortXcvrEncodingType OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "If wwpLeosPortXcvrIdentiferType is SFP, then the following values is defined for the encoding type:
	             unspecified(1),
		     8B10B(2),
		     4b5b(3),
		     NRZ(4),
		     Manchester(5),
		     SONET(6),
		     reserved(7-256)
	     If wwpLeosPortXcvrIdentiferType is XFP, then the following values is defined for the encoding type:
	             Bit 7:  64B/66B (yes/no)
	             Bit 6:  8B10B   (yes/no)
	             Bit 5:  Sonet Scrambled (yes/no)
	             Bit 4:  NRZ (yes/no)
	             Bit 3:  RZ (yes/no)
	             Bit 2:  Tx Dither Support (yes/no) 
	             Bit 1:  Reserved 
	             Bit 0:  Reserved
	     Multiple bits can be set at once in the case of XFP. 
	     For instance, to indicate support for NRZ(4) and Sonet scrambled (5), 
	     the user would see this object with the value of 16 + 32 = 48" 
    ::= { wwpLeosPortXcvrEntry 12 }

 wwpLeosPortXcvrMfgDate OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "The transceiver's manufacture date in string."
    ::= { wwpLeosPortXcvrEntry 13 }

 wwpLeosPortXcvrComplianceVer OBJECT-TYPE
    SYNTAX        INTEGER(1..4)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the compliance version.
	     Value 1 means digital diagnostic functionality 
	     not included or undefined
	     Value 2 means includes functionality defined in 
	     Rev 9.0 SFF-8472
	     Value 3 means TBD
	     Value 4 means TBD."
    ::= { wwpLeosPortXcvrEntry 14 }

 wwpLeosPortXcvrWaveLength OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the wavelength of the transceiver. Units are nano meter."
    ::= { wwpLeosPortXcvrEntry 15 }

 wwpLeosPortXcvrTemperature OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the temperature of the transceiver."
    ::= { wwpLeosPortXcvrEntry 16 }
 
 wwpLeosPortXcvrVcc OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the voltage of the transceiver."
    ::= { wwpLeosPortXcvrEntry 17 }
 
 wwpLeosPortXcvrBias OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the bias of the transceiver."
    ::= { wwpLeosPortXcvrEntry 18 }

 wwpLeosPortXcvrRxPower OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the measured receive power of the transceiver. 
	     Units are Watts."
    ::= { wwpLeosPortXcvrEntry 19 }

 wwpLeosPortXcvrTxState OBJECT-TYPE
    SYNTAX       INTEGER {	
		      enabled(1),
		      disabled(2)
	         }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
	    "Indicates whether this transceiver is currently set to transmit."
    ::= { wwpLeosPortXcvrEntry 20 }		
 		
 wwpLeosPortXcvrTxFaultStatus OBJECT-TYPE
    SYNTAX        INTEGER {	
		       fault(1),
		       noFault(2)
	     	  }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the fault status of this transceiver."
    ::= { wwpLeosPortXcvrEntry 21 }
 
 wwpLeosPortXcvrRxRateStatus OBJECT-TYPE
    SYNTAX        INTEGER {
			enabled(1),
			disabled(2)
			}
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the Rx rate status of this transceiver."
    ::= { wwpLeosPortXcvrEntry 22 }

 wwpLeosPortXcvr9by125um OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the link length for 9/125um fiber."
    ::= { wwpLeosPortXcvrEntry 23 }
 
 wwpLeosPortXcvr50by125um OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the link length for 50/125um fiber."
    ::= { wwpLeosPortXcvrEntry 24 }

 wwpLeosPortXcvr62dot5by125um OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the link length for 62.5/125um fiber."
    ::= { wwpLeosPortXcvrEntry 25 }

 wwpLeosPortXcvrCu OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the link length for copper."
    ::= { wwpLeosPortXcvrEntry 26 }

 wwpLeosPortXcvrTxOutputPw OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the Tx Output power for the transceiver.
	     Units are Watts."
    ::= { wwpLeosPortXcvrEntry 27 }
 
 wwpLeosPortXcvrLosState OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the LOS State for the transceiver."
    ::= { wwpLeosPortXcvrEntry 28 }

 wwpLeosPortXcvrDiagSupported OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates if diagnostics are supported on this transceiver."
    ::= { wwpLeosPortXcvrEntry 29 }

 wwpLeosPortXcvrEnhDiagAlarmSupported OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates if enhanced diagnostics alarms / warnings implemented."
    ::= { wwpLeosPortXcvrEntry 30 }

 wwpLeosPortXcvrEnhDiagSoftTxDisableSupported OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates if enhanced diagnostics soft Tx disable control is implemented."
    ::= { wwpLeosPortXcvrEntry 31 }

 wwpLeosPortXcvrEnhDiagSoftTxFaultSupported OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates if enhanced diagnostics soft Tx fault monitoring is implemented."
    ::= { wwpLeosPortXcvrEntry 32 }

 wwpLeosPortXcvrEnhDiagRxLosSupported OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates if enhanced diagnostics Rx LOS monitoring is implemented."
    ::= { wwpLeosPortXcvrEntry 33 }

  wwpLeosPortXcvrHighTempAlarmThreshold OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the higher threshold for temperature alarm."
    ::= { wwpLeosPortXcvrEntry 34 }
  
  wwpLeosPortXcvrLowTempAlarmThreshold OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the lower threshold for temperature alarm."
    ::= { wwpLeosPortXcvrEntry 35 } 

  wwpLeosPortXcvrHighVccAlarmThreshold OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the higher threshold for voltage alarm."
    ::= { wwpLeosPortXcvrEntry 36 }
  
  wwpLeosPortXcvrLowVccAlarmThreshold OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the lower threshold for voltage alarm."
    ::= { wwpLeosPortXcvrEntry 37 }
 
 wwpLeosPortXcvrHighBiasAlarmThreshold OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the higher threshold for bias alarm."
    ::= { wwpLeosPortXcvrEntry 38 }

 wwpLeosPortXcvrLowBiasAlarmThreshold OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the lower threshold for bias alarm."
    ::= { wwpLeosPortXcvrEntry 39 }

 wwpLeosPortXcvrHighTxPwAlarmThreshold OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the higher threshold for Tx power alarm.
	     Units are watts"
    ::= { wwpLeosPortXcvrEntry 40 }

 wwpLeosPortXcvrLowTxPwAlarmThreshold OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the lower threshold for Tx power alarm.
	     Units are watts."
    ::= { wwpLeosPortXcvrEntry 41 }

  wwpLeosPortXcvrHighRxPwAlarmThreshold OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the higher threshold for Rx power alarm.
	     Units are watts."
    ::= { wwpLeosPortXcvrEntry 42 }

  wwpLeosPortXcvrLowRxPwAlarmThreshold OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates the lower threshold for Rx power alarm.
	     Units are watts."
    ::= { wwpLeosPortXcvrEntry 43 }
    
 wwpLeosPortXcvrEnhDiagRateSelectSupported OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "Indicates if enhanced diagnostics soft rate select control is implemented."
    ::= { wwpLeosPortXcvrEntry 44 }
    
 wwpLeosPortXcvrAdminState OBJECT-TYPE
    SYNTAX           INTEGER {
                        disabled(1),
                        enabled(2),
                        loopback(3)                        
                     }
    MAX-ACCESS       read-write
    STATUS           current
    DESCRIPTION
	    "The admin state of the transceiver."
    ::= { wwpLeosPortXcvrEntry 45 }

  wwpLeosPortXcvrXfpMinBitRate OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the minimum bit rate."
    ::= { wwpLeosPortXcvrEntry 70 }   

  wwpLeosPortXcvrXfpMaxBitRate OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the maximum bit rate."
    ::= { wwpLeosPortXcvrEntry 71 }

  wwpLeosPortXcvrXfpLinkLenSmf1km OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the length (SMF fiber) 1km."
    ::= { wwpLeosPortXcvrEntry 72 }

  wwpLeosPortXcvrXfpLinkLenE50u2m OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the length (ext. BW MMF) 2m."
    ::= { wwpLeosPortXcvrEntry 73 }
   
  wwpLeosPortXcvrXfpLinkLen50u1m OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the length (50um) 1m."
    ::= { wwpLeosPortXcvrEntry 74 }
   
  wwpLeosPortXcvrXfpLinkLen62dot5u1m OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the length (62.5um) 1m."
    ::= { wwpLeosPortXcvrEntry 75 }
   
  wwpLeosPortXcvrXfpLinkLenCopper1m OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the length (copper) 1m."
    ::= { wwpLeosPortXcvrEntry 76 }
   
  wwpLeosPortXcvrXfpDevTech OBJECT-TYPE
    SYNTAX        INTEGER {
                    vcsel850nm(1),
                    vcsel1310nm(2),
                    vcsel1550nm(3),
                    fp1310nm(4),
                    dfb1310nm(5),
                    dfb1550nm(6),
                    eml1310nm(7),
                    eml1550nm(8),
                    copperOrOther(9),
		    tunable1550nm(10),
                    reserved(11)
                  }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the device technology."
    ::= { wwpLeosPortXcvrEntry 77 }
   
  wwpLeosPortXcvrXfpTransmitterTech OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the device transmitter technology:
        Bit 3: Wavelength Control (active/none)
        Bit 2: Transmitter Cooling (cooled/uncooled)
        Bit 1: Detector Type (apd/pin)
        Bit 0: Transmitter Tuning (Tunable/non-Tunable)
        "
    ::= { wwpLeosPortXcvrEntry 78 }
   
  wwpLeosPortXcvrXfpCdrSupport OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the CDR support:
         Bit 7:  9.95 Gb/s (yes/no)
         Bit 6:  10.3  Gb/s (yes/no)
         Bit 5:  10.5  Gb/s (yes/no)
         Bit 4:  10.7  Gb/s (yes/no)
         Bit 3:  11.1  Gb/s (yes/no)
         Bit 2:  N/A
         Bit 1:  Lineside Loopback (yes/no)
         Bit 0:  XFI Loopback (yes/no)
        "
    ::= { wwpLeosPortXcvrEntry 79 }
   
  wwpLeosPortXcvrXfpWaveLengthTol OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the wavelength tolerance."
    ::= { wwpLeosPortXcvrEntry 80 }
   
  wwpLeosPortXcvrXfpMaxCaseTemp OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the maximum case temperature."
    ::= { wwpLeosPortXcvrEntry 81 }
   
  wwpLeosPortXcvrXfpMaxPower OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the maximum power dissipation."
    ::= { wwpLeosPortXcvrEntry 82 }
   
  wwpLeosPortXcvrXfpMax5vCurrent OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the 5.0 Volt Max Current."
    ::= { wwpLeosPortXcvrEntry 83 }
   
  wwpLeosPortXcvrXfpMax3p3vCurrent OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the 3.3 Volt Max Current."
    ::= { wwpLeosPortXcvrEntry 84 }
   
  wwpLeosPortXcvrXfpMax1p8vCurrent OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the 1.8 Volt Max Current."
    ::= { wwpLeosPortXcvrEntry 85 }
   
  wwpLeosPortXcvrXfpMaxNeg5p2vCurrent OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the -5.2 Volt Max Current."
    ::= { wwpLeosPortXcvrEntry 86 }
   
  wwpLeosPortXcvrXfpDiagMonitorType OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the diag monitor type:
         Bit 4 indicates BER support.
         Bit 3 indidates the Rx Power Meas. type of Avg or OMA."
    ::= { wwpLeosPortXcvrEntry 87 }
   
  wwpLeosPortXcvrXfpEnhancedOptions OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the enhanced options:
         Bit 7: VPS Support (yes/no)
         Bit 6: Soft TX_DISABLE (yes/no)
         Bit 5: Soft P_down (yes/no)
         Bit 4: VPS LV Regulator Mode (yes/no)
         Bit 3: VPS bypassed Reg. Mode (yes/no)
         Bit 2: Active FEC Ctrl (yes/no)
         Bit 1: Wavelength or frequency Tunability (yes/no)
         Bit 0: CMU Support Mode (yes/no)
        "
    ::= { wwpLeosPortXcvrEntry 88 }
   
  wwpLeosPortXcvrXfpAuxMonitoringInput1 OBJECT-TYPE
    SYNTAX        INTEGER {
                    none(1),
                    aPDBiasVoltage(2),
                    reserved(3),
                    tECCurrentMa(4),
                    laserTemp(5),
                    laserWavelength(6),
                    voltage5V(7),
                    voltage3p3V(8),
                    voltage1p8V(9),
                    voltageNeg5p2V(10),
                    voltage5VCurrent(11),
                    voltage3p3VCurrent(12),
                    voltage1p8VCurrent(13),
                    voltageNeg5p2VCurrent(14),
                    unknown(15)
                  }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the Aux monitoring of A/D input 1."
    ::= { wwpLeosPortXcvrEntry 89 }

  wwpLeosPortXcvrXfpAuxMonitoringInput2 OBJECT-TYPE
    SYNTAX        INTEGER {
                    none(1),
                    aPDBiasVoltage(2),
                    reserved(3),
                    tECCurrentMa(4),
                    laserTemp(5),
                    laserWavelength(6),
                    voltage5V(7),
                    voltage3p3V(8),
                    voltage1p8V(9),
                    voltageNeg5p2V(10),
                    voltage5VCurrent(11),
                    voltage3p3VCurrent(12),
                    voltage1p8VCurrent(13),
                    voltageNeg5p2VCurrent(14),
                    unknown(15)
                  }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the Aux monitoring of A/D input 2."
    ::= { wwpLeosPortXcvrEntry 90 }

   wwpLeosPortXcvrAdminFrequency OBJECT-TYPE
    SYNTAX        Unsigned32(0..4294967295)
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The admin frequency of the transceiver in GHz"
    ::= { wwpLeosPortXcvrEntry 91 }

  wwpLeosPortXcvrXfpLaserFirstFrequency OBJECT-TYPE
    SYNTAX        Unsigned32(0..4294967295)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the first frequency in GHz"
    ::= { wwpLeosPortXcvrEntry 92 }

  wwpLeosPortXcvrXfpLaserLastFrquency OBJECT-TYPE
    SYNTAX        Unsigned32(0..4294967295)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the last frequency in GHz"
    ::= { wwpLeosPortXcvrEntry 93 }

  wwpLeosPortXcvrXfpMaxGridScacing OBJECT-TYPE
    SYNTAX        INTEGER (0..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the maximun support grid spacing in GHz"
    ::= { wwpLeosPortXcvrEntry 94 }

  wwpLeosPortXcvrXfpChannelNum OBJECT-TYPE
    SYNTAX        INTEGER (1..65535)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the channel number"
    ::= { wwpLeosPortXcvrEntry 95 }

   wwpLeosPortXcvrXfpFrequencyError OBJECT-TYPE
    SYNTAX        INTEGER (-32768..32767)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
	    "This represents the frequency error"
    ::= { wwpLeosPortXcvrEntry 96 }

   wwpLeosPortXcvrAdminWavelength OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The admin wavelength of the transceiver in pico-meter"
    ::= { wwpLeosPortXcvrEntry 97 }

   wwpLeosPortXcvrAdminChannel OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "The admin channel number of the transceiver"
    ::= { wwpLeosPortXcvrEntry 98 }

   wwpLeosPortXcvrXfpLaserFirstWavelenth OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "This represents the first wavelength in pico meter"
    ::= { wwpLeosPortXcvrEntry 99 }

   wwpLeosPortXcvrXfpLaserLastWavelength OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "This represents the last wavelength in pico meter"
    ::= { wwpLeosPortXcvrEntry 100 }

    wwpLeosPortXcvrXfpLaserFirstChannel OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "This represents the first channel number"
    ::= { wwpLeosPortXcvrEntry 101 }

    wwpLeosPortXcvrXfpLaserLastChannel OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "This represents the last channel number"
    ::= { wwpLeosPortXcvrEntry 102 }

   wwpLeosPortXcvrOperFrequency OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The operational frequency  of the transceiver in GHz"
    ::= { wwpLeosPortXcvrEntry 103 }

   wwpLeosPortXcvrOperWavelength OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The operational wavelength of the transceiver in pico-meter"
    ::= { wwpLeosPortXcvrEntry 104 }



    
 wwpLeosPortXcvrEventType OBJECT-TYPE
    SYNTAX         INTEGER {
                        inserted(1),
                        removed(2),
                        enabled(3),
                        disabled(4)
                   }                         
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
	    "Indicates if the Xcvr specified by the wwpLeosPortXcvrId has come up, 
	     gone down or has been selected."
    ::= { wwpLeosPortXcvrNotif 1}

  wwpLeosPortXcvrErrorType OBJECT-TYPE
    SYNTAX         INTEGER {
                        none(0),
                        chksumFailed(1),
                        opticalFault(2)                        
                   }
    MAX-ACCESS     read-only
    STATUS         current
    DESCRIPTION
	    "Indicates if the Xcvr specified by the wwpLeosPortXcvrId is faulted because of 
	     checksum failure or optical fault. This object only makes sense if transceiver has 
	     been detected faulted otherwise it returns none."
    ::= { wwpLeosPortXcvrNotif 2 } 
 
 wwpLeosPortXcvrLinkStateChangeNotification NOTIFICATION-TYPE
	OBJECTS	{                
                wwpLeosPortXcvrId,
                wwpLeosPortXcvrEventType        
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrLinkStateChangeNotification is sent if the Xcvr state has changed."
	::= { wwpLeosPortXcvrMIBNotifications 4 }

 wwpLeosPortXcvrErrorTypeNotification NOTIFICATION-TYPE
	OBJECTS	{                
		wwpLeosPortXcvrId,
		wwpLeosPortXcvrErrorType        
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrErrorTypeNotification is sent if the Xcvr is detected faulted because of some reason. 
		 Reason of failure is specified by wwpLeosPortXcvrErrorType."
	::= { wwpLeosPortXcvrMIBNotifications 5 }

 wwpLeosPortXcvrTempHighNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrTempHighNotification is sent if the Xcvr 
		 temperature exceeds the threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 6 }
 
 wwpLeosPortXcvrTempLowNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrTempLowNotification is sent if the Xcvr 
		 temperature decreases the threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 7 }

 wwpLeosPortXcvrTempNormalNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrTempNormalNotification is sent if the Xcvr 
		 temperature returns back to normal state."		 
	::= { wwpLeosPortXcvrMIBNotifications 8 }
 
 wwpLeosPortXcvrVoltageHighNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrVoltageHighNotification is sent if the Xcvr 
		 voltage exceeds the threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 9 }
 
 wwpLeosPortXcvrVoltageLowNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrVoltageLowNotification is sent if the Xcvr 
		 voltage decreases the threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 10 }

 wwpLeosPortXcvrVoltageNormalNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrVoltageNormalNotification is sent if the Xcvr 
		 voltage returns back to normal state."		 
	::= { wwpLeosPortXcvrMIBNotifications 11 }
 
 wwpLeosPortXcvrBiasHighNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrBiasHighNotification is sent if the Xcvr 
		 Bias exceeds the threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 12 }
 
 wwpLeosPortXcvrBiasLowNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrBiasLowNotification is sent if the Xcvr 
		 voltage decreases the threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 13 }

 wwpLeosPortXcvrBiasNormalNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrBiasNormalNotification is sent if the Xcvr 
		 Bias returns back to normal state."		 
	::= { wwpLeosPortXcvrMIBNotifications 14 }
 
 wwpLeosPortXcvrTxPowerHighNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrTxPowerHighNotification is sent if the Xcvr 
		 TxPower exceeds the threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 15 }
 
 wwpLeosPortXcvrTxPowerLowNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrTxPowerLowNotification is sent if the Xcvr 
		 voltage decreases the threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 16 }

 wwpLeosPortXcvrTxPowerNormalNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrTxPowerNormalNotification is sent if the Xcvr 
		 TxPower returns back to normal state."		 
	::= { wwpLeosPortXcvrMIBNotifications 17 }
 
 wwpLeosPortXcvrRxPowerHighNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrRxPowerHighNotification is sent if the Xcvr 
		 RxPower exceeds the threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 18 }
 
 wwpLeosPortXcvrRxPowerLowNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrRxPowerLowNotification is sent if the Xcvr 
		 voltage decreases the threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 19 }

 wwpLeosPortXcvrRxPowerNormalNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrRxPowerNormalNotification is sent if the Xcvr 
		 RxPower returns back to normal state."		 
	::= { wwpLeosPortXcvrMIBNotifications 20 }
   
  wwpLeosPortXcvrSpeedInfoMissingNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrSpeedInfoMissingNotification is sent if the Xcvr 
		 speed information is not found."		 
	::= { wwpLeosPortXcvrMIBNotifications 21 }

 wwpLeosPortXcvrBiasHighWarningNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrBiasHighNotification is sent if the Xcvr 
		 Bias exceeds the warning threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 22 }
 
 wwpLeosPortXcvrBiasLowWarningNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrBiasLowNotification is sent if the Xcvr 
		 voltage decreases below the warning threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 23 }

 wwpLeosPortXcvrTempHighWarningNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrTempHighNotification is sent if the Xcvr 
		 temperature exceeds the warning threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 24 }
 
 wwpLeosPortXcvrTempLowWarningNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrTempLowNotification is sent if the Xcvr 
		 temperature decreases below the warning threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 25 }
 
 wwpLeosPortXcvrVoltageHighWarningNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrVoltageHighNotification is sent if the Xcvr 
		 voltage exceeds the warning threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 26 }
 
 wwpLeosPortXcvrVoltageLowWarningNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrVoltageLowNotification is sent if the Xcvr 
		 voltage decreases below  the warning threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 27 }

 wwpLeosPortXcvrTxPowerHighWarningNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrTxPowerHighNotification is sent if the Xcvr 
		 TxPower exceeds the warning threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 28 }
 
 wwpLeosPortXcvrTxPowerLowWarningNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrTxPowerLowNotification is sent if the Xcvr 
		 TxPower decreases below the warning threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 29 }

 wwpLeosPortXcvrRxPowerHighWarningNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrRxPowerHighNotification is sent if the Xcvr 
		 RxPower exceeds the warning threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 30 }
 
 wwpLeosPortXcvrRxPowerLowWarningNotification NOTIFICATION-TYPE
	OBJECTS	{                
		     wwpLeosPortXcvrId		
		}
	STATUS	current
	DESCRIPTION
		"A wwpLeosPortXcvrRxPowerLowNotification is sent if the Xcvr 
		 RxPower decreases below the warning threshold."		 
	::= { wwpLeosPortXcvrMIBNotifications 31 }


 END

 --
 -- WWP-XCVR-MIB
 --
