-- This file was included in WWP MIB release 04-07-01-0008
--
-- WWP-LEOS-OAM-MIB.my
-- MIB generated by MG-SOFT Visual MIB Builder Version 6.0  Build 88

        WWP-LEOS-OAM-MIB DEFINITIONS ::= BEGIN
 
                IMPORTS
                        OBJECT-GROUP, NOTIFICATION-GROUP                        
                                FROM SNMPv2-CONF                
                          
                        Integer32, Unsigned32, Counter32, OBJECT-TYPE, 
                        MODULE-IDENTITY                 
                                FROM SNMPv2-SMI   
                         TimeStamp, TruthValue
                                FROM SNMPv2-TC
                        wwpModulesLeos                  
                                FROM WWP-SMI;
        
         
                -- 1.3.6.1.4.1.6141.2.60.400
                wwpLeosOamMibModule MODULE-IDENTITY 
                        LAST-UPDATED "200801030000Z"            -- January 3,2008 at 00:00GMT 
                        ORGANIZATION "Ciena, Inc"
                        CONTACT-INFO
                                "   Mib Meister
                                        115 North Sullivan Road
                                        Spokane Valley, WA 99037
                                USA                             
                                Phone:  +1 509 242 9000
                                        Email:  support@ciena.com"
                        DESCRIPTION 
                                "The MIB module for managing the new Ethernet OAM features
                                         introduced by the Ethernet in the First Mile task force (IEEE
                                         802.3ah).  The functionality presented here is based on IEEE
                                         802.3ah [802.3ah], released in October, 2004.  
                                  
                                         In particular, this MIB focused on the changes to Clause 30 of
                                         the draft that are not specific to any physical layer.  These
                                         changes are primarily reflected in the new OAM features
                                         developed under this project, that can be applied to any
                                         Ethernet like interface. The OAM features are described in
                                         Clause 57 of [802.3ah].
                                  
                                         The following reference is used throughout this MIB module:  
                                  
                                           [802.3ah] refers to:
                                             IEEE Std 802.3ah-2004: 'Draft amendment to -
                                             Information technology - Telecommunications and
                                             information exchange between systems - Local and
                                             metropolitan are networks - Specific requirements - Part
                                             3: Carrier sense multiple access with collision detection
                                             (CSMA/CD) access method and physical layer specifications
                                             - Media Access Control Parameters, Physical Layers and
                                             Management Parameters for subscriber access networks',
                                             October 2004.
                                  
                                           [802-2001] refers to:
                                             'IEEE Standard for LAN/MAN (Local Area
                                             Network/Metropolitan Area Network): Overview and
                                             Architecture', IEEE 802, June 2001.  
                                  
                                         Copyright (c) The Internet Society (2005). This version of
                                         this MIB module is part of RFC XXXX; See the RFC itself for
                                         full legal notices."
                        ::= { wwpModulesLeos 400 }


        
--
-- Node definitions
--
        
                -- 1.3.6.1.4.1.6141.2.60.400.1
                wwpLeosOamMIB OBJECT IDENTIFIER ::= { wwpLeosOamMibModule 1 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.1
                wwpLeosOamConf OBJECT IDENTIFIER ::= { wwpLeosOamMIB 1 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.1.1
                wwpLeosOamGroups OBJECT IDENTIFIER ::= { wwpLeosOamConf 1 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.1.1.1
                --wwpLeosOamObjectGroup OBJECT-GROUP
                --      OBJECTS { object1 }
                --      STATUS current
                --      DESCRIPTION 
                --              "Description."
                --      ::= { wwpLeosOamGroups 1 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.1.1.2
                --wwpLeosOamNotificationGroup NOTIFICATION-GROUP
                --      NOTIFICATIONS { notification1 }
                --      STATUS current
                --      DESCRIPTION 
                --              "Description."
                --      ::= { wwpLeosOamGroups 2 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.1.2
                wwpLeosOamCompls OBJECT IDENTIFIER ::= { wwpLeosOamConf 2 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2
                wwpLeosOamObjs OBJECT IDENTIFIER ::= { wwpLeosOamMIB 2 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.1
                wwpLeosOamTable OBJECT-TYPE
                        SYNTAX SEQUENCE OF WwpLeosOamEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "Primary controls and status for the OAM capabilities of an
                                         Ethernet like interface.  There will be one row in this table
                                         for each Ethernet like interface in the system that supports
                                         the Ethernet OAM functions defined in [802.3ah]."
                        ::= { wwpLeosOamObjs 1 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.1.1
                wwpLeosOamEntry OBJECT-TYPE
                        SYNTAX WwpLeosOamEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "An entry in the table. Contains an Ethernet like interface
                                		in the system that supports the Ethernet OAM functions
                                		defined in [802.3ah]."
                        INDEX { wwpLeosOamPort }
                        ::= { wwpLeosOamTable 1 }

                
                WwpLeosOamEntry ::=
                        SEQUENCE { 
                                wwpLeosOamAdminState
                                        INTEGER,
                                wwpLeosOamOperStatus
                                        INTEGER,
                                wwpLeosOamMode
                                        INTEGER,
                                wwpLeosMaxOamPduSize
                                        Integer32,
                                wwpLeosOamConfigRevision
                                        Unsigned32,
                                wwpLeosOamFunctionsSupported
                                        BITS,
                                wwpLeosOamPort
                                        Integer32,
                                wwpLeosOamPduTimer
                                		INTEGER,
                                wwpLeosOamLinkLostTimer
                                		INTEGER
                         }

                -- 1.3.6.1.4.1.6141.2.60.400.1.2.1.1.1
                wwpLeosOamAdminState OBJECT-TYPE
                        SYNTAX INTEGER
                                {
                                disabled(1),
                                enabled(2)
                                }
                        MAX-ACCESS read-write
                        STATUS current
                        DESCRIPTION
                                "This object is used to provision the default administrative OAM mode for this 
                                interface.  This object represents the desired state of OAM for this interface.  
                                  
                                The wwpLeosOamAdminState always starts in the disabled(1) state
                                         until an explicit management action or configuration
                                         information retained by the system causes a transition to the
                                         enabled(2) state. 
                                  
                                         Note that the value of this object is ignored when the
                                         interface is not operating in full-duplex mode. OAM is not
                                         supported on half-duplex links."
                        ::= { wwpLeosOamEntry 1 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.1.1.2
                wwpLeosOamOperStatus OBJECT-TYPE
                        SYNTAX INTEGER
                                {
                                disabled(1),
                                linkfault(2),
                                passiveWait(3),
                                activeSendLocal(4),
                                sendLocalAndRemote(5),
                                sendLocalAndRemoteOk(6),
                                oamPeeringLocallyRejected(7),
                                oamPeeringRemotelyRejected(8),
                                operational(9)
                                }
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "At initialization and failure conditions, two OAM entities on
                                         the same full-duplex Ethernet link begin a discovery phase to
                                         determine what OAM capabilities may be used on that link.  The
                                         progress of this initialization is controlled by the OAM
                                         sub layer.  
                                                    
                                         This value is always disabled(1) if OAM is disabled on this
                                         interface via the wwpLeosOamAdminState.  
                                  
                                         If the link has detected a fault and is transmitting OAMPDUs
                                         with a link fault indication, the value is linkFault(2). 
                                                          
                                         The passiveWait(3) state is returned only by OAM entities in
                                         passive mode (wwpLeosOamMode) and reflects the state in which the
                                         OAM entity is waiting to see if the peer device is OAM
                                         capable.  The activeSendLocal(4) is used by active mode
                                         devices (wwpLeosOamMode) and reflects the OAM entity actively
                                         trying to discover whether the peer has OAM capability but has
                                         not yet made that determination.  
                                                          
                                         The state sendLocalAndRemote(5) reflects that the local OAM
                                         entity has discovered the peer but has not yet accepted or
                                         rejected the configuration of the peer.  The local device can,
                                         for whatever reason, decide that the peer device is
                                         unacceptable and decline OAM peering.  If the local OAM entity
                                         rejects the peer OAM entity, the state becomes
                                         oamPeeringLocallyRejected(7).  If the OAM peering is allowed
                                         by the local device, the state moves to
                                         sendLocalAndRemoteOk(6).  Note that both the
                                         sendLocalAndRemote(5) and oamPeeringLocallyRejected(7) states
                                         fall within the state SEND_LOCAL_REMOTE of the Discovery state
                                         diagram [802.3ah, Figure 57-5], with the difference being
                                         whether the local OAM client has actively rejected the peering
                                         or has just not indicated any decision yet.  Whether a peering
                                         decision has been made is indicated via the local flags field
                                         in the OAMPDU (reflected in the aOAMLocalFlagsField of
                                         30.3.6.1.10).  
                                  
                                         If the remote OAM entity rejects the peering, the state
                                         becomes oamPeeringRemotelyRejected(8).  Note that both the
                                         sendLocalAndRemoteOk(6) and oamPeeringRemotelyRejected(8)
                                         states fall within the state SEND_LOCAL_REMOTE_OK of the
                                         Discovery state diagram [802.3ah, Figure 57-5], with the
                                         difference being whether the remote OAM client has rejected
                                         the peering or has just not yet decided.  This is indicated
                                         via the remote flags field in the OAM PDU (reflected in the
                                         aOAMRemoteFlagsField of 30.3.6.1.11).  
                                                          
                                         When the local OAM entity learns that both it and the remote
                                         OAM entity have accepted the peering, the state moves to
                                         operational(9) corresponding to the SEND_ANY state of the
                                         Discovery state diagram [802.3ah, Figure 57-5]. "
                        ::= { wwpLeosOamEntry 2 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.1.1.3
                wwpLeosOamMode OBJECT-TYPE
                        SYNTAX INTEGER
                                {
                                active(1),
                                passive(2)
                                }
                        MAX-ACCESS read-write
                        STATUS current
                        DESCRIPTION
                                "This object configures the mode of OAM operation for this
                                         Ethernet like interface.  OAM on Ethernet interfaces may be in
                                         'active' mode or 'passive' mode.  These two modes differ in
                                         that active mode provides additional capabilities to initiate
                                         monitoring activities with the remote OAM peer entity, while
                                         passive mode generally waits for the peer to initiate OAM
                                         actions with it.  As an example, an active OAM entity can put
                                         the remote OAM entity in a loopback state, where a passive OAM
                                         entity cannot.  
                                  
                                         The default value of wwpLeosOamMode is dependent on the type of
                                         system on which this Ethernet like interface resides.  The
                                         default value should be 'active(1)' unless it is known that
                                         this system should take on a subservient role to the other
                                         device connected over this interface.  
                                  
                                         Changing this value results in incrementing the configuration
                                         revision field of locally generated OAMPDUs (30.3.6.1.12) and
                                         potentially re-doing the OAM discovery process if the
                                         wwpLeosOamOperStatus was already operational(9). "
                        ::= { wwpLeosOamEntry 3 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.1.1.4
                wwpLeosMaxOamPduSize OBJECT-TYPE
                        SYNTAX Integer32
                        UNITS "bytes"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "The largest OAMPDU that the OAM entity supports.  OAM
                                         entities exchange maximum OAMPDU sizes and negotiate to use
                                         the smaller of the two maximum OAMPDU sizes between the peers.
                                         This value is determined by the local implementation."
                        ::= { wwpLeosOamEntry 4 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.1.1.5
                wwpLeosOamConfigRevision OBJECT-TYPE
                        SYNTAX Unsigned32
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "The configuration revision of the OAM entity as reflected in
                                         the latest OAMPDU sent by the OAM entity.  The configuration revision
                                         is used by OAM entities to indicate configuration changes have
                                         occurred which might require the peer OAM entity to re-evaluate
                                         whether the peering is allowed.  See local_satisfied in
                                         [802.3ah, 57.3.1.2]."
                        ::= { wwpLeosOamEntry 5 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.1.1.6
                wwpLeosOamFunctionsSupported OBJECT-TYPE
                        SYNTAX BITS
                                {
                                unidirectionalSupport(0),
                                loopbackSupport(1),
                                eventSupport(2),
                                variableSupport(3)
                                }
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "The OAM functions supported on this Ethernet like interface.
                                         OAM consists of separate functional sets beyond the basic
                                         discovery process which is always required.  These functional
                                         groups can be supported independently by any implementation.
                                         These values are communicated to the peer via the local
                                         configuration field of Information OAMPDUs. "
                        ::= { wwpLeosOamEntry 6 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.1.1.7
                wwpLeosOamPort OBJECT-TYPE
                        SYNTAX Integer32 (1..1000)
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "An Ethernet port on the switch."
                        ::= { wwpLeosOamEntry 7 }


                -- 1.3.6.1.4.1.6141.2.60.400.1.2.1.1.8
                wwpLeosOamPduTimer OBJECT-TYPE
                        SYNTAX INTEGER (100..1000)
                        MAX-ACCESS read-write
                        STATUS current
                        DESCRIPTION
                                "The time in milliseconds between Information OAMPDUs
                                being transmitted via the Ethernet port."
                        ::= { wwpLeosOamEntry 8 }

                -- 1.3.6.1.4.1.6141.2.60.400.1.2.1.1.9
                wwpLeosOamLinkLostTimer OBJECT-TYPE
                        SYNTAX INTEGER (500..5000)
                        MAX-ACCESS read-write
                        STATUS current
                        DESCRIPTION
                                "The time in milliseconds to wait for an Information OAMPDU
                                via the Ethernet port, from a peer, before declaring the link lost."
                        ::= { wwpLeosOamEntry 9 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.2
                wwpLeosOamPeerTable OBJECT-TYPE
                        SYNTAX SEQUENCE OF WwpLeosOamPeerEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "Information about the OAM peer for a particular Ethernet like
                                         interface. OAM entities communicate with a single OAM peer
                                         entity on full-duplex Ethernet links on which OAM is enabled
                                         and operating properly.  
                                         
                                         In certain states, the OAM peer information is not available.
                                         Whether peer information is available is communicated via the
                                         wwpLeosOamPeerStatus object.  When this object is inactive, all
                                         other information in the row is to be considered invalid."
                        ::= { wwpLeosOamObjs 2 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.2.1
                wwpLeosOamPeerEntry OBJECT-TYPE
                        SYNTAX WwpLeosOamPeerEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "An entry in the table, containing information on the peer OAM
                                         entity for a single Ethernet like interface.  
                                  
                                         Note that there is at most one OAM peer for each Ethernet like
                                         interface.  There is exactly one row in this table for each
                                         Ethernet like interface supporting OAM. "
                        INDEX { wwpLeosOamLocalPort }
                        ::= { wwpLeosOamPeerTable 1 }

                
                WwpLeosOamPeerEntry ::=
                        SEQUENCE {                              
                                wwpLeosOamPeerStatus                                    INTEGER,
                                wwpLeosOamPeerMacAddress                                        OCTET STRING(SIZE(6)),
                                wwpLeosOamPeerVendorOui                                 OCTET STRING(SIZE(3)),
                                wwpLeosOamPeerVendorInfo                                        Unsigned32,
                                wwpLeosOamPeerMode                                      INTEGER,
                                wwpLeosOamPeerMaxOamPduSize                                     Integer32,
                                wwpLeosOamPeerConfigRevision                                    Unsigned32,
                                wwpLeosOamPeerFunctionsSupported                                        BITS,
                                wwpLeosOamLocalPort                                     Integer32                                                              

                         }

                -- 1.3.6.1.4.1.6141.2.60.400.1.2.2.1.1
                wwpLeosOamPeerStatus OBJECT-TYPE
                        SYNTAX INTEGER
                                {
                                active(1),
                                inactive(2)
                                }
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "This object indicates whether the information in this row
                                         should be considered valid.  When active(1), the information
                                         is valid and represents the current peer of the OAM entity.
                                         When inactive(2), the information in this row is invalid.  
                                  
                                         A value of inactive(2) is returned if the wwpLeosOamOperStatus is
                                         disabled, passiveWait, or activeSendLocal.  For all other
                                         values of wwpLeosOamOperStatus, a value of active(1) is returned."
                        ::= { wwpLeosOamPeerEntry 1 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.2.1.2
                wwpLeosOamPeerMacAddress OBJECT-TYPE
                        SYNTAX OCTET STRING(SIZE(6))
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "The MAC address of the peer OAM entity.  The MAC address is
                                         derived from the most recently received OAMPDU.  This value is
                                         initialized to all zeros (0x000000000000).  This value is
                                         invalid if the wwpLeosOamPeerStatus is inactive.  
                                  
                                         An OAMPDU is indicated by a valid frame with (1) destination
                                         MAC address equal to that of the reserved MAC address for Slow
                                         Protocols (See 43B of [802.3ah]), (2) a lengthOrType field
                                         equal to the reserved type for Slow Protocols, (3) and a Slow
                                         Protocols subtype equal to that of the subtype reserved for
                                         OAM."
                        ::= { wwpLeosOamPeerEntry 2 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.2.1.3
                wwpLeosOamPeerVendorOui OBJECT-TYPE
                        SYNTAX OCTET STRING(SIZE(3))
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "The OUI of the OAM peer as reflected in the latest
                                         Information OAMPDU received with a Local Information TLV.  The
                                         OUI can be used to identify the vendor of the remote OAM
                                         entity.  This value is initialized to all zeros (0x000000).
                                         This value is considered invalid if the wwpLeosOamPeerStatus is
                                         inactive.  
                                  
                                         An Information OAMPDU is indicated by a valid frame with (1)
                                         destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, (4) a OAM code that equals the code
                                         reserved for Information OAMPDUs."
                        ::= { wwpLeosOamPeerEntry 3 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.2.1.4
                wwpLeosOamPeerVendorInfo OBJECT-TYPE
                        SYNTAX Unsigned32
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "The Vendor Info of the OAM peer as reflected in the latest
                                         Information OAMPDU received with a Local Information TLV.  The
                                         vendor information field is within the Local Information TLV,
                                         and can be used to determine additional information about the
                                         peer entity.  The format of the vendor information is
                                         unspecified within the 32-bit field.  This value is initialized
                                         to all zeros (0x00000000).  This value is invalid if the
                                         wwpLeosOamPeerStatus is inactive.  
                                  
                                         An Information OAMPDU is indicated by a valid frame with (1)
                                         destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) a OAM code that equals the
                                         code reserved for Information OAMPDUs. "
                        ::= { wwpLeosOamPeerEntry 4 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.2.1.5
                wwpLeosOamPeerMode OBJECT-TYPE
                        SYNTAX INTEGER
                                {
                                active(1),
                                passive(2),
                                unknown(3)
                                }
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "The mode of the OAM peer as reflected in the latest
                                         Information OAMPDU received with a Local Information TLV.  The
                                         mode of the peer can be determined from the Configuration
                                         field in the Local Information TLV of the last Information
                                         OAMPDU received from the peer.  This value is initialized to
                                         unknown(3), and is not valid if the wwpLeosOamPeerStatus is
                                         inactive.  
                                  
                                         An Information OAMPDU is indicated by a valid frame with (1)
                                         destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) a OAM code that equals the
                                         code reserved for Information OAMPDUs."
                        ::= { wwpLeosOamPeerEntry 5 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.2.1.6
                wwpLeosOamPeerMaxOamPduSize OBJECT-TYPE
                        SYNTAX Integer32
                        UNITS "bytes"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "The maximum size of OAMPDU supported by the peer as reflected
                                         in the latest Information OAMPDU received with a Local
                                         Information TLV.   Ethernet OAM on this interface must not use
                                         OAMPDUs that exceed this size.  The maximum OAMPDU size can be
                                         determined from the PDU Configuration field of the Local
                                         Information TLV of the last Information OAMPDU received from
                                         the peer.  This value is initialized to 64, and is invalid if
                                         the wwpLeosOamPeerStatus is inactive.  
                                  
                                         An Information OAMPDU is indicated by a valid frame with (1)
                                         destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) a OAM code that equals the
                                         code reserved for Information OAMPDUs."
                        ::= { wwpLeosOamPeerEntry 6 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.2.1.7
                wwpLeosOamPeerConfigRevision OBJECT-TYPE
                        SYNTAX Unsigned32
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "The configuration revision of the OAM peer as reflected in
                                         the latest OAMPDU.  This attribute is changed by the peer
                                         whenever it has a local configuration change for Ethernet OAM
                                         this interface.  This value is initialized to all zeros
                                         (0x00000000), and is invalid if the wwpLeosOamPeerStatus is
                                         inactive.   
                                  
                                         The configuration revision can be determined from the Revision
                                
                                         field of the Local Information TLV of the most recently
                                         received Information OAMPDU with a Local Information TLV.  
                                                         
                                         An Information OAMPDU is indicated by a valid frame with (1)
                                         destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) a OAM code that equals the
                                         code reserved for Information OAMPDUs."
                        ::= { wwpLeosOamPeerEntry 7 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.2.1.8
                wwpLeosOamPeerFunctionsSupported OBJECT-TYPE
                        SYNTAX BITS
                                {
                                unidirectionalSupport(0),
                                loopbackSupport(1),
                                eventSupport(2),
                                variableSupport(3)
                                }
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "The OAM functions supported on this Ethernet like interface.
                                         OAM consists of separate functionality sets above the basic
                                         discovery process.  This value indicates the capabilities of
                                         the peer OAM entity with respect to these functions.  This
                                         value is initialized so all bits are clear, and is invalid if
                                         the wwpLeosOamPeerStatus is inactive.  
                                  
                                         The capbilities of the OAM peer can be determined from the
                                         configuration field of the Local Information TLV of the most
                                         recently received Information OAMPDU with a Local Information
                                         TLV.  
                                                         
                                         An Information OAMPDU is indicated by a valid frame with (1)
                                         destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) a OAM code that equals the
                                         code reserved for Information OAMPDUs. "
                        ::= { wwpLeosOamPeerEntry 8 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.2.1.9
                wwpLeosOamLocalPort OBJECT-TYPE
                        SYNTAX Integer32 (1..1000)
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "An Ethernet port on the local switch."
                        ::= { wwpLeosOamPeerEntry 9 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.3
                wwpLeosOamLoopbackTable OBJECT-TYPE
                        SYNTAX SEQUENCE OF WwpLeosOamLoopbackEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "This table contains methods to control the loopback state of
                                         the local link as well as indicating the status of the
                                         loopback function.  
                                  
                                         Loopback can be used to place the remote OAM entity in a state
                                         where every received frame (except OAMPDUs) are echoed back
                                         over the same interface on which they were received.   In this
                                         state, at the remote entity, 'normal' traffic is disabled as
                                         only the looped back frames are transmitted on the interface.
                                         Loopback is thus an intrusive operation that prohibits normal
                                         data flow and should be used accordingly."
                        ::= { wwpLeosOamObjs 3 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.3.1
                wwpLeosOamLoopbackEntry OBJECT-TYPE
                        SYNTAX WwpLeosOamLoopbackEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "An entry in the table, containing information on the loopback
                                         status for a single Ethernet like interface.  There is an
                                         entry in this table for every Ethernet like interface on which
                                         supports OAM and loopback function within OAM (as indicated in
                                         wwpLeosOamFunctionsSupported)."
                        INDEX { wwpLeosOamLoopbackPort }
                        ::= { wwpLeosOamLoopbackTable 1 }

                
                WwpLeosOamLoopbackEntry ::=
                        SEQUENCE { 
                                wwpLeosOamLoopbackCommand
                                        INTEGER,
                                wwpLeosOamLoopbackStatus
                                        INTEGER,
                                wwpLeosOamLoopbackIgnoreRx
                                        INTEGER,
                                wwpLeosOamLoopbackPort
                                        Integer32
                         }

                -- 1.3.6.1.4.1.6141.2.60.400.1.2.3.1.1
                wwpLeosOamLoopbackCommand OBJECT-TYPE
                        SYNTAX INTEGER
                                {
                                noLoopback(1),
                                startRemoteLoopback(2),
                                stopRemoteLoopback(3)
                                }
                        MAX-ACCESS read-write
                        STATUS current
                        DESCRIPTION
                                "This attribute initiates or terminates remote loopback with
                                         an OAM peer.  Writing startRemoteLoopback(2) to this attribute
                                         cause the local OAM client to send a loopback OAMPDU to the
                                         OAM peer with the loopback enable flags set.  Writing
                                         stopRemoteLoopback(3) to this attribute will cause the local
                                         OAM client to send a loopback OAMPDU to the OAM peer with the
                                         loopback enable flags cleared.  Writing noLoopback to this
                                         attribute has no effect.  
                                  
                                         Writes to this attribute are ignored unless the OAM status of
                                         this interface is 'operational' (wwpLeosOamOperStatus).  
                                                          
                                         The attribute always returns noLoopback on a read.  To
                                         determine the loopback status, use the attribute
                                         wwpLeosOamLoopbackStatus. "
                        ::= { wwpLeosOamLoopbackEntry 1 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.3.1.2
                wwpLeosOamLoopbackStatus OBJECT-TYPE
                        SYNTAX INTEGER
                                {
                                noLoopback(1),
                                initiatingLoopback(2),
                                remoteLoopback(3),
                                terminatingLoopback(4),
                                localLoopback(5),
                                unknown(6)
                                }
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "The loopback status of the OAM entity.  This status is
                                         determined by a combination of the local parser and
                                         multiplexer states, the remote parser and multiplexer states,
                                         as well as by the actions of the local OAM client.  When
                                         operating in normal mode with no loopback in progress, the
                                         status reads noLoopback(1).  
                                                         
                                         If the OAM client has sent an Loopback OAMPDU and is waiting
                                         for a response, where the local parser and multiplexer states
                                         are DISCARD (see [802.3ah, 57.2.11.1]), the status is
                                         'initiatingLoopback'.  In this case, the local OAM entity has
                                         yet to receive any acknowledgement that the remote OAM entity
                                         has received its loopback command request.  
                                                         
                                         If the local OAM client knows that the remote OAM entity is in
                                         loopback mode (via the remote state information as described
                                         in [802.3ah, 57.2.11.1, 30.3.6.1.15]), the status is remoteLoopback(3).  If the local OAM client is in the process
                                         of terminating the remote loopback [802.3ah, 57.2.11.3,
                                         30.3.6.1.14], with its local multiplexer and parser states in
                                         DISCARD, the status is terminatingLoopback(4).  If the remote
                                         OAM client has put the local OAM entity in loopback mode as
                                         indicated by its local parser state, the status is
                                         localLoopback(5).  
                                  
                                         The unknown(6) status indicates the parser and multiplexer
                                         combination is unexpected.  This status may be returned if the
                                         OAM loopback is in a transition state but should not persist. 
                                  
                                         The values of this attribute correspond to the following
                                         values of the local and remote parser and multiplexer states. 
                                  
                                           value            LclPrsr   LclMux    RmtPrsr   RmtMux
                                           noLoopback         FWD       FWD       FWD       FWD  
                                           initLoopback     DISCARD   DISCARD     FWD       FWD 
                                           rmtLoopback      DISCARD     FWD      LPBK    DISCARD
                                           tmtngLoopback    DISCARD   DISCARD    LPBK    DISCARD
                                           lclLoopback        LPBK    DISCARD   DISCARD     FWD
                                           unknown            ***   any other combination   ***"
                        ::= { wwpLeosOamLoopbackEntry 2 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.3.1.3
                wwpLeosOamLoopbackIgnoreRx OBJECT-TYPE
                        SYNTAX INTEGER
                                {
                                ignore(1),
                                process(2)
                                }
                        MAX-ACCESS read-write
                        STATUS current
                        DESCRIPTION
                                "Since OAM loopback is a disruptive operation (user traffic
                                         does not pass), this attribute provides a mechanism to provide
                                         controls over whether received OAM loopback commands are
                                         processed or ignored.  When the value is ignore(1), received
                                         loopback commands are ignored.  When the value is process(2),
                                         OAM loopback commands are processed.  The default value is to
                                         ignore loopback commands (ignore(1)).  
                                  
                                         The attribute has no meaning if the local OAM entity does not
                                         support the loopback function (as defined in
                                         wwpLeosOamFunctionsSupported). "
                        ::= { wwpLeosOamLoopbackEntry 3 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.3.1.4
                wwpLeosOamLoopbackPort OBJECT-TYPE
                        SYNTAX Integer32 (1..1000)
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "An Ethernet port on the switch"
                        ::= { wwpLeosOamLoopbackEntry 4 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4
                wwpLeosOamStatsTable OBJECT-TYPE
                        SYNTAX SEQUENCE OF WwpLeosOamStatsEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "Statistics for the OAM function on a particular Ethernet like
                                         interface."
                        ::= { wwpLeosOamObjs 4 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1
                wwpLeosOamStatsEntry OBJECT-TYPE
                        SYNTAX WwpLeosOamStatsEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "An entry in the table, containing statistics information on
                                         the Ethernet OAM function for a single Ethernet like
                                         interface."
                        INDEX { wwpLeosOamStatsPort }
                        ::= { wwpLeosOamStatsTable 1 }

                
                WwpLeosOamStatsEntry ::=
                        SEQUENCE { 
                                wwpLeosOamInformationTx
                                        Counter32,
                                wwpLeosOamInformationRx
                                        Counter32,
                                wwpLeosOamUniqueEventNotificationTx
                                        Counter32,
                                wwpLeosOamUniqueEventNotificationRx
                                        Counter32,
                                wwpLeosOamLoopbackControlTx
                                        Counter32,
                                wwpLeosOamLoopbackControlRx
                                        Counter32,
                                wwpLeosOamVariableRequestTx
                                        Counter32,
                                wwpLeosOamVariableRequestRx
                                        Counter32,
                                wwpLeosOamVariableResponseTx
                                        Counter32,
                                wwpLeosOamVariableResponseRx
                                        Counter32,
                                wwpLeosOamOrgSpecificTx
                                        Counter32,
                                wwpLeosOamOrgSpecificRx
                                        Counter32,
                                wwpLeosOamUnsupportedCodesTx
                                        Counter32,
                                wwpLeosOamUnsupportedCodesRx
                                        Counter32,
                                wwpLeosOamframesLostDueToOam
                                        Counter32,
                                wwpLeosOamStatsPort
                                        Integer32,
                                wwpLeosOamDuplicateEventNotificationTx
                                        Counter32,
                                wwpLeosOamDuplicateEventNotificationRx
                                        Counter32
                         }

                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.1
                wwpLeosOamInformationTx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of Information OAMPDUs transmitted on
                                         this interface.
                                  
                                         An Information OAMPDU is indicated by a valid frame with (1)
                                         destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Information code.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime."
                        ::= { wwpLeosOamStatsEntry 1 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.2
                wwpLeosOamInformationRx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of Information OAMPDUs received on this
                                         interface.
                                  
                                         An Information OAMPDU is indicated by a valid frame with (1)
                                         destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Information code.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime. "
                        ::= { wwpLeosOamStatsEntry 2 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.3
                wwpLeosOamUniqueEventNotificationTx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of unique Event OAMPDUs transmitted on
                                         this interface.  Event notifications may be sent in duplicate
                                         to increase the probability of successfully being received,
                                         given the possibility that a frame may be lost in transit.  
                                  
                                         An Event Notification OAMPDU is indicated by a valid frame
                                         with (1) destination MAC address equal to that of the reserved
                                         MAC address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Event code.  
                                  
                                         A unique Event Notification OAMPDU is indicated as an Event
                                         Notification OAMPDU with a Sequence Number field that is
                                         distinct from the previously transmitted Event Notification
                                         OAMPDU Sequence Number.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime."
                        ::= { wwpLeosOamStatsEntry 3 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.4
                wwpLeosOamUniqueEventNotificationRx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of unique Event OAMPDUs received on
                                         this interface.  Event notification OAMPDUs may be sent in
                                         duplicate to increase the probability of successfully being
                                         received, given the possibility that a frame may be lost in
                                         transit.  
                                  
                                         An Event Notification OAMPDU is indicated by a valid frame
                                         with (1) destination MAC address equal to that of the reserved
                                         MAC address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Event code.  
                                  
                                         A unique Event Notification OAMPDU is indicated as an Event
                                         Notification OAMPDU with a Sequence Number field that is
                                         distinct from the previously received Event Notification
                                
                                
                                                         
                                         OAMPDU Sequence Number.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime."
                        ::= { wwpLeosOamStatsEntry 4 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.5
                wwpLeosOamLoopbackControlTx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of Loopback Control OAMPDUs transmitted
                                         on this interface.  
                                  
                                         An Loopback Control OAMPDU is indicated by a valid frame with
                                         (1) destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Loopback Control code.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime.  "
                                       REFERENCE   "[802.3ah], 30.3.6.1.26."
                        ::= { wwpLeosOamStatsEntry 5 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.6
                wwpLeosOamLoopbackControlRx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of Loopback Control OAMPDUs transmitted
                                         on this interface.  
                                  
                                         An Loopback Control OAMPDU is indicated by a valid frame with
                                         (1) destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Loopback Control code.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime.  "
                                       REFERENCE   "[802.3ah], 30.3.6.1.27."
                        ::= { wwpLeosOamStatsEntry 6 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.7
                wwpLeosOamVariableRequestTx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of Variable Request OAMPDUs transmitted
                                         on this interface.  
                                  
                                         An Variable Request OAMPDU is indicated by a valid frame with
                                         (1) destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Variable Request code.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime.  "
                                       REFERENCE   "[802.3ah], 30.3.6.1.28."
                        ::= { wwpLeosOamStatsEntry 7 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.8
                wwpLeosOamVariableRequestRx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of Variable Request OAMPDUs received on
                                         this interface.  
                                
                                
                                                         
                                  
                                         An Variable Request OAMPDU is indicated by a valid frame with
                                         (1) destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Variable Request code.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime."
                        ::= { wwpLeosOamStatsEntry 8 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.9
                wwpLeosOamVariableResponseTx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of Variable Response OAMPDUs
                                         transmitted on this interface.  
                                  
                                         An Variable Response OAMPDU is indicated by a valid frame with
                                         (1) destination MAC address equal to that of the reserved MAC
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Variable Response code.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime. "
                        ::= { wwpLeosOamStatsEntry 9 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.10
                wwpLeosOamVariableResponseRx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of Variable Response OAMPDUs received
                                         on this interface.  
                                  
                                         An Variable Response OAMPDU is indicated by a valid frame with
                                         (1) destination MAC address equal to that of the reserved MAC
                                
                                
                                                         
                                         address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Variable Response code.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime. "
                        ::= { wwpLeosOamStatsEntry 10 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.11
                wwpLeosOamOrgSpecificTx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of Organization Specific OAMPDUs
                                         transmitted on this interface.  
                                  
                                         An Organization Specific OAMPDU is indicated by a valid frame
                                         with (1) destination MAC address equal to that of the reserved
                                         MAC address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Organization Specific code.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime. "
                        ::= { wwpLeosOamStatsEntry 11 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.12
                wwpLeosOamOrgSpecificRx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of Organization Specific OAMPDUs
                                         received on this interface.  
                                  
                                         An Organization Specific OAMPDU is indicated by a valid frame
                                         with (1) destination MAC address equal to that of the reserved
                                         MAC address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                
                                
                                                         
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Organization Specific code.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime. "
                        ::= { wwpLeosOamStatsEntry 12 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.13
                wwpLeosOamUnsupportedCodesTx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of OAMPDUs transmitted on this
                                         interface with an unsupported op-code.  
                                  
                                         An unsupported op-code OAMPDU is indicated by a valid frame
                                         with (1) destination MAC address equal to that of the reserved
                                         MAC address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         op-code for a function that is not supported by the device.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime. "
                        ::= { wwpLeosOamStatsEntry 13 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.14
                wwpLeosOamUnsupportedCodesRx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of OAMPDUs received on this interface
                                         with an unsupported op-code.  
                                  
                                         An unsupported op-code OAMPDU is indicated by a valid frame
                                         with (1) destination MAC address equal to that of the reserved
                                         MAC address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         opcode for a function that is not supported by the device.  
                                
                                
                                                         
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime."
                        ::= { wwpLeosOamStatsEntry 14 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.15
                wwpLeosOamframesLostDueToOam OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of frames that were dropped by the OAM
                                         multiplexer.  Since the OAM multiplexer has multiple inputs
                                         and a single output, there may be cases where frames are
                                         dropped due to transmit resource contention.  This counter is
                                         incremented whenever a frame is dropped by the OAM layer.
                                         When this counter is incremented, no other counters in this
                                         MIB are incremented.  
                                                       
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime."
                        ::= { wwpLeosOamStatsEntry 15 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.16
                wwpLeosOamStatsPort OBJECT-TYPE
                        SYNTAX Integer32 (1..1000)
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "An Ethernet port on the switch"
                        ::= { wwpLeosOamStatsEntry 16 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.17
                wwpLeosOamDuplicateEventNotificationTx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of duplicate Event OAMPDUs transmitted
                                         on this interface.  Event notification OAMPDUs may be sent in
                                         duplicate to increase the probability of successfully being
                                         received, given the possibility that a frame may be lost in
                                         transit.  
                                  
                                         An Event Notification OAMPDU is indicated by a valid frame
                                         with (1) destination MAC address equal to that of the reserved
                                         MAC address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Event code.  
                                  
                                         A duplicate Event Notification OAMPDU is indicated as an Event
                                         Notification OAMPDU with a Sequence Number field that is
                                         identical to the previously transmitted Event Notification
                                         OAMPDU Sequence Number.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime."
                        ::= { wwpLeosOamStatsEntry 17 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.4.1.18
                wwpLeosOamDuplicateEventNotificationRx OBJECT-TYPE
                        SYNTAX Counter32
                        UNITS "frames"
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A count of the number of duplicate Event OAMPDUs received on
                                         this interface.  Event notification OAMPDUs may be sent in
                                         duplicate to increase the probability of successfully being
                                         received, given the possibility that a frame may be lost in
                                
                                
                                                         
                                         transit.  
                                  
                                         An Event Notification OAMPDU is indicated by a valid frame
                                         with (1) destination MAC address equal to that of the reserved
                                         MAC address for Slow Protocols (See 43B of [802.3ah]), (2) a
                                         lengthOrType field equal to the reserved type for Slow
                                         Protocols, (3) a Slow Protocols subtype equal to that of the
                                         subtype reserved for OAM, and (4) an OAMPDU code equals the
                                         OAM Event code.  
                                  
                                         A duplicate Event Notification OAMPDU is indicated as an Event
                                         Notification OAMPDU with a Sequence Number field that is
                                         identical to the previously received Event Notification OAMPDU
                                         Sequence Number.  
                                  
                                         Discontinuities of this counter can occur at re-initialization
                                         of the management system, and at other times as indicated by
                                         the value of the ifCounterDiscontinuityTime. "
                        ::= { wwpLeosOamStatsEntry 18 }

                
                -- 1.3.6.1.4.1.6141.2.60.400.1.2.5
                wwpLeosOamSystemEnableDisable OBJECT-TYPE
                        SYNTAX INTEGER
                                {
                                enable(1),
                                disable(2)
                                }
                        MAX-ACCESS read-write
                        STATUS current
                        DESCRIPTION
                                "Global Enable/disable OAM on the switch"
                        ::= { wwpLeosOamObjs 5 }

                
                wwpLeosOamEventConfigTable OBJECT-TYPE  
                        SYNTAX SEQUENCE OF WwpLeosOamEventConfigEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "Ethernet OAM includes the ability to generate and receive
                                         event notifications to indicate various link problems.  This
                                         table contains the mechanisms to configure the thresholds to
                                         generate the standard Ethernet OAM Event.
                                These events are:
                                        - Errored Symbol Period Event.  Generated when the number of
                                        symbol errors exceeds a threshold within a given window 
                                        defined by a number of symbols (e.g. 1,000 symbols out of 
                                        1,000,000 had errors).  

                                   - Errored Frame Period Event.  Generated when the number of 
                                         frame errors exceeds a threshold within a given window 
                                        defined by a number of frames (e.g. 10 frames out of 1000 
                                        had errors).  
                                        - Errored Frame Event.  Generated when the number of frame 
                                        errors exceeds a threshold within a given window defined 
                                        by a period of time (e.g. 10 frames in 1 second had 
                                        errors).
                                        - Errored Frame Seconds Summary Event.  Generated when the 
                                        number of errored frame seconds exceeds a threshold within
                                        a given time period (e.g. 10 errored frame seconds within 
                                        the last 100 seconds).  An errored frame second is defined
                                        as a 1 second interval which had >0 frame errors.  
                        "   
                        ::= { wwpLeosOamObjs 6 }
  
                -- 1.3.6.1.4.1.6141.2.60.400.1.3.1.1
                wwpLeosOamEventConfigEntry OBJECT-TYPE
                        SYNTAX WwpLeosOamEventConfigEntry
                                                MAX-ACCESS not-accessible
                                        STATUS current
                                        DESCRIPTION
                                                 "Event configuration information is available for every
                                                 Ethernet like interface that supports OAM and the event
                                                 function of OAM as indicated in the wwpLeosOamFunctionsSupported
                                                 attribute.  
                                          
                                                 Event configuration controls when the local management entity
                                                 sends Event Notification OAMPDUs to its OAM peer.  "
                  
                        INDEX { wwpLeosOamEventPort }
                        ::= { wwpLeosOamEventConfigTable 1 }
                
                WwpLeosOamEventConfigEntry ::=
                        SEQUENCE { 
                         wwpLeosOamEventPort                               Integer32,
                                wwpLeosOamErrFramePeriodWindow                                  Unsigned32,
                                wwpLeosOamErrFramePeriodThreshold                                       Unsigned32,
                                wwpLeosOamErrFramePeriodEvNotifEnable                                   INTEGER,
                                wwpLeosOamErrFrameWindow                                        Unsigned32,             
                                wwpLeosOamErrFrameThreshold                                     Unsigned32,
                                wwpLeosOamErrFrameEvNotifEnable                                 INTEGER,
                                wwpLeosOamErrFrameSecsSummaryWindow                                     Integer32,
                                wwpLeosOamErrFrameSecsSummaryThreshold                                  Integer32,
                                wwpLeosOamErrFrameSecsEvNotifEnable                                     INTEGER,
                                wwpLeosOamDyingGaspEnable                                       INTEGER,
                                wwpLeosOamCriticalEventEnable                                   INTEGER
                                        }
        
        wwpLeosOamEventPort OBJECT-TYPE
                SYNTAX Integer32 (1..1000)
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "An Ethernet port on the switch"
                ::= { wwpLeosOamEventConfigEntry 1 }

                -- 1.3.6.1.4.1.6141.2.60.400.1.3.1.1.1

                        wwpLeosOamErrFramePeriodWindow OBJECT-TYPE
                                        SYNTAX      Unsigned32 (14880..8928000)
                        UNITS       "frames"
                        MAX-ACCESS  read-write
                        STATUS      current
                        DESCRIPTION 
                                "The number of frames over which the threshold is defined. 
                                             The default value of the window is the number of minimum size
                                             Ethernet frames that can be received over the physical layer in
                                             one second.  
                                                 
                                 If wwpLeosOamErrFramePeriodThreshold frame errors occur within a
                                 window of wwpLeosOamErrFramePeriodWindow frames, an Event
                                 Notification OAMPDU should be generated with an Errored Frame
                                 Period Event TLV indicating the threshold has been crossed in
                                 this window.  "
                                       REFERENCE   "[802.3ah], 30.3.6.1.38"  
                        ::= { wwpLeosOamEventConfigEntry 2 }

                -- 1.3.6.1.4.1.6141.2.60.400.1.3.1.1.2
       wwpLeosOamErrFramePeriodThreshold OBJECT-TYPE
       SYNTAX      Unsigned32 (0..4294967293)
                        UNITS       "frames"
                        MAX-ACCESS  read-write
                        STATUS      current
                        DESCRIPTION 
                                "The number of frame errors that must occur for this event to
                                         be triggered.  The default value is one frame error.  
                                                         
                                         If wwpLeosOamErrFramePeriodThreshold frame errors occur within a
                                         window of wwpLeosOamErrFramePeriodWindow frames, an Event
                                         Notification OAMPDU should be generated with an Errored Frame
                                         Period Event TLV indicating the threshold has been crossed in
                                         this window.  "
       REFERENCE   "[802.3ah], 30.3.6.1.38"  
                        ::= { wwpLeosOamEventConfigEntry 3 }
                       
                -- 1.3.6.1.4.1.6141.2.60.400.1.3.1.1.3
                wwpLeosOamErrFramePeriodEvNotifEnable OBJECT-TYPE 
                        SYNTAX      INTEGER { enabled(1), disabled(2) }
                        MAX-ACCESS  read-write
                        STATUS      current
                        DESCRIPTION 
                                "Indicates whether the occurrence of an Errored Frame Period
                                         Event should result in an Event Notification OAMPDU generated
                                         by the OAM layer.  
                                                         
                                         By default, this object should have the value enabled(1) for
                                         Ethernet like interfaces that support OAM.  If the OAM layer
                                         does not support event notifications (as indicated via the
                                         wwpLeosOamFunctionsSupported attribute), this value is ignored. "
                        ::= { wwpLeosOamEventConfigEntry 4 }
                        
                -- 1.3.6.1.4.1.6141.2.60.400.1.3.1.1.4     
                wwpLeosOamErrFrameWindow OBJECT-TYPE
       SYNTAX      Unsigned32 (10..600)
                        UNITS       "tenths of a second"
                        MAX-ACCESS  read-write
                        STATUS      current
                        DESCRIPTION 
                                "The amount of time (in 100ms increments) over which the
                                         threshold is defined.  The default value is 10 (1 second).  
                                                         
                                        If wwpLeosOamErrFrameThreshold frame errors occur within a window
                                        of wwpLeosOamErrFrameWindow seconds (measured in tenths of
                                        seconds), an Event Notification OAMPDU should be generated with
                                        an Errored Frame Event TLV indicating the threshold has been
                                        crossed in this window.  "
       REFERENCE   "[802.3ah], 30.3.6.1.36"  
                        ::= { wwpLeosOamEventConfigEntry 5 }
                       
                -- 1.3.6.1.4.1.6141.2.60.400.1.3.1.1.5
       wwpLeosOamErrFrameThreshold OBJECT-TYPE
       SYNTAX      Unsigned32 (0..4294967293)
                        UNITS       "frames"
                        MAX-ACCESS  read-write
                        STATUS      current
                        DESCRIPTION 
                                "The number of frame errors that must occur for this event to
                                         be triggered.  The default value is one frame error.  
                                                         
                                         If wwpLeosOamErrFrameThreshold frame errors occur within a window
                                         of wwpLeosOamErrFrameWindow (in tenths of seconds), an Event
                                         Notification OAMPDU should be generated with an Errored Frame
                                         Event TLV indicating the threshold has been crossed in this
                                         window.  "
       REFERENCE   "[802.3ah], 30.3.6.1.36"  
                        ::= { wwpLeosOamEventConfigEntry 6 }
                       
                -- 1.3.6.1.4.1.6141.2.60.400.1.3.1.1.6
                wwpLeosOamErrFrameEvNotifEnable OBJECT-TYPE 
                        SYNTAX      INTEGER { enabled(1), disabled(2) }
                        MAX-ACCESS  read-write
                        STATUS      current
                        DESCRIPTION 
                                "Indicates whether the occurrence of an Errored Frame Event
                                         should result in an Event Notification OAMPDU generated by the
                                         OAM layer.  
                                                         
                                         By default, this object should have the value enabled(1) for
                                         Ethernet like interfaces that support OAM.  If the OAM layer
                                         does not support event notifications (as indicated via the
                                         wwpLeosOamFunctionsSupported attribute), this value is ignored. "
                        ::= { wwpLeosOamEventConfigEntry 7 }
                          
                -- 1.3.6.1.4.1.6141.2.60.400.1.3.1.1.7   
                wwpLeosOamErrFrameSecsSummaryWindow OBJECT-TYPE
       SYNTAX      Integer32 (100..9000)
                        UNITS       "tenths of a second"
                        MAX-ACCESS  read-write
                        STATUS      current
                        DESCRIPTION 
                                "The amount of time (in 100ms intervals) over which the
                                         threshold is defined.  The default value is 100 (10 seconds).  
                                                         
                                         If wwpLeosOamErrFrameSecsSummaryThreshold frame errors occur
                                         within a window of wwpLeosOamErrFrameSecsSummaryWindow (in tenths
                                         of seconds), an Event Notification OAMPDU should be generated
                                         with an Errored Frame Seconds Summary Event TLV indicating the
                                         threshold has been crossed in this window.  "
                        REFERENCE   "[802.3ah], 30.3.6.1.40"  
                        ::= { wwpLeosOamEventConfigEntry 8 }
                
                -- 1.3.6.1.4.1.6141.2.60.400.1.3.1.1.8
                wwpLeosOamErrFrameSecsSummaryThreshold OBJECT-TYPE
       SYNTAX      Integer32 (0..65535)
                        UNITS       "errored frame seconds"
                        MAX-ACCESS  read-write
                        STATUS      current
                        DESCRIPTION 
                                "The number of errored frame seconds that must occur for this
                                         event to be triggered.  The default value is one errored frame
                                         second.  
                                                         
                                         If wwpLeosOamErrFrameSecsSummaryThreshold frame errors occur
                                         within a window of wwpLeosOamErrFrameSecsSummaryWindow (in tenths
                                         of seconds), an Event Notification OAMPDU should be generated
                                         with an Errored Frame Seconds Summary Event TLV indicating the
                                         threshold has been crossed in this window.  "
       REFERENCE   "[802.3ah], 30.3.6.1.40"  
                        ::= { wwpLeosOamEventConfigEntry 9 }
                       
                -- 1.3.6.1.4.1.6141.2.60.400.1.3.1.1.9
                wwpLeosOamErrFrameSecsEvNotifEnable OBJECT-TYPE 
                        SYNTAX      INTEGER { enabled(1), disabled(2) }
                        MAX-ACCESS  read-write
                        STATUS      current
                        DESCRIPTION 
                                "Indicates whether the occurrence of an Errored Frame Seconds
                                         Summary Event should result in an Event Notification OAMPDU
                                         generated by the OAM layer.  
                                                         
                                         By default, this object should have the value enabled(1) for
                                         Ethernet like interfaces that support OAM.  If the OAM layer
                                         does not support event notifications (as indicated via the
                                         wwpLeosOamFunctionsSupported attribute), this value is ignored."
                        ::= { wwpLeosOamEventConfigEntry 10 }
                       
                -- 1.3.6.1.4.1.6141.2.60.400.1.3.1.1.10      
                wwpLeosOamDyingGaspEnable OBJECT-TYPE 
                        SYNTAX      INTEGER { enabled(1), disabled(2) }
                        MAX-ACCESS  read-write
                        STATUS      current
                        DESCRIPTION 
                                "Indicates whether the local device should attempt to indicate
                                         a dying gasp fault via the OAMPDU flags field to its peer OAM
                                         entity.  If the system does not support dying gasp capability,
                                         setting this object has no effect, and reading the object
                                         should always result in 'disabled(2)'.  
                                         
                                         By default, this object should have the value enabled(1) for
                                         Ethernet like interfaces that support OAM.  If the OAM layer
                                         does not support event notifications (as indicated via the
                                         OamFunctionsSupported attribute), this value is ignored."
                        ::= { wwpLeosOamEventConfigEntry 11 }
                 
                -- 1.3.6.1.4.1.6141.2.60.400.1.3.1.1.11      

                wwpLeosOamCriticalEventEnable OBJECT-TYPE 
                        SYNTAX      INTEGER { enabled(1), disabled(2) }
                        MAX-ACCESS  read-write
                        STATUS      current
                        DESCRIPTION 
                                "Indicates whether the local device should attempt to indicate
                                         a critical event has occurred via the OAMPDU flags field to its peer OAM
                                         entity.  If the system does not support dying gasp capability,
                                         setting this object has no effect, and reading the object
                                         should always result in 'disabled(2)'.  
                                         
                                         By default, this object should have the value enabled(1) for
                                         Ethernet like interfaces that support OAM.  If the OAM layer
                                         does not support event notifications (as indicated via the
                                         OamFunctionsSupported attribute), this value is ignored."
                        ::= { wwpLeosOamEventConfigEntry 12 }
       
                                

                -- 1.3.6.1.4.1.6141.2.60.400.1.3.2
                wwpLeosOamEventLogTable   OBJECT-TYPE 
                        SYNTAX       SEQUENCE OF WwpLeosOamEventLogEntry 
                        MAX-ACCESS   not-accessible 
                        STATUS       current 
                        DESCRIPTION 
                                "This table records a history of the events that have occurred
                                         at the Ethernet OAM level.  These events can include locally
                                         detected events, which may result in locally generated
                                         OAMPDUs, and remotely detected events, which are detected by
                                         the OAM peer entity and signaled to the local entity via
                                         Ethernet OAM.  Ethernet OAM events can be signaled by Event
                                         Notification OAMPDUs or by the flags field in any OAMPDU.  "
                        ::= { wwpLeosOamObjs 7 } 
  
                -- 1.3.6.1.4.1.6141.2.60.400.1.3.2.1
                wwpLeosOamEventLogEntry OBJECT-TYPE 
                        SYNTAX      WwpLeosOamEventLogEntry 
                        MAX-ACCESS  not-accessible 
                        STATUS      current 
                        DESCRIPTION "An entry in the wwpLeosOamEventLogTable." 
                        INDEX       { wwpLeosOamEventLogPort, wwpLeosOamEventLogIndex }
                        ::= { wwpLeosOamEventLogTable 1 } 
  
                WwpLeosOamEventLogEntry ::=
                        SEQUENCE {
                                                        wwpLeosOamEventLogPort                 Integer32,
                                wwpLeosOamEventLogIndex                Unsigned32,
                                wwpLeosOamEventLogTimestamp            TimeStamp,
                                wwpLeosOamEventLogOui                  OCTET STRING(SIZE(3)), 
                                wwpLeosOamEventLogType                 Unsigned32,
                                wwpLeosOamEventLogLocation             INTEGER,
                                                        wwpLeosOamEventLogWindowHi             Unsigned32,
                                                        wwpLeosOamEventLogWindowLo             Unsigned32,                                                              
                                                        wwpLeosOamEventLogThresholdHi          Unsigned32,
                                                        wwpLeosOamEventLogThresholdLo          Unsigned32,
                                wwpLeosOamEventLogValue                Counter64,
                                wwpLeosOamEventLogRunningTotal         Counter64,
                                wwpLeosOamEventLogEventTotal           Unsigned32
                        }
        
                                wwpLeosOamEventLogPort OBJECT-TYPE
                                        SYNTAX Integer32 (1..1000)
                                        MAX-ACCESS read-only
                                        STATUS current
                                        DESCRIPTION
                                                        "An Ethernet port on the switch"
                                        ::= { wwpLeosOamEventLogEntry 1 }       
  
                wwpLeosOamEventLogIndex       OBJECT-TYPE
                        SYNTAX      Unsigned32
                                        MAX-ACCESS  read-only
                        STATUS      current 
                        DESCRIPTION 
                                "An arbitrary integer for identifying individual events
                                        within the event log.  "
                        ::= { wwpLeosOamEventLogEntry 2 }
  
                wwpLeosOamEventLogTimestamp  OBJECT-TYPE 
                        SYNTAX      TimeStamp 
                        MAX-ACCESS  read-only
                        STATUS      current 
                        DESCRIPTION 
                                "The value of sysUpTime at the time of the logged event.  For
                                         locally generated events, the time of the event can be
                                         accurately retrieved from sysUpTime.  For remotely generated
                                         events, the time of the event is indicated by the reception of
                                         the Event Notification OAMPDU indicating the event occurred on
                                         the peer.  A system may attempt to adjust the timestamp value
                                         to more accurately reflect the time of the event at the peer
                                         OAM entity by using other information, such as that found in
                                         the timestamp found of the Event Notification TLVs, which
                                         provides an indication of the relative time between events at
                                         the peer entity.  "
                        ::= { wwpLeosOamEventLogEntry 3 }
  
                wwpLeosOamEventLogOui  OBJECT-TYPE 
                        SYNTAX      OCTET STRING(SIZE(3))
                        MAX-ACCESS  read-only
                        STATUS      current 
                        DESCRIPTION 
                                "The OUI of the entity defining the object type.  All IEEE
                                         802.3 defined events (as appearing in [802.3ah] except for the
                                         Organizationally Unique Event TLVs) use the IEEE 802.3 OUI of
                                         0x0180C2.  Organizations defining their own Event Notification
                                         TLVs include their OUI in the Event Notification TLV which
                                         gets reflected here.  "
                        ::= { wwpLeosOamEventLogEntry 4 }
  
                wwpLeosOamEventLogType      OBJECT-TYPE
                        SYNTAX      Unsigned32 
                        MAX-ACCESS  read-only
                        STATUS      current 
                        DESCRIPTION 
                                "The type of event that generated this entry in the event log.
  
                                        When the OUI is the IEEE 802.3 OUI of 0x0180C2, the following
                                        event types are defined:
                                             erroredSymbolEvent(1), 
                                             erroredFramePeriodEvent (2), 
                                             erroredFrameEvent(3),
                                             erroredFrameSecondsEvent(4), 
                                             linkFault(256), 
                                             dyingGaspEvent(257),
                                             criticalLinkEvent(258)
                                         The first four are considered threshold crossing events as
                                         they are generated when a metric exceeds a given value within
                                         a specified window.  The other three are not threshold
                                         crossing events.  
                                  
                                         When the OUI is not 0x0180C2, then some other organization has
                                         defined the event space.  If event subtyping is known to the
                                         implementation, it may be reflected here.  Otherwise, this
                                         value should return all F's (0xFFFFFFFF).  
                                         "
                        REFERENCE   "[802.3ah], 30.3.6.1.10 and 57.5.3."
                        ::= { wwpLeosOamEventLogEntry 5 }
  
                wwpLeosOamEventLogLocation OBJECT-TYPE 
                        SYNTAX      INTEGER { local(1), remote(2) }
                        MAX-ACCESS  read-only
                        STATUS      current 
                        DESCRIPTION 
                                "Whether this event occurred locally, or was received from the
                                        OAM peer via Ethernet OAM."
                        ::= { wwpLeosOamEventLogEntry 6 }
                                
                        wwpLeosOamEventLogWindowHi      OBJECT-TYPE
                                        SYNTAX      Unsigned32
                                        MAX-ACCESS  read-only
                                        STATUS      current 
                                        DESCRIPTION 
                                                "If the event represents a threshold crossing event, the two
                                                objects wwpLeosOamEventWindowHi and wwpLeosOamEventWindowLo form an
                                                unsigned 64-bit integer yielding the window over which the
                                                value was measured for the threshold crossing event (e.g. 5,
                                                when 11 occurrences happened in 5 seconds while the threshold
                                                was 10).   The two objects are combined as:
                
                                                wwpLeosOamEventLogWindow = ((2^32) * wwpLeosOamEventLogWindowHi)
                                                + wwpLeosOamEventLogWindowLo
  
         
                                                Otherwise, this value is returned as all F's (0xFFFFFFFF) and 
                                                adds no useful information.  "
                                        REFERENCE   "[802.3ah], 30.3.6.1.37 and 57.5.3.2."
                                        ::= { wwpLeosOamEventLogEntry 7 }     
               
                       wwpLeosOamEventLogWindowLo      OBJECT-TYPE
                                        SYNTAX      Unsigned32
                                        MAX-ACCESS  read-only
                                        STATUS      current 
                                        DESCRIPTION 
                                                "If the event represents a threshold crossing event, the two
                                                objects wwpLeosOamEventWindowHi and wwpLeosOamEventWindowLo form an
                                                unsigned 64-bit integer yielding the window over which the
                                                value was measured for the threshold crossing event (e.g. 5,
                                                when 11 occurrences happened in 5 seconds while the threshold
                                                was 10).   The two objects are combined as:
  
                                                wwpLeosOamEventLogWindow = ((2^32) * wwpLeosOamEventLogWindowHi)
                                                                     + wwpLeosOamEventLogWindowLo
  
                                               Otherwise, this value is returned as all F's (0xFFFFFFFF) and 
                                                adds no useful information.  "
                                        REFERENCE   "[802.3ah], 30.3.6.1.37 and 57.5.3.2."
                        ::= { wwpLeosOamEventLogEntry 8 }
     
                        wwpLeosOamEventLogThresholdHi      OBJECT-TYPE
                                        SYNTAX      Unsigned32
                                        MAX-ACCESS  read-only
                                        STATUS      current 
                                        DESCRIPTION 
                                                        "If the event represents a threshold crossing event, the two
                                                        objects wwpLeosOamEventThresholdHi and wwpLeosOamEventThresholdLo 
                                                        form an unsigned 64-bit integer yielding the value that was
                                                        crossed for the threshold crossing event (e.g. 10, when 11 
                                                        occurrences happened in 5 seconds while the threshold was 10).
                                                        The two objects are combined as:
  
                                                         wwpLeosOamEventLogThreshold = ((2^32) * wwpLeosOamEventLogThresholdHi)
                                                 + wwpLeosOamEventLogThresholdLo
  
                                                        Otherwise, this value is returned as all F's (0xFFFFFFFF) and 
                                                        adds no useful information.  "
                                        REFERENCE   "[802.3ah], 30.3.6.1.37 and 57.5.3.2."
                                        ::= { wwpLeosOamEventLogEntry 9 }
     
     -- 1.3.6.1.4.1.6141.2.400.1.2.7.1.10
     wwpLeosOamEventLogThresholdLo      OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current 
       DESCRIPTION 
         "If the event represents a threshold crossing event, the two
         objects wwpLeosOamEventThresholdHi and wwpLeosOamEventThresholdLo 
         form an unsigned 64-bit integer yielding the value that was
         crossed for the threshold crossing event (e.g. 10, when 11 
         occurrences happened in 5 seconds while the threshold was 10).
         The two objects are combined as:
  
       wwpLeosOamEventLogThreshold = ((2^32) * wwpLeosOamEventLogThresholdHi)
                                          + wwpLeosOamEventLogThresholdLo
  
         Otherwise, this value is returned as all F's (0xFFFFFFFF) and
         adds no useful information.  "
       REFERENCE   "[802.3ah], 30.3.6.1.37 and 57.5.3.2."
       ::= { wwpLeosOamEventLogEntry 10 }
  
                
                wwpLeosOamEventLogValue      OBJECT-TYPE
                        SYNTAX      Counter64 
                        MAX-ACCESS  read-only
                        STATUS      current 
                        DESCRIPTION 
                                "If the event represents a threshold crossing event, this
                                         value indicates the value of the parameter within the given
                                         window that generated this event (e.g. 11, when 11 occurrences
                                         happened in 5 seconds while the threshold was 10).  
                                  
                                         Otherwise, this value is returned as all F's 
                                         (0xFFFFFFFFFFFFFFFF) and adds no useful information.  
                                         "
                        REFERENCE   "[802.3ah], 30.3.6.1.37 and 57.5.3.2."
                        ::= { wwpLeosOamEventLogEntry 11 }
  
                wwpLeosOamEventLogRunningTotal      OBJECT-TYPE
                        SYNTAX      Counter64
                        MAX-ACCESS  read-only
                        STATUS      current 
                        DESCRIPTION 
                                "This value represents the total number of times this
                                         occurrence has happened since the last reset (e.g. 3253, when
                                         3253 symbol errors have occurred since the last reset, which
                                         has resulted in 51 symbol error threshold crossing events
                                         since the last reset).  "
                        REFERENCE   "[802.3ah], 30.3.6.1.37 and 57.5.3.2."
                        ::= { wwpLeosOamEventLogEntry 12 }
  
                wwpLeosOamEventLogEventTotal      OBJECT-TYPE
                        SYNTAX      Unsigned32
                        MAX-ACCESS  read-only
                        STATUS      current 
                        DESCRIPTION 
                                "This value represents the total number of times one or more
                                         of these occurrences have resulted in an event (e.g. 51 when
                                         3253 symbol errors have occurred since the last reset, which
                                         has resulted in 51 symbol error threshold crossing events
                                         since the last reset)."
                        REFERENCE   "[802.3ah], 30.3.6.1.37 and 57.5.3.2."
                        ::= { wwpLeosOamEventLogEntry 13 }
                        
    --
    -- OAM Global Attributes
    --
    wwpLeosOamGlobal OBJECT IDENTIFIER ::= { wwpLeosOamObjs 8 }
    
    wwpLeosOamStatsClear      OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-write
        STATUS      current 
        DESCRIPTION           
                    "Setting this object to 'true' will cause the values of all objects maintained within the wwpLeosOamStatsTable to reset to the value of zero.  
                     When read, this object always returns the value of false."
             ::= { wwpLeosOamGlobal 1 }
                                                               
                                                               
    --
    -- Notifications
    --  
    wwpLeosOamNotifMIBNotificationPrefix  OBJECT IDENTIFIER ::= { wwpLeosOamMIB 3 } 
    wwpLeosOamNotifMIBNotification        OBJECT IDENTIFIER ::= { wwpLeosOamNotifMIBNotificationPrefix 0 }

    wwpLeosOamLinkEventTrap  NOTIFICATION-TYPE
        OBJECTS     {                                                        
                     wwpLeosOamEventLogPort,
                     wwpLeosOamEventLogType,
                     wwpLeosOamEventLogLocation
                    }
         STATUS     current
         DESCRIPTION
                     "A wwpLeosOamLinkEventTrap notification is sent whenever a local or remote link event is detected
                      and recorded in the wwpLeosOamEventLogTable."
            ::= { wwpLeosOamNotifMIBNotification 1 }

        END

--
-- WWP-LEOS-OAM-MIB.my
--
