-- This file was included in WWP MIB release 04-07-01-0008
 --
 -- WWP-LEOS-PORT-STATSMIB.my
 --
 --
 -- NOTE WELL
 -- Starting from LE21X 2.0, the object wwpPortStatsReset mentioned 
 -- in this MIB has been deprecated. The WWP products no longer
 -- will provide the functionlaity to reset port stats.
 -- NOTE WELL

 WWP-LEOS-PORT-STATS-MIB DEFINITIONS ::= BEGIN

 IMPORTS                
   Unsigned32, Counter64, Counter32, OBJECT-TYPE, MODULE-IDENTITY                  
            FROM SNMPv2-SMI                                                     
   wwpModules, wwpModulesLeos                   
            FROM WWP-SMI;
        
        
 wwpLeosPortStatsMIB MODULE-IDENTITY
            LAST-UPDATED "200908061700Z"
            ORGANIZATION "Ciena, Inc"
            CONTACT-INFO
                    "   Mib Meister
                                        115 North Sullivan Road
                                        Spokane Valley, WA 99037
                                USA                             
                                Phone:  +1 509 242 9000
                                        Email:  support@ciena.com"
            DESCRIPTION
                    "The MIB module for the WWP Port ether Stats."
            REVISION    "200104031700Z"
            DESCRIPTION
                    "Initial creation."
            ::= { wwpModulesLeos 3 }
                                                
 --
 -- Node definitions
 --
        
 wwpLeosPortStatsMIBObjects OBJECT IDENTIFIER ::= { wwpLeosPortStatsMIB 1 }
 

 -- PortStats
 --
 wwpLeosPortStats OBJECT IDENTIFIER ::= { wwpLeosPortStatsMIBObjects 1 }

  
 -- Notifications 
  
 wwpLeosPortStatsMIBNotificationPrefix  OBJECT IDENTIFIER ::= { wwpLeosPortStatsMIB 2 } 
 wwpLeosPortStatsMIBNotifications       OBJECT IDENTIFIER ::=  
                       { wwpLeosPortStatsMIBNotificationPrefix 0 }

 -- Conformance information 
 
 wwpLeosPortStatsMIBConformance OBJECT IDENTIFIER ::= { wwpLeosPortStatsMIB 3 } 
 wwpLeosPortStatsMIBCompliances OBJECT IDENTIFIER ::= { wwpLeosPortStatsMIBConformance 1 }              
 wwpLeosPortStatsMIBGroups      OBJECT IDENTIFIER ::= { wwpLeosPortStatsMIBConformance 2 }


 wwpLeosPortStatsReset OBJECT-TYPE
    SYNTAX          INTEGER {
                        none(0),
                                reset(1)
                    } 
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
            "Setting this object to 'reset' will clear the stats of all ports. A read on this object will
             always return the 'none'."
    ::= { wwpLeosPortStats 1 }
                
 wwpLeosPortStatsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosPortStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "The table specifying the stats for the ports."
     ::= { wwpLeosPortStats 2 }

 wwpLeosPortStatsEntry OBJECT-TYPE
     SYNTAX       WwpLeosPortStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "An entry in the port stats table."
     INDEX { wwpLeosPortStatsPortId }
     ::= { wwpLeosPortStatsTable 1 }



                
 WwpLeosPortStatsEntry ::= SEQUENCE { 
     wwpLeosPortStatsPortId                INTEGER,
     wwpLeosPortStatsRxBytes               Counter32,
     wwpLeosPortStatsRxPkts                Counter32,
     wwpLeosPortStatsRxCrcErrorPkts        Counter32,
     wwpLeosPortStatsRxBcastPkts           Counter32,
     wwpLeosPortStatsUndersizePkts         Counter32,
     wwpLeosPortStatsOversizePkts          Counter32,
     wwpLeosPortStatsFragmentPkts          Counter32,
     wwpLeosPortStatsJabberPkts            Counter32,
     wwpLeosPortStats64BytePkts            Counter32,
     wwpLeosPortStats65To127BytePkts       Counter32,
     wwpLeosPortStats128To255BytePkts      Counter32,
     wwpLeosPortStats256To511BytePkts      Counter32,
     wwpLeosPortStats512To1023BytePkts     Counter32,
     wwpLeosPortStats1024To1518BytePkts    Counter32,
     wwpLeosPortStatsTxBytes               Counter32,
     wwpLeosPortStatsTxTBytes              Counter32,
     wwpLeosPortStatsTxPkts                Counter32,
     wwpLeosPortStatsTxExDeferPkts         Counter32,
     wwpLeosPortStatsTxGiantPkts           Counter32,
     wwpLeosPortStatsTxUnderRunPkts        Counter32,
     wwpLeosPortStatsTxCrcErrorPkts        Counter32,
     wwpLeosPortStatsTxLCheckErrorPkts     Counter32,
     wwpLeosPortStatsTxLOutRangePkts       Counter32,
     wwpLeosPortStatsTxLateCollPkts        Counter32,
     wwpLeosPortStatsTxExCollPkts          Counter32,
     wwpLeosPortStatsTxSingleCollPkts      Counter32,
     wwpLeosPortStatsTxCollPkts            Counter32,
     wwpLeosPortStatsTxPausePkts           Counter32,
     wwpLeosPortStatsTxMcastPkts           Counter32,
     wwpLeosPortStatsTxBcastPkts           Counter32,
     wwpLeosPortStatsPortReset             INTEGER,
     wwpLeosPortStatsRxMcastPkts           Counter32,
     wwpLeosPortStatsRxPausePkts           Counter32,
     wwpLeosPortStats1519To2047BytePkts    Counter32,
     wwpLeosPortStats2048To4095BytePkts    Counter32,
     wwpLeosPortStats4096To9216BytePkts    Counter32,
     wwpLeosPortStatsTxDeferPkts           Counter32,
     wwpLeosPortStatsTx64BytePkts          Counter32,
     wwpLeosPortStatsTx65To127BytePkts     Counter32,
     wwpLeosPortStatsTx128To255BytePkts    Counter32,
     wwpLeosPortStatsTx256To511BytePkts    Counter32,
     wwpLeosPortStatsTx512To1023BytePkts   Counter32,
     wwpLeosPortStatsTx1024To1518BytePkts  Counter32,
     wwpLeosPortStatsTx1519To2047BytePkts  Counter32,
     wwpLeosPortStatsTx2048To4095BytePkts  Counter32,
     wwpLeosPortStatsTx4096To9216BytePkts  Counter32,
     wwpLeosPortStatsRxFpgaDropPkts        Counter32,
     wwpLeosPortStatsPortLinkUp			    Counter32,
     wwpLeosPortStatsPortLinkDown		    Counter32,
     wwpLeosPortStatsPortLinkFlap		    Counter32,
     wwpLeosPortStatsRxUcastPkts           Counter32,
     wwpLeosPortStatsTxUcastPkts           Counter32,
     wwpLeosPortStatsRxDropPkts            Counter32,
     wwpLeosPortStatsRxDiscardPkts         Counter32,
     wwpLeosPortStatsRxLOutRangePkts       Counter32,
     wwpLeosPortStatsRxFpgaBufferDropPkts  Counter32, 
     wwpLeosPortStatsTxFpgaBufferDropPkts  Counter32,    
     wwpLeosPortStatsFpgaVlanPriFilterDropPkts  Counter32,
     wwpLeosPortStatsFpgaRxErrorPkts       Counter32,
     wwpLeosPortStatsFpgaRxCrcErrorPkts    Counter32,
     wwpLeosPortStatsFpgaRxIpCrcErrorPkts  Counter32
 }

 wwpLeosPortStatsPortId OBJECT-TYPE
    SYNTAX       INTEGER (1..65535)
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The Id of the port for which this entry
            contains the stats."
    ::= { wwpLeosPortStatsEntry 1 }

 wwpLeosPortStatsRxBytes OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of bytes received by this port."
    ::= { wwpLeosPortStatsEntry 2 }

 wwpLeosPortStatsRxPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of packets received by this port."
    ::= { wwpLeosPortStatsEntry 3 }
        
 wwpLeosPortStatsRxCrcErrorPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of packets received with CRC errors by this port."
    ::= { wwpLeosPortStatsEntry 4 }

 wwpLeosPortStatsRxBcastPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of Broadcast packets received by this port."
    ::= { wwpLeosPortStatsEntry 5 }

 wwpLeosPortStatsUndersizePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were
            less than 64 octets long (excluding framing bits,
            but including FCS octets) and were otherwise well
            formed."
    ::= { wwpLeosPortStatsEntry 6 }

 wwpLeosPortStatsOversizePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were
            longer than 1518 octets (excluding framing bits,
            but including FCS octets) and were otherwise
            well formed."
    ::= { wwpLeosPortStatsEntry 7 }

 wwpLeosPortStatsFragmentPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were less
            than 64 octets in length (excluding framing bits but
            including FCS octets) and had either a bad Frame
            Check Sequence (FCS) with an integral number of
            octets (FCS Error) or a bad FCS with a non-integral
            number of octets (Alignment Error)."
    ::= { wwpLeosPortStatsEntry 8 }


 wwpLeosPortStatsJabberPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were
            longer than 1518 octets (excluding framing bits,
            but including FCS octets), and had either a bad
            Frame Check Sequence (FCS) with an integral number
            of octets (FCS Error) or a bad FCS with a
            non-integral number of octets (Alignment Error)."
    ::= { wwpLeosPortStatsEntry 9 }
        
        
 wwpLeosPortStats64BytePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were 64 octets in length
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortStatsEntry 10 }

        
 wwpLeosPortStats65To127BytePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            65 and 127 octets in length inclusive
            (excluding framing bits but including FCS octets)." 
    ::= { wwpLeosPortStatsEntry 11 }
        
 wwpLeosPortStats128To255BytePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            128 and 255 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortStatsEntry 12 }
        
 wwpLeosPortStats256To511BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            256 and 511 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortStatsEntry 13 }
        
 wwpLeosPortStats512To1023BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            512 and 1023 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortStatsEntry 14 }
        
 wwpLeosPortStats1024To1518BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            1024 and 1518 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortStatsEntry 15 }
        
 wwpLeosPortStatsTxBytes OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The number of Octets transmitted for this port."
    ::= { wwpLeosPortStatsEntry 16 }
        
 wwpLeosPortStatsTxTBytes OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      deprecated
    DESCRIPTION
            "The total number of Octets transmitted for this port."
    ::= { wwpLeosPortStatsEntry 17 }

 wwpLeosPortStatsTxPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The total number of packets transmitted for this port."
    ::= { wwpLeosPortStatsEntry 18 }
        
        
 wwpLeosPortStatsTxExDeferPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit excessive defer packet count for a port."
    ::= { wwpLeosPortStatsEntry 19 }
        
 wwpLeosPortStatsTxGiantPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit too big packet count for a port."
    ::= { wwpLeosPortStatsEntry 20 }
        
 wwpLeosPortStatsTxUnderRunPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit underrun packet count for a port."
    ::= { wwpLeosPortStatsEntry 21 }
        
 wwpLeosPortStatsTxCrcErrorPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit CRC error packet count for a port."
    ::= { wwpLeosPortStatsEntry 22 }
        
 wwpLeosPortStatsTxLCheckErrorPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit length check error packet count for a port."
    ::= { wwpLeosPortStatsEntry 23 }
        
 wwpLeosPortStatsTxLOutRangePkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit length out of range packet count for a port."
    ::= { wwpLeosPortStatsEntry 24 }
        
 wwpLeosPortStatsTxLateCollPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit late collision packet count for a port."
    ::= { wwpLeosPortStatsEntry 25 }
        
 wwpLeosPortStatsTxExCollPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit excessive collision packet count for a port."
    ::= { wwpLeosPortStatsEntry 26 }
        
 wwpLeosPortStatsTxSingleCollPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit single collision packet count for a port."
    ::= { wwpLeosPortStatsEntry 27 }
        
 wwpLeosPortStatsTxCollPkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit collision packet count for the port."
    ::= { wwpLeosPortStatsEntry 28 }
 
 wwpLeosPortStatsTxPausePkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit pause packets for the port."
    ::= { wwpLeosPortStatsEntry 29 }

 wwpLeosPortStatsTxMcastPkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit multicast packets for the port."
    ::= { wwpLeosPortStatsEntry 30 }

 wwpLeosPortStatsTxBcastPkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit broadcast packets for the port."
    ::= { wwpLeosPortStatsEntry 31 }
    
 wwpLeosPortStatsPortReset OBJECT-TYPE
    SYNTAX          INTEGER {
                        none(0),
                                reset(1)
                    } 
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
            "Setting this object will reset the stats of given port.
             Doing read on this object will always return 'none'"
    ::= { wwpLeosPortStatsEntry 32 }
 
 wwpLeosPortStatsRxMcastPkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total number of multicast packets received for the given port."
    ::= { wwpLeosPortStatsEntry 33 }
 
 wwpLeosPortStatsRxPausePkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The receive pause packets for the port."
    ::= { wwpLeosPortStatsEntry 34 }
        
 wwpLeosPortStats1519To2047BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            1519 and 2047 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 35 }
        
 wwpLeosPortStats2048To4095BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            2048 and 4095 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 36 }
        
 wwpLeosPortStats4096To9216BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            4096 and 9216 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 37 }
        
 wwpLeosPortStatsTxDeferPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit single deferral packet count for a port.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 38 }
        
 wwpLeosPortStatsTx64BytePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were 64 octets in length
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 39 }
        
 wwpLeosPortStatsTx65To127BytePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            65 and 127 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x" 
    ::= { wwpLeosPortStatsEntry 40 }
        
 wwpLeosPortStatsTx128To255BytePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            128 and 255 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 41 }
        
 wwpLeosPortStatsTx256To511BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            256 and 511 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 42 }
        
 wwpLeosPortStatsTx512To1023BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            512 and 1023 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 43 }
        
 wwpLeosPortStatsTx1024To1518BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            1024 and 1518 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 44 }
        
 wwpLeosPortStatsTx1519To2047BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            1519 and 2047 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 45 }
        
 wwpLeosPortStatsTx2048To4095BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            2048 and 4095 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 46 }
        
 wwpLeosPortStatsTx4096To9216BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            4096 and 9216 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 47 }
        
 wwpLeosPortStatsRxFpgaDropPkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total number of dropped packets on a port when 
             traffic profiles are enabled on the port. (311v only)"
    ::= { wwpLeosPortStatsEntry 48 } 
 
 wwpLeosPortStatsPortLinkUp OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total number of port link up events on the port."
    ::= { wwpLeosPortStatsEntry 49 }
 
 wwpLeosPortStatsPortLinkDown OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total number of port link down events on the port."
    ::= { wwpLeosPortStatsEntry 50 }
 
 wwpLeosPortStatsPortLinkFlap OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total number of port link flap events on the port."
    ::= { wwpLeosPortStatsEntry 51 }
       
 wwpLeosPortStatsRxUcastPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of Unicast packets received by this port.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 52 }
        
 wwpLeosPortStatsTxUcastPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of Unicast packets transmitted by this port.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 53 }
        
  wwpLeosPortStatsRxDropPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of discarded received frames for this port."
    ::= { wwpLeosPortStatsEntry 54 }
        
  wwpLeosPortStatsRxDiscardPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of discarded received frames for this port including
            IPv6 L3, L3 IP Header and runt discards."
    ::= { wwpLeosPortStatsEntry 55 }
        
  wwpLeosPortStatsRxLOutRangePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of frames received by this port that exceeded
            the maximum permitted frame size.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortStatsEntry 56 }
 wwpLeosPortStatsRxFpgaBufferDropPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "number of frames dropped because the FPGA RX buffer was full
				Only supported on the 311V"
    ::= { wwpLeosPortStatsEntry 57 }
 wwpLeosPortStatsTxFpgaBufferDropPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "number of frames dropped because the FPGA TX buffer was full
				Only supported on the 311V"
    ::= { wwpLeosPortStatsEntry 58 }
    
 wwpLeosPortStatsFpgaVlanPriFilterDropPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "number of frames dropped by the transmit VLAN Priority Filter
				Only supported on the 311V"
    ::= { wwpLeosPortStatsEntry 59 }

 wwpLeosPortStatsFpgaRxErrorPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "Number of frames dropped by the FPGA because of receive errors.
            Only supported on the 311V"
    ::= { wwpLeosPortStatsEntry 60 }
    
 wwpLeosPortStatsFpgaRxCrcErrorPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "Number of frames dropped by the FPGA because of CRC errors.
            Only supported on the 311V"
    ::= { wwpLeosPortStatsEntry 61 }
    
 wwpLeosPortStatsFpgaRxIpCrcErrorPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "Number of frames dropped by the FPGA because of IP Checksum errors
             Only supported on the 311V"
    ::= { wwpLeosPortStatsEntry 62 }


        
--
-- Total Port stats
--
 wwpLeosPortTotalStatsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosPortTotalStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "The table specifying the stats for the ports."
     ::= { wwpLeosPortStats 3 }  
 
 wwpLeosPortTotalStatsEntry OBJECT-TYPE
     SYNTAX       WwpLeosPortTotalStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "An entry in the port stats table."
     INDEX { wwpLeosPortTotalStatsPortId }
     ::= { wwpLeosPortTotalStatsTable 1 }       
   
     WwpLeosPortTotalStatsEntry ::= SEQUENCE { 
     wwpLeosPortTotalStatsPortId                INTEGER,
     wwpLeosPortTotalStatsRxBytes               Counter32,
     wwpLeosPortTotalStatsRxPkts                Counter32,
     wwpLeosPortTotalStatsRxCrcErrorPkts        Counter32,
     wwpLeosPortTotalStatsRxBcastPkts           Counter32,
     wwpLeosPortTotalStatsUndersizePkts         Counter32,
     wwpLeosPortTotalStatsOversizePkts          Counter32,
     wwpLeosPortTotalStatsFragmentPkts          Counter32,
     wwpLeosPortTotalStatsJabberPkts            Counter32,
     wwpLeosPortTotalStats64BytePkts            Counter32,
     wwpLeosPortTotalStats65To127BytePkts       Counter32,
     wwpLeosPortTotalStats128To255BytePkts      Counter32,
     wwpLeosPortTotalStats256To511BytePkts      Counter32,
     wwpLeosPortTotalStats512To1023BytePkts     Counter32,
     wwpLeosPortTotalStats1024To1518BytePkts    Counter32,
     wwpLeosPortTotalStatsTxBytes               Counter32,
     wwpLeosPortTotalStatsTxTBytes              Counter32,
     wwpLeosPortTotalStatsTxPkts                Counter32,
     wwpLeosPortTotalStatsTxExDeferPkts         Counter32,
     wwpLeosPortTotalStatsTxGiantPkts           Counter32,
     wwpLeosPortTotalStatsTxUnderRunPkts        Counter32,
     wwpLeosPortTotalStatsTxCrcErrorPkts        Counter32,
     wwpLeosPortTotalStatsTxLCheckErrorPkts     Counter32,
     wwpLeosPortTotalStatsTxLOutRangePkts       Counter32,
     wwpLeosPortTotalStatsTxLateCollPkts        Counter32,
     wwpLeosPortTotalStatsTxExCollPkts          Counter32,
     wwpLeosPortTotalStatsTxSingleCollPkts      Counter32,
     wwpLeosPortTotalStatsTxCollPkts            Counter32,
     wwpLeosPortTotalStatsTxPausePkts           Counter32,
     wwpLeosPortTotalStatsTxMcastPkts           Counter32,
     wwpLeosPortTotalStatsTxBcastPkts           Counter32,
     wwpLeosPortTotalStatsPortReset             INTEGER,
     wwpLeosPortTotalStatsRxMcastPkts           Counter32,
     wwpLeosPortTotalStatsRxPausePkts           Counter32,
     wwpLeosPortTotalStats1519To2047BytePkts    Counter32,
     wwpLeosPortTotalStats2048To4095BytePkts    Counter32,
     wwpLeosPortTotalStats4096To9216BytePkts    Counter32,
     wwpLeosPortTotalStatsTxDeferPkts           Counter32,
     wwpLeosPortTotalStatsTx64BytePkts          Counter32,
     wwpLeosPortTotalStatsTx65To127BytePkts     Counter32,
     wwpLeosPortTotalStatsTx128To255BytePkts    Counter32,
     wwpLeosPortTotalStatsTx256To511BytePkts    Counter32,
     wwpLeosPortTotalStatsTx512To1023BytePkts   Counter32,
     wwpLeosPortTotalStatsTx1024To1518BytePkts  Counter32,
     wwpLeosPortTotalStatsTx1519To2047BytePkts  Counter32,
     wwpLeosPortTotalStatsTx2048To4095BytePkts  Counter32,
     wwpLeosPortTotalStatsTx4096To9216BytePkts  Counter32,
     wwpLeosPortTotalStatsRxFpgaDropPkts        Counter32,
     wwpLeosPortTotalStatsPortLinkUp			Counter32,
     wwpLeosPortTotalStatsPortLinkDown			Counter32,
     wwpLeosPortTotalStatsPortLinkFlap			Counter32,
     wwpLeosPortTotalStatsRxUcastPkts           Counter32,
     wwpLeosPortTotalStatsTxUcastPkts           Counter32,
     wwpLeosPortTotalStatsRxDropPkts            Counter32,
     wwpLeosPortTotalStatsRxDiscardPkts         Counter32,
     wwpLeosPortTotalStatsRxLOutRangePkts       Counter32,
     wwpLeosPortTotalStatsRxFpgaBufferDropPkts       Counter32, 
     wwpLeosPortTotalStatsTxFpgaBufferDropPkts       Counter32,    
     wwpLeosPortTotalStatsFpgaVlanPriFilterDropPkts  Counter32,
     wwpLeosPortTotalStatsFpgaRxErrorPkts       Counter32,
     wwpLeosPortTotalStatsFpgaRxCrcErrorPkts    Counter32,
     wwpLeosPortTotalStatsFpgaRxIpCrcErrorPkts  Counter32
 }

 wwpLeosPortTotalStatsPortId OBJECT-TYPE
    SYNTAX       INTEGER (1..65535)
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The Id of the port for which this entry
            contains the stats."
    ::= { wwpLeosPortTotalStatsEntry 1 }

 wwpLeosPortTotalStatsRxBytes OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of bytes received by this port."
    ::= { wwpLeosPortTotalStatsEntry 2 }

 wwpLeosPortTotalStatsRxPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of packets received by this port."
    ::= { wwpLeosPortTotalStatsEntry 3 }
        
 wwpLeosPortTotalStatsRxCrcErrorPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of packets received with CRC errors by this port."
    ::= { wwpLeosPortTotalStatsEntry 4 }

 wwpLeosPortTotalStatsRxBcastPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of Broadcast packets received by this port."
    ::= { wwpLeosPortTotalStatsEntry 5 }

 wwpLeosPortTotalStatsUndersizePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were
            less than 64 octets long (excluding framing bits,
            but including FCS octets) and were otherwise well
            formed."
    ::= { wwpLeosPortTotalStatsEntry 6 }

 wwpLeosPortTotalStatsOversizePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were
            longer than 1518 octets (excluding framing bits,
            but including FCS octets) and were otherwise
            well formed."
    ::= { wwpLeosPortTotalStatsEntry 7 }

 wwpLeosPortTotalStatsFragmentPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were less
            than 64 octets in length (excluding framing bits but
            including FCS octets) and had either a bad Frame
            Check Sequence (FCS) with an integral number of
            octets (FCS Error) or a bad FCS with a non-integral
            number of octets (Alignment Error)."
    ::= { wwpLeosPortTotalStatsEntry 8 }


 wwpLeosPortTotalStatsJabberPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were
            longer than 1518 octets (excluding framing bits,
            but including FCS octets), and had either a bad
            Frame Check Sequence (FCS) with an integral number
            of octets (FCS Error) or a bad FCS with a
            non-integral number of octets (Alignment Error)."
    ::= { wwpLeosPortTotalStatsEntry 9 }
        
        
 wwpLeosPortTotalStats64BytePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were 64 octets in length
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortTotalStatsEntry 10 }

        
 wwpLeosPortTotalStats65To127BytePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            65 and 127 octets in length inclusive
            (excluding framing bits but including FCS octets)." 
    ::= { wwpLeosPortTotalStatsEntry 11 }
        
 wwpLeosPortTotalStats128To255BytePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            128 and 255 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortTotalStatsEntry 12 }
        
 wwpLeosPortTotalStats256To511BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            256 and 511 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortTotalStatsEntry 13 }
        
 wwpLeosPortTotalStats512To1023BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            512 and 1023 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortTotalStatsEntry 14 }
        
 wwpLeosPortTotalStats1024To1518BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            1024 and 1518 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortTotalStatsEntry 15 }
        
 wwpLeosPortTotalStatsTxBytes OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The number of Octets transmitted for this port."
    ::= { wwpLeosPortTotalStatsEntry 16 }
        
 wwpLeosPortTotalStatsTxTBytes OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      deprecated
    DESCRIPTION
            "The total number of Octets transmitted for this port."
    ::= { wwpLeosPortTotalStatsEntry 17 }

 wwpLeosPortTotalStatsTxPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The total number of packets transmitted for this port."
    ::= { wwpLeosPortTotalStatsEntry 18 }
        
        
 wwpLeosPortTotalStatsTxExDeferPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit excessive defer packet count for a port."
    ::= { wwpLeosPortTotalStatsEntry 19 }
        
 wwpLeosPortTotalStatsTxGiantPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit too big packet count for a port."
    ::= { wwpLeosPortTotalStatsEntry 20 }
        
 wwpLeosPortTotalStatsTxUnderRunPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit underrun packet count for a port."
    ::= { wwpLeosPortTotalStatsEntry 21 }
        
 wwpLeosPortTotalStatsTxCrcErrorPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit CRC error packet count for a port."
    ::= { wwpLeosPortTotalStatsEntry 22 }
        
 wwpLeosPortTotalStatsTxLCheckErrorPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit length check error packet count for a port."
    ::= { wwpLeosPortTotalStatsEntry 23 }
        
 wwpLeosPortTotalStatsTxLOutRangePkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit length out of range packet count for a port."
    ::= { wwpLeosPortTotalStatsEntry 24 }
        
 wwpLeosPortTotalStatsTxLateCollPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit late collision packet count for a port."
    ::= { wwpLeosPortTotalStatsEntry 25 }
        
 wwpLeosPortTotalStatsTxExCollPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit excessive collision packet count for a port."
    ::= { wwpLeosPortTotalStatsEntry 26 }
        
 wwpLeosPortTotalStatsTxSingleCollPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit single collision packet count for a port."
    ::= { wwpLeosPortTotalStatsEntry 27 }
        
 wwpLeosPortTotalStatsTxCollPkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit collision packet count for the port."
    ::= { wwpLeosPortTotalStatsEntry 28 }
 
 wwpLeosPortTotalStatsTxPausePkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit pause packets for the port."
    ::= { wwpLeosPortTotalStatsEntry 29 }

 wwpLeosPortTotalStatsTxMcastPkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit multicast packets for the port."
    ::= { wwpLeosPortTotalStatsEntry 30 }

 wwpLeosPortTotalStatsTxBcastPkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit broadcast packets for the port."
    ::= { wwpLeosPortTotalStatsEntry 31 }
    
 wwpLeosPortTotalStatsPortReset OBJECT-TYPE
    SYNTAX          INTEGER {
                        none(0),
                                reset(1)
                    } 
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
            "Setting this object will reset the stats of given port.
             Doing read on this object will always return 'none'"
    ::= { wwpLeosPortTotalStatsEntry 32 }
 
 wwpLeosPortTotalStatsRxMcastPkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total number of multicast packets received for the given port."
    ::= { wwpLeosPortTotalStatsEntry 33 }
 
 wwpLeosPortTotalStatsRxPausePkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total receive pause packets for the port."
    ::= { wwpLeosPortTotalStatsEntry 34 }
        
 wwpLeosPortTotalStats1519To2047BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            1519 and 2047 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 35 }
        
 wwpLeosPortTotalStats2048To4095BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            2048 and 4095 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 36 }
        
 wwpLeosPortTotalStats4096To9216BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            4096 and 9216 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 37 }
        
 wwpLeosPortTotalStatsTxDeferPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The total transmit single deferral packet count for a port.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 38 }
        
 wwpLeosPortTotalStatsTx64BytePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were 64 octets in length
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 39 }
        
 wwpLeosPortTotalStatsTx65To127BytePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            65 and 127 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x" 
    ::= { wwpLeosPortTotalStatsEntry 40 }
        
 wwpLeosPortTotalStatsTx128To255BytePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            128 and 255 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 41 }
        
 wwpLeosPortTotalStatsTx256To511BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            256 and 511 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 42 }
        
 wwpLeosPortTotalStatsTx512To1023BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            512 and 1023 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 43 }
        
 wwpLeosPortTotalStatsTx1024To1518BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            1024 and 1518 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 44 }
        
 wwpLeosPortTotalStatsTx1519To2047BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            1519 and 2047 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 45 }
        
 wwpLeosPortTotalStatsTx2048To4095BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            2048 and 4095 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 46 }
        
 wwpLeosPortTotalStatsTx4096To9216BytePkts OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            4096 and 9216 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 47 }
        
 wwpLeosPortTotalStatsRxFpgaDropPkts OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total number of dropped packets on a port when 
             traffic profiles are enabled on the port.(311v only)"
    ::= { wwpLeosPortTotalStatsEntry 48 }
  
 wwpLeosPortTotalStatsPortLinkUp OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total number of port link up events on the port."
    ::= { wwpLeosPortTotalStatsEntry 49 }

 wwpLeosPortTotalStatsPortLinkDown OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total number of port link down events on the port."
    ::= { wwpLeosPortTotalStatsEntry 50 }
    
 wwpLeosPortTotalStatsPortLinkFlap OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total number of port link flap events on the port."
    ::= { wwpLeosPortTotalStatsEntry 51 }
       
 wwpLeosPortTotalStatsRxUcastPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of Unicast packets received by this port.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 52 }
        
 wwpLeosPortTotalStatsTxUcastPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of Unicast packets transmitted by this port.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 53 }
        
 wwpLeosPortTotalStatsRxDropPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of discarded received frames for this port."
    ::= { wwpLeosPortTotalStatsEntry 54 }
        
 wwpLeosPortTotalStatsRxDiscardPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of discarded received frames for this port
             including IPv6 L3, L3 IP Header and runt discards."
    ::= { wwpLeosPortTotalStatsEntry 55 }
        
 wwpLeosPortTotalStatsRxLOutRangePkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of frames received by this port that exceeded
            the maximum permitted frame size.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalStatsEntry 56 }
    
 wwpLeosPortTotalStatsRxFpgaBufferDropPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "number of frames dropped because the FPGA RX buffer was full
				Only supported on the 311V"
    ::= { wwpLeosPortTotalStatsEntry 57 }
    
 wwpLeosPortTotalStatsTxFpgaBufferDropPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "number of frames dropped because the FPGA TX buffer was full
				Only supported on the 311V"
    ::= { wwpLeosPortTotalStatsEntry 58 }
    
 wwpLeosPortTotalStatsFpgaVlanPriFilterDropPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "number of frames dropped by the transmit VLAN Priority Filter
				Only supported on the 311V"
    ::= { wwpLeosPortTotalStatsEntry 59 }
    
 wwpLeosPortTotalStatsFpgaRxErrorPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "Number of frames dropped by the FPGA because of receive errors.
            Only supported on the 311V"
    ::= { wwpLeosPortTotalStatsEntry 60 }
    
 wwpLeosPortTotalStatsFpgaRxCrcErrorPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "Number of frames dropped by the FPGA because of CRC errors.
            Only supported on the 311V"
    ::= { wwpLeosPortTotalStatsEntry 61 }
    
 wwpLeosPortTotalStatsFpgaRxIpCrcErrorPkts OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "Number of frames dropped by the FPGA because of IP Checksum errors
             Only supported on the 311V"
    ::= { wwpLeosPortTotalStatsEntry 62 }
        

wwpLeosPortHCStatsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosPortHCStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "The table specifying the 64 bit statistics for the ports."
     ::= { wwpLeosPortStats 4 }

 wwpLeosPortHCStatsEntry OBJECT-TYPE
     SYNTAX       WwpLeosPortHCStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "An entry in the port stats table."
     INDEX { wwpLeosPortHCStatsPortId }
     ::= { wwpLeosPortHCStatsTable 1 }



                
 WwpLeosPortHCStatsEntry ::= SEQUENCE { 
     wwpLeosPortHCStatsPortId                INTEGER,
     wwpLeosPortHCStatsRxBytes               Counter64,
     wwpLeosPortHCStatsRxPkts                Counter64,
     wwpLeosPortHCStatsRxCrcErrorPkts        Counter64,
     wwpLeosPortHCStatsRxBcastPkts           Counter64,
     wwpLeosPortHCStatsUndersizePkts         Counter64,
     wwpLeosPortHCStatsOversizePkts          Counter64,
     wwpLeosPortHCStatsFragmentPkts          Counter64,
     wwpLeosPortHCStatsJabberPkts            Counter64,
     wwpLeosPortHCStats64BytePkts            Counter64,
     wwpLeosPortHCStats65To127BytePkts       Counter64,
     wwpLeosPortHCStats128To255BytePkts      Counter64,
     wwpLeosPortHCStats256To511BytePkts      Counter64,
     wwpLeosPortHCStats512To1023BytePkts     Counter64,
     wwpLeosPortHCStats1024To1518BytePkts    Counter64,
     wwpLeosPortHCStatsTxBytes               Counter64,
     wwpLeosPortHCStatsTxTBytes              Counter64,
     wwpLeosPortHCStatsTxPkts                Counter64,
     wwpLeosPortHCStatsTxExDeferPkts         Counter64,
     wwpLeosPortHCStatsTxGiantPkts           Counter64,
     wwpLeosPortHCStatsTxUnderRunPkts        Counter64,
     wwpLeosPortHCStatsTxCrcErrorPkts        Counter64,
     wwpLeosPortHCStatsTxLCheckErrorPkts     Counter64,
     wwpLeosPortHCStatsTxLOutRangePkts       Counter64,
     wwpLeosPortHCStatsTxLateCollPkts        Counter64,
     wwpLeosPortHCStatsTxExCollPkts          Counter64,
     wwpLeosPortHCStatsTxSingleCollPkts      Counter64,
     wwpLeosPortHCStatsTxCollPkts            Counter64,
     wwpLeosPortHCStatsTxPausePkts           Counter64,
     wwpLeosPortHCStatsTxMcastPkts           Counter64,
     wwpLeosPortHCStatsTxBcastPkts           Counter64,
     wwpLeosPortHCStatsPortReset                     INTEGER,
     wwpLeosPortHCStatsRxMcastPkts                   Counter64,
     wwpLeosPortHCStatsRxPausePkts           Counter64,
     wwpLeosPortHCStats1519To2047BytePkts      Counter64,
     wwpLeosPortHCStats2048To4095BytePkts     Counter64,
     wwpLeosPortHCStats4096To9216BytePkts    Counter64,
     wwpLeosPortHCStatsTxDeferPkts         Counter64,
     wwpLeosPortHCStatsTx64BytePkts            Counter64,
     wwpLeosPortHCStatsTx65To127BytePkts       Counter64,
     wwpLeosPortHCStatsTx128To255BytePkts      Counter64,
     wwpLeosPortHCStatsTx256To511BytePkts      Counter64,
     wwpLeosPortHCStatsTx512To1023BytePkts     Counter64,
     wwpLeosPortHCStatsTx1024To1518BytePkts    Counter64,
     wwpLeosPortHCStatsTx1519To2047BytePkts      Counter64,
     wwpLeosPortHCStatsTx2048To4095BytePkts     Counter64,
     wwpLeosPortHCStatsTx4096To9216BytePkts    Counter64,
     wwpLeosPortHCStatsRxUcastPkts           Counter64,
     wwpLeosPortHCStatsTxUcastPkts           Counter64,
     wwpLeosPortHCStatsRxDropPkts      Counter64,
     wwpLeosPortHCStatsRxDiscardPkts      Counter64,
     wwpLeosPortHCStatsRxLOutRangePkts      Counter64
 }

 wwpLeosPortHCStatsPortId OBJECT-TYPE
    SYNTAX       INTEGER (1..65535)
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The Id of the port for which this entry
            contains the stats."
    ::= { wwpLeosPortHCStatsEntry 1 }

 wwpLeosPortHCStatsRxBytes OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of bytes received by this port."
    ::= { wwpLeosPortHCStatsEntry 2 }

 wwpLeosPortHCStatsRxPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of packets received by this port."
    ::= { wwpLeosPortHCStatsEntry 3 }
        
 wwpLeosPortHCStatsRxCrcErrorPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of packets received with CRC errors by this port."
    ::= { wwpLeosPortHCStatsEntry 4 }

 wwpLeosPortHCStatsRxBcastPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of Broadcast packets received by this port."
    ::= { wwpLeosPortHCStatsEntry 5 }

 wwpLeosPortHCStatsUndersizePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were
            less than 64 octets long (excluding framing bits,
            but including FCS octets) and were otherwise well
            formed."
    ::= { wwpLeosPortHCStatsEntry 6 }

 wwpLeosPortHCStatsOversizePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were
            longer than 1518 octets (excluding framing bits,
            but including FCS octets) and were otherwise
            well formed."
    ::= { wwpLeosPortHCStatsEntry 7 }

 wwpLeosPortHCStatsFragmentPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were less
            than 64 octets in length (excluding framing bits but
            including FCS octets) and had either a bad Frame
            Check Sequence (FCS) with an integral number of
            octets (FCS Error) or a bad FCS with a non-integral
            number of octets (Alignment Error)."
    ::= { wwpLeosPortHCStatsEntry 8 }


 wwpLeosPortHCStatsJabberPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were
            longer than 1518 octets (excluding framing bits,
            but including FCS octets), and had either a bad
            Frame Check Sequence (FCS) with an integral number
            of octets (FCS Error) or a bad FCS with a
            non-integral number of octets (Alignment Error)."
    ::= { wwpLeosPortHCStatsEntry 9 }
        
        
 wwpLeosPortHCStats64BytePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were 64 octets in length
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortHCStatsEntry 10 }

        
 wwpLeosPortHCStats65To127BytePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            65 and 127 octets in length inclusive
            (excluding framing bits but including FCS octets)." 
    ::= { wwpLeosPortHCStatsEntry 11 }
        
 wwpLeosPortHCStats128To255BytePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            128 and 255 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortHCStatsEntry 12 }
        
 wwpLeosPortHCStats256To511BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            256 and 511 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortHCStatsEntry 13 }
        
 wwpLeosPortHCStats512To1023BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            512 and 1023 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortHCStatsEntry 14 }
        
 wwpLeosPortHCStats1024To1518BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            1024 and 1518 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortHCStatsEntry 15 }
        
 wwpLeosPortHCStatsTxBytes OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The number of Octets transmitted for this port."
    ::= { wwpLeosPortHCStatsEntry 16 }
        
 wwpLeosPortHCStatsTxTBytes OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      deprecated
    DESCRIPTION
            "The total number of Octets transmitted for this port."
    ::= { wwpLeosPortHCStatsEntry 17 }

 wwpLeosPortHCStatsTxPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The total number of packets transmitted for this port."
    ::= { wwpLeosPortHCStatsEntry 18 }
        
        
 wwpLeosPortHCStatsTxExDeferPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit excessive defer packet count for a port."
    ::= { wwpLeosPortHCStatsEntry 19 }
        
 wwpLeosPortHCStatsTxGiantPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit too big packet count for a port."
    ::= { wwpLeosPortHCStatsEntry 20 }
        
 wwpLeosPortHCStatsTxUnderRunPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit underrun packet count for a port."
    ::= { wwpLeosPortHCStatsEntry 21 }
        
 wwpLeosPortHCStatsTxCrcErrorPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit CRC error packet count for a port."
    ::= { wwpLeosPortHCStatsEntry 22 }
        
 wwpLeosPortHCStatsTxLCheckErrorPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit length check error packet count for a port."
    ::= { wwpLeosPortHCStatsEntry 23 }
        
 wwpLeosPortHCStatsTxLOutRangePkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit length out of range packet count for a port."
    ::= { wwpLeosPortHCStatsEntry 24 }
        
 wwpLeosPortHCStatsTxLateCollPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit late collision packet count for a port."
    ::= { wwpLeosPortHCStatsEntry 25 }
        
 wwpLeosPortHCStatsTxExCollPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit excessive collision packet count for a port."
    ::= { wwpLeosPortHCStatsEntry 26 }
        
 wwpLeosPortHCStatsTxSingleCollPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit single collision packet count for a port."
    ::= { wwpLeosPortHCStatsEntry 27 }
        
 wwpLeosPortHCStatsTxCollPkts OBJECT-TYPE
    SYNTAX       Counter64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit collision packet count for the port."
    ::= { wwpLeosPortHCStatsEntry 28 }
 
 wwpLeosPortHCStatsTxPausePkts OBJECT-TYPE
    SYNTAX       Counter64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit pause packets for the port."
    ::= { wwpLeosPortHCStatsEntry 29 }

 wwpLeosPortHCStatsTxMcastPkts OBJECT-TYPE
    SYNTAX       Counter64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit multicast packets for the port."
    ::= { wwpLeosPortHCStatsEntry 30 }

 wwpLeosPortHCStatsTxBcastPkts OBJECT-TYPE
    SYNTAX       Counter64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit broadcast packets for the port."
    ::= { wwpLeosPortHCStatsEntry 31 }
    
 wwpLeosPortHCStatsPortReset OBJECT-TYPE
    SYNTAX          INTEGER {
                        none(0),
                                reset(1)
                    } 
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
            "Setting this object will reset the stats of given port.
             Doing read on this object will always return 'none'"
    ::= { wwpLeosPortHCStatsEntry 32 }
 
 wwpLeosPortHCStatsRxMcastPkts OBJECT-TYPE
    SYNTAX       Counter64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total number of multicast packets received for the given port."
    ::= { wwpLeosPortHCStatsEntry 33 }
 
 wwpLeosPortHCStatsRxPausePkts OBJECT-TYPE
    SYNTAX       Counter64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The receive pause packets for the port."
    ::= { wwpLeosPortHCStatsEntry 34 }
        
 wwpLeosPortHCStats1519To2047BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            1519 and 2047 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 35 }
        
 wwpLeosPortHCStats2048To4095BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            2048 and 4095 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 36 }
        
 wwpLeosPortHCStats4096To9216BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            4096 and 9216 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 37 }
        
 wwpLeosPortHCStatsTxDeferPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit single deferral packet count for a port.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 38 }
        
 wwpLeosPortHCStatsTx64BytePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were 64 octets in length
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 39 }
        
 wwpLeosPortHCStatsTx65To127BytePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            65 and 127 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x" 
    ::= { wwpLeosPortHCStatsEntry 40 }
        
 wwpLeosPortHCStatsTx128To255BytePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            128 and 255 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 41 }
        
 wwpLeosPortHCStatsTx256To511BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            256 and 511 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 42 }
        
 wwpLeosPortHCStatsTx512To1023BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            512 and 1023 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 43 }
        
 wwpLeosPortHCStatsTx1024To1518BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            1024 and 1518 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 44 }
        
 wwpLeosPortHCStatsTx1519To2047BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            1519 and 2047 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 45 }
        
 wwpLeosPortHCStatsTx2048To4095BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            2048 and 4095 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 46 }
        
 wwpLeosPortHCStatsTx4096To9216BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            4096 and 9216 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 47 }  
    
 wwpLeosPortHCStatsRxUcastPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of Unicast packets received by this port."
    ::= { wwpLeosPortHCStatsEntry 48 }
        
 wwpLeosPortHCStatsTxUcastPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of Unicast packets transmitted by this port.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 49 }
        
  wwpLeosPortHCStatsRxDropPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of discarded received frames for this port."
    ::= { wwpLeosPortHCStatsEntry 50 }
        
  wwpLeosPortHCStatsRxDiscardPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of discarded received frames for this port including
            IPv6 L3, L3 IP Header and runt discards."
    ::= { wwpLeosPortHCStatsEntry 51 }
        
  wwpLeosPortHCStatsRxLOutRangePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of frames received by this port that exceeded
            the maximum permitted frame size.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortHCStatsEntry 52 }
        
--
-- Total Port stats
--
 wwpLeosPortTotalHCStatsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosPortTotalHCStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "The table specifying the 64 bit statistics for the ports."
     ::= { wwpLeosPortStats 5 }  
 
 wwpLeosPortTotalHCStatsEntry OBJECT-TYPE
     SYNTAX       WwpLeosPortTotalHCStatsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "An entry in the port stats table."
     INDEX { wwpLeosPortTotalHCStatsPortId }
     ::= { wwpLeosPortTotalHCStatsTable 1 }       
   
     WwpLeosPortTotalHCStatsEntry ::= SEQUENCE { 
     wwpLeosPortTotalHCStatsPortId                INTEGER,
     wwpLeosPortTotalHCStatsRxBytes               Counter64,
     wwpLeosPortTotalHCStatsRxPkts                Counter64,
     wwpLeosPortTotalHCStatsRxCrcErrorPkts        Counter64,
     wwpLeosPortTotalHCStatsRxBcastPkts           Counter64,
     wwpLeosPortTotalHCStatsUndersizePkts         Counter64,
     wwpLeosPortTotalHCStatsOversizePkts          Counter64,
     wwpLeosPortTotalHCStatsFragmentPkts          Counter64,
     wwpLeosPortTotalHCStatsJabberPkts            Counter64,
     wwpLeosPortTotalHCStats64BytePkts            Counter64,
     wwpLeosPortTotalHCStats65To127BytePkts       Counter64,
     wwpLeosPortTotalHCStats128To255BytePkts      Counter64,
     wwpLeosPortTotalHCStats256To511BytePkts      Counter64,
     wwpLeosPortTotalHCStats512To1023BytePkts     Counter64,
     wwpLeosPortTotalHCStats1024To1518BytePkts    Counter64,
     wwpLeosPortTotalHCStatsTxBytes               Counter64,
     wwpLeosPortTotalHCStatsTxTBytes              Counter64,
     wwpLeosPortTotalHCStatsTxPkts                Counter64,
     wwpLeosPortTotalHCStatsTxExDeferPkts         Counter64,
     wwpLeosPortTotalHCStatsTxGiantPkts           Counter64,
     wwpLeosPortTotalHCStatsTxUnderRunPkts        Counter64,
     wwpLeosPortTotalHCStatsTxCrcErrorPkts        Counter64,
     wwpLeosPortTotalHCStatsTxLCheckErrorPkts     Counter64,
     wwpLeosPortTotalHCStatsTxLOutRangePkts       Counter64,
     wwpLeosPortTotalHCStatsTxLateCollPkts        Counter64,
     wwpLeosPortTotalHCStatsTxExCollPkts          Counter64,
     wwpLeosPortTotalHCStatsTxSingleCollPkts      Counter64,
     wwpLeosPortTotalHCStatsTxCollPkts            Counter64,
     wwpLeosPortTotalHCStatsTxPausePkts           Counter64,
     wwpLeosPortTotalHCStatsTxMcastPkts           Counter64,
     wwpLeosPortTotalHCStatsTxBcastPkts           Counter64,
     wwpLeosPortTotalHCStatsPortReset                     INTEGER,
     wwpLeosPortTotalHCStatsRxMcastPkts                   Counter64,
     wwpLeosPortTotalHCStatsRxPausePkts           Counter64,
     wwpLeosPortTotalHCStats1519To2047BytePkts      Counter64,
     wwpLeosPortTotalHCStats2048To4095BytePkts     Counter64,
     wwpLeosPortTotalHCStats4096To9216BytePkts    Counter64,
     wwpLeosPortTotalHCStatsTxDeferPkts         Counter64,
     wwpLeosPortTotalHCStatsTx64BytePkts            Counter64,
     wwpLeosPortTotalHCStatsTx65To127BytePkts       Counter64,
     wwpLeosPortTotalHCStatsTx128To255BytePkts      Counter64,
     wwpLeosPortTotalHCStatsTx256To511BytePkts      Counter64,
     wwpLeosPortTotalHCStatsTx512To1023BytePkts     Counter64,
     wwpLeosPortTotalHCStatsTx1024To1518BytePkts    Counter64,
     wwpLeosPortTotalHCStatsTx1519To2047BytePkts      Counter64,
     wwpLeosPortTotalHCStatsTx2048To4095BytePkts     Counter64,
     wwpLeosPortTotalHCStatsTx4096To9216BytePkts    Counter64,
     wwpLeosPortTotalHCStatsRxUcastPkts           Counter64,
     wwpLeosPortTotalHCStatsTxUcastPkts           Counter64,
     wwpLeosPortTotalHCStatsRxDropPkts      Counter64,
     wwpLeosPortTotalHCStatsRxDiscardPkts           Counter64,
     wwpLeosPortTotalHCStatsRxLOutRangePkts           Counter64
 }

 wwpLeosPortTotalHCStatsPortId OBJECT-TYPE
    SYNTAX       INTEGER (1..65535)
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The Id of the port for which this entry
            contains the stats."
    ::= { wwpLeosPortTotalHCStatsEntry 1 }

 wwpLeosPortTotalHCStatsRxBytes OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of bytes received by this port."
    ::= { wwpLeosPortTotalHCStatsEntry 2 }

 wwpLeosPortTotalHCStatsRxPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of packets received by this port."
    ::= { wwpLeosPortTotalHCStatsEntry 3 }
        
 wwpLeosPortTotalHCStatsRxCrcErrorPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of packets received with CRC errors by this port."
    ::= { wwpLeosPortTotalHCStatsEntry 4 }

 wwpLeosPortTotalHCStatsRxBcastPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The number of Broadcast packets received by this port."
    ::= { wwpLeosPortTotalHCStatsEntry 5 }

 wwpLeosPortTotalHCStatsUndersizePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were
            less than 64 octets long (excluding framing bits,
            but including FCS octets) and were otherwise well
            formed."
    ::= { wwpLeosPortTotalHCStatsEntry 6 }

 wwpLeosPortTotalHCStatsOversizePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were
            longer than 1518 octets (excluding framing bits,
            but including FCS octets) and were otherwise
            well formed."
    ::= { wwpLeosPortTotalHCStatsEntry 7 }

 wwpLeosPortTotalHCStatsFragmentPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were less
            than 64 octets in length (excluding framing bits but
            including FCS octets) and had either a bad Frame
            Check Sequence (FCS) with an integral number of
            octets (FCS Error) or a bad FCS with a non-integral
            number of octets (Alignment Error)."
    ::= { wwpLeosPortTotalHCStatsEntry 8 }


 wwpLeosPortTotalHCStatsJabberPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets received that were
            longer than 1518 octets (excluding framing bits,
            but including FCS octets), and had either a bad
            Frame Check Sequence (FCS) with an integral number
            of octets (FCS Error) or a bad FCS with a
            non-integral number of octets (Alignment Error)."
    ::= { wwpLeosPortTotalHCStatsEntry 9 }
        
        
 wwpLeosPortTotalHCStats64BytePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were 64 octets in length
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortTotalHCStatsEntry 10 }

        
 wwpLeosPortTotalHCStats65To127BytePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            65 and 127 octets in length inclusive
            (excluding framing bits but including FCS octets)." 
    ::= { wwpLeosPortTotalHCStatsEntry 11 }
        
 wwpLeosPortTotalHCStats128To255BytePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            128 and 255 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortTotalHCStatsEntry 12 }
        
 wwpLeosPortTotalHCStats256To511BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            256 and 511 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortTotalHCStatsEntry 13 }
        
 wwpLeosPortTotalHCStats512To1023BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            512 and 1023 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortTotalHCStatsEntry 14 }
        
 wwpLeosPortTotalHCStats1024To1518BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            1024 and 1518 octets in length inclusive
            (excluding framing bits but including FCS octets)."
    ::= { wwpLeosPortTotalHCStatsEntry 15 }
        
 wwpLeosPortTotalHCStatsTxBytes OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The number of Octets transmitted for this port."
    ::= { wwpLeosPortTotalHCStatsEntry 16 }
        
 wwpLeosPortTotalHCStatsTxTBytes OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      deprecated
    DESCRIPTION
            "The total number of Octets transmitted for this port."
    ::= { wwpLeosPortTotalHCStatsEntry 17 }

 wwpLeosPortTotalHCStatsTxPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The total number of packets transmitted for this port."
    ::= { wwpLeosPortTotalHCStatsEntry 18 }
        
        
 wwpLeosPortTotalHCStatsTxExDeferPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit excessive defer packet count for a port."
    ::= { wwpLeosPortTotalHCStatsEntry 19 }
        
 wwpLeosPortTotalHCStatsTxGiantPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit too big packet count for a port."
    ::= { wwpLeosPortTotalHCStatsEntry 20 }
        
 wwpLeosPortTotalHCStatsTxUnderRunPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit underrun packet count for a port."
    ::= { wwpLeosPortTotalHCStatsEntry 21 }
        
 wwpLeosPortTotalHCStatsTxCrcErrorPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The transmit CRC error packet count for a port."
    ::= { wwpLeosPortTotalHCStatsEntry 22 }
        
 wwpLeosPortTotalHCStatsTxLCheckErrorPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit length check error packet count for a port."
    ::= { wwpLeosPortTotalHCStatsEntry 23 }
        
 wwpLeosPortTotalHCStatsTxLOutRangePkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit length out of range packet count for a port."
    ::= { wwpLeosPortTotalHCStatsEntry 24 }
        
 wwpLeosPortTotalHCStatsTxLateCollPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit late collision packet count for a port."
    ::= { wwpLeosPortTotalHCStatsEntry 25 }
        
 wwpLeosPortTotalHCStatsTxExCollPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit excessive collision packet count for a port."
    ::= { wwpLeosPortTotalHCStatsEntry 26 }
        
 wwpLeosPortTotalHCStatsTxSingleCollPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The transmit single collision packet count for a port."
    ::= { wwpLeosPortTotalHCStatsEntry 27 }
        
 wwpLeosPortTotalHCStatsTxCollPkts OBJECT-TYPE
    SYNTAX       Counter64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit collision packet count for the port."
    ::= { wwpLeosPortTotalHCStatsEntry 28 }
 
 wwpLeosPortTotalHCStatsTxPausePkts OBJECT-TYPE
    SYNTAX       Counter64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit pause packets for the port."
    ::= { wwpLeosPortTotalHCStatsEntry 29 }

 wwpLeosPortTotalHCStatsTxMcastPkts OBJECT-TYPE
    SYNTAX       Counter64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit multicast packets for the port."
    ::= { wwpLeosPortTotalHCStatsEntry 30 }

 wwpLeosPortTotalHCStatsTxBcastPkts OBJECT-TYPE
    SYNTAX       Counter64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The transmit broadcast packets for the port."
    ::= { wwpLeosPortTotalHCStatsEntry 31 }
    
 wwpLeosPortTotalHCStatsPortReset OBJECT-TYPE
    SYNTAX          INTEGER {
                        none(0),
                                reset(1)
                    } 
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
            "Setting this object will reset the stats of given port.
             Doing read on this object will always return 'none'"
    ::= { wwpLeosPortTotalHCStatsEntry 32 }
 
 wwpLeosPortTotalHCStatsRxMcastPkts OBJECT-TYPE
    SYNTAX       Counter64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total number of multicast packets received for the given port."
    ::= { wwpLeosPortTotalHCStatsEntry 33 }
 
 wwpLeosPortTotalHCStatsRxPausePkts OBJECT-TYPE
    SYNTAX       Counter64
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
            "The total receive pause packets for the port."
    ::= { wwpLeosPortTotalHCStatsEntry 34 }
        
 wwpLeosPortTotalHCStats1519To2047BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            1519 and 2047 octets in length inclusive
            (excluding framing bits but including FCS octets)
				Not Supported in leos 4.x.
				"
    ::= { wwpLeosPortTotalHCStatsEntry 35 }
        
 wwpLeosPortTotalHCStats2048To4095BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            2048 and 4095 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 36 }
        
 wwpLeosPortTotalHCStats4096To9216BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) received that were between
            4096 and 9216 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 37 }
        
 wwpLeosPortTotalHCStatsTxDeferPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only 
    STATUS      current
    DESCRIPTION
            "The total transmit single deferral packet count for a port.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 38 }
        
 wwpLeosPortTotalHCStatsTx64BytePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were 64 octets in length
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 39 }
        
 wwpLeosPortTotalHCStatsTx65To127BytePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            65 and 127 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x" 
    ::= { wwpLeosPortTotalHCStatsEntry 40 }
        
 wwpLeosPortTotalHCStatsTx128To255BytePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            128 and 255 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 41 }
        
 wwpLeosPortTotalHCStatsTx256To511BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            256 and 511 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 42 }
        
 wwpLeosPortTotalHCStatsTx512To1023BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            512 and 1023 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 43 }
        
 wwpLeosPortTotalHCStatsTx1024To1518BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            1024 and 1518 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 44 }
        
 wwpLeosPortTotalHCStatsTx1519To2047BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            1519 and 2047 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 45 }
        
 wwpLeosPortTotalHCStatsTx2048To4095BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            2048 and 4095 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 46 }
        
 wwpLeosPortTotalHCStatsTx4096To9216BytePkts OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The total number of packets (including bad
            packets) transmitted that were between
            4096 and 9216 octets in length inclusive
            (excluding framing bits but including FCS octets).
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 47 } 
    
 wwpLeosPortTotalHCStatsRxUcastPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of Unicast packets received by this port.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 48 }
        
 wwpLeosPortTotalHCStatsTxUcastPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of Unicast packets transmitted by this port.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 49 }
        
 wwpLeosPortTotalHCStatsRxDropPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of discarded received frames for this port."
    ::= { wwpLeosPortTotalHCStatsEntry 50 }
        
 wwpLeosPortTotalHCStatsRxDiscardPkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of discarded received frames for this port
             including IPv6 L3, L3 IP Header and runt discards."
    ::= { wwpLeosPortTotalHCStatsEntry 51 }
        
 wwpLeosPortTotalHCStatsRxLOutRangePkts OBJECT-TYPE
    SYNTAX        Counter64
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
            "The total number of frames received by this port that exceeded
            the maximum permitted frame size.
				Not Supported in leos 4.x"
    ::= { wwpLeosPortTotalHCStatsEntry 52 }
 

        
END

