| AnyConnect Secure Mobility Client 5.1.2.42

- Main Page
- Related Pages
- Classes
- Files

- File List
- File Members

# include/VPNStats.h

    00001 /**************************************************************************
    00002 *       Copyright (c) 2006, Cisco Systems, All Rights Reserved
    00003 ***************************************************************************
    00004 *
    00005 *  File:    VpnStats.h
    00006 *  Date:    08/2006
    00007 *
    00008 ***************************************************************************
    00009 *
    00010 *   VPN Statistics class implementation for the Client API.
    00011 *
    00012 ***************************************************************************/
    00013 #ifndef _VPNSTATS_
    00014 #define _VPNSTATS_
    00015
    00016 #include "VPNStatsBase.h"
    00017
    00018
    00019 /**
    00020  * Use this class to retrieve statistics related to the tunnel and
    00021  * protocol being used.
    00022  *
    00023  * The class has two uses: it provides a consistent localized label
    00024  * definition mechanism and it uses this label mechanism to do
    00025  * values lookups.
    00026  *
    00027  * Labels are automatically localized at application startup.
    00028  * See the AnyConnect Release notes for additional information on localization.
    00029  *
    00030  * To retrieve a value for one of the labels, use the method getStatValue().
    00031  * For example, to get Time connected use: getStatValue(VPNStats::TimeConnected)
    00032  */
    00033
    00034
    00035 class VPN_VPNAPI VPNStats : public VPNStatsBase
    00036 {
    00037     public:
    00038
    00039         /**
    00040          * Get a list of Secure Routes.
    00041          * Method returns a list of RouteInfo pointers
    00042          */
    00043         const std::list<RouteInfo *> &getSecureRoutes();
    00044
    00045         /**
    00046          * Get a list of Nonsecure Routes.
    00047          * Method returns a list of RouteInfo pointers
    00048          */
    00049         const std::list<RouteInfo *> &getNonsecureRoutes();
    00050
    00051         /**
    00052          * Get a list of protocol Info objects.
    00053          * Method returns a list of ProtocolInfo pointers
    00054          */
    00055         const std::list<ProtocolInfo *> &getProtocolInfo();
    00056
    00057         /**
    00058         * Get a list of firewall Info objects.
    00059         * Method returns a list of FirewallInfo pointers
    00060         */
    00061         const std::list<FirewallInfo *> &getFirewallInfo();
    00062
    00063         /**
    00064          * Method used to retrieve statistics by name.
    00065          */
    00066         const tstring &getStatValue(tstring &label);
    00067
    00068         /**
    00069          * Alias for getStatValue.
    00070          */
    00071         const tstring &getValue(tstring &label) { return getStatValue(label); }
    00072
    00073         /**
    00074          * Return a translated stats label.  As an example, passing
    00075          * VPNStats::State will return a translated label for State text.
    00076          *
    00077          * NOTE: Do not use this translated label to retrieve stats
    00078          *       values; it is meant only as a label translation mechanism.
    00079          */
    00080         static tstring getTranslatedLabel(tstring &label);
    00081
    00082         //
    00083         // These static localized strings can be used in conjunction with the
    00084         // getStatValue method to retrieve VPN statisitics.
    00085         //
    00086         static tstring State;                           /**< Current state (see ::VPNState) of
    00087                                                              the VPN tunnel. */
    00088         static tstring MgmtTunState;                    /**< Current state (see ::VPNState) of
    00089                                                              the management VPN tunnel. */
    00090         static tstring TimeConnected;                   /**< Time hh:mm:ss the VPN tunnel has
    00091                                                              been active. */
    00092         static tstring SessionDisconnect;               /**< Estimate of time left until VPN session is
    00093                                                              disconnected due to ASA configured timeout. */
    00094
    00095         //
    00096         // Data byte/packet counts, does not include encap/encrypt overhead
    00097         //
    00098         static tstring BytesSent;       /**< Bytes sent to the remote network. */
    00099         static tstring BytesReceived;   /**< Bytes received from the remote
    00100                                              network. */
    00101         static tstring PacketsSent;     /**< Packets sent to the remote
    00102                                              network. */
    00103         static tstring PacketsReceived; /**< Packets received from the remote
    00104                                              network. */
    00105
    00106         //
    00107         // Control byte/packet count include size of DPD/Keepalive/etc
    00108         //
    00109         static tstring ControlBytesSent;        /**< Control bytes sent to the
    00110                                                      remote gateway. */
    00111         static tstring ControlBytesReceived;    /**< Control bytes received
    00112                                                      from the remote gateway. */
    00113         static tstring ControlPacketsSent;      /**< Control packets sent to the
    00114                                                      remote gateway. */
    00115         static tstring ControlPacketsReceived;  /**< Control packets received
    00116                                                      from the remote gateway. */
    00117
    00118         //
    00119         // Encrypted byte counts include both control and data, as well as
    00120         // encryption and encapsulation headers
    00121         //
    00122         static tstring EncryptedBytesSent;      /**< Encrypted bytes sent to the
    00123                                                      remote network. */
    00124         static tstring EncryptedBytesReceived;  /**< Encrypted bytes received
    00125                                                      from the remote network. */
    00126         static tstring EncryptedPacketsSent;    /**< Encrypted packets sent to the
    00127                                                      remote network. */
    00128         static tstring EncryptedPacketsReceived;/**< Encrypted packets received
    00129                                                      from the remote network. */
    00130
    00131         //
    00132         // Encrypted byte counts include both control and data (if protocol
    00133         // is TLS), as well as encryption and encapsulation headers
    00134         //
    00135         static tstring CompressedBytesSent;      /**< Compressed bytes sent
    00136                                                       to the remote network. */
    00137         static tstring CompressedBytesReceived;  /**< Compressed bytes received
    00138                                                       from the remote network. */
    00139         static tstring CompressedPacketsSent;    /**< Compressed packets sent
    00140                                                       to the remote network. */
    00141         static tstring CompressedPacketsReceived;/**< Compressed packets
    00142                                                       received from the remote
    00143                                                       network. */
    00144
    00145         static tstring InboundDiscarded;    /**< Incoming discarded bytes. */
    00146         static tstring OutboundDiscarded;   /**< Outgoing discarded bytes. */
    00147         static tstring InboundBypassed;     /**< Incoming skipped bytes. */
    00148         static tstring OutboundBypassed;    /**< Outgoing skipped bytes. */
    00149
    00150         static tstring ClientAddress;   /**< Client IPv4 address. */
    00151         static tstring ServerAddress;   /**< Remote gateway IP address. */
    00152         static tstring ClientAddressV6; /**< Client IPv6 address. */
    00153
    00154         static tstring ServerHostName;  /**< Host name of the remote gateway. */
    00155         static tstring ProxyAddress;    /**< Proxy server IP address. */
    00156         static tstring ProxyHostName;   /**< Proxy server host name. */
    00157         static tstring ProxyPort;       /**< Port used for communicating with
    00158                                              proxy server. */
    00159         static tstring TunnelingMode;   /**< Mode IPv4 traffic is being passed over
    00160                                              the tunnel.  Values are "Tunnel All Traffic",
    00161                                              "Split Include", "Split Exclude", "Application Tunnel",
    00162                                              "Drop All Traffic" or "Bypass All Traffic". */
    00163         static tstring TunnelingModeV6; /**< Mode IPv6 traffic is being passed over
    00164                                              the tunnel.  Values are "Tunnel All Traffic",
    00165                                              "Split Include", "Split Exclude",
    00166                                              "Drop All Traffic" or "Bypass All Traffic". */
    00167         static tstring DynamicTunnelExclusion; /**< Domain names dynamically excluded from tunneling */
    00168         static tstring DynamicTunnelInclusion; /**< Domain names dynamically added to tunnel */
    00169
    00170         static tstring Enabled;     /**< */
    00171         static tstring Disabled;    /**< */
    00172         static tstring Unconfirmed;     /**< Used for Secure Mobility Solution. If the
    00173                                              WSA is not reachable from the agent, it might be
    00174                                              due to private side proxy configuration. In such a case
    00175                                              report Unconfirmed to the UI */
    00176
    00177         static tstring FipsMode;        /**< FIPS mode (Federal security standard).
    00178                                              Values are "Enabled" or "Disabled" */
    00179
    00180         static tstring TrustedNetworkDetectionMode;  /** < Trusted Network Detection.
    00181                                                            Values are "Enabled" or "Disabled" */
    00182         static tstring AlwaysOnMode;    /**< Always On. Values are "Enabled" or
    00183                                              "Disabled" */
    00184
    00185         static tstring NetworkStatus;     /**< Network Status.
    00186                                                Values include are: "No Networks Detected",
    00187                                                                    "DNS Services Unavailable",
    00188                                                                    "Web Authentication Required",
    00189                                                                    "Proxy Authentication Required",
    00190                                                                    "Access Restricted",
    00191                                                                    "Access Unrestricted" */
    00192
    00193         static tstring DAPMessage;     /**< DAP message received from gateway.  Used for Quarantine
    00194                                             mode, etc. */
    00195
    00196         static tstring MUSHost;        /**< MUS Host delivered from secure gateway. */
    00197         static tstring MUSStatus;      /**< MUS Status: Enabled, Disabled. */
    00198
    00199         static tstring AdministrativeDomain;   /**<Administrative Domain Name:
    00200                                                    - domain name of the SG that the user connects to for the first time
    00201                                                    - "Admin Defined" if there are authorized SGs specified in
    00202                                                      the local policy file
    00203                                                    - "Not Applicable" otherwise. */
    00204
    00205         static tstring ProfileName;      /**< Active profile name. */
    00206
    00207         VPNStats();
    00208
    00209         virtual ~VPNStats();
    00210
    00211 };
    00212
    00213
    00214 #endif // _VPNSATS_