> # Configuring an LDAP Server

> ## Detailed Steps

> To configure an LDAP server and all of its options, follow these steps:

> 1. Expand Switches > Security > AAA, and then select LDAP.

> You see the LDAP configuration in the Information pane.

> 2. Click the Servers tab.

> You see any existing RADIUS servers.

> 3. Click Create Row to add a new LDAP server.

> You see the Create LDAP Server dialog box.

> 4. Select the switches that you want to assign as LDAP servers.
> 5. Assign an index number to identify the LDAP server.
> 6. Select the IP address type for the LDAP server.
> 7. Fill in the IP address or name for the LDAP server.
> 8. (Optional) Modify the authentication and accounting ports used by this LDAP server.
> 9. Select the appropriate key type for the LDAP server.
> 10. Select the TimeOut value in seconds. The valid range is 0 to 60 seconds.
> 11. Select the number of times the switch tries to connect to an LDAP server(s) before reverting to local authentication.
> 12. Enter the test idle time interval value in minutes. The valid range is 1 to 1440 minutes.
> 13. Enter the test user with the default password. The default username is test.
> 14. Click Create to save these changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.