> # FC

> # VSAN General

> Field | Description
> --- | ---
> Name | The name of the VSAN. Note that default value will be the string VSANxxxx where xxxx is value of vsanIndex expressed as 4 digits. For example, if vsanIndex is 23, the default value is VSAN0023.
> Mtu | The MTU of the VSAN. Normally, this is 2112.
> LoadBalancing | The type of load balancing used on this VSAN. srcdst - use source and destination ID for path selection srcdst 0xld - use source, destination, and exchange IDs
> InterOp | The interoperability mode of the local switch on this VSAN. standard interop-1 interop-2 interop-3
> AdminState | The state of this VSAN.
> OperState | The operational state of the VSAN.
> InOrderDelivery | The InorderDelivery guarantee flag of device. If true, then the inorder delivery is guaranteed. If false, it is not guaranteed.
> DomainId | Specifies an insistent domain ID.
> FICON | True if the VSAN is FICON-enabled.
> Network Latency | Network latency of this switch on this VSAN. This is the time interval after which the frames are dropped if they are not delivered in the order they were transmitted.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.