> # FICON Port Attributes

> Field | Description
> --- | ---
> TypeNumber | The type number for this FICON Director.
> SerialNumber | The sequence number assigned to this FICON Director during manufacturing.
> Tag | This is the identifier of the peer port. If the peer port's unit type is channel, then PortId will be the CHPID (Channel Path Identifier) of the channel path that contains this peer port. If the peer port is controlUnit, then PortId will be 0. If the peer port is fabric, then PortId will be port address of the interface on the peer switch.
> FcId | The fabric Id of the other side port (initiator /target). This will be filled only in the case of Fabric ports.
> Status | valid—If this information is current. old—If this information is cached. Click Clear Old Attributes to clear the cache.
> Name | The FICON port name.
> Manufacturer | The name of the company that manufactured this FICON Director.
> ModelNumber | The model number for this FICON Director.
> PlantOfMfg | The plant code that identifies the plant of manufacture of this FICON Director.
> UnitType | The peer type of the port that this port is communicating. ==Channel - host ==Control Unit - disk == Fabric - ISL
> Alert | Displays one of the following: bitErrThreshExceeded lossOfSignalOrSync nosReceived primitiveSeqTimeOut invalidPrimitiveSeq Click Clear to acknowledge and clear this alert.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.