> # Ethernet Interfaces iSCSI

> Field | Description
> --- | ---
> Description | An alias name for the interface as specified by a network manager.
> Speed | Operational speed.
> PhysAddress | The interface's WWN.
> Admin | The desired state of the interface.
> Oper | The current operational state of the interface.
> LastChange | When the interface entered its current operational state. If the current state was entered prior to the last re-initialization of the local network management subsystem, then this value contains a N/A value.
> PortVSAN | The VSAN that the interface belongs to.
> ForwardingMode | Use Store and Forward if the HBA has problems with passthrough.
> Initiator ID Mode | How the initiator is identified on this interface, either by its iSCSI name (name) or by its IP address (ipaddress).
> Enable | The intiator proxy mode for this interface. If true, then all the initiators coming on this interface would use the intiator configuration provided by this interface. The initiator configuration include port WWN and node WWN.
> Assignment | How the initiator proxy mode FC addresses are assigned. If auto, then the FC addresses are automatically assigned. If it is manual, then they have to be manually configured.
> Port WWN | The Port FC address used by the intiators on this interface when the intiator proxy mode is on.
> Node WWN | The Node FC address used by the initiators on this interface when the initiator proxy mode is on.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.