> # MTU Frame Size Configuration

> You can configure the interfaces on a switch to transfer large (or jumbo) frames on a port. The default IP maximum transmission unit (MTU) frame size is 1500 bytes for all Ethernet ports. By configuring jumbo frames on a port, the MTU size can be increased up to 9000 bytes.

> Note The minimum MTU size is 576 bytes.

> Tip MTU changes are disruptive, all FCIP links and iSCSI sessions flap when the software detects a change in the MTU size.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.