> # Configuring Retransmitting Intervals

> ## Detailed Steps

> To configure the FSPF retransmit time interval, follow these steps:

> 1. Expand Switches, expand FC Interfaces, and then select Physical.

> You see the interface configuration in the Information pane.

> 2. Click the FSPF tab.

> You see the FSPF interface configuration in the Information pane.

> 3. Double-click the ReTx Interval field and enter a value.
> 4. Click Apply Changes to save these changes, or click Undo Changes to discard any unsaved changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.